<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<text>rst</text>
<text>3.3v</text>
<text>gnd</text>
<text>en</text>
<text>bat</text>
<text>usb</text>
<text>sda</text>
<text>scl</text>
<text>mi</text>
<text>mo</text>
<text>sck</text>
<text>TinyPICO[+]</text>
<text>4</text>
<text>14</text>
<text>15</text>
<text>27</text>
<text>26</text>
<text>25</text>
<text>21</text>
<text>33</text>
<text>22</text>
<text>5</text>
<text>18</text>
<text>19</text>
<text>23</text>
<text>32</text>
<text>26</text>
<text>3V3</text>
<text>4</text>
<text>27</text>
<text>14</text>
<text>GND</text>
<text>21</text>
<text>RST</text>
<text>33</text>
<text>22</text>
<text>5</text>
<text>18</text>
<text>25</text>
<text>15</text>
<text>BAT</text>
<text>5V</text>
<text>19</text>
<text>23</text>
<text>GND</text>
<text>32</text>
<text>sck</text>
<text>mo</text>
<text>mi</text>
<text>scl</text>
<text>sda</text>
<text>rst</text>
<text>gnd</text>
<text>bat</text>
<text>usb</text>
<text>3.3v</text>
<text>gnd</text>
<text>tx</text>
<text>rx</text>
<text>0</text>
<text>TX</text>
<text>RX</text>
<text>tx</text>
<text>rx</text>
<text>TP[+]2FW
TinyPICO[+]
to
FeatherWing
Adapter</text>
<text>0</text>
<text>rst</text>
<text>3.3v</text>
<text>gnd</text>
<text>en</text>
<text>bat</text>
<text>usb</text>
<text>sda</text>
<text>scl</text>
<text>mi</text>
<text>mo</text>
<text>sck</text>
<text>tx</text>
<text>rx</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="FEATHERWING">
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_4.6X2.8MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.ck-components.com/media/1479/kmr2.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X11">
<description>&lt;h3&gt;Plated Through Hole -11 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X12">
<description>&lt;h3&gt;Plated Through Hole -12 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_4.6X2.8MM" value="MOMENTARY-SWITCH-SPST-SMD-4.6X2.8MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-13065"/>
<attribute name="VALUE"/>
</element>
<element name="MS2" library="microbuilder" package="FEATHERWING" value="FEATHERWING"/>
<element name="LEFT1" library="SparkFun-Connectors" package="1X11" value="">
<attribute name="VALUE"/>
</element>
<element name="RIGHT1" library="SparkFun-Connectors" package="1X12" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="MISO">
<contactref element="MS2" pad="13"/>
<contactref element="RIGHT1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="MS2" pad="12"/>
<contactref element="RIGHT1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="MS2" pad="11"/>
<contactref element="RIGHT1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="MS2" pad="4"/>
<contactref element="RIGHT1" pad="10"/>
<contactref element="LEFT1" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
</signal>
<signal name="EN">
<contactref element="MS2" pad="27"/>
</signal>
<signal name="SCL">
<contactref element="MS2" pad="18"/>
<contactref element="RIGHT1" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="MS2" pad="17"/>
<contactref element="RIGHT1" pad="6"/>
</signal>
<signal name="3.3V">
<contactref element="MS2" pad="2"/>
<contactref element="LEFT1" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="MS2" pad="1"/>
<contactref element="RIGHT1" pad="9"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="GPIO32">
<contactref element="MS2" pad="9"/>
<contactref element="RIGHT1" pad="7"/>
</signal>
<signal name="GPIO33">
<contactref element="MS2" pad="10"/>
<contactref element="RIGHT1" pad="8"/>
</signal>
<signal name="GPIO25">
<contactref element="MS2" pad="19"/>
<contactref element="LEFT1" pad="10"/>
</signal>
<signal name="GPIO26">
<contactref element="MS2" pad="20"/>
<contactref element="LEFT1" pad="9"/>
</signal>
<signal name="GPIO27">
<contactref element="MS2" pad="21"/>
<contactref element="LEFT1" pad="8"/>
</signal>
<signal name="GPIO14">
<contactref element="MS2" pad="23"/>
<contactref element="LEFT1" pad="6"/>
</signal>
<signal name="GPIO15">
<contactref element="MS2" pad="22"/>
<contactref element="LEFT1" pad="7"/>
</signal>
<signal name="GPIO4">
<contactref element="MS2" pad="24"/>
<contactref element="LEFT1" pad="5"/>
</signal>
<signal name="GPIO5">
<contactref element="MS2" pad="8"/>
<contactref element="RIGHT1" pad="4"/>
</signal>
<signal name="VBAT">
<contactref element="MS2" pad="28"/>
<contactref element="LEFT1" pad="1"/>
</signal>
<signal name="USB">
<contactref element="MS2" pad="26"/>
<contactref element="LEFT1" pad="3"/>
</signal>
<signal name="TX">
<contactref element="RIGHT1" pad="11"/>
<contactref element="MS2" pad="15"/>
</signal>
<signal name="RX">
<contactref element="RIGHT1" pad="12"/>
<contactref element="MS2" pad="14"/>
</signal>
<signal name="0">
<contactref element="LEFT1" pad="11"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
