<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="99.5" y1="69" x2="58" y2="69" width="0" layer="20"/>
<wire x1="58" y1="69" x2="56" y2="67" width="0" layer="20" curve="90"/>
<wire x1="58" y1="35" x2="118" y2="35" width="0" layer="20"/>
<wire x1="118" y1="35" x2="120" y2="37" width="0" layer="20" curve="90"/>
<wire x1="120" y1="37" x2="120" y2="43.5" width="0" layer="20"/>
<wire x1="58" y1="35" x2="56" y2="37" width="0" layer="20" curve="-90"/>
<wire x1="56" y1="37" x2="56" y2="67" width="0" layer="20"/>
<wire x1="120" y1="43.5" x2="118.5" y2="45" width="0" layer="20"/>
<wire x1="118.5" y1="45" x2="118.5" y2="54" width="0" layer="20"/>
<wire x1="118.5" y1="54" x2="120" y2="55.5" width="0" layer="20"/>
<wire x1="120" y1="55.5" x2="120" y2="67" width="0" layer="20"/>
<wire x1="120" y1="67" x2="118" y2="69" width="0" layer="20" curve="90"/>
<wire x1="118" y1="69" x2="109.5" y2="69" width="0" layer="20"/>
<wire x1="109.5" y1="69" x2="108.5" y2="67.5" width="0" layer="20"/>
<wire x1="108.5" y1="67.5" x2="100.5" y2="67.5" width="0" layer="20"/>
<wire x1="100.5" y1="67.5" x2="99.5" y2="69" width="0" layer="20"/>
<text>RST</text>
<text>BT0</text>
<text>SWD</text>
<text>diag</text>
<text>SD card</text>
<text>JAW 2017-08</text>
<text>www.AMIKETO.com</text>
<text>F7MINI Rev.0</text>
<text>use screw: M2.5,
No. 3, or 3/32"</text>
<text>64mm</text>
<text>34mm</text>
<text>Pb</text>
<text>L</text>
<text>Designed in Philly
Built by robots</text>
<text>2</text>
<text>3</text>
<text>1</text>
<text>LED</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>ARM Cortex</text>
<text>Much Fast!
Such Memories!</text>
<text>AMIKETO
F7 Mini</text>
<text>VIN
VUSB</text>
<text>3v3
GND</text>
<text>A0
A1</text>
<text>A2
A3</text>
<text>A4
A5</text>
<text>A6
A7</text>
<text>C4
C5</text>
<text>B0
B1</text>
<text>E7
E8</text>
<text>E9
E10</text>
<text>B13
E11</text>
<text>B15
B14</text>
<text>D9
D8</text>
<text>D11
D10</text>
<text>GND</text>
<text>3v3</text>
<text>i2CK
i2DA</text>
<text>CSd
GND</text>
<text>MOSI
DC</text>
<text>3v3
nRST</text>
<text>SCK</text>
<text>MISO</text>
<text>GND RST CK  IO  V</text>
<text>USB</text>
<text>JAW 2017-08</text>
<text>M7</text>
<text>STM32F7</text>
<text>*</text>
<text>*</text>
<text>5V MAX</text>
<text>3v3
MAX</text>
</plain>
<libraries>
<library name="jaw">
<packages>
<package name="SMD0402">
</package>
<package name="SMD0603">
</package>
<package name="MICROSD/EJECTOR">
</package>
<package name="HEADER-3X2-POGO">
</package>
<package name="KMR211">
</package>
<package name="SMD0805">
</package>
<package name="SMD0603D">
</package>
<package name="SOT-23-5">
</package>
<package name="USB-MICRO-B-192">
<description>USB micro-b connector SMT 0.65 mm pitch,
1.45mm from center to PCB edge,
Based on TE part number 1981568-1,
FCI - 10118192</description>
</package>
<package name="TQFP-100-14X14MM">
</package>
<package name="PUI-0540">
</package>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
<package name="SOT-23">
</package>
<package name="HEADER-5X1-SMD127-NOCR">
</package>
<package name="XTAL-32X15">
</package>
<package name="XTAL-32X25">
</package>
<package name="ROBOTMAN-LOGO">
</package>
<package name="SOT-23-6">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C8" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="jaw" package="SMD0402" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB1" library="jaw" package="USB-MICRO-B-192" value="USB-F-B-MICRO-B-192">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN1" library="jaw" package="MICROSD/EJECTOR" value="MICROSD-EJECT">
<attribute name="NAME"/>
</element>
<element name="CN5" library="adafruit" package="2X20" value="DO NOT PLACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CN3" library="jaw" package="HEADER-3X2-POGO" value="DO NOT PLACE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="jaw" package="KMR211" value="SWITCHKMR211">
<attribute name="NAME"/>
</element>
<element name="SW2" library="jaw" package="KMR211" value="SWITCHKMR211">
<attribute name="NAME"/>
</element>
<element name="C21" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="jaw" package="SMD0603" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jaw" package="SMD0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jaw" package="SMD0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="jaw" package="SMD0805" value="750mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="jaw" package="SMD0603D" value="white">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="jaw" package="SMD0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="jaw" package="SOT-23-5" value="3v3, 500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="jaw" package="SMD0402" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="jaw" package="SMD0402" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="jaw" package="SMD0603" value="10u 10V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="jaw" package="SMD0603D" value="green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="jaw" package="SMD0603D" value="orange">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="jaw" package="TQFP-100-14X14MM" value="STM32F7/100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="jaw" package="SMD0402" value="2u2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jaw" package="SMD0402" value="2u2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPKR1" library="jaw" package="PUI-0540" value="SPKR-PUI-0540"/>
<element name="D1" library="jaw" package="SOD-323" value="any">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="jaw" package="SOT-23" value="IRLML6344TRPBF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jaw" package="SMD0402" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="jaw" package="SMD0402" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="jaw" package="HEADER-5X1-SMD127-NOCR" value="HEADER-5X1"/>
<element name="X2" library="jaw" package="XTAL-32X15" value="32kHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="jaw" package="SMD0402" value="4p7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="jaw" package="SMD0402" value="4p7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="jaw" package="XTAL-32X25" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="jaw" package="SMD0402" value="7p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="jaw" package="SMD0402" value="7p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$3" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$4" library="jaw" package="ROBOTMAN-LOGO" value="ROBOTMAN-LOGO"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="FD1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FD2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="L1" library="jaw" package="SMD0603" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="jaw" package="SMD0603" value="4u7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="jaw" package="SMD0402" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="jaw" package="SOT-23-6" value="FDC6392S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="jaw" package="SMD0402" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="USB1" pad="P5"/>
<contactref element="CN3" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="C23" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="USB1" pad="P4"/>
<contactref element="CN1" pad="6"/>
<contactref element="CN1" pad="SHELL1"/>
<contactref element="C24" pad="1"/>
<contactref element="CN5" pad="8"/>
<contactref element="CN5" pad="12"/>
<contactref element="CN5" pad="38"/>
<contactref element="VR1" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="49"/>
<contactref element="U1" pad="99"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="74"/>
<contactref element="U1" pad="19"/>
<contactref element="Q1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="J1" pad="P$5"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="3"/>
<contactref element="CN1" pad="4"/>
<contactref element="C24" pad="2"/>
<contactref element="CN5" pad="1"/>
<contactref element="CN5" pad="11"/>
<contactref element="VR1" pad="5"/>
<contactref element="CN5" pad="37"/>
<contactref element="U1" pad="50"/>
<contactref element="U1" pad="75"/>
<contactref element="U1" pad="100"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="6"/>
<contactref element="SPKR1" pad="P1"/>
<contactref element="D1" pad="C"/>
<contactref element="J1" pad="P$1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="USBDP">
<contactref element="USB1" pad="P3"/>
<contactref element="U1" pad="71"/>
</signal>
<signal name="USBDM">
<contactref element="USB1" pad="P2"/>
<contactref element="U1" pad="70"/>
</signal>
<signal name="NRST">
<contactref element="CN3" pad="6"/>
<contactref element="C23" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="2"/>
<contactref element="CN5" pad="2"/>
<contactref element="U1" pad="14"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="VUSB">
<contactref element="CN3" pad="1"/>
<contactref element="USB1" pad="P1"/>
<contactref element="F1" pad="1"/>
<contactref element="CN5" pad="40"/>
</signal>
<signal name="TX">
<contactref element="CN3" pad="4"/>
<contactref element="U1" pad="68"/>
</signal>
<signal name="RX">
<contactref element="CN3" pad="3"/>
<contactref element="U1" pad="69"/>
</signal>
<signal name="N$13">
</signal>
<signal name="N$14">
</signal>
<signal name="SWDIO">
<contactref element="J1" pad="P$2"/>
<contactref element="U1" pad="72"/>
</signal>
<signal name="N$16">
<contactref element="R5" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="IOLED1">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="61"/>
</signal>
<signal name="SDIOD0">
<contactref element="CN1" pad="7"/>
<contactref element="U1" pad="65"/>
</signal>
<signal name="SDIOD1">
<contactref element="CN1" pad="8"/>
<contactref element="U1" pad="66"/>
</signal>
<signal name="SDIOD2">
<contactref element="CN1" pad="1"/>
<contactref element="U1" pad="78"/>
</signal>
<signal name="SDIOD3">
<contactref element="CN1" pad="2"/>
<contactref element="U1" pad="79"/>
</signal>
<signal name="SDIOCK">
<contactref element="CN1" pad="5"/>
<contactref element="U1" pad="80"/>
</signal>
<signal name="SDIOCM">
<contactref element="CN1" pad="3"/>
<contactref element="U1" pad="83"/>
</signal>
<signal name="CARDIO">
<contactref element="CN1" pad="CD1"/>
<contactref element="U1" pad="62"/>
</signal>
<signal name="SPIMISO">
<contactref element="CN5" pad="3"/>
<contactref element="U1" pad="43"/>
</signal>
<signal name="SPIMOSI">
<contactref element="CN5" pad="5"/>
<contactref element="U1" pad="44"/>
</signal>
<signal name="DPYCS">
<contactref element="CN5" pad="7"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="I2CCK">
<contactref element="CN5" pad="9"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="SPISCK">
<contactref element="CN5" pad="4"/>
<contactref element="U1" pad="42"/>
</signal>
<signal name="DPYDC">
<contactref element="CN5" pad="6"/>
<contactref element="U1" pad="45"/>
</signal>
<signal name="I2CDA">
<contactref element="CN5" pad="10"/>
<contactref element="U1" pad="47"/>
</signal>
<signal name="IOA1">
<contactref element="CN5" pad="36"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="IOA0">
<contactref element="CN5" pad="35"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="IOA3">
<contactref element="CN5" pad="34"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="IOA2">
<contactref element="CN5" pad="33"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="IOLED2">
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="60"/>
</signal>
<signal name="IOLED3">
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="59"/>
</signal>
<signal name="VSYS">
<contactref element="VR1" pad="3"/>
<contactref element="C25" pad="1"/>
<contactref element="VR1" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q2" pad="6"/>
</signal>
<signal name="VIN">
<contactref element="CN5" pad="39"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="R8" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="73"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="48"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="12"/>
<contactref element="X1" pad="1"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="BOOT0">
<contactref element="U1" pad="94"/>
<contactref element="SW2" pad="4"/>
<contactref element="SW2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="CN3" pad="5"/>
<contactref element="U1" pad="95"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="3"/>
<contactref element="SPKR1" pad="P2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="SWDCK">
<contactref element="J1" pad="P$3"/>
<contactref element="U1" pad="76"/>
</signal>
<signal name="N$8">
<contactref element="X2" pad="P$1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="X2" pad="P$2"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="13"/>
<contactref element="X1" pad="3"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="PZO">
<contactref element="U1" pad="96"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="IOD8">
<contactref element="U1" pad="55"/>
<contactref element="CN5" pad="16"/>
</signal>
<signal name="IOD9">
<contactref element="U1" pad="56"/>
<contactref element="CN5" pad="15"/>
</signal>
<signal name="IOD10">
<contactref element="U1" pad="57"/>
<contactref element="CN5" pad="14"/>
</signal>
<signal name="IOD11">
<contactref element="U1" pad="58"/>
<contactref element="CN5" pad="13"/>
</signal>
<signal name="IOB13">
<contactref element="U1" pad="52"/>
<contactref element="CN5" pad="19"/>
</signal>
<signal name="IOB14">
<contactref element="U1" pad="53"/>
<contactref element="CN5" pad="18"/>
</signal>
<signal name="IOB15">
<contactref element="U1" pad="54"/>
<contactref element="CN5" pad="17"/>
</signal>
<signal name="IOE11">
<contactref element="CN5" pad="20"/>
<contactref element="U1" pad="41"/>
</signal>
<signal name="IOE8">
<contactref element="U1" pad="38"/>
<contactref element="CN5" pad="24"/>
</signal>
<signal name="IOE9">
<contactref element="U1" pad="39"/>
<contactref element="CN5" pad="21"/>
</signal>
<signal name="IOE10">
<contactref element="U1" pad="40"/>
<contactref element="CN5" pad="22"/>
</signal>
<signal name="IOE7">
<contactref element="U1" pad="37"/>
<contactref element="CN5" pad="23"/>
</signal>
<signal name="IOB0">
<contactref element="U1" pad="34"/>
<contactref element="CN5" pad="25"/>
</signal>
<signal name="IOB1">
<contactref element="U1" pad="35"/>
<contactref element="CN5" pad="26"/>
</signal>
<signal name="IOC4">
<contactref element="U1" pad="32"/>
<contactref element="CN5" pad="27"/>
</signal>
<signal name="IOC5">
<contactref element="U1" pad="33"/>
<contactref element="CN5" pad="28"/>
</signal>
<signal name="IOA4">
<contactref element="U1" pad="28"/>
<contactref element="CN5" pad="31"/>
</signal>
<signal name="IOA5">
<contactref element="U1" pad="29"/>
<contactref element="CN5" pad="32"/>
</signal>
<signal name="IOA6">
<contactref element="U1" pad="30"/>
<contactref element="CN5" pad="29"/>
</signal>
<signal name="IOA7">
<contactref element="U1" pad="31"/>
<contactref element="CN5" pad="30"/>
</signal>
<signal name="VCCA">
<contactref element="L1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="VIN1">
<contactref element="Q2" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="Q2" pad="3"/>
<contactref element="F1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
