<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.1">
<drawing>
<board>
<plain>
<wire x1="0.0254" y1="47.5996" x2="0.0254" y2="3.2004" width="0" layer="20" locked="yes"/>
<wire x1="0.0254" y1="3.2004" x2="3.2004" y2="0.0254" width="0" layer="20" curve="90" locked="yes"/>
<wire x1="3.2004" y1="0.0254" x2="72.9996" y2="0.0254" width="0" layer="20" locked="yes"/>
<wire x1="72.9996" y1="0.0254" x2="76.1746" y2="3.2004" width="0" layer="20" curve="90" locked="yes"/>
<wire x1="76.1746" y1="3.2004" x2="76.1746" y2="47.5996" width="0" layer="20" locked="yes"/>
<wire x1="76.1746" y1="47.5996" x2="72.9996" y2="50.7746" width="0" layer="20" curve="90" locked="yes"/>
<wire x1="72.9996" y1="50.7746" x2="3.2004" y2="50.7746" width="0" layer="20" locked="yes"/>
<wire x1="3.2004" y1="50.7746" x2="0.0254" y2="47.5996" width="0" layer="20" curve="90" locked="yes"/>
<text>RA0</text>
<text>RB1</text>
<text>5
4
3
2
1
0
PORTB</text>
<text>7
6
5
4
3
2
1
0
PORTC</text>
<text>0
1
2
3
4
5
6
7
PORTA</text>
<text>VDD
GND</text>
<text>VDD
GND</text>
<text>GND</text>
<text>GND</text>
<text>VDD</text>
<text>v1.a 2018</text>
<text>GND</text>
<text>PIC-APRS</text>
<text>TX</text>
</plain>
<libraries>
<library name="library1">
<packages>
<package name="AA-BAT">
<description>AA Battery Clips
Memory Protection Devices BK-92</description>
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CONN4-SMD">
</package>
<package name="CONN8-SMD">
</package>
<package name="TY-NRS5030">
</package>
<package name="2WIRE-18AWG">
</package>
<package name="28SOIC-7.5MM">
</package>
<package name="8MSOP">
</package>
<package name="APRS-RF1">
</package>
<package name="UBLOX-GPS">
</package>
<package name="SOT23-3">
</package>
<package name="CAP-6.3MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint with Long Pads&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B2" library="library1" package="AA-BAT" value=""/>
<element name="B1" library="library1" package="AA-BAT" value=""/>
<element name="C1" library="library1" package="0805" value="1uF"/>
<element name="C8" library="library1" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="library1" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="library1" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="library1" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="library1" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="library1" package="0805" value="10uF">
<attribute name="NAME"/>
</element>
<element name="H2" library="library1" package="CONN4-SMD" value="HEADER-1X4-SMD"/>
<element name="H1" library="library1" package="CONN8-SMD" value="HEADER-1X8-SMD"/>
<element name="J4" library="SparkFun-Connectors" package="1X06_LOCK_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="L1" library="library1" package="TY-NRS5030" value="4.7 uH"/>
<element name="R1" library="library1" package="0805" value="10k"/>
<element name="R6" library="library1" package="0805" value="10k"/>
<element name="SW1" library="library1" package="2WIRE-18AWG" value="SPST-SW-EXT"/>
<element name="U1" library="library1" package="28SOIC-7.5MM" value="PIC16F1716-SOIC">
<attribute name="NAME"/>
</element>
<element name="U2" library="library1" package="8MSOP" value="MCP1642B-ADJ">
<attribute name="NAME"/>
</element>
<element name="U$1" library="library1" package="APRS-RF1" value=""/>
<element name="U$2" library="library1" package="UBLOX-GPS" value=""/>
<element name="D1" library="library1" package="0805" value="PWR">
<attribute name="VALUE"/>
</element>
<element name="D2" library="library1" package="0805" value="GPS">
<attribute name="VALUE"/>
</element>
<element name="D3" library="library1" package="0805" value="RF">
<attribute name="VALUE"/>
</element>
<element name="R2" library="library1" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R3" library="library1" package="0805" value="RB2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="library1" package="0805" value="RA3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="library1" package="0805" value="ACT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="library1" package="0805" value="RB0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="library1" package="SOT23-3" value="MCP9700A-SOT23-3">
<attribute name="NAME"/>
</element>
<element name="U4" library="library1" package="SOT23-3" value="MCP9700A-SOT23-3">
<attribute name="NAME"/>
</element>
<element name="C11" library="library1" package="0603" value="1uF">
<attribute name="NAME"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
</element>
<element name="C12" library="library1" package="0603" value="1uF"/>
<element name="C5" library="library1" package="CAP-6.3MM" value="22uF"/>
<element name="C9" library="library1" package="0805" value="1uF"/>
<element name="C10" library="library1" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="B2" pad="P1" route="any" routetag="B.+"/>
<contactref element="B2" pad="P2" route="any" routetag="B.+"/>
<contactref element="B1" pad="N1" route="any" routetag="B.-"/>
<contactref element="B1" pad="N2" route="any" routetag="B.-"/>
</signal>
<signal name="GND">
<contactref element="B2" pad="N1" route="any" routetag="B.-"/>
<contactref element="B2" pad="N2" route="any" routetag="B.-"/>
<contactref element="H1" pad="1"/>
<contactref element="H2" pad="3"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="19"/>
<contactref element="C1" pad="2"/>
<contactref element="J4" pad="3"/>
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="6"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="D4" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U4" pad="3"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="C5" pad="-"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="J6" pad="2"/>
<contactref element="J6" pad="3"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="V+">
<contactref element="SW1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="L1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="C5" pad="+"/>
</signal>
<signal name="RF_TXD">
<contactref element="H2" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="RF_EN">
<contactref element="H2" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="GPS_TP">
<contactref element="H1" pad="3"/>
</signal>
<signal name="GPS_EN">
<contactref element="H1" pad="4"/>
<contactref element="U1" pad="24"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="GPS_RX">
<contactref element="H1" pad="5"/>
<contactref element="U1" pad="25"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="GPS_TX">
<contactref element="H1" pad="6"/>
<contactref element="U1" pad="26"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="GPS_SCL">
<contactref element="H1" pad="7"/>
</signal>
<signal name="GPS_SDA">
<contactref element="H1" pad="8"/>
</signal>
<signal name="VDD">
<contactref element="U1" pad="20"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="J4" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="R6" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="H2" pad="2"/>
<contactref element="H1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="!MCLR">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="ICSP_DAT">
<contactref element="J4" pad="4"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="ICSP_CLK">
<contactref element="J4" pad="5"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="SW">
<contactref element="U2" pad="5"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="18"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="17"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="16"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="15"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="14"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="13"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="12"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$9">
<contactref element="U1" pad="11"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="GPS_LED">
<contactref element="U1" pad="23"/>
<contactref element="R3" pad="2"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="ACT_LED">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="MAIN_TEMP">
<contactref element="U3" pad="2"/>
<contactref element="U1" pad="22"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="9"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="10"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="EXT_TMP">
<contactref element="U1" pad="2"/>
<contactref element="J1" pad="8"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="PG">
<contactref element="R6" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="VBAT">
<contactref element="SW1" pad="2"/>
<contactref element="B1" pad="P1" route="any" routetag="B.+"/>
<contactref element="B1" pad="P2" route="any" routetag="B.+"/>
</signal>
<signal name="N$10">
<contactref element="R2" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R3" pad="1"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R4" pad="1"/>
<contactref element="D3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R5" pad="1"/>
<contactref element="D4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
