(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 526)
    (no_connects 0)
    (area 50.609499 50.609499 167.830501 205.930501)
    (thickness 1.6002)
    (drawings 25)
    (tracks 2605)
    (zones 0)
    (modules 61)
    (nets 84)
  )
  (page User 431.8 279.4)
  (title_block
    (date "18 mar 2013")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.37846)
    (user_trace_width 1.01346)
    (user_trace_width 1.905)
    (trace_clearance 0.254)
    (zone_clearance 0.37846)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.381)
    (edge_width 0.381)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.254)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 2.60096 2.60096)
    (pad_drill 1.6002)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber))
  )
  (net 0 "")
  (net 1 /-12V)
  (net 2 /-5V)
  (net 3 /-5V_ATX)
  (net 4 /12V)
  (net 5 /A0)
  (net 6 /A1)
  (net 7 /A10)
  (net 8 /A11)
  (net 9 /A12)
  (net 10 /A13)
  (net 11 /A14)
  (net 12 /A15)
  (net 13 /A16)
  (net 14 /A17)
  (net 15 /A18)
  (net 16 /A19)
  (net 17 /A2)
  (net 18 /A3)
  (net 19 /A4)
  (net 20 /A5)
  (net 21 /A6)
  (net 22 /A7)
  (net 23 /A8)
  (net 24 /A9)
  (net 25 /AEN)
  (net 26 /ALE)
  (net 27 /CLK)
  (net 28 /D0)
  (net 29 /D1)
  (net 30 /D2)
  (net 31 /D3)
  (net 32 /D4)
  (net 33 /D5)
  (net 34 /D6)
  (net 35 /D7)
  (net 36 /DRQ1)
  (net 37 /DRQ2)
  (net 38 /DRQ3)
  (net 39 /IRQ3)
  (net 40 /IRQ4)
  (net 41 /IRQ5)
  (net 42 /IRQ6)
  (net 43 /IRQ7)
  (net 44 /OSC)
  (net 45 /TC)
  (net 46 /~0WS)
  (net 47 /~DACK0)
  (net 48 /~DACK1)
  (net 49 /~DACK2)
  (net 50 /~DACK3)
  (net 51 /~IOCHK)
  (net 52 /~IOR)
  (net 53 /~IOW)
  (net 54 /~MEMR)
  (net 55 /~MEMW)
  (net 56 /~PS_ON)
  (net 57 GND)
  (net 58 VCC)
  (net 59 /RSTDRV)
  (net 60 /+5V)
  (net 61 /IRQ2)
  (net 62 /IORDY)
  (net 63 "Net-(D1-Pad2)")
  (net 64 "Net-(D2-Pad2)")
  (net 65 "Net-(D2-Pad1)")
  (net 66 "Net-(P1-Pad2)")
  (net 67 "Net-(P2-Pad2)")
  (net 68 "Net-(P3-Pad1)")
  (net 69 "Net-(R3-Pad2)")
  (net 70 "Net-(R5-Pad2)")
  (net 71 "Net-(U1-Pad12)")
  (net 72 "Net-(U1-Pad10)")
  (net 73 "Net-(U1-Pad11)")
  (net 74 "Net-(U2-Pad4)")
  (net 75 "Net-(RR5-Pad2)")
  (net 76 "Net-(C20-Pad1)")
  (net 77 "Net-(C19-Pad1)")
  (net 78 "Net-(U2-Pad8)")
  (net 79 "Net-(U2-Pad10)")
  (net 80 "Net-(U2-Pad12)")
  (net 81 "Net-(P1-Pad8)")
  (net 82 "Net-(P1-Pad11)")
  (net 83 "Net-(P1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.37846)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AEN)
    (add_net /ALE)
    (add_net /CLK)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DRQ1)
    (add_net /DRQ2)
    (add_net /DRQ3)
    (add_net /IORDY)
    (add_net /IRQ2)
    (add_net /IRQ3)
    (add_net /IRQ4)
    (add_net /IRQ5)
    (add_net /IRQ6)
    (add_net /IRQ7)
    (add_net /OSC)
    (add_net /RSTDRV)
    (add_net /TC)
    (add_net /~0WS)
    (add_net /~DACK0)
    (add_net /~DACK1)
    (add_net /~DACK2)
    (add_net /~DACK3)
    (add_net /~IOCHK)
    (add_net /~IOR)
    (add_net /~IOW)
    (add_net /~MEMR)
    (add_net /~MEMW)
    (add_net /~PS_ON)
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(RR5-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad8)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.50546)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /+5V)
    (add_net /-12V)
    (add_net /-5V)
    (add_net /-5V_ATX)
    (add_net /12V)
    (add_net GND)
    (add_net VCC)
  )
  (module my_components:IC_DIP14_300 (layer Front) (tedit 5A2F1791)
    (at 124.46 67.31)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U1 (at -10.8585 3.81 90) (layer F.SilkS))
    (fp_text value 74HCT74 (at -10.8585 -1.27 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(R5-Pad2)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(R3-Pad2)"))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(D2-Pad2)"))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(R5-Pad2)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(U1-Pad12)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /~PS_ON))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Edge_ISA8 (layer Front) (tedit 5A2F1DCC)
    (at 114.3 77.47 180)
    (descr "ISA8 Edge Connector")
    (tags "ISA ISA8 EDGE CONN")
    (fp_text reference BUS1 (at 43.815 0.635 270) (layer F.SilkS))
    (fp_text value BUSPC_DEV (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RSTDRV))
    (pad 3 thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 4 thru_hole circle (at 30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /IRQ2))
    (pad 5 thru_hole circle (at 27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (pad 6 thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /DRQ2))
    (pad 7 thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 8 thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~0WS))
    (pad 9 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 10 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 11 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /~MEMW))
    (pad 12 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~MEMR))
    (pad 13 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~IOW))
    (pad 14 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~IOR))
    (pad 15 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~DACK3))
    (pad 16 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /DRQ3))
    (pad 17 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~DACK1))
    (pad 18 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /DRQ1))
    (pad 19 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~DACK0))
    (pad 20 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CLK))
    (pad 21 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /IRQ7))
    (pad 22 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /IRQ6))
    (pad 23 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /IRQ5))
    (pad 24 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /IRQ4))
    (pad 25 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /IRQ3))
    (pad 26 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~DACK2))
    (pad 27 thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TC))
    (pad 28 thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ALE))
    (pad 29 thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 30 thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /OSC))
    (pad 31 thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 32 thru_hole circle (at 38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~IOCHK))
    (pad 33 thru_hole circle (at 35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D7))
    (pad 34 thru_hole circle (at 33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D6))
    (pad 35 thru_hole circle (at 30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D5))
    (pad 36 thru_hole circle (at 27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D4))
    (pad 37 thru_hole circle (at 25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D3))
    (pad 38 thru_hole circle (at 22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D2))
    (pad 39 thru_hole circle (at 20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D1))
    (pad 40 thru_hole circle (at 17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D0))
    (pad 41 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /IORDY))
    (pad 42 thru_hole circle (at 12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AEN))
    (pad 43 thru_hole circle (at 10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A19))
    (pad 44 thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A18))
    (pad 45 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A17))
    (pad 46 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A16))
    (pad 47 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A15))
    (pad 48 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A14))
    (pad 49 thru_hole circle (at -5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A13))
    (pad 50 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A12))
    (pad 51 thru_hole circle (at -10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A11))
    (pad 52 thru_hole circle (at -12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A10))
    (pad 53 thru_hole circle (at -15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A9))
    (pad 54 thru_hole circle (at -17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 55 thru_hole circle (at -20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
    (pad 56 thru_hole circle (at -22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 57 thru_hole circle (at -25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A5))
    (pad 58 thru_hole circle (at -27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A4))
    (pad 59 thru_hole circle (at -30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A3))
    (pad 60 thru_hole circle (at -33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 61 thru_hole circle (at -35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (pad 62 thru_hole circle (at -38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
  )
  (module my_components:Conn_Edge_ISA8 (layer Front) (tedit 5A2F1DC1)
    (at 114.3 97.79 180)
    (descr "ISA8 Edge Connector")
    (tags "ISA ISA8 EDGE CONN")
    (fp_text reference BUS2 (at 43.815 0 270) (layer F.SilkS))
    (fp_text value BUSPC_HOST (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RSTDRV))
    (pad 3 thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 4 thru_hole circle (at 30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /IRQ2))
    (pad 5 thru_hole circle (at 27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (pad 6 thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /DRQ2))
    (pad 7 thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 8 thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~0WS))
    (pad 9 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 10 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 11 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /~MEMW))
    (pad 12 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~MEMR))
    (pad 13 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~IOW))
    (pad 14 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~IOR))
    (pad 15 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~DACK3))
    (pad 16 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /DRQ3))
    (pad 17 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~DACK1))
    (pad 18 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /DRQ1))
    (pad 19 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~DACK0))
    (pad 20 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CLK))
    (pad 21 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /IRQ7))
    (pad 22 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /IRQ6))
    (pad 23 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /IRQ5))
    (pad 24 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /IRQ4))
    (pad 25 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /IRQ3))
    (pad 26 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~DACK2))
    (pad 27 thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TC))
    (pad 28 thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ALE))
    (pad 29 thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 30 thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /OSC))
    (pad 31 thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 32 thru_hole circle (at 38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~IOCHK))
    (pad 33 thru_hole circle (at 35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D7))
    (pad 34 thru_hole circle (at 33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D6))
    (pad 35 thru_hole circle (at 30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D5))
    (pad 36 thru_hole circle (at 27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D4))
    (pad 37 thru_hole circle (at 25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D3))
    (pad 38 thru_hole circle (at 22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D2))
    (pad 39 thru_hole circle (at 20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D1))
    (pad 40 thru_hole circle (at 17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D0))
    (pad 41 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /IORDY))
    (pad 42 thru_hole circle (at 12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AEN))
    (pad 43 thru_hole circle (at 10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A19))
    (pad 44 thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A18))
    (pad 45 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A17))
    (pad 46 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A16))
    (pad 47 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A15))
    (pad 48 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A14))
    (pad 49 thru_hole circle (at -5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A13))
    (pad 50 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A12))
    (pad 51 thru_hole circle (at -10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A11))
    (pad 52 thru_hole circle (at -12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A10))
    (pad 53 thru_hole circle (at -15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A9))
    (pad 54 thru_hole circle (at -17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 55 thru_hole circle (at -20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
    (pad 56 thru_hole circle (at -22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 57 thru_hole circle (at -25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A5))
    (pad 58 thru_hole circle (at -27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A4))
    (pad 59 thru_hole circle (at -30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A3))
    (pad 60 thru_hole circle (at -33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 61 thru_hole circle (at -35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (pad 62 thru_hole circle (at -38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
  )
  (module my_components:Conn_Edge_ISA8 (layer Front) (tedit 5A2F1D1F)
    (at 114.3 118.11 180)
    (descr "ISA8 Edge Connector")
    (tags "ISA ISA8 EDGE CONN")
    (fp_text reference BUS3 (at 43.815 0 270) (layer F.SilkS))
    (fp_text value BUSPC_HOST (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RSTDRV))
    (pad 3 thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 4 thru_hole circle (at 30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /IRQ2))
    (pad 5 thru_hole circle (at 27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (pad 6 thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /DRQ2))
    (pad 7 thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 8 thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~0WS))
    (pad 9 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 10 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 11 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /~MEMW))
    (pad 12 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~MEMR))
    (pad 13 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~IOW))
    (pad 14 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~IOR))
    (pad 15 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~DACK3))
    (pad 16 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /DRQ3))
    (pad 17 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~DACK1))
    (pad 18 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /DRQ1))
    (pad 19 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~DACK0))
    (pad 20 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CLK))
    (pad 21 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /IRQ7))
    (pad 22 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /IRQ6))
    (pad 23 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /IRQ5))
    (pad 24 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /IRQ4))
    (pad 25 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /IRQ3))
    (pad 26 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~DACK2))
    (pad 27 thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TC))
    (pad 28 thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ALE))
    (pad 29 thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 30 thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /OSC))
    (pad 31 thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 32 thru_hole circle (at 38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~IOCHK))
    (pad 33 thru_hole circle (at 35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D7))
    (pad 34 thru_hole circle (at 33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D6))
    (pad 35 thru_hole circle (at 30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D5))
    (pad 36 thru_hole circle (at 27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D4))
    (pad 37 thru_hole circle (at 25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D3))
    (pad 38 thru_hole circle (at 22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D2))
    (pad 39 thru_hole circle (at 20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D1))
    (pad 40 thru_hole circle (at 17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D0))
    (pad 41 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /IORDY))
    (pad 42 thru_hole circle (at 12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AEN))
    (pad 43 thru_hole circle (at 10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A19))
    (pad 44 thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A18))
    (pad 45 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A17))
    (pad 46 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A16))
    (pad 47 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A15))
    (pad 48 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A14))
    (pad 49 thru_hole circle (at -5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A13))
    (pad 50 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A12))
    (pad 51 thru_hole circle (at -10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A11))
    (pad 52 thru_hole circle (at -12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A10))
    (pad 53 thru_hole circle (at -15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A9))
    (pad 54 thru_hole circle (at -17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 55 thru_hole circle (at -20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
    (pad 56 thru_hole circle (at -22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 57 thru_hole circle (at -25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A5))
    (pad 58 thru_hole circle (at -27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A4))
    (pad 59 thru_hole circle (at -30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A3))
    (pad 60 thru_hole circle (at -33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 61 thru_hole circle (at -35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (pad 62 thru_hole circle (at -38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
  )
  (module my_components:Conn_Edge_ISA8 (layer Front) (tedit 5A2F1D15)
    (at 114.3 138.43 180)
    (descr "ISA8 Edge Connector")
    (tags "ISA ISA8 EDGE CONN")
    (fp_text reference BUS4 (at 43.815 0 270) (layer F.SilkS))
    (fp_text value BUSPC_HOST (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RSTDRV))
    (pad 3 thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 4 thru_hole circle (at 30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /IRQ2))
    (pad 5 thru_hole circle (at 27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (pad 6 thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /DRQ2))
    (pad 7 thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 8 thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~0WS))
    (pad 9 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 10 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 11 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /~MEMW))
    (pad 12 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~MEMR))
    (pad 13 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~IOW))
    (pad 14 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~IOR))
    (pad 15 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~DACK3))
    (pad 16 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /DRQ3))
    (pad 17 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~DACK1))
    (pad 18 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /DRQ1))
    (pad 19 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~DACK0))
    (pad 20 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CLK))
    (pad 21 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /IRQ7))
    (pad 22 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /IRQ6))
    (pad 23 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /IRQ5))
    (pad 24 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /IRQ4))
    (pad 25 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /IRQ3))
    (pad 26 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~DACK2))
    (pad 27 thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TC))
    (pad 28 thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ALE))
    (pad 29 thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 30 thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /OSC))
    (pad 31 thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 32 thru_hole circle (at 38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~IOCHK))
    (pad 33 thru_hole circle (at 35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D7))
    (pad 34 thru_hole circle (at 33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D6))
    (pad 35 thru_hole circle (at 30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D5))
    (pad 36 thru_hole circle (at 27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D4))
    (pad 37 thru_hole circle (at 25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D3))
    (pad 38 thru_hole circle (at 22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D2))
    (pad 39 thru_hole circle (at 20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D1))
    (pad 40 thru_hole circle (at 17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D0))
    (pad 41 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /IORDY))
    (pad 42 thru_hole circle (at 12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AEN))
    (pad 43 thru_hole circle (at 10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A19))
    (pad 44 thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A18))
    (pad 45 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A17))
    (pad 46 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A16))
    (pad 47 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A15))
    (pad 48 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A14))
    (pad 49 thru_hole circle (at -5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A13))
    (pad 50 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A12))
    (pad 51 thru_hole circle (at -10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A11))
    (pad 52 thru_hole circle (at -12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A10))
    (pad 53 thru_hole circle (at -15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A9))
    (pad 54 thru_hole circle (at -17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 55 thru_hole circle (at -20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
    (pad 56 thru_hole circle (at -22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 57 thru_hole circle (at -25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A5))
    (pad 58 thru_hole circle (at -27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A4))
    (pad 59 thru_hole circle (at -30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A3))
    (pad 60 thru_hole circle (at -33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 61 thru_hole circle (at -35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (pad 62 thru_hole circle (at -38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
  )
  (module my_components:Conn_Edge_ISA8 (layer Front) (tedit 5A2F1D0B)
    (at 114.3 158.75 180)
    (descr "ISA8 Edge Connector")
    (tags "ISA ISA8 EDGE CONN")
    (fp_text reference BUS5 (at 43.815 0 270) (layer F.SilkS))
    (fp_text value BUSPC_HOST (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RSTDRV))
    (pad 3 thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 4 thru_hole circle (at 30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /IRQ2))
    (pad 5 thru_hole circle (at 27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (pad 6 thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /DRQ2))
    (pad 7 thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 8 thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~0WS))
    (pad 9 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 10 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 11 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /~MEMW))
    (pad 12 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~MEMR))
    (pad 13 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~IOW))
    (pad 14 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~IOR))
    (pad 15 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~DACK3))
    (pad 16 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /DRQ3))
    (pad 17 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~DACK1))
    (pad 18 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /DRQ1))
    (pad 19 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~DACK0))
    (pad 20 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CLK))
    (pad 21 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /IRQ7))
    (pad 22 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /IRQ6))
    (pad 23 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /IRQ5))
    (pad 24 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /IRQ4))
    (pad 25 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /IRQ3))
    (pad 26 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~DACK2))
    (pad 27 thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TC))
    (pad 28 thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ALE))
    (pad 29 thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 30 thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /OSC))
    (pad 31 thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 32 thru_hole circle (at 38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~IOCHK))
    (pad 33 thru_hole circle (at 35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D7))
    (pad 34 thru_hole circle (at 33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D6))
    (pad 35 thru_hole circle (at 30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D5))
    (pad 36 thru_hole circle (at 27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D4))
    (pad 37 thru_hole circle (at 25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D3))
    (pad 38 thru_hole circle (at 22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D2))
    (pad 39 thru_hole circle (at 20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D1))
    (pad 40 thru_hole circle (at 17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D0))
    (pad 41 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /IORDY))
    (pad 42 thru_hole circle (at 12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AEN))
    (pad 43 thru_hole circle (at 10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A19))
    (pad 44 thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A18))
    (pad 45 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A17))
    (pad 46 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A16))
    (pad 47 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A15))
    (pad 48 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A14))
    (pad 49 thru_hole circle (at -5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A13))
    (pad 50 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A12))
    (pad 51 thru_hole circle (at -10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A11))
    (pad 52 thru_hole circle (at -12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A10))
    (pad 53 thru_hole circle (at -15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A9))
    (pad 54 thru_hole circle (at -17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 55 thru_hole circle (at -20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
    (pad 56 thru_hole circle (at -22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 57 thru_hole circle (at -25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A5))
    (pad 58 thru_hole circle (at -27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A4))
    (pad 59 thru_hole circle (at -30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A3))
    (pad 60 thru_hole circle (at -33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 61 thru_hole circle (at -35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (pad 62 thru_hole circle (at -38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
  )
  (module my_components:Conn_Edge_ISA8 (layer Front) (tedit 5A2F1CFF)
    (at 114.3 179.07 180)
    (descr "ISA8 Edge Connector")
    (tags "ISA ISA8 EDGE CONN")
    (fp_text reference BUS6 (at 43.815 0 270) (layer F.SilkS))
    (fp_text value BUSPC_HOST (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RSTDRV))
    (pad 3 thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 4 thru_hole circle (at 30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /IRQ2))
    (pad 5 thru_hole circle (at 27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (pad 6 thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /DRQ2))
    (pad 7 thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 8 thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~0WS))
    (pad 9 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 10 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 11 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /~MEMW))
    (pad 12 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~MEMR))
    (pad 13 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~IOW))
    (pad 14 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~IOR))
    (pad 15 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~DACK3))
    (pad 16 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /DRQ3))
    (pad 17 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~DACK1))
    (pad 18 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /DRQ1))
    (pad 19 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~DACK0))
    (pad 20 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CLK))
    (pad 21 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /IRQ7))
    (pad 22 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /IRQ6))
    (pad 23 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /IRQ5))
    (pad 24 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /IRQ4))
    (pad 25 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /IRQ3))
    (pad 26 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~DACK2))
    (pad 27 thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TC))
    (pad 28 thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ALE))
    (pad 29 thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 30 thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /OSC))
    (pad 31 thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 32 thru_hole circle (at 38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~IOCHK))
    (pad 33 thru_hole circle (at 35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D7))
    (pad 34 thru_hole circle (at 33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D6))
    (pad 35 thru_hole circle (at 30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D5))
    (pad 36 thru_hole circle (at 27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D4))
    (pad 37 thru_hole circle (at 25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D3))
    (pad 38 thru_hole circle (at 22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D2))
    (pad 39 thru_hole circle (at 20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D1))
    (pad 40 thru_hole circle (at 17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D0))
    (pad 41 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /IORDY))
    (pad 42 thru_hole circle (at 12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AEN))
    (pad 43 thru_hole circle (at 10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A19))
    (pad 44 thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A18))
    (pad 45 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A17))
    (pad 46 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A16))
    (pad 47 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A15))
    (pad 48 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A14))
    (pad 49 thru_hole circle (at -5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A13))
    (pad 50 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A12))
    (pad 51 thru_hole circle (at -10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A11))
    (pad 52 thru_hole circle (at -12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A10))
    (pad 53 thru_hole circle (at -15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A9))
    (pad 54 thru_hole circle (at -17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 55 thru_hole circle (at -20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
    (pad 56 thru_hole circle (at -22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 57 thru_hole circle (at -25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A5))
    (pad 58 thru_hole circle (at -27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A4))
    (pad 59 thru_hole circle (at -30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A3))
    (pad 60 thru_hole circle (at -33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 61 thru_hole circle (at -35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (pad 62 thru_hole circle (at -38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5A2F27C8)
    (at 76.2 68.58)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C1 (at -0.3175 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.556) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 149.86 87.3125)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C2 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 83.82 107.95)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C3 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 149.86 107.95)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C4 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 83.82 148.59)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C5 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 149.86 148.59)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C6 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5A2F282E)
    (at 81.28 186.69)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C7 (at -5.715 -0.9525) (layer F.SilkS))
    (fp_text value 10uF (at -5.715 0.635) (layer F.SilkS))
    (fp_text user + (at -3.175 -1.905) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5A2F282B)
    (at 149.86 186.69)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C8 (at -5.715 -0.9525) (layer F.SilkS))
    (fp_text value 10uF (at -5.715 0.635) (layer F.SilkS))
    (fp_text user + (at -3.175 -1.905) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 99.06 87.63)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C9 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 99.06 128.27)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C10 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 99.06 168.91)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C11 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 91.44 107.95)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C13 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 91.44 148.59)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C14 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 83.82 87.63)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C15 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 83.82 128.27)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C16 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5298D611)
    (at 83.82 168.91)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C17 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5A3028F2)
    (at 106.68 68.58)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C18 (at 0 -3.7465) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.556) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5A2F27CD)
    (at 91.44 68.58)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C19 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.556) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5A2F27CF)
    (at 99.06 68.58)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C20 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 1uF (at -0.3175 3.556) (layer F.SilkS))
    (fp_text user + (at -3.175 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:LED_3mm (layer Front) (tedit 57E95C70)
    (at 156.21 55.88 180)
    (descr "LED 3mm, 100mil (2.54mm) lead spacing")
    (tags "LED 3mm T1")
    (fp_text reference D1 (at 0 -3.175 180) (layer F.SilkS))
    (fp_text value POWER (at 0 3.175 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:LED_3mm (layer Front) (tedit 57E95C70)
    (at 162.56 55.88 180)
    (descr "LED 3mm, 100mil (2.54mm) lead spacing")
    (tags "LED 3mm T1")
    (fp_text reference D2 (at 0 -3.175 180) (layer F.SilkS))
    (fp_text value ACTIVITY (at 0 3.175 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(D2-Pad1)"))
    (model discret/leds/led3_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Diode_762 (layer Front) (tedit 5A2F1C7D)
    (at 139.7 67.31 270)
    (descr "Diode, 7.62mm lead spacing")
    (tags "DIODE 7.62mm")
    (fp_text reference D3 (at -5.715 -1.905 270) (layer F.SilkS))
    (fp_text value 1N4148 (at -9.8425 -1.905 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(C20-Pad1)"))
    (pad 1 thru_hole rect (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Diode_762 (layer Front) (tedit 5A2F1C81)
    (at 142.24 67.31 270)
    (descr "Diode, 7.62mm lead spacing")
    (tags "DIODE 7.62mm")
    (fp_text reference D4 (at -5.715 -0.9525 270) (layer F.SilkS))
    (fp_text value 1N4148 (at -9.8425 -0.9525 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(C19-Pad1)"))
    (pad 1 thru_hole rect (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Hole_4mm (layer Front) (tedit 5298E8A8)
    (at 60.96 171.45 90)
    (descr "Mounting Hole, 4mm")
    (tags "HOLE 4MM")
    (fp_text reference HOLE1 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.00126 5.00126) (drill 4.0005) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
  )
  (module my_components:Hole_4mm (layer Front) (tedit 5298E8A8)
    (at 60.96 125.73 90)
    (descr "Mounting Hole, 4mm")
    (tags "HOLE 4MM")
    (fp_text reference HOLE2 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.00126 5.00126) (drill 4.0005) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
  )
  (module my_components:Hole_4mm (layer Front) (tedit 5298E8A8)
    (at 162.56 64.77 90)
    (descr "Mounting Hole, 4mm")
    (tags "HOLE 4MM")
    (fp_text reference HOLE3 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.00126 5.00126) (drill 4.0005) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
  )
  (module my_components:Hole_4mm (layer Front) (tedit 5298E8A8)
    (at 162.56 191.77 90)
    (descr "Mounting Hole, 4mm")
    (tags "HOLE 4MM")
    (fp_text reference HOLE4 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.00126 5.00126) (drill 4.0005) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
  )
  (module my_components:Hole_4mm (layer Front) (tedit 5298E8A8)
    (at 162.56 171.45 90)
    (descr "Mounting Hole, 4mm")
    (tags "HOLE 4MM")
    (fp_text reference HOLE5 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.00126 5.00126) (drill 4.0005) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
  )
  (module my_components:Hole_4mm (layer Front) (tedit 5298E8A8)
    (at 162.56 125.73 90)
    (descr "Mounting Hole, 4mm")
    (tags "HOLE 4MM")
    (fp_text reference HOLE6 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.00126 5.00126) (drill 4.0005) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
  )
  (module my_components:Hole_4mm (layer Front) (tedit 5298E8A8)
    (at 60.96 191.77 90)
    (descr "Mounting Hole, 4mm")
    (tags "HOLE 4MM")
    (fp_text reference HOLE7 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.81 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.00126 5.00126) (drill 4.0005) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
  )
  (module my_components:Hole_4mm (layer Front) (tedit 5298E8A8)
    (at 60.96 64.77)
    (descr "Mounting Hole, 4mm")
    (tags "HOLE 4MM")
    (fp_text reference HOLE8 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value HOLE (at 0 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.00126 5.00126) (drill 4.0005) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
  )
  (module my_components:Conn_Pin_Header_2x1_2.54mm (layer Front) (tedit 5A2F18B2)
    (at 162.56 85.09 90)
    (descr "Pin Header, 2x1, 2.54mm pitch")
    (tags "CONN 2x1")
    (fp_text reference P2 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value POWER_SW (at 1.27 2.8575 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P2-Pad2)"))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_Power_ATX_20pin (layer Front) (tedit 5A2F3465)
    (at 86.36 57.15)
    (descr "Connector, ATX Power, 20pin")
    (tags "ATX POWER CONN 20PIN")
    (fp_text reference P1 (at -19.05 5.715) (layer F.SilkS))
    (fp_text value POWER (at -13.335 5.715) (layer F.SilkS))
    (pad 5 thru_hole circle (at 2.10058 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 6 thru_hole circle (at -2.10058 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 7 thru_hole circle (at -6.2992 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 8 thru_hole circle (at -10.50036 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(P1-Pad8)"))
    (pad 9 thru_hole circle (at -14.69898 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 10 thru_hole circle (at -18.90014 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 11 thru_hole circle (at 18.90014 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(P1-Pad11)"))
    (pad 12 thru_hole circle (at 14.69898 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 13 thru_hole circle (at 10.50036 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 14 thru_hole circle (at 6.2992 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 56 /~PS_ON))
    (pad 15 thru_hole circle (at 2.10058 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 16 thru_hole circle (at -2.10058 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 17 thru_hole circle (at -6.2992 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 18 thru_hole circle (at -10.50036 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 3 /-5V_ATX))
    (pad 19 thru_hole circle (at -14.69898 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 20 thru_hole circle (at -18.90014 -2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 4 thru_hole circle (at 6.2992 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 3 thru_hole circle (at 10.50036 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 14.69898 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at 18.90014 2.75082) (size 2.60096 2.60096) (drill 1.6002) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(P1-Pad1)"))
  )
  (module my_components:Res_762 (layer Front) (tedit 5A2F1CA8)
    (at 147.32 67.31 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 6.35 0.1905 270) (layer F.SilkS))
    (fp_text value 10k (at 6.35 1.5875 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P2-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 5A2F1CC4)
    (at 144.78 67.31 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 6.35 -0.0635 90) (layer F.SilkS))
    (fp_text value 10k (at 6.35 1.3335 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(C19-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 5A2F1A7C)
    (at 137.16 67.31 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R3 (at -3.81 -2.9845 90) (layer F.SilkS))
    (fp_text value 1k (at -3.81 -1.5875 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(R3-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 5A2F1CB3)
    (at 149.86 67.31 90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 6.35 0.4445 90) (layer F.SilkS))
    (fp_text value 470 (at 6.35 1.8415 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P2-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 5A2F1A75)
    (at 137.16 57.15 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R5 (at -4.1275 2.9845 270) (layer F.SilkS))
    (fp_text value 470 (at -4.1275 1.5875 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(R5-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 5A2F1935)
    (at 139.7 57.15 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R6 (at -4.1275 -1.905 270) (layer F.SilkS))
    (fp_text value 470 (at -4.1275 -3.4925 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Res_762 (layer Front) (tedit 5A2F1AC0)
    (at 152.4 67.31 270)
    (descr "Resistor, 7.62mm lead spacing")
    (tags RESISTOR)
    (autoplace_cost180 10)
    (fp_text reference R7 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value 470 (at -1.5875 -1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_SIL10 (layer Front) (tedit 5A2F188A)
    (at 143.51 191.77)
    (descr "Footprint, SIL-10")
    (tags "CONN SIL-10")
    (fp_text reference RR1 (at -10.16 2.2225) (layer F.SilkS))
    (fp_text value 10k (at 10.16 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A5))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A4))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ALE))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A3))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /OSC))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (pad 10 thru_hole circle (at 11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
  )
  (module my_components:Conn_SIL10 (layer Front) (tedit 5A2F1887)
    (at 123.19 186.69)
    (descr "Footprint, SIL-10")
    (tags "CONN SIL-10")
    (fp_text reference RR2 (at -10.16 2.2225) (layer F.SilkS))
    (fp_text value 10k (at 10.16 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A14))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A13))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A12))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CLK))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A11))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A10))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A9))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 10 thru_hole circle (at 11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
  )
  (module my_components:Conn_SIL10 (layer Front) (tedit 5A2F187B)
    (at 85.09 191.77)
    (descr "Footprint, SIL-10")
    (tags "CONN SIL-10")
    (fp_text reference RR3 (at -10.16 2.2225) (layer F.SilkS))
    (fp_text value 10k (at 10.16 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at -8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D7))
    (pad 3 thru_hole circle (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D6))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D5))
    (pad 5 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D4))
    (pad 6 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D3))
    (pad 7 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D2))
    (pad 8 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D1))
    (pad 9 thru_hole circle (at 8.89 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D0))
    (pad 10 thru_hole circle (at 11.43 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AEN))
  )
  (module my_components:Switch_Tactile_6mm (layer Front) (tedit 5A2F1A49)
    (at 148.59 55.88)
    (descr "Switch, Tactile, 6mm")
    (tags "SWITCH TACTILE 6MM")
    (fp_text reference SW1 (at 4.445 0 90) (layer F.SilkS))
    (fp_text value POWER (at 0 -3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at 3.2512 -2.25044) (size 1.39954 1.39954) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 3.2512 2.25044) (size 1.39954 1.39954) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P2-Pad2)"))
    (pad 1 thru_hole circle (at -3.2512 -2.25044) (size 1.39954 1.39954) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at -3.2512 2.25044) (size 1.39954 1.39954) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P2-Pad2)"))
  )
  (module my_components:Conn_Edge_ISA8 (layer Front) (tedit 5A2F1CF3)
    (at 114.3 199.39 180)
    (descr "ISA8 Edge Connector")
    (tags "ISA ISA8 EDGE CONN")
    (fp_text reference BUS7 (at 43.815 0 270) (layer F.SilkS))
    (fp_text value BUSPC_HOST (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RSTDRV))
    (pad 3 thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 4 thru_hole circle (at 30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /IRQ2))
    (pad 5 thru_hole circle (at 27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (pad 6 thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /DRQ2))
    (pad 7 thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 8 thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~0WS))
    (pad 9 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /12V))
    (pad 10 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 11 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /~MEMW))
    (pad 12 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~MEMR))
    (pad 13 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~IOW))
    (pad 14 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~IOR))
    (pad 15 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /~DACK3))
    (pad 16 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /DRQ3))
    (pad 17 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /~DACK1))
    (pad 18 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /DRQ1))
    (pad 19 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~DACK0))
    (pad 20 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /CLK))
    (pad 21 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /IRQ7))
    (pad 22 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /IRQ6))
    (pad 23 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /IRQ5))
    (pad 24 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /IRQ4))
    (pad 25 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /IRQ3))
    (pad 26 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /~DACK2))
    (pad 27 thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TC))
    (pad 28 thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ALE))
    (pad 29 thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 30 thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /OSC))
    (pad 31 thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 32 thru_hole circle (at 38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /~IOCHK))
    (pad 33 thru_hole circle (at 35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /D7))
    (pad 34 thru_hole circle (at 33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /D6))
    (pad 35 thru_hole circle (at 30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /D5))
    (pad 36 thru_hole circle (at 27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /D4))
    (pad 37 thru_hole circle (at 25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /D3))
    (pad 38 thru_hole circle (at 22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /D2))
    (pad 39 thru_hole circle (at 20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /D1))
    (pad 40 thru_hole circle (at 17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /D0))
    (pad 41 thru_hole circle (at 15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /IORDY))
    (pad 42 thru_hole circle (at 12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /AEN))
    (pad 43 thru_hole circle (at 10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A19))
    (pad 44 thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A18))
    (pad 45 thru_hole circle (at 5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A17))
    (pad 46 thru_hole circle (at 2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A16))
    (pad 47 thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A15))
    (pad 48 thru_hole circle (at -2.54 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A14))
    (pad 49 thru_hole circle (at -5.08 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A13))
    (pad 50 thru_hole circle (at -7.62 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A12))
    (pad 51 thru_hole circle (at -10.16 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A11))
    (pad 52 thru_hole circle (at -12.7 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A10))
    (pad 53 thru_hole circle (at -15.24 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A9))
    (pad 54 thru_hole circle (at -17.78 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A8))
    (pad 55 thru_hole circle (at -20.32 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /A7))
    (pad 56 thru_hole circle (at -22.86 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /A6))
    (pad 57 thru_hole circle (at -25.4 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A5))
    (pad 58 thru_hole circle (at -27.94 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A4))
    (pad 59 thru_hole circle (at -30.48 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /A3))
    (pad 60 thru_hole circle (at -33.02 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A2))
    (pad 61 thru_hole circle (at -35.56 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A1))
    (pad 62 thru_hole circle (at -38.1 2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A0))
  )
  (module my_components:Conn_Pin_Header_2x1_2.54mm (layer Front) (tedit 5A2F18B5)
    (at 162.56 90.17 90)
    (descr "Pin Header, 2x1, 2.54mm pitch")
    (tags "CONN 2x1")
    (fp_text reference P3 (at 0.3175 -2.54 90) (layer F.SilkS))
    (fp_text value POWER_LED (at -1.905 2.8575 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model pin_array/pins_array_8x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Conn_SIL6 (layer Front) (tedit 5A2F1883)
    (at 107.95 191.77)
    (descr "Footprint, SIL-6")
    (tags "CONN SIL-6")
    (fp_text reference RR4 (at -5.08 2.2225) (layer F.SilkS))
    (fp_text value 10k (at 5.08 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A19))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /A18))
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A17))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A16))
    (pad 6 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A15))
  )
  (module my_components:Conn_SIL6 (layer Front) (tedit 5A2F1880)
    (at 100.33 186.69)
    (descr "Footprint, SIL-6")
    (tags "CONN SIL-6")
    (fp_text reference RR5 (at -5.08 2.2225) (layer F.SilkS))
    (fp_text value 4.7k (at 5.08 2.2225) (layer F.SilkS))
    (pad 1 thru_hole rect (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 /+5V))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(RR5-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 /~MEMW))
    (pad 4 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /~MEMR))
    (pad 5 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /~IOW))
    (pad 6 thru_hole circle (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /~IOR))
  )
  (module my_components:IC_DIP14_300 (layer Front) (tedit 5A2F1788)
    (at 124.46 57.15)
    (descr "14 pins DIL package, round pads")
    (tags "DIP DIP DIP14 DIL14")
    (fp_text reference U2 (at -10.8585 3.81 90) (layer F.SilkS))
    (fp_text value 74HCT14 (at -10.8585 -1.27 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(U1-Pad11)"))
    (pad 3 thru_hole circle (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(C19-Pad1)"))
    (pad 4 thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(U2-Pad4)"))
    (pad 6 thru_hole circle (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(U1-Pad10)"))
    (pad 7 thru_hole circle (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 8 thru_hole circle (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(U2-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 10 thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(U2-Pad10)"))
    (pad 11 thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 12 thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(U2-Pad12)"))
    (pad 13 thru_hole circle (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 14 thru_hole circle (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (model dil/dil_14.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 5A2F27BE)
    (at 111.76 67.31 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C22 (at 3.81 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.905 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Tant_508 (layer Front) (tedit 5A2F27CA)
    (at 83.82 68.58)
    (descr "Capacitor Tantalum, 5.08mm lead spacing")
    (tags CAPACITOR)
    (fp_text reference C12 (at 0 -3.81) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.556) (layer F.SilkS))
    (fp_text user + (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:Cap_Cer_508 (layer Front) (tedit 5A2F1756)
    (at 111.76 57.15 270)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags Cap_Cer_508)
    (fp_text reference C21 (at 2.54 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at -2.54 1.905 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 VCC))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (model discret/capa_2pas_5x5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module my_components:IC_TO220-3_Horiz (layer Front) (tedit 5A2F15E5)
    (at 60.96 72.39 180)
    (descr "TO220, 3 Leads, Horizontal")
    (tags TO220-3)
    (fp_text reference U3 (at 6.35 -19.05 270) (layer F.SilkS))
    (fp_text value LM7905CT (at 6.35 -9.525 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 57 GND))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 1 /-12V))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 2 /-5V))
    (pad 4 thru_hole rect (at 0 -16.51 180) (size 8.89 8.89) (drill 3.048) (layers *.Cu *.SilkS *.Mask))
    (model discret/to220_horiz.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OSHW-logo:OSHW-logo_silkscreen-front_8mm (layer Front) (tedit 0)
    (at 66.04 107.95 90)
    (fp_text reference G*** (at 0 4.2418 90) (layer F.SilkS) hide)
    (fp_text value OSHW-logo_silkscreen-front_8mm (at 0 -4.2418 90) (layer F.SilkS) hide)
  )
  (gr_line (start 165.1 205.74) (end 53.34 205.74) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 167.64 53.34) (end 167.64 203.2) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 53.34 50.8) (end 165.1 50.8) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 50.8 203.2) (end 50.8 53.34) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_text www.malinov.com (at 59.055 107.95 90) (layer F.SilkS))
  (gr_text "ISA 8-Bit Backplane - Version 1.0\nCopyright (C) 2017 Sergey Kiselev" (at 60.96 148.59 90) (layer F.SilkS))
  (gr_arc (start 165.1 203.2) (end 167.64 203.2) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 165.1 53.34) (end 165.1 50.8) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 53.34 53.34) (end 50.8 53.34) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 53.34 203.2) (end 53.34 205.74) (angle 90) (layer Edge.Cuts) (width 0.381))
  (zone (net 57) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.37846))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.005 52.705) (xy 167.005 203.835) (xy 165.735 205.105) (xy 52.705 205.105) (xy 51.435 203.835)
        (xy 51.435 52.705) (xy 52.705 51.435) (xy 165.735 51.435) (xy 167.005 52.705)
      )
    )
  )
  (zone (net 57) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.37846))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.005 203.835) (xy 167.005 52.705) (xy 165.735 51.435) (xy 109.855 51.435) (xy 108.585 52.705)
        (xy 108.585 60.96) (xy 107.315 62.23) (xy 99.695 62.23) (xy 98.425 60.96) (xy 98.425 59.055)
        (xy 97.155 57.785) (xy 75.565 57.785) (xy 74.295 59.055) (xy 74.295 62.23) (xy 73.025 63.5)
        (xy 65.405 63.5) (xy 64.135 62.23) (xy 64.135 52.705) (xy 62.865 51.435) (xy 52.705 51.435)
        (xy 51.435 52.705) (xy 51.435 203.835) (xy 52.705 205.105) (xy 165.735 205.105)
      )
    )
  )
  (zone (net 60) (net_name /+5V) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.37846))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.315 52.07) (xy 107.95 52.705) (xy 107.95 60.325) (xy 106.68 61.595) (xy 100.33 61.595)
        (xy 99.06 60.325) (xy 99.06 58.42) (xy 97.79 57.15) (xy 74.93 57.15) (xy 73.66 58.42)
        (xy 73.66 61.595) (xy 72.39 62.865) (xy 66.04 62.865) (xy 64.77 61.595) (xy 64.77 52.705)
        (xy 65.405 52.07)
      )
    )
  )
)
