(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 160)
    (tracks 493)
    (zones 0)
    (modules 31)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.3048)
    (user_trace_width 0.508)
    (user_trace_width 0.8)
    (user_trace_width 0.85)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 SDA)
  (net 4 SCL)
  (net 5 33)
  (net 6 SCK)
  (net 7 MOSI)
  (net 8 MISO)
  (net 9 "Net-(J11-Pad1)")
  (net 10 14)
  (net 11 15)
  (net 12 27)
  (net 13 26)
  (net 14 25)
  (net 15 36)
  (net 16 16)
  (net 17 17)
  (net 18 21)
  (net 19 VBUS)
  (net 20 34)
  (net 21 39)
  (net 22 32)
  (net 23 4)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 17)
    (add_net 21)
    (add_net 25)
    (add_net 26)
    (add_net 27)
    (add_net 32)
    (add_net 33)
    (add_net 34)
    (add_net 36)
    (add_net 39)
    (add_net 4)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(J11-Pad1)")
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net VBUS)
  )
  (module Button_Switch_THT:SW_TH_Tactile_Omron_B3F-10xx (layer B.Cu) (tedit 5A02FE31)
    (at 103.5304 45.974 90)
    (descr SW_TH_Tactile_Omron_B3F-10xx_https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "Omron B3F-10xx")
    (fp_text reference SW1 (at 1.0922 -2.286 180) (layer B.SilkS))
    (fp_text value SW_Push_Dual (at 3.2 -6.5 90) (layer B.Fab))
    (fp_text user %R (at 3.25 -2.25 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 34))
    (pad 2 thru_hole circle (at 6.5 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 34))
    (pad 3 thru_hole circle (at 0 -4.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 6.5 -4.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_TH_Tactile_Omron_B3F-10xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pvos_logo:pvos15 (layer F.Cu) (tedit 6019A876)
    (at 100.4316 19.7866 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Button_Switch_THT:SW_TH_Tactile_Omron_B3F-10xx (layer B.Cu) (tedit 5A02FE31)
    (at 80.3656 53.0098)
    (descr SW_TH_Tactile_Omron_B3F-10xx_https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "Omron B3F-10xx")
    (fp_text reference SW2 (at 3.302 0.1016) (layer B.SilkS))
    (fp_text value SW_Push_Dual (at 3.2 -6.5) (layer B.Fab))
    (fp_text user %R (at 3.25 -2.25) (layer B.Fab))
    (pad 4 thru_hole circle (at 6.5 -4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 -4.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 6.5 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 36))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 36))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_TH_Tactile_Omron_B3F-10xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 65.925 22.9 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 11.95 0.1 180) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 SDA))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5B36C52B)
    (at 80.85 30 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2173904347826087)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2173904347826087)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 62.3 3.65 90)
    (descr "Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x07 2.54mm single row")
    (fp_text reference J13 (at 0 2.77 -90) (layer B.SilkS))
    (fp_text value Conn_01x07_Female (at 0 -18.01 -90) (layer B.Fab))
    (fp_text user %R (at 0 -7.62) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 4))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 39))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VBUS))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal (layer B.Cu) (tedit 5B78AD87)
    (at 102.743 10.7442 270)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J7 (at 0.1016 -0.2286 180) (layer B.SilkS))
    (fp_text value Conn_01x04_Female (at 0 -3.98 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.5 2 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at -0.5 2 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +3V3))
    (pad 3 smd roundrect (at 0.5 2 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 SDA))
    (pad 4 smd roundrect (at 1.5 2 270) (size 0.6 1.55) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 SCL))
    (pad MP smd roundrect (at -2.8 -1.875 270) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2083325))
    (pad MP smd roundrect (at 2.8 -1.875 270) (size 1.2 1.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2083325))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-2-5.0-H_1x02_P5.00mm_Horizontal (layer B.Cu) (tedit 5B294F69)
    (at 5.4 28.4)
    (descr "Terminal Block Phoenix PT-1,5-2-5.0-H, 2 pins, pitch 5mm, size 10x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-2-5.0-H pitch 5mm size 10x9mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J1 (at 2.5 5.06) (layer B.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 2.5 -6.06) (layer B.Fab))
    (fp_text user %R (at 2.5 -2.9) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 VBUS))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-2-5.0-H_1x02_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 59.65 12.75 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at -1.875 -0.175 180) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 17))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 56.475 12.75 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at -1.875 -0.025 180) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 16))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:DM3D-SF (layer B.Cu) (tedit 5951123E)
    (at 97.88398 24.91232 270)
    (descr "Micro SD")
    (tags "Micro SD")
    (attr smd)
    (fp_text reference J10 (at -0.69342 1.37414 270) (layer B.SilkS))
    (fp_text value Micro_SD_Card (at 1.5 7 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -3.25 270) (layer B.Fab))
    (pad 8 smd rect (at -4.5 -0.875 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -5.7 -0.75 270) (size 1.3 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -5.95 6.85 270) (size 0.8 1.5) (layers B.Cu B.Paste B.Mask))
    (pad B smd rect (at -5.625 8.35 270) (size 1.45 1) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 6 7.5 270) (size 0.8 1.4) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -3.4 -0.875 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 8 MISO))
    (pad 6 smd rect (at -2.3 -0.875 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.2 -0.875 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 6 SCK))
    (pad 4 smd rect (at -0.1 -0.875 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 1 -0.875 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 7 MOSI))
    (pad 2 smd rect (at 2.1 -0.875 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 5 33))
    (pad 1 smd rect (at 3.2 -0.875 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 5.65 -0.75 270) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask))
    (pad A smd rect (at 5.6 9.925 270) (size 1 1.55) (layers B.Cu B.Paste B.Mask))
    (model C:/Cad/Footprint/Hirose/3D/DM3D-SF.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 93.853 51.435)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H8 (at 1.9812 2.54) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 93.8276 4.572)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H7 (at 2.0574 -2.2606) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 11.9888 4.572)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H6 (at -2.0066 -2.2098) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 11.9888 51.435)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H5 (at -1.9888 2.465) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 44.525 12.75 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at -1.85674 0.03556 180) (layer F.SilkS))
    (fp_text value 4.7K (at 4.8641 -0.03302 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 36))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A434)
    (at 52.95 54.1 270)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J11 (at -2.284 0.118) (layer B.SilkS))
    (fp_text value Conn_01x01_Female (at 1 -0.05) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J11-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 79.2734 4.6482 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J12 (at -0.40894 -2.38252 90) (layer F.SilkS))
    (fp_text value ssd1306 (at 0 10.39 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 16))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 17))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A420)
    (at 44.2976 45.0596 270)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J8 (at 2.3622 19.304 180) (layer F.SilkS))
    (fp_text value BME390 (at 0 20.55 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A433)
    (at 49.3776 32.0294 90)
    (descr "Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x07 2.54mm single row")
    (fp_text reference J6 (at -0.4318 17.4498 270) (layer F.SilkS))
    (fp_text value SCD30 (at 0 18.01 90) (layer F.Fab))
    (fp_text user %R (at 0 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A420)
    (at 71.88454 16.15186 180)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (fp_text reference J5 (at 0 2.77 180) (layer B.SilkS))
    (fp_text value uSD (at 0 -20.55 180) (layer B.Fab))
    (fp_text user %R (at 0 -8.89 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 33))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 MOSI))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 MISO))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 SCK))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A429)
    (at 22.17772 43.2808)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0.10668 -7.32282) (layer B.SilkS))
    (fp_text value M4466 (at 0 -7.85) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 270) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 39))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 40.4 12.75 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at -1.83646 -0.02408 180) (layer F.SilkS))
    (fp_text value 4.7K (at 4.9047 0.10546 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 34))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x16_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41E)
    (at 62.3062 27.6606 270)
    (descr "Through hole straight socket strip, 1x16, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x16 2.54mm single row")
    (fp_text reference J3 (at 0.0762 -2.286 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Female (at 2.82 5.676 180) (layer F.Fab))
    (fp_text user %R (at 0 19.05) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 21))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 17))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 16))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 MISO))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 MOSI))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 SCK))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 4))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 36))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 39))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 34))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 25))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 26))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41D)
    (at 34.35 7.2796 90)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference J2 (at -0.061 30.2422 90) (layer F.SilkS))
    (fp_text value Conn_01x12_Female (at -2.6822 22.1424 180) (layer F.Fab))
    (fp_text user %R (at 0 13.97) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 14))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 32))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 15))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 33))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 27))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VBUS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:RFM95 (layer B.Cu) (tedit 585E5D4C)
    (at 71.8 40.2 180)
    (fp_text reference U1 (at 15.2342 1.8968) (layer B.SilkS))
    (fp_text value RFM95HW (at 13.5 1.8) (layer B.Fab))
    (pad 1 smd oval (at 0 0 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd oval (at 0 -2 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 14 25))
    (pad 3 smd oval (at 0 -4 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 18 21))
    (pad 4 smd oval (at 0 -6 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 13 26))
    (pad 5 smd oval (at 0 -8 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 10 14))
    (pad 6 smd oval (at 0 -10 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 12 27))
    (pad 7 smd oval (at 0 -12 180) (size 2 1) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd oval (at 0 -14 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd oval (at 16 -14 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J11-Pad1)"))
    (pad 10 smd oval (at 16 -12 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd oval (at 16 -10 180) (size 2 1) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd oval (at 16 -8 180) (size 2 1) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd oval (at 16 -6 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 14 smd oval (at 16 -4 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 11 15))
    (pad 15 smd oval (at 16 -2 180) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 22 32))
    (pad 16 smd oval (at 16 0 180) (size 2 1) (layers B.Cu B.Paste B.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 102.15 52.2 90)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at -2.7148 0.1358 180) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 3.85 3.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at -0.0146 2.9818) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 102.15 3.8)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0.212 3.0072) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 3.85 52.2)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at -2.1736 2.3084) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 62.8002 22.908 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 12.01474 -0.03994) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 SCL))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Please consult\nuser guide for\ncalibration\nprocedures." (at 1.905 41.7068) (layer F.SilkS))
  (gr_text pvos.org/co2/g (at 84.6582 42.6212) (layer F.SilkS))
  (gr_text " \"REV_G\"" (at 84.3026 38.4048) (layer F.SilkS))
  (gr_text Monitor (at 91.2368 33.5788) (layer F.SilkS))
  (gr_text 16 (at 86.9188 7.3406 90) (layer F.SilkS))
  (gr_text 17 (at 84.5058 7.5438 90) (layer F.SilkS))
  (gr_text GND (at 79.375 7.5692 90) (layer F.SilkS))
  (gr_text 3V (at 81.9404 7.3406 90) (layer F.SilkS))
  (gr_text SDA (at 62.738 1.524) (layer B.SilkS))
  (gr_text SCL (at 59.7408 1.5748) (layer B.SilkS))
  (gr_text 4 (at 57.2516 1.6002) (layer B.SilkS))
  (gr_text 39 (at 54.6354 1.6002) (layer B.SilkS))
  (gr_text 5V (at 14.1224 28.2956 90) (layer B.SilkS))
  (gr_text 5V (at 52.1462 1.524) (layer B.SilkS))
  (gr_text 3V (at 49.6316 1.6002) (layer B.SilkS))
  (gr_text GND (at 46.8122 1.6002) (layer B.SilkS))
  (gr_text 3V (at 75.0824 31.4452) (layer B.SilkS))
  (gr_text GND (at 75.1078 29.0068) (layer B.SilkS))
  (gr_text SCK (at 75.311 26.4414) (layer B.SilkS))
  (gr_text MISO (at 75.311 23.6728) (layer B.SilkS))
  (gr_text MOSI (at 75.311 21.3868) (layer B.SilkS))
  (gr_text 33 (at 74.8792 18.9484) (layer B.SilkS))
  (gr_text adafruit.com/product/254 (at 87.7062 35.9664) (layer B.SilkS))
  (gr_text "Hirose DM3D" (at 92.8624 24.8158 270) (layer B.SilkS))
  (gr_text qwiic (at 97.409 10.5664) (layer B.SilkS))
  (gr_text GND (at 1.6002 28.3972 90) (layer B.SilkS))
  (gr_text B (at 83.4644 55.1688) (layer B.SilkS))
  (gr_text A (at 105.3592 42.6974) (layer B.SilkS))
  (gr_text MOSI (at 68.707 44.196) (layer B.SilkS))
  (gr_text MISO (at 68.6054 42.3672) (layer B.SilkS))
  (gr_text ANA (at 58.6486 54.1274) (layer B.SilkS))
  (gr_text GND (at 68.8594 40.3352) (layer B.SilkS))
  (gr_text GND (at 68.6562 54.1274) (layer B.SilkS))
  (gr_text ANT (at 49.784 54.356) (layer B.SilkS))
  (gr_text "(DISPLAY)" (at 83.3628 17.018) (layer F.SilkS))
  (gr_text "Usage & Assembly Guides:" (at 18.8468 50.0126) (layer F.SilkS))
  (gr_text http://pvos.org/co2/g (at 17.1 52) (layer F.SilkS))
  (gr_text CO2 (at 84.0232 33.5788) (layer F.SilkS))
  (gr_text "NOTE:\nCO2 sensing requires\nregular calibration!" (at 1.905 34.5186) (layer F.SilkS))
  (gr_text adafruit.com/product/3405 (at 27.8 21.5) (layer F.SilkS))
  (gr_text 4.7K (at 40.4114 17.5514 90) (layer F.SilkS))
  (gr_text 4.7K (at 44.525 17.6 90) (layer F.SilkS))
  (gr_text 4.7K (at 62.81166 17.6149 90) (layer F.SilkS))
  (gr_text 4.7K (at 59.625 17.45 90) (layer F.SilkS))
  (gr_text 4.7K (at 56.4 17.625 90) (layer F.SilkS))
  (gr_text RFM95 (at 63.7286 37.973) (layer B.SilkS))
  (gr_text "uSD Card" (at 87.9348 15.3416) (layer B.SilkS))
  (gr_line (start 0 56) (end 0 22.606) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 11.5062 22.606) (end 0 22.606) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 11.5062 12.319) (end 11.5062 22.606) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 12.319) (end 11.5062 12.319) (layer Edge.Cuts) (width 0.05))
  (gr_text SSD1306 (at 82.9564 14.5288) (layer F.SilkS))
  (gr_line (start 106 0) (end 106 56) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 0) (end 0 12.319) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 56) (end 106 56) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 0 0) (end 106 0) (layer Edge.Cuts) (width 0.05))
  (gr_text SDA (at 57.0484 35.179 90) (layer F.SilkS))
  (gr_text SCL (at 54.4576 35.2806 90) (layer F.SilkS))
  (gr_text adafruit.com/product/1063 (at 13.4222 45.9994) (layer B.SilkS))
  (gr_text adafruit.com/product/4816 (at 35.4532 37.8792) (layer F.SilkS))
  (gr_text 4.7K (at 65.9384 17.6022 90) (layer F.SilkS))
  (gr_text SCL (at 34.4088 41.7522 90) (layer F.SilkS))
  (gr_text GND (at 31.8088 41.7522 90) (layer F.SilkS))
  (gr_text SDA (at 39.5088 41.8522 90) (layer F.SilkS))
  (gr_text 3V (at 26.5848 41.7462 90) (layer F.SilkS))
  (gr_text 3V (at 18.46002 43.32484) (layer B.SilkS))
  (gr_text GND (at 18.71402 40.78484) (layer B.SilkS))
  (gr_text 39 (at 18.7284 38.277) (layer B.SilkS))
  (gr_text GND (at 51.8922 35.2552 90) (layer F.SilkS))
  (gr_text 3V (at 49.5554 34.7472 90) (layer F.SilkS))
  (gr_text "Feather\nESP32" (at 18.796 17.272) (layer F.SilkS))
  (gr_text "(mic, optional)" (at 10.2222 40.7994) (layer B.SilkS))
  (gr_text "(CO2)" (at 54.2036 46.8122) (layer F.SilkS))
  (gr_text "(pressure, optional)" (at 35.6532 32.7792) (layer F.SilkS))
  (gr_text MAX4466 (at 10.0222 43.6994) (layer B.SilkS))
  (gr_text sparkfun.com/products/15112 (at 61.468 51.816) (layer F.SilkS))
  (gr_text BMP388/390 (at 35.8532 35.5792) (layer F.SilkS))
  (gr_text SCD30 (at 54.5084 49.7078) (layer F.SilkS))
)
