(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 396)
    (zones 0)
    (modules 14)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /RESET)
  (net 2 GND)
  (net 3 +5V)
  (net 4 +3V3)
  (net 5 /GPIO18)
  (net 6 /GPIO17)
  (net 7 /GPIO16)
  (net 8 /GPIO15)
  (net 9 /GPIO14)
  (net 10 /GPIO13)
  (net 11 /GPIO12)
  (net 12 /GPIO11)
  (net 13 /GPIO10)
  (net 14 /GPIO9)
  (net 15 /GPIO8)
  (net 16 /GPIO7)
  (net 17 /GPIO6)
  (net 18 /GPIO5)
  (net 19 /GPIO4)
  (net 20 /GPIO3)
  (net 21 /GPIO2)
  (net 22 /GPIO1)
  (net 23 /GPIO0)
  (net 24 /GPIO19)
  (net 25 /GPIO20)
  (net 26 /GPIO21)
  (net 27 /GPIO26)
  (net 28 /GPIO33)
  (net 29 /GPIO34)
  (net 30 /GPIO35)
  (net 31 /GPIO36)
  (net 32 /GPIO37)
  (net 33 /GPIO38)
  (net 34 /GPIO39)
  (net 35 /GPIO40)
  (net 36 /GPIO41)
  (net 37 /GPIO42)
  (net 38 /TX)
  (net 39 /RX)
  (net 40 /GPIO45)
  (net 41 /GPIO46)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /GPIO0)
    (add_net /GPIO1)
    (add_net /GPIO10)
    (add_net /GPIO11)
    (add_net /GPIO12)
    (add_net /GPIO13)
    (add_net /GPIO14)
    (add_net /GPIO15)
    (add_net /GPIO16)
    (add_net /GPIO17)
    (add_net /GPIO18)
    (add_net /GPIO19)
    (add_net /GPIO2)
    (add_net /GPIO20)
    (add_net /GPIO21)
    (add_net /GPIO26)
    (add_net /GPIO3)
    (add_net /GPIO33)
    (add_net /GPIO34)
    (add_net /GPIO35)
    (add_net /GPIO36)
    (add_net /GPIO37)
    (add_net /GPIO38)
    (add_net /GPIO39)
    (add_net /GPIO4)
    (add_net /GPIO40)
    (add_net /GPIO41)
    (add_net /GPIO42)
    (add_net /GPIO45)
    (add_net /GPIO46)
    (add_net /GPIO5)
    (add_net /GPIO6)
    (add_net /GPIO7)
    (add_net /GPIO8)
    (add_net /GPIO9)
    (add_net /RESET)
    (add_net /RX)
    (add_net /TX)
    (add_net GND)
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57)
    (at 194.3735 101.2825 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value TC2117-3.3VDBTR (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.15 2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 3.15 0 270) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Espressif:ESP32-S2-MINI-1 (layer F.Cu) (tedit 60F56B8A)
    (at 199.39 76.962)
    (descr "ESP32-S2-MINI-1 and ESP32-S2-MINI-1U: https://www.espressif.com/sites/default/files/documentation/esp32-s2-mini-1_esp32-s2-mini-1u_datasheet_en.pdf")
    (tags ESP32-S2)
    (attr smd)
    (fp_text reference U2 (at -8.763 -6.985 90) (layer F.SilkS))
    (fp_text value ESP32-S2-MINI-1 (at 0 9.4) (layer F.Fab))
    (fp_text user "Antenna Area" (at 0 -10.45) (layer F.SilkS))
    (fp_text user REF** (at 0 0) (layer F.Fab))
    (pad 46 smd rect (at -1.65 1.65) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 1.65 1.65) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 1.65 -1.65) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd custom (at -1.65 -1.65) (size 0.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.6 0.6) (xy 0.6 0.6) (xy 0.6 -0.6) (xy 0 -0.6) (xy -0.6 0)
) (width 0))
      ))
    (pad 46 smd rect (at 0 1.65) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -1.65 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 0 -1.65) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 1.65 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 0 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 7 7 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -7 7 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 6.95 -7 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -7 -7 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -5.95 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -5.1 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -4.25 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -3.4 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -2.55 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -1.7 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at -0.85 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 0 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 0.85 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 1.7 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 2.55 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 3.4 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 4.25 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 5.1 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 5.95 -7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 45 smd rect (at 7 -5.95 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /RESET))
    (pad 44 smd rect (at 7 -5.1 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 41 /GPIO46))
    (pad 43 smd rect (at 7 -4.25 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 42 smd rect (at 7 -3.4 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 41 smd rect (at 7 -2.55 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 40 /GPIO45))
    (pad 40 smd rect (at 7 -1.7 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 39 /RX))
    (pad 39 smd rect (at 7 -0.85 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 /TX))
    (pad 38 smd rect (at 7 0 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 /GPIO42))
    (pad 37 smd rect (at 7 0.85 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 /GPIO41))
    (pad 36 smd rect (at 7 1.7 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 /GPIO40))
    (pad 35 smd rect (at 7 2.55 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 /GPIO39))
    (pad 34 smd rect (at 7 3.4 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 /GPIO38))
    (pad 33 smd rect (at 7 4.25 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /GPIO37))
    (pad 32 smd rect (at 7 5.1 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 /GPIO36))
    (pad 31 smd rect (at 7 5.95 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 /GPIO35))
    (pad 30 smd rect (at 5.95 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 29 smd rect (at 5.1 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 /GPIO34))
    (pad 28 smd rect (at 4.25 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 /GPIO33))
    (pad 27 smd rect (at 3.4 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 2.55 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 27 /GPIO26))
    (pad 25 smd rect (at 1.7 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 /GPIO21))
    (pad 24 smd rect (at 0.85 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 /GPIO20))
    (pad 23 smd rect (at 0 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /GPIO19))
    (pad 22 smd rect (at -0.85 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /GPIO18))
    (pad 21 smd rect (at -1.7 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 /GPIO17))
    (pad 20 smd rect (at -2.55 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /GPIO16))
    (pad 19 smd rect (at -3.4 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /GPIO15))
    (pad 18 smd rect (at -4.25 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 /GPIO14))
    (pad 17 smd rect (at -5.1 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 /GPIO13))
    (pad 16 smd rect (at -5.95 7) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 /GPIO12))
    (pad 15 smd rect (at -7 5.95 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 /GPIO11))
    (pad 14 smd rect (at -7 5.1 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 /GPIO10))
    (pad 13 smd rect (at -7 4.25 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 /GPIO9))
    (pad 12 smd rect (at -7 3.4 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 /GPIO8))
    (pad 11 smd rect (at -7 2.55 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 /GPIO7))
    (pad 10 smd rect (at -7 1.7 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 /GPIO6))
    (pad 9 smd rect (at -7 0.85 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 /GPIO5))
    (pad 8 smd rect (at -7 0 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 /GPIO4))
    (pad 7 smd rect (at -7 -0.85 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 /GPIO3))
    (pad 6 smd rect (at -7 -1.7 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 /GPIO2))
    (pad 5 smd rect (at -7 -2.55 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 /GPIO1))
    (pad 4 smd rect (at -7 -3.4 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 /GPIO0))
    (pad 3 smd rect (at -7 -4.25 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -7 -5.1 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -7 -5.95 90) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${ESPRESSIF_3DMODELS}/ESP32-S2-MINI-1.STEP
      (offset (xyz -7.7 -7.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 192.532 111.125 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /GPIO18))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 196.088 109.1715 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 5EAC9A07)
    (at 202.692 90.932)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J4 (at -4.445 -4.699 90) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 1.27 16.26) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 10 thru_hole circle (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /GPIO41))
    (pad 6 thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /GPIO40))
    (pad 4 thru_hole circle (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /GPIO39))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /GPIO42))
    (pad 9 thru_hole circle (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 5EAC9A07)
    (at 202.692 112.776)
    (descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x03 2.54mm double row")
    (fp_text reference J3 (at -4.572 -4.572 90) (layer F.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 1.27 11.18) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /GPIO0))
    (pad 4 thru_hole circle (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /RX))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /TX))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 /RESET))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x21_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 210.82 71.12 180)
    (descr "Through hole straight pin header, 1x21, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x21 2.54mm single row")
    (fp_text reference J2 (at 0 1.905) (layer B.SilkS))
    (fp_text value Conn_01x21 (at 0 -53.13) (layer B.Fab))
    (fp_text user %R (at 0 -25.4 270) (layer B.Fab))
    (pad 21 thru_hole oval (at 0 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /GPIO18))
    (pad 20 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /GPIO19))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /GPIO20))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /GPIO21))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /GPIO26))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /GPIO33))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /GPIO34))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /GPIO35))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /GPIO36))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /GPIO37))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /GPIO38))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /GPIO39))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /GPIO40))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /GPIO41))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /GPIO42))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /TX))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /RX))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /GPIO45))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /GPIO46))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /RESET))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x21_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x21_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 187.96 71.12 180)
    (descr "Through hole straight pin header, 1x21, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x21 2.54mm single row")
    (fp_text reference J1 (at 0 1.905) (layer B.SilkS))
    (fp_text value Conn_01x21 (at 0 -53.13) (layer F.Fab))
    (fp_text user %R (at 0 -25.4 -90) (layer F.Fab))
    (pad 21 thru_hole oval (at 0 -50.8 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /GPIO17))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /GPIO16))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /GPIO15))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GPIO14))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /GPIO13))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /GPIO12))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /GPIO11))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /GPIO10))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GPIO9))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /GPIO8))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /GPIO7))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /GPIO6))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /GPIO5))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /GPIO4))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /GPIO3))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /GPIO2))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /GPIO1))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /GPIO0))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x21_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm (layer F.Cu) (tedit 5AA4B285)
    (at 194.31 119.38 270)
    (descr https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf)
    (tags "LED RGB NeoPixel")
    (attr smd)
    (fp_text reference D1 (at -4.318 1.778 180) (layer F.SilkS))
    (fp_text value WS2812B (at 0 4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (fp_text user 1 (at -4.15 -1.6 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at -2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.45 -1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /GPIO18))
    (pad 3 smd rect (at 2.45 1.6 270) (size 1.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 192.405 88.138)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 192.405 91.694 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.651) (layer F.SilkS))
    (fp_text value 22uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 196.2935 95.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 1.524) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 192.405 95.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.524) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 196.088 112.9815 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /RESET))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "G\nEN\n46\n45\nRX\nTX\n42\n41\n40\n39\n38\n37\n36\n35\n34\n33\n26\n21\n20\n19\n18" (at 212.5345 96.647) (layer F.SilkS))
  (gr_text "3V\n0\n1\n2\n3\n4\n5\n6\n7\n8\n9\n10\n11\n12\n13\n14\n15\n16\n17\n5V\nG" (at 186.2455 96.647) (layer F.SilkS))
  (gr_line (start 213.36 68.58) (end 213.36 124.46) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.42 68.58) (end 213.36 68.58) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.42 124.46) (end 185.42 68.58) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 213.36 124.46) (end 185.42 124.46) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.725 123.825) (xy 186.055 123.825) (xy 186.055 69.215) (xy 212.725 69.215)
      )
    )
  )
)
