(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.556512)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(3 "In3.Cu" signal)
		(4 "In4.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0254)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.04318)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.110744)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.017272)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.1016)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.017272)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.925576)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In3.Cu"
				(type "copper")
				(thickness 0.017272)
			)
			(layer "dielectric 4"
				(type "core")
				(color "FR4 natural")
				(thickness 0.1016)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In4.Cu"
				(type "copper")
				(thickness 0.017272)
			)
			(layer "dielectric 5"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.110744)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.04318)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0254)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints yes)
		(aux_axis_origin 57.785 137.123)
		(grid_origin 57.785 137.123)
		(pcbplotparams
			(layerselection 0x0000020_7fffffe0)
			(plot_on_all_layers_selection 0x0021000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref yes)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 4)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "CAM/")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(K1A-P10_3-Pad4)")
	(net 2 "unconnected-(K1B-VDD_USB-Pad70)")
	(net 3 "Net-(U21-OUT-)")
	(net 4 "unconnected-(K1A-P10_5-Pad8)")
	(net 5 "unconnected-(K1B-P6_4-Pad66)")
	(net 6 "/QSPI.SCLK")
	(net 7 "/FP_87")
	(net 8 "Net-(U21-OUT+)")
	(net 9 "/FP_83")
	(net 10 "Net-(J23-Pin_1)")
	(net 11 "/QSPI.I1")
	(net 12 "Net-(C90-Pad1)")
	(net 13 "unconnected-(K1A-P0_4-Pad31)")
	(net 14 "unconnected-(K1B-VBACKUP-Pad43)")
	(net 15 "/QSPI.I3")
	(net 16 "Net-(J23-Pin_4)")
	(net 17 "Net-(U21-TTL_IN)")
	(net 18 "/FPGA/FM_1P8")
	(net 19 "/AD_TCLK")
	(net 20 "unconnected-(K1A-P13_7-Pad29)")
	(net 21 "+5.0V")
	(net 22 "/QSPI.~{CE}")
	(net 23 "/SPI2.MISO")
	(net 24 "/QSPI.I0")
	(net 25 "Net-(J23-Pin_3)")
	(net 26 "unconnected-(K1A-VDDIO_0-Pad21)")
	(net 27 "/FP_84")
	(net 28 "unconnected-(K1A-VTARG-Pad2)")
	(net 29 "/FP_86")
	(net 30 "/FP_85")
	(net 31 "unconnected-(K1A-BT_UART_RTS-Pad39)")
	(net 32 "/FP_80")
	(net 33 "/FP_82")
	(net 34 "unconnected-(K1C-VCC_3V6-Pad83)")
	(net 35 "unconnected-(K1A-BT_UART_RXD-Pad37)")
	(net 36 "unconnected-(K1B-P6_VDD-Pad64)")
	(net 37 "unconnected-(K1A-BT_UART_CTS-Pad38)")
	(net 38 "/FPGA/F_1P8")
	(net 39 "unconnected-(K1A-BT_UART_TXD-Pad40)")
	(net 40 "/AD_TMS")
	(net 41 "/FP_81")
	(net 42 "/SPI2.MOSI")
	(net 43 "/SPI2.CE")
	(net 44 "unconnected-(K1A-P10_4-Pad5)")
	(net 45 "/SPI2.CLK")
	(net 46 "/SCLK_HARM_FLT_1V8")
	(net 47 "unconnected-(K1B-VTARG-Pad72)")
	(net 48 "/FP_52")
	(net 49 "/FP_51")
	(net 50 "unconnected-(K1A-P10_2-Pad6)")
	(net 51 "unconnected-(K1B-P1_0-Pad57)")
	(net 52 "/FP_55")
	(net 53 "Net-(J23-Pin_5)")
	(net 54 "/FP_56")
	(net 55 "/FPGA/N_1P8")
	(net 56 "unconnected-(K1B-Vref-Pad41)")
	(net 57 "/QSPI.I2")
	(net 58 "/FP_50")
	(net 59 "/FP_54")
	(net 60 "/Power Supply/ap3445_3P3V")
	(net 61 "/FPGA/STM_~{RST}")
	(net 62 "Net-(U1H-INITN)")
	(net 63 "/Power Supply/FV_1P8")
	(net 64 "Net-(U5-PD0)")
	(net 65 "Net-(U5-PD1)")
	(net 66 "/FPGA/FPGA_nPROG")
	(net 67 "/FPGA/USB_P")
	(net 68 "Net-(U1H-CFG_1)")
	(net 69 "/FPGA/FLASH.IO3")
	(net 70 "unconnected-(U1A-PL20C{slash}GR_PCLK7_0{slash}+{slash}LDQ20-PadJ3)")
	(net 71 "/FPGA/USB_N")
	(net 72 "Net-(F1-Pad1)")
	(net 73 "unconnected-(U1E-PR20D{slash}-{slash}RDQ20-PadK14)")
	(net 74 "unconnected-(U1G-PT4B{slash}--PadB3)")
	(net 75 "unconnected-(J1-SBU1-PadA8)")
	(net 76 "unconnected-(U1B-PL32C{slash}+{slash}LDQ32-PadL3)")
	(net 77 "unconnected-(U1B-PL23D{slash}-{slash}LDQ32-PadM3)")
	(net 78 "/FPGA/JTAG1.TCK")
	(net 79 "unconnected-(J1-SBU2-PadB8)")
	(net 80 "unconnected-(U1F-PT62A{slash}+-PadD13)")
	(net 81 "unconnected-(U1B-PL29D{slash}-{slash}LDQ32-PadL5)")
	(net 82 "/VDIG_1P0")
	(net 83 "unconnected-(U1F-PT58B{slash}--PadE12)")
	(net 84 "unconnected-(J7-Pad7)")
	(net 85 "/FPGA/FLASH.CLK")
	(net 86 "unconnected-(U1F-PT47A{slash}+-PadD10)")
	(net 87 "Net-(J1-CC1_B)")
	(net 88 "+2.5V")
	(net 89 "Net-(J1-CC1_A)")
	(net 90 "unconnected-(U1F-PT40B{slash}--PadE9)")
	(net 91 "unconnected-(J8-Pad10)")
	(net 92 "Net-(U5-BOOT0)")
	(net 93 "unconnected-(U1B-PL29C{slash}GR_PCLK6_1{slash}+{slash}LDQ32-PadL4)")
	(net 94 "Net-(U5-PB2)")
	(net 95 "unconnected-(U1F-PT47B{slash}--PadE10)")
	(net 96 "/VDIGIO_1P8")
	(net 97 "+3.3V")
	(net 98 "Net-(D2-A)")
	(net 99 "unconnected-(U1F-PT62B{slash}--PadE13)")
	(net 100 "/FPGA/JTAG1.TDO")
	(net 101 "unconnected-(U1A-PL11D{slash}-{slash}LDQ8-PadE1)")
	(net 102 "unconnected-(U1E-PR20C{slash}GR_PCLK2_0{slash}+{slash}RDQ20-PadJ14)")
	(net 103 "unconnected-(U1A-PL8A{slash}HS+{slash}LDQS8-PadD1)")
	(net 104 "/FPGA/SDRAM_DQ11")
	(net 105 "unconnected-(U1A-PL8B{slash}HS-{slash}LDQSN8-PadE2)")
	(net 106 "/FPGA/SDRAM_A7")
	(net 107 "+1.1V")
	(net 108 "unconnected-(U1G-PT4A{slash}+-PadA2)")
	(net 109 "/FPGA/SDRAM_A2")
	(net 110 "/FPGA/SDRAM_x.nRAS")
	(net 111 "unconnected-(U1E-PR17C{slash}+{slash}RDQ20-PadJ13)")
	(net 112 "unconnected-(U1A-PL20D{slash}-{slash}LDQ20-PadK3)")
	(net 113 "/FPGA/SDRAM_DQ12")
	(net 114 "unconnected-(U1A-PL11C{slash}-{slash}LDQ8-PadF2)")
	(net 115 "/FPGA/JTAG1.TDI")
	(net 116 "/FPGA/SDRAM_x.CKE")
	(net 117 "/FPGA/SDRAM_A0")
	(net 118 "unconnected-(U1E-PR17D{slash}-{slash}RDQ20-PadJ12)")
	(net 119 "/FPGA/SDRAM_DQ7")
	(net 120 "/FPGA/SDRAM_DQ4")
	(net 121 "/FPGA/SDRAM_DQ14")
	(net 122 "unconnected-(U1B-PL35C{slash}+{slash}LDQ32-PadM4)")
	(net 123 "/FPGA/SDRAM_DQ10")
	(net 124 "/FPGA/SDRAM_DQ9")
	(net 125 "unconnected-(U1A-PL23C{slash}PCLKT7_0{slash}+{slash}LDQ20-PadK1)")
	(net 126 "/FPGA/JTAG1.TMS")
	(net 127 "/FPGA/SDRAM_x.mCS")
	(net 128 "/FPGA/FLASH.IO2")
	(net 129 "unconnected-(U1F-PT51B{slash}--PadE11)")
	(net 130 "/FPGA/SDRAM_DQM0")
	(net 131 "unconnected-(U1G-PT20A{slash}+-PadE6)")
	(net 132 "/FPGA/SDRAM_x.CLK")
	(net 133 "/FPGA/SDRAM_BA0")
	(net 134 "/FPGA/FLASH.CS")
	(net 135 "/FPGA/JTAG2.TDO")
	(net 136 "unconnected-(J8-Pad7)")
	(net 137 "/FPGA/SDRAM_A3")
	(net 138 "/FPGA/SDRAM_DQ5")
	(net 139 "/FPGA/SDRAM_DQ3")
	(net 140 "unconnected-(U1E-PR2C{slash}+{slash}RDQ8-PadC14)")
	(net 141 "/FPGA/JTAG2.TDI")
	(net 142 "unconnected-(J12-Pad7)")
	(net 143 "unconnected-(U1G-PT24A{slash}GR_PCLK0_1{slash}+-PadE7)")
	(net 144 "Net-(U1C-PB6B{slash}D4{slash}MOSI2{slash}IO4{slash}-)")
	(net 145 "unconnected-(U1A-PL117C{slash}+{slash}LDQ20-PadJ4)")
	(net 146 "/FPGA/SDRAM_A6")
	(net 147 "/FPGA/SDRAM_A12")
	(net 148 "unconnected-(U1A-PL23D{slash}PCLKC7_0{slash}-{slash}LDQ20-PadK2)")
	(net 149 "unconnected-(U1G-PT13A{slash}+-PadE5)")
	(net 150 "unconnected-(U1B-PL38B{slash}HS-{slash}LDQ44-PadP3)")
	(net 151 "/FPGA/JTAG2.TCK")
	(net 152 "/FPGA/SDRAM_A1")
	(net 153 "/FPGA/SDRAM_A8")
	(net 154 "Net-(U1C-PB4B{slash}D6{slash}IO6{slash}-)")
	(net 155 "/FPGA/UART1_RX")
	(net 156 "/FPGA/SDRAM_A9")
	(net 157 "/FPGA/SDRAM_DQ8")
	(net 158 "/FPGA/SDRAM_DQ1")
	(net 159 "/FPGA/FLASH.MOSI")
	(net 160 "unconnected-(U1G-PT9A{slash}+-PadE4)")
	(net 161 "/FPGA/SDRAM_DQ2")
	(net 162 "/FPGA/SDRAM_x.nWE")
	(net 163 "/VDIGIO_1P8_F")
	(net 164 "Net-(U2B-RX1A+)")
	(net 165 "/VANA_1P8_F")
	(net 166 "/VANA_1P8")
	(net 167 "Net-(T1-SECONDARY_DOT)")
	(net 168 "/RX1_ST+")
	(net 169 "/RX1_QD+")
	(net 170 "Net-(T1-SECONDARY)")
	(net 171 "Net-(U2B-RX1A-)")
	(net 172 "unconnected-(C74-Pad2)")
	(net 173 "Net-(U2B-RX1B+)")
	(net 174 "unconnected-(C75-Pad2)")
	(net 175 "/RX2_QD+")
	(net 176 "Net-(U2B-RX1B-)")
	(net 177 "Net-(U2C-RX2A+)")
	(net 178 "/RX1_ID-")
	(net 179 "/VANA_1P3")
	(net 180 "/RX2_ID-")
	(net 181 "/AD_TDI")
	(net 182 "Net-(T2-SECONDARY_DOT)")
	(net 183 "Net-(U1C-PB13B{slash}CS1N{slash}-)")
	(net 184 "/RX2_EN")
	(net 185 "/VANA_1P3_F")
	(net 186 "/RX1_DCLK-")
	(net 187 "/VSYN_1P3")
	(net 188 "/AD_TDO")
	(net 189 "/RX2_QD-")
	(net 190 "Net-(T2-SECONDARY)")
	(net 191 "unconnected-(U2G-VANA2_1P0-PadC6)")
	(net 192 "/FP_57")
	(net 193 "Net-(U2C-RX2A-)")
	(net 194 "/FP_53")
	(net 195 "Net-(U2C-RX2B+)")
	(net 196 "unconnected-(C78-Pad2)")
	(net 197 "/VSYN_1P3_F")
	(net 198 "unconnected-(C79-Pad2)")
	(net 199 "/I2C_SDA")
	(net 200 "/RX1_ID+")
	(net 201 "Net-(U2C-RX2B-)")
	(net 202 "/FP_124")
	(net 203 "/RX1_DCLK+")
	(net 204 "unconnected-(U2G-VANA1_1P0-PadC9)")
	(net 205 "Net-(C80-Pad2)")
	(net 206 "/FP_132")
	(net 207 "/RX2_ST+")
	(net 208 "Net-(C80-Pad1)")
	(net 209 "/RX2_ID+")
	(net 210 "/AD_~{RST}")
	(net 211 "/RX1_EN")
	(net 212 "Net-(U1C-PB18A{slash}WRITEN)")
	(net 213 "Net-(C81-Pad1)")
	(net 214 "/RX1_QD-")
	(net 215 "/RX1_ST-")
	(net 216 "Net-(C81-Pad2)")
	(net 217 "unconnected-(U2G-VTX1LO_1P0-PadH12)")
	(net 218 "/RX2_DCLK-")
	(net 219 "Net-(C82-Pad1)")
	(net 220 "unconnected-(U2G-VTX2LO_1P0-PadH3)")
	(net 221 "Net-(U2G-VDIG_0P9)")
	(net 222 "Net-(U2G-VRFLO2_1P0)")
	(net 223 "Net-(U2G-VRFLO1_1P0)")
	(net 224 "/RX2_ST-")
	(net 225 "Net-(C82-Pad2)")
	(net 226 "/RX2_DCLK+")
	(net 227 "/TX1_CLK_O+")
	(net 228 "Net-(U2G-VCLKVCO_1P0)")
	(net 229 "Net-(U2G-VAUXVCO_1P0)")
	(net 230 "Net-(U2G-VRX1LO_1P0)")
	(net 231 "Net-(U2G-VRX2LO_1P0)")
	(net 232 "GND")
	(net 233 "Net-(U2G-VCONV_1P0)")
	(net 234 "unconnected-(U4-NC-PadE2)")
	(net 235 "/FPGA/FLASH.MISO")
	(net 236 "/FPGA/FPGA_DONE")
	(net 237 "/FPGA/SDRAM_A10")
	(net 238 "/FPGA/SDRAM_DQ13")
	(net 239 "/FPGA/JTAG2.TMS")
	(net 240 "/FPGA/SDRAM_DQ15")
	(net 241 "/FPGA/SDRAM_A4")
	(net 242 "/FPGA/SDRAM_A5")
	(net 243 "/FPGA/UART1_TX")
	(net 244 "/FPGA/SDRAM_DQ0")
	(net 245 "/FPGA/SDRAM_BA1")
	(net 246 "/FPGA/SDRAM_A11")
	(net 247 "/FPGA/SDRAM_DQ6")
	(net 248 "/FPGA/SDRAM_DQM1")
	(net 249 "/FPGA/SDRAM_x.nCAS")
	(net 250 "/FPGA/LED_RUN")
	(net 251 "/FPGA/MCO")
	(net 252 "/FPGA/D_UART2_RX")
	(net 253 "/FPGA/D_UART2_TX")
	(net 254 "/FPGA/USB_ENUM")
	(net 255 "/TX2_ST+")
	(net 256 "/TX1_QD+")
	(net 257 "/TX1_ST-")
	(net 258 "/TX1_CLK_I+")
	(net 259 "/TX2_ID-")
	(net 260 "/TX2_CLK_O-")
	(net 261 "/TX1_ID-")
	(net 262 "/TX2_CLK_I-")
	(net 263 "/TX1_EN")
	(net 264 "/TX1_QD-")
	(net 265 "/TX2_ID+")
	(net 266 "/TX2_CLK_I+")
	(net 267 "/TX2_QD+")
	(net 268 "/TX1_CLK_I-")
	(net 269 "/TX2_CLK_O+")
	(net 270 "/TX1_CLK_O-")
	(net 271 "/TX2_EN")
	(net 272 "/TX1_ID+")
	(net 273 "/TX1_ST+")
	(net 274 "/TX2_QD-")
	(net 275 "/TX2_ST-")
	(net 276 "/I2C_SCL")
	(net 277 "/VDIG_1P0_F")
	(net 278 "/I2C_SEL")
	(net 279 "/FPGA/UART1_TX_FPGA")
	(net 280 "/FPGA/UART1_RX_FPGA")
	(net 281 "+1.8V")
	(net 282 "Net-(U6-Standby)")
	(net 283 "/FPGA/CLK_25MHz")
	(net 284 "Net-(Q1-B)")
	(net 285 "Net-(U17-OE)")
	(net 286 "/FPGA/sJTAG2_TDO")
	(net 287 "/FPGA/sJTAG2_TMS")
	(net 288 "/FPGA/sJTAG2_CLK")
	(net 289 "/FPGA/sJTAG2_TDI")
	(net 290 "Net-(U10-SCL)")
	(net 291 "Net-(Q1-C)")
	(net 292 "Net-(U10-A0)")
	(net 293 "unconnected-(U7-ALERT-Pad8)")
	(net 294 "/Power Supply/V_1P3")
	(net 295 "Net-(U13-SDA)")
	(net 296 "Net-(U13-A0)")
	(net 297 "/Power Supply/V_1P8")
	(net 298 "/Power Supply/V_1P0")
	(net 299 "Net-(U1C-PB15B{slash}DOUT{slash}CS0N{slash}-)")
	(net 300 "unconnected-(U10-ALERT-Pad8)")
	(net 301 "unconnected-(U11-ALERT-Pad8)")
	(net 302 "Net-(U1C-PB6A{slash}D5{slash}MISO2{slash}IO5{slash}+)")
	(net 303 "unconnected-(U12-ALERT-Pad8)")
	(net 304 "unconnected-(U13-ALERT-Pad8)")
	(net 305 "unconnected-(U14-ALERT-Pad8)")
	(net 306 "unconnected-(U15-ALERT-Pad8)")
	(net 307 "unconnected-(U16-ALERT-Pad8)")
	(net 308 "Net-(U1C-PB13A{slash}SN{slash}CSN{slash}+)")
	(net 309 "Net-(U1C-PB4A{slash}D7{slash}IO7{slash}+)")
	(net 310 "Net-(U18-OE)")
	(net 311 "Net-(C83-Pad2)")
	(net 312 "Net-(C83-Pad1)")
	(net 313 "Net-(U2F-DEV_CLK_IN+)")
	(net 314 "/SFL_BPFS_1V8")
	(net 315 "Net-(U2F-DEV_CLK_IN-)")
	(net 316 "/RX_PATH_DISABLE_1V8")
	(net 317 "Net-(U2D-TX1+)")
	(net 318 "Net-(U2D-TX1-)")
	(net 319 "Net-(U2E-TX2+)")
	(net 320 "Net-(U2E-TX2-)")
	(net 321 "Net-(U2F-EXT_LO2-)")
	(net 322 "Net-(U2F-EXT_LO2+)")
	(net 323 "Net-(U2F-EXT_LO1+)")
	(net 324 "Net-(U2F-EXT_LO1-)")
	(net 325 "Net-(U2F-MCS+)")
	(net 326 "Net-(U2F-MCS-)")
	(net 327 "Net-(U2A-RBIAS)")
	(net 328 "unconnected-(T1-NC-Pad1)")
	(net 329 "unconnected-(T2-NC-Pad1)")
	(net 330 "Net-(J3-RF)")
	(net 331 "Net-(U2F-DEV_CLK_OUT)")
	(net 332 "unconnected-(T3-Pad2)")
	(net 333 "unconnected-(T4-Pad2)")
	(net 334 "Net-(J4-RF)")
	(net 335 "Net-(Q2-C)")
	(net 336 "Net-(Q2-B)")
	(net 337 "Net-(Q3-B)")
	(net 338 "Net-(Q3-C)")
	(net 339 "Net-(Q4-C)")
	(net 340 "Net-(Q4-B)")
	(net 341 "/FPGA/F_LED_B")
	(net 342 "/FPGA/F_LED_G")
	(net 343 "/FPGA/F_LED_R")
	(net 344 "Net-(D1-RK)")
	(net 345 "Net-(D1-GK)")
	(net 346 "Net-(D1-BK)")
	(net 347 "/AG_03")
	(net 348 "Net-(U24-FB)")
	(net 349 "Net-(U22-EN)")
	(net 350 "/Power Supply/adp5056_1P8V")
	(net 351 "Net-(U22-FB)")
	(net 352 "Net-(U8-FB)")
	(net 353 "/Power Supply/adp5056_1P0V")
	(net 354 "/Power Supply/adp5056_1P3V")
	(net 355 "Net-(U25-VREG)")
	(net 356 "Net-(U25-PVIN3)")
	(net 357 "Net-(C158-Pad2)")
	(net 358 "Net-(C159-Pad2)")
	(net 359 "Net-(C160-Pad2)")
	(net 360 "Net-(U25-BST1)")
	(net 361 "Net-(C161-Pad2)")
	(net 362 "Net-(U25-BST2)")
	(net 363 "Net-(C162-Pad1)")
	(net 364 "Net-(U25-SW3)")
	(net 365 "Net-(U25-BST3)")
	(net 366 "Net-(U25-FB1)")
	(net 367 "Net-(U25-FB2)")
	(net 368 "Net-(U25-FB3)")
	(net 369 "Net-(U23-FB)")
	(net 370 "/Power Supply/ALT_1P8")
	(net 371 "Net-(U8-LX)")
	(net 372 "Net-(U22-LX)")
	(net 373 "Net-(U24-LX)")
	(net 374 "Net-(U23-LX)")
	(net 375 "Net-(R44-Pad2)")
	(net 376 "Net-(R47-Pad2)")
	(net 377 "/Power Supply/PGOOD")
	(net 378 "Net-(U25-RAMP1)")
	(net 379 "Net-(U25-COMP1)")
	(net 380 "Net-(U25-RAMP2)")
	(net 381 "Net-(U25-COMP2)")
	(net 382 "Net-(U25-RAMP3)")
	(net 383 "Net-(U25-COMP3)")
	(net 384 "Net-(U25-EN1)")
	(net 385 "Net-(U25-EN2)")
	(net 386 "Net-(U25-EN3)")
	(net 387 "Net-(U25-CFG1)")
	(net 388 "Net-(U25-CFG2)")
	(net 389 "Net-(U25-RT)")
	(net 390 "unconnected-(U8-PG-Pad5)")
	(net 391 "unconnected-(U22-PG-Pad5)")
	(net 392 "unconnected-(U23-PG-Pad5)")
	(net 393 "unconnected-(U24-PG-Pad5)")
	(net 394 "unconnected-(U25-SYNC{slash}MODE-Pad11)")
	(net 395 "/AG_02")
	(net 396 "Net-(U2A-MODE)")
	(net 397 "Net-(U2A-MODEA)")
	(net 398 "Net-(Q5-C)")
	(net 399 "Net-(Q5-B)")
	(net 400 "Net-(U1H-CFG_2)")
	(net 401 "Net-(U1H-CFG_0)")
	(net 402 "Net-(C145-Pad2)")
	(net 403 "Net-(C146-Pad2)")
	(net 404 "Net-(C147-Pad2)")
	(net 405 "/AG_00")
	(net 406 "/AG_10")
	(net 407 "/AG_06")
	(net 408 "/AG_08")
	(net 409 "/AG_11")
	(net 410 "/AG_07")
	(net 411 "/AG_09")
	(net 412 "/ADC_3")
	(net 413 "/ADC_0")
	(net 414 "/ADC_2")
	(net 415 "/ADC_1")
	(net 416 "/DG_01")
	(net 417 "/DG_02")
	(net 418 "/DG_00")
	(net 419 "/DG_09")
	(net 420 "/DG_10")
	(net 421 "/DG_11")
	(net 422 "/DG_08")
	(net 423 "/AG_05")
	(net 424 "/AG_04")
	(net 425 "/AG_01")
	(net 426 "unconnected-(T3-Pad5)")
	(net 427 "unconnected-(T4-Pad5)")
	(net 428 "Net-(Z1-K)")
	(net 429 "Net-(D3-A)")
	(net 430 "Net-(Q6-G)")
	(net 431 "/{slash}CS_EXPANDER_1V8")
	(net 432 "/Power Supply/Vin")
	(net 433 "/FPGA/PR47B")
	(net 434 "/FPGA/PR47D")
	(net 435 "/FPGA/PR47C")
	(net 436 "/FPGA/PR44D")
	(net 437 "/FPGA/PR41A")
	(net 438 "/FPGA/PR38A")
	(net 439 "/FPGA/PR44C")
	(net 440 "/FPGA/PR38B")
	(net 441 "/FPGA/PR35C")
	(net 442 "/FPGA/PR32D")
	(net 443 "/FPGA/PR32C")
	(net 444 "/FPGA/PR29C")
	(net 445 "/FPGA/PR29D")
	(net 446 "/FPGA/PR29B")
	(net 447 "/FPGA/PR29A")
	(net 448 "unconnected-(U1D-PR47A{slash}HS+{slash}RDQ44-PadM11)")
	(net 449 "/FPGA/PR17B")
	(net 450 "/FPGA/PR14D")
	(net 451 "/FPGA/PR17A")
	(net 452 "/FPGA/PR11B")
	(net 453 "/FPGA/PR14C")
	(net 454 "/FPGA/PR8C")
	(net 455 "/FPGA/PR11A")
	(net 456 "/FPGA/PR5D")
	(net 457 "/FPGA/PR5C")
	(net 458 "/FPGA/PR8D")
	(net 459 "/FP_121")
	(net 460 "/FP_133")
	(net 461 "/FP_125")
	(net 462 "/FP_130")
	(net 463 "/FP_131")
	(net 464 "/FP_120")
	(net 465 "/FP_05")
	(net 466 "/FP_123")
	(net 467 "Net-(U2A-SPI_CLK)")
	(net 468 "Net-(U2A-SPI_DIO)")
	(net 469 "Net-(U2A-SPI_DO)")
	(net 470 "Net-(U2A-SPI_EN)")
	(net 471 "/SPI2x.CLK")
	(net 472 "/SPI2x.MOSI")
	(net 473 "/SPI2x.MISO")
	(net 474 "/SPI2x.CE")
	(net 475 "/RX_ATTEN_LE_1V8")
	(net 476 "unconnected-(JSDB2-Pad16)")
	(net 477 "unconnected-(JSDB2-Pad18)")
	(net 478 "unconnected-(JSDB2-Pad13)")
	(net 479 "unconnected-(JSDB2-Pad14)")
	(net 480 "unconnected-(JSDB2-Pad15)")
	(net 481 "unconnected-(JSDB2-Pad12)")
	(net 482 "unconnected-(JSDB2-Pad7)")
	(net 483 "unconnected-(JSDB2-Pad17)")
	(net 484 "unconnected-(JSDB2-Pad11)")
	(net 485 "unconnected-(JSDB2-Pad10)")
	(net 486 "unconnected-(JSDB3-Pad9)")
	(net 487 "/AGPIO_1")
	(net 488 "unconnected-(JSDB3-Pad11)")
	(net 489 "unconnected-(JSDB3-Pad7)")
	(net 490 "/DGPIO_0_1P8_THRU")
	(net 491 "/SCLK_RX_PATH_1V8")
	(net 492 "unconnected-(JSDB3-Pad13)")
	(net 493 "/NDB_RESET_1P8")
	(net 494 "/NDB_FMC_INT_1P8")
	(net 495 "unconnected-(JSDB4-Pin_26-Pad26)")
	(net 496 "/MUX{slash}CS_1V8")
	(net 497 "unconnected-(JSDB4-Pin_29-Pad29)")
	(net 498 "unconnected-(JSDB4-Pin_30-Pad30)")
	(net 499 "/nTOP_PTT_1P8")
	(net 500 "/DGPIO_2_1P8_THRU")
	(net 501 "unconnected-(JSDB4-Pin_25-Pad25)")
	(net 502 "unconnected-(JSDB4-Pin_27-Pad27)")
	(net 503 "/MISO_BPFS_1V8")
	(net 504 "/NDB_FMCA_SDA_1P8")
	(net 505 "unconnected-(JSDB4-Pin_28-Pad28)")
	(net 506 "/RX{slash}RESET_1V8")
	(net 507 "/RF_TX_SPI_DI_1P8")
	(net 508 "/RF_TX_SPI_DO_1P8")
	(net 509 "/RF_READY")
	(net 510 "/RF_RX_SPI_CLK_1P8")
	(net 511 "/RF_RX_SPI_DI_1P8")
	(net 512 "/DGPIO_1_1P8_THRU")
	(net 513 "/RF_RX_SPI_CS_1P8")
	(net 514 "/RF_TX_SPI_CS_1P8")
	(net 515 "unconnected-(JSDB5-Pin_29-Pad29)")
	(net 516 "/DGPIO_3_1P8_THRU")
	(net 517 "/RF_RX_SPI_DO_1P8")
	(net 518 "/RF_TX_SPI_CLK_1P8")
	(net 519 "Net-(X3-OUT)")
	(net 520 "Net-(X3-OE)")
	(net 521 "Net-(T1-PRIMARY_DOT)")
	(net 522 "Net-(T4-Pad4)")
	(net 523 "/DGPIO_4_1P8_THRU")
	(net 524 "/MOSI_RX_PATH_1V8")
	(net 525 "/MOSI_HARM_FLT_1V8")
	(net 526 "/MISO_HARM_FLT_1V8")
	(net 527 "/{slash}CS_HARM_FILT_EXPANDER_1V8")
	(net 528 "/TX_ATTEN_LE_1V8")
	(net 529 "/DGPIO_9_1P8_THRU")
	(net 530 "/MOSI_TX_BOARD_1V8")
	(net 531 "/DGPIO_11_1P8_THRU")
	(net 532 "/DGPIO_10_1P8_THRU")
	(net 533 "/SCLK_TX_BOARD_1V8")
	(net 534 "/DGPIO_8_1P8_THRU")
	(net 535 "/NDB_FMCA_SCL_1P8")
	(net 536 "/+12V")
	(net 537 "/DGPIO_6_1P8_THRU")
	(net 538 "/DGPIO_5_1P8_THRU")
	(net 539 "/DGPIO_7_1P8_THRU")
	(net 540 "Net-(K1B-P6_0)")
	(net 541 "Net-(K1B-P6_1)")
	(net 542 "Net-(K1B-P6_5)")
	(net 543 "Net-(K1B-P6_2)")
	(net 544 "Net-(K1B-P6_3)")
	(net 545 "unconnected-(SW2-Pad1)")
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 112.7252 85.307 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R36"
			(at -2.0828 0.2032 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 336 "Net-(Q2-B)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 341 "/FPGA/F_LED_B")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 129.159 65.4696 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R5"
			(at -2.3876 0.1778 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "/FPGA/FPGA_nPROG")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 107.0102 85.7134)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R39"
			(at -0.0254 -1.0668 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 335 "Net-(Q2-C)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 344 "Net-(D1-RK)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 144.0434 60.8136 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R68"
			(at -1.9226 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 467 "Net-(U2A-SPI_CLK)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/SPI2.CLK")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_Mini_Circuits:DB1627_MNC"
		(layer "F.Cu")
		(at 163.576 86.6913 90)
		(tags "TCM2-33X+ ")
		(property "Reference" "T1"
			(at 2.7813 2.921 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCM2-33X+"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_Mini_Circuits:DB1627_MNC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/TCM2-33WX+.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RF Transformer 10 to 3000 MHz"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB1627_MNC")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -3.302 1.27 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 -90)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -3.302 1.27 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5875 1.27 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 328 "unconnected-(T1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "2" smd rect
			(at -1.5875 0 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "PRIMARY/GND")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -1.5875 -1.27 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 170 "Net-(T1-SECONDARY)")
			(pinfunction "SECONDARY")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.5875 -1.27 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 167 "Net-(T1-SECONDARY_DOT)")
			(pinfunction "SECONDARY_DOT")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 1.5875 0 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 1.5875 1.27 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 521 "Net-(T1-PRIMARY_DOT)")
			(pinfunction "PRIMARY_DOT")
			(pintype "unspecified")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 154.559 157.57)
		(property "Reference" "TP19"
			(at 0 2.54 -90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 518 "/RF_TX_SPI_CLK_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 106.9252 90.9204)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R40"
			(at -0.0166 1.0414 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 338 "Net-(Q3-C)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 345 "Net-(D1-GK)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 126.365 99.2008)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x1"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 396 "Net-(U2A-MODE)")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "2")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 194.183 76.671 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R114"
			(at 0 -1.27 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 496 "/MUX{slash}CS_1V8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 192 "/FP_57")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_switch:Switch_PB_6_5mm"
		(layer "F.Cu")
		(at 91.013 96.388 90)
		(property "Reference" "SW1"
			(at -1.778 4.191 -90)
			(layer "F.SilkS")
		)
		(property "Value" "SWITCH_PB"
			(at 0 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_switch:Switch_PB_6_5mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 2.875 2 90)
			(size 2.75 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "/FPGA/FPGA_nPROG")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.875 2 90)
			(size 2.75 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "/FPGA/FPGA_nPROG")
			(pinfunction "x")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.875 -2 90)
			(size 2.75 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.875 -2 90)
			(size 2.75 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "x")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_switch/PB_Switch_6_2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 161.6964 74.0294)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R24"
			(at 1.9812 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 321 "Net-(U2F-EXT_LO2-)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 135.255 94.1208 90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "P2"
			(at -0.0508 -2.667 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X04"
			(at 0 9.95 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X04 Pin_Header_Angled_1X04 Socket_Strip_Straight_1X04 Socket_Strip_Angled_1X04")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 406 "/AG_10")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 419 "/DG_09")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 420 "/DG_10")
			(pinfunction "P4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_qfn:WSON8-8x6"
		(layer "F.Cu")
		(at 135.5598 58.8148 90)
		(property "Reference" "U3"
			(at -2.9718 5.6388 0)
			(layer "F.SilkS")
		)
		(property "Value" "W25Q256JW"
			(at 0 -1 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_qfn:WSON8-8x6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.winbond.com/resource-files/w25q256jv%20spi%20revg%2008032017.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32 MBit SPI FLASH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.3 0.2 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.905 3.8 90)
			(size 0.5 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "/FPGA/FLASH.CS")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.635 3.8 90)
			(size 0.5 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 235 "/FPGA/FLASH.MISO")
			(pinfunction "MISO/IO1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at 0.635 3.8 90)
			(size 0.5 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "/FPGA/FLASH.IO2")
			(pinfunction "~{WP}/IO2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at 1.905 3.8 90)
			(size 0.5 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.91 -3.8 90)
			(size 0.5 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 159 "/FPGA/FLASH.MOSI")
			(pinfunction "MOSI/IO0")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at 0.64 -3.8 90)
			(size 0.5 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "/FPGA/FLASH.CLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -0.63 -3.8 90)
			(size 0.5 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "/FPGA/FLASH.IO3")
			(pinfunction "~{HOLD}/IO3")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -1.9 -3.8 90)
			(size 0.5 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 0 0 90)
			(size 4.2 3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_qfn/WSON8-6x8.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 169.884 80.989 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R35"
			(at -0.381 0.889 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U21-TTL_IN)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:sot-23"
		(layer "F.Cu")
		(at 109.728 85.7134 180)
		(descr "SOT-23")
		(property "Reference" "Q2"
			(at -0.0254 2.159 180)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904"
			(at 0 0.0762 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 336 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 335 "Net-(Q2-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-3.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SSOP-8_TEX"
		(layer "F.Cu")
		(at 108.46435 102.741199)
		(tags "TCA9406")
		(property "Reference" "U9"
			(at -0.08255 -2.448199 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCA9406"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_sot:SSOP-8_TEX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9406.pdf?ts=1710769372418&ref_url=https%253A%252F%252Fwww.google.com%252F"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "I2C Level Translator"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.2 -1.55 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.2 -1.55 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 -0.974999)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 295 "Net-(U13-SDA)")
			(pinfunction "SDA_B")
			(pintype "open_collector")
		)
		(pad "2" smd rect
			(at -1.7 -0.325001)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.7 0.325001)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.7 0.974999)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 199 "/I2C_SDA")
			(pinfunction "SDA_A")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at 1.7 0.974999)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 276 "/I2C_SCL")
			(pinfunction "SCL_A")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.7 0.325001)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 278 "/I2C_SEL")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 1.7 -0.325001)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 1.7 -0.974999)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 296 "Net-(U13-A0)")
			(pinfunction "SCL_B")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.3 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 112.7164 87.1866 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R37"
			(at -2.117 -0.1778 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 337 "Net-(Q3-B)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 342 "/FPGA/F_LED_G")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 168.5748 71.5656 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J10"
			(at 2.413 3.7896 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x1"
			(at 0 4.87 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 397 "Net-(U2A-MODEA)")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "2")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_USB:AMPHENOL_12402012E212A"
		(layer "F.Cu")
		(at 97.157 50.3312 180)
		(property "Reference" "J1"
			(at 6.098 -3.5814 180)
			(layer "F.SilkS")
		)
		(property "Value" "12402012E212A"
			(at 9.175 -6.715 180)
			(layer "F.Fab")
		)
		(property "Footprint" "t_USB:AMPHENOL_12402012E212A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/2614/C12402012-4.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.26 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(pad "" np_thru_hole circle
			(at -2.89 -3.68 180)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -3.68 180)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1_B12" smd rect
			(at -3.2 -4.75 180)
			(size 0.6 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "A4_B9" smd rect
			(at -2.4 -4.75 180)
			(size 0.6 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 429 "Net-(D3-A)")
			(pinfunction "VBUS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "A5" smd rect
			(at -1.25 -4.75 180)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "Net-(J1-CC1_A)")
			(pinfunction "CC1_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A6" smd rect
			(at -0.25 -4.75 180)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "/FPGA/USB_P")
			(pinfunction "D+_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A7" smd rect
			(at 0.25 -4.75 180)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "/FPGA/USB_N")
			(pinfunction "D-_A")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "A8" smd rect
			(at 1.25 -4.75 180)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "B1_A12" smd rect
			(at 3.2 -4.75 180)
			(size 0.6 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "B4_A9" smd rect
			(at 2.4 -4.75 180)
			(size 0.6 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 429 "Net-(D3-A)")
			(pinfunction "VBUS__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "B5" smd rect
			(at 1.75 -4.75 180)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "Net-(J1-CC1_B)")
			(pinfunction "CC1_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B6" smd rect
			(at 0.75 -4.75 180)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "/FPGA/USB_P")
			(pinfunction "D+_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B7" smd rect
			(at -0.75 -4.75 180)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "/FPGA/USB_N")
			(pinfunction "D-_B")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "B8" smd rect
			(at -1.75 -4.75 180)
			(size 0.3 1.14)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "SH1" thru_hole oval
			(at -4.32 -4.18 180)
			(size 1.05 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "SH2" thru_hole oval
			(at 4.32 -4.18 180)
			(size 1.05 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "SHIELD__1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "SH3" thru_hole oval
			(at -4.32 0 180)
			(size 0.9 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "SHIELD__2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "SH4" thru_hole oval
			(at 4.32 0 180)
			(size 0.9 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "SHIELD__3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "${T_LIBS}/3d/t_USB/12402012E212A.step"
			(offset
				(xyz 40 2.25 1.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 117.1194 64.3774)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R7"
			(at -1.7272 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "Net-(U5-BOOT0)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_Mini_Circuits:DB1627_MNC"
		(layer "F.Cu")
		(at 158.6992 60.9484)
		(tags "TCM2-33X+ ")
		(property "Reference" "T4"
			(at 3.3528 -2.4384 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TC1-1-13MX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_Mini_Circuits:DB1627_MNC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5875 1.27)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 225 "Net-(C82-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.5875 0)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 333 "unconnected-(T4-Pad2)")
			(pinfunction "2")
			(pintype "input+no_connect")
		)
		(pad "3" smd rect
			(at -1.5875 -1.27)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 311 "Net-(C83-Pad2)")
			(pinfunction "3")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 1.5875 -1.27)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 522 "Net-(T4-Pad4)")
			(pinfunction "4")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 1.5875 0)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 427 "unconnected-(T4-Pad5)")
			(pinfunction "5")
			(pintype "no_connect")
		)
		(pad "6" smd rect
			(at 1.5875 1.27)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "6")
			(pintype "input")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 81.026 157.697)
		(property "Reference" "TP15"
			(at 0 2.667 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/FP_83")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 161.6964 71.9974 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C78"
			(at -1.8796 0.1524 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 195 "Net-(U2C-RX2B+)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 196 "unconnected-(C78-Pad2)")
			(pintype "passive+no_connect")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 199.644 62.193 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R31"
			(at -0.127 -1.143 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 475 "/RX_ATTEN_LE_1V8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 542 "Net-(K1B-P6_5)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 84.455 98.388)
		(property "Reference" "TP8"
			(at 3.175 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 142.24 86.323)
		(property "Reference" "TP4"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 88.646 142.33)
		(property "Reference" "TP27"
			(at 0 -2.286 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 499 "/nTOP_PTT_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 105.029 102.3378 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R23"
			(at 2.5274 0.0508 -90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 0.9652 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 291 "Net-(Q1-C)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 161.671 76.2392)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R28"
			(at 2.032 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 325 "Net-(U2F-MCS+)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 86.6648 90.2854 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R20"
			(at -3.0988 0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.02 Ohms"
			(at 0 0.9652 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "+5.0V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 432 "/Power Supply/Vin")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 113.8466 120.7008 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C163"
			(at -2.46 -0.0138 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 365 "Net-(U25-BST3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 364 "Net-(U25-SW3)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 88.9 72.353)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J20"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 435 "/FPGA/PR47C")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 440 "/FPGA/PR38B")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 445 "/FPGA/PR29D")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 451 "/FPGA/PR17A")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 456 "/FPGA/PR5D")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 209.338 79.211 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R104"
			(at -0.466 1.143 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 544 "Net-(K1B-P6_3)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 527 "/{slash}CS_HARM_FILT_EXPANDER_1V8")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:sot-23"
		(layer "F.Cu")
		(at 102.63124 102.6679 -90)
		(descr "SOT-23")
		(property "Reference" "Q1"
			(at -2.3749 -0.16256 180)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904"
			(at 0 0.0762 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 284 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.9525 1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1.05664 270)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 291 "Net-(Q1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-3.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 75.565 67.273)
		(property "Reference" "TP5"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 114.5286 50.9916 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -2.3876 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED_RED"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LED_GREEN"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 98 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 113.8632 119.5578)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C162"
			(at 2.4434 -0.037 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 363 "Net-(C162-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 362 "Net-(U25-BST2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 128.0414 65.495 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R6"
			(at -2.3876 0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "Net-(U1H-CFG_1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 113.8466 121.8438 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C161"
			(at -2.4346 0.0116 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 360 "Net-(U25-BST1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 361 "Net-(C161-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 162.179 142.457)
		(property "Reference" "TP28"
			(at 0 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 509 "/RF_READY")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_connectors:Banana_Horiz_Red"
		(layer "F.Cu")
		(at 69.27 79.553 180)
		(property "Reference" "J16"
			(at 8.945 5.803 180)
			(layer "F.SilkS")
		)
		(property "Value" "BANANA_JACK"
			(at 0 -0.5 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_connectors:Banana_Horiz_Red"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 7.6454 0 180)
			(size 3.048 3.048)
			(drill 2.032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(F1-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.6454 0 180)
			(size 3.048 3.048)
			(drill 2.032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(F1-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_connectors/AB2_90DEG_4MM_JACK_PTH-RED.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.394 0.394 0.394)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${T_LIBS}/3d/t_connectors/DELTRON_RED.STEP"
			(offset
				(xyz 7.8 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "t_LED:LED_Cree_PLCC6_3.4x3.4mm"
		(layer "F.Cu")
		(at 103.3272 89.244 180)
		(tags "LED Cree PLCC-6 CLX6F-FKC")
		(property "Reference" "D1"
			(at 0 -2.75 180)
			(layer "F.Fab")
		)
		(property "Value" "LED_RGB"
			(at 0 2.75 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_LED:LED_Cree_PLCC6_3.4x3.4mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DNP" "YES"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Cree"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFN" "CLX6F-FKC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.55 -1 180)
			(size 1.2 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 344 "Net-(D1-RK)")
			(pinfunction "RK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.55 0 180)
			(size 1.2 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 345 "Net-(D1-GK)")
			(pinfunction "GK")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.55 1 180)
			(size 1.2 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 346 "Net-(D1-BK)")
			(pinfunction "BK")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.55 1 180)
			(size 1.2 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pinfunction "BA")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.55 0 180)
			(size 1.2 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pinfunction "GA")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.55 -1 180)
			(size 1.2 0.6)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pinfunction "RA")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_RGB_5050-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 0.6 0.6 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 103.6828 55.8596 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C28"
			(at -2.455 0.1524 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:sot-23"
		(layer "F.Cu")
		(at 109.728 88.4058 180)
		(descr "SOT-23")
		(property "Reference" "Q4"
			(at -2.5146 -0.254 180)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904"
			(at 0 0.0762 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 340 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 339 "Net-(Q4-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-3.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 156.3624 86.565 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C72"
			(at -1.8662 0.0508 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "Net-(U2B-RX1A+)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 170 "Net-(T1-SECONDARY)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:sot-23-5"
		(layer "F.Cu")
		(at 171.1325 77.39236 180)
		(descr "SOT-23")
		(property "Reference" "U21"
			(at 0.0254 -0.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "DSLVDS1001"
			(at 0 0.3302 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23-5"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/dslvds1001.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1711410112338"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Channel LVDS Driver"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at 0 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U21-OUT-)")
			(pinfunction "OUT-")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.9525 -1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U21-OUT+)")
			(pinfunction "OUT+")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.9525 -1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U21-TTL_IN)")
			(pinfunction "TTL_IN")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-5-2.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 77.1906 85.8912 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R65"
			(at -2.4892 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.9652 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 430 "Net-(Q6-G)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 207.264 79.169)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R112"
			(at -0.254 -1.101 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 544 "Net-(K1B-P6_3)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 431 "/{slash}CS_EXPANDER_1V8")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "hornet phase 2:SULLINS_SBH11-PBPC-D10-ST-BK"
		(layer "F.Cu")
		(at 219.456 144.108 90)
		(property "Reference" "JSDB3"
			(at 17.653 -2.921 0)
			(layer "F.SilkS")
		)
		(property "Value" "SBH11-PBPC-D10-ST-BK"
			(at 1.08 6.115 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "hornet phase 2:SULLINS_SBH11-PBPC-D10-ST-BK"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "J"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "9.4mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Sullins Connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -11.43 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -11.43 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -8.89 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 533 "/SCLK_TX_BOARD_1V8")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -8.89 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 530 "/MOSI_TX_BOARD_1V8")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at -6.35 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/FP_80")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at -6.35 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 528 "/TX_ATTEN_LE_1V8")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at -3.81 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 489 "unconnected-(JSDB3-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -3.81 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 281 "+1.8V")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at -1.27 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 486 "unconnected-(JSDB3-Pad9)")
			(pinfunction "9")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at -1.27 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at 1.27 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 488 "unconnected-(JSDB3-Pad11)")
			(pinfunction "11")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at 1.27 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 506 "/RX{slash}RESET_1V8")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at 3.81 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 492 "unconnected-(JSDB3-Pad13)")
			(pinfunction "13")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 3.81 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/FP_81")
			(pinfunction "14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 6.35 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 534 "/DGPIO_8_1P8_THRU")
			(pinfunction "15")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 6.35 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 529 "/DGPIO_9_1P8_THRU")
			(pinfunction "16")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at 8.89 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 532 "/DGPIO_10_1P8_THRU")
			(pinfunction "17")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at 8.89 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 531 "/DGPIO_11_1P8_THRU")
			(pinfunction "18")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at 11.43 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at 11.43 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "C:/Users/yh5034/Desktop/hornet phase 2/SBH11-PBPC-D10-ST-BK.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_misc:SMT_PAD_40"
		(layer "F.Cu")
		(at 120.65 54.446)
		(property "Reference" "TP2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEST_POINT"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_misc:SMT_PAD_40"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 253 "/FPGA/D_UART2_TX")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 152.019 157.57)
		(property "Reference" "TP18"
			(at 0 2.667 -90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 514 "/RF_TX_SPI_CS_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 85.09 72.353)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "P8"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X04"
			(at 0 9.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X04 Pin_Header_Angled_1X04 Socket_Strip_Straight_1X04 Socket_Strip_Angled_1X04")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_Mini_Circuits:DB1627_MNC"
		(layer "F.Cu")
		(at 163.449 66.6634 90)
		(tags "TCM2-33X+ ")
		(property "Reference" "T2"
			(at 2.9464 2.667 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCM2-33X+"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_Mini_Circuits:DB1627_MNC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/TCM2-33WX+.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RF Transformer 10 to 3000 MHz"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DB1627_MNC")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -3.302 1.27 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 -90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -3.302 1.27 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5875 1.27 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 329 "unconnected-(T2-NC-Pad1)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "2" smd rect
			(at -1.5875 0 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "PRIMARY/GND")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -1.5875 -1.27 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 190 "Net-(T2-SECONDARY)")
			(pinfunction "SECONDARY")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.5875 -1.27 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 182 "Net-(T2-SECONDARY_DOT)")
			(pinfunction "SECONDARY_DOT")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 1.5875 0 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 1.5875 1.27 90)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 330 "Net-(J3-RF)")
			(pinfunction "PRIMARY_DOT")
			(pintype "unspecified")
		)
	)
	(footprint "t_coilcraft:ind_0603cs"
		(layer "F.Cu")
		(at 154.7114 66.7054 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "L5"
			(at -0.1358 1.1684 -90)
			(layer "F.SilkS")
		)
		(property "Value" "220nH"
			(at 0 0.6096 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:ind_0603cs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 319 "Net-(U2E-TX2+)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-0603CS.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 169.164 86.45 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R99"
			(at 1.397001 -1.016001 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.381 0.127 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 520 "Net-(X3-OE)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 96.52 72.353)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J19"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 434 "/FPGA/PR47D")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 439 "/FPGA/PR44C")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 444 "/FPGA/PR29C")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 450 "/FPGA/PR14D")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 455 "/FPGA/PR11A")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 120.5572 58.7894 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C1"
			(at -1.7692 -0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "/FPGA/STM_~{RST}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "F.Cu")
		(at 125.857 58.5608 180)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C45"
			(at -1.7526 -0.1016 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 0.5 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 180)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "+1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 180)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 113.7158 53.7768 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R60"
			(at 0.042 1.0414 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 98 "Net-(D2-A)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 250 "/FPGA/LED_RUN")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 150.495 101.7408 90)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "P5"
			(at 0.0254 20.3708 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X08"
			(at 0 20.11 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X08 Pin_Header_Angled_1X08 Socket_Strip_Straight_1X08 Socket_Strip_Angled_1X08")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/AD_TMS")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/AD_TCLK")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 188 "/AD_TDO")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 181 "/AD_TDI")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 210 "/AD_~{RST}")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 421 "/DG_11")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 103.9368 50.213 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R61"
			(at -0.55 -1.0922 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 310 "Net-(U18-OE)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 172.212 80.989 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C90"
			(at 0 -1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(C90-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U21-TTL_IN)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 169.037 91.276 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C22"
			(at 0 -1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 165.5572 75.1724 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C88"
			(at 1.397 0.2286 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U21-OUT-)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 313 "Net-(U2F-DEV_CLK_IN+)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 149.9362 91.911)
		(property "Reference" "TP1"
			(at -1.9304 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 331 "Net-(U2F-DEV_CLK_OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "hornet phase 2:SULLINS_SBH11-PBPC-D10-ST-BK"
		(layer "F.Cu")
		(at 220.091 72.861 90)
		(property "Reference" "JSDB2"
			(at -18.542 -1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "SBH11-PBPC-D10-ST-BK"
			(at 1.08 6.115 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "hornet phase 2:SULLINS_SBH11-PBPC-D10-ST-BK"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "J"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "9.4mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Sullins Connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -11.43 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -11.43 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -8.89 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/SCLK_HARM_FLT_1V8")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -8.89 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 525 "/MOSI_HARM_FLT_1V8")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at -6.35 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 526 "/MISO_HARM_FLT_1V8")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at -6.35 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 527 "/{slash}CS_HARM_FILT_EXPANDER_1V8")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at -3.81 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 482 "unconnected-(JSDB2-Pad7)")
			(pinfunction "7")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -3.81 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 281 "+1.8V")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at -1.27 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 506 "/RX{slash}RESET_1V8")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at -1.27 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 485 "unconnected-(JSDB2-Pad10)")
			(pinfunction "10")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at 1.27 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 484 "unconnected-(JSDB2-Pad11)")
			(pinfunction "11")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at 1.27 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 481 "unconnected-(JSDB2-Pad12)")
			(pinfunction "12")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at 3.81 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 478 "unconnected-(JSDB2-Pad13)")
			(pinfunction "13")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 3.81 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 479 "unconnected-(JSDB2-Pad14)")
			(pinfunction "14")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 6.35 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 480 "unconnected-(JSDB2-Pad15)")
			(pinfunction "15")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 6.35 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 476 "unconnected-(JSDB2-Pad16)")
			(pinfunction "16")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at 8.89 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 483 "unconnected-(JSDB2-Pad17)")
			(pinfunction "17")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at 8.89 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 477 "unconnected-(JSDB2-Pad18)")
			(pinfunction "18")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at 11.43 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at 11.43 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "C:/Users/yh5034/Desktop/hornet phase 2/SBH11-PBPC-D10-ST-BK.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 122.0978 60.5132 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C3"
			(at 0.0034 -1.1176 90)
			(layer "F.SilkS")
		)
		(property "Value" "20pF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U5-PD1)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_BGA:BC-196-16_ADI"
		(layer "F.Cu")
		(at 152.0124 76.9442 -90)
		(tags "ADRV9002BBCZ ")
		(property "Reference" "U2"
			(at -7.0296 -7.4996 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ADRV9002"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_BGA:BC-196-16_ADI"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adrv9002.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "14"
			(at 5.4926 -7.271 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "1"
			(at -5.2008 -6.8392 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "P"
			(at -6.6802 5.199999 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "A"
			(at -6.6802 -5.199999 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "A"
			(at -7.2582 -5.2898 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -5.7342 -7.1186 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "14"
			(at 5.3148 -7.3726 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "P"
			(at -7.055 5.3274 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A"
			(at -6.6802 -5.199999 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "14"
			(at 5.199999 -6.6802 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "P"
			(at -6.6802 5.199999 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at -5.199999 -6.6802 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -5.199999 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "A2" smd circle
			(at -4.399999 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "A3" smd circle
			(at -3.6 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 322 "Net-(U2F-EXT_LO2+)")
			(pinfunction "EXT_LO2+")
			(pintype "input")
		)
		(pad "A4" smd circle
			(at -2.8 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 321 "Net-(U2F-EXT_LO2-)")
			(pinfunction "EXT_LO2-")
			(pintype "input")
		)
		(pad "A5" smd circle
			(at -2 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "VRFVCO2_1P3")
			(pintype "power_in")
		)
		(pad "A6" smd circle
			(at -1.2 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 222 "Net-(U2G-VRFLO2_1P0)")
			(pinfunction "VRFLO2_1P0")
			(pintype "power_in")
		)
		(pad "A7" smd circle
			(at -0.4 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 397 "Net-(U2A-MODEA)")
			(pinfunction "MODEA")
			(pintype "input")
		)
		(pad "A8" smd circle
			(at 0.4 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 327 "Net-(U2A-RBIAS)")
			(pinfunction "RBIAS")
			(pintype "passive")
		)
		(pad "A9" smd circle
			(at 1.2 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 223 "Net-(U2G-VRFLO1_1P0)")
			(pinfunction "VRFLO1_1P0")
			(pintype "power_in")
		)
		(pad "A10" smd circle
			(at 2 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "VRFVCO1_1P3")
			(pintype "power_in")
		)
		(pad "A11" smd circle
			(at 2.8 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 324 "Net-(U2F-EXT_LO1-)")
			(pinfunction "EXT_LO1-")
			(pintype "input")
		)
		(pad "A12" smd circle
			(at 3.6 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 323 "Net-(U2F-EXT_LO1+)")
			(pinfunction "EXT_LO1+")
			(pintype "input")
		)
		(pad "A13" smd circle
			(at 4.4 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "A14" smd circle
			(at 5.199999 -5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B1" smd circle
			(at -5.199999 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 193 "Net-(U2C-RX2A-)")
			(pinfunction "RX2A-")
			(pintype "input")
		)
		(pad "B2" smd circle
			(at -4.399999 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B3" smd circle
			(at -3.6 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B4" smd circle
			(at -2.8 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B5" smd circle
			(at -2 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B6" smd circle
			(at -1.2 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 222 "Net-(U2G-VRFLO2_1P0)")
			(pinfunction "VRFVCO2_1P0")
			(pintype "power_in")
		)
		(pad "B7" smd circle
			(at -0.4 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 414 "/ADC_2")
			(pinfunction "AUXADC_2")
			(pintype "input")
		)
		(pad "B8" smd circle
			(at 0.4 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 415 "/ADC_1")
			(pinfunction "AUXADC_1")
			(pintype "input")
		)
		(pad "B9" smd circle
			(at 1.2 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 223 "Net-(U2G-VRFLO1_1P0)")
			(pinfunction "VRFVCO1_1P0")
			(pintype "power_in")
		)
		(pad "B10" smd circle
			(at 2 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B11" smd circle
			(at 2.8 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B12" smd circle
			(at 3.6 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B13" smd circle
			(at 4.4 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "B14" smd circle
			(at 5.199999 -4.399999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "Net-(U2B-RX1A-)")
			(pinfunction "RX1A-")
			(pintype "input")
		)
		(pad "C1" smd circle
			(at -5.199999 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 177 "Net-(U2C-RX2A+)")
			(pinfunction "RX2A+")
			(pintype "input")
		)
		(pad "C2" smd circle
			(at -4.399999 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "C3" smd circle
			(at -3.6 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 195 "Net-(U2C-RX2B+)")
			(pinfunction "RX2B+")
			(pintype "input")
		)
		(pad "C4" smd circle
			(at -2.8 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 201 "Net-(U2C-RX2B-)")
			(pinfunction "RX2B-")
			(pintype "input")
		)
		(pad "C5" smd circle
			(at -2 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "C6" smd circle
			(at -1.2 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 191 "unconnected-(U2G-VANA2_1P0-PadC6)")
			(pinfunction "VANA2_1P0")
			(pintype "power_in+no_connect")
		)
		(pad "C7" smd circle
			(at -0.4 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "VANA2_1P3")
			(pintype "power_in")
		)
		(pad "C8" smd circle
			(at 0.4 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "VANA1_1P3")
			(pintype "power_in")
		)
		(pad "C9" smd circle
			(at 1.2 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 204 "unconnected-(U2G-VANA1_1P0-PadC9)")
			(pinfunction "VANA1_1P0")
			(pintype "power_in+no_connect")
		)
		(pad "C10" smd circle
			(at 2 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "C11" smd circle
			(at 2.8 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 176 "Net-(U2B-RX1B-)")
			(pinfunction "RX1B-")
			(pintype "input")
		)
		(pad "C12" smd circle
			(at 3.6 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "Net-(U2B-RX1B+)")
			(pinfunction "RX1B+")
			(pintype "input")
		)
		(pad "C13" smd circle
			(at 4.4 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "C14" smd circle
			(at 5.199999 -3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 164 "Net-(U2B-RX1A+)")
			(pinfunction "RX1A+")
			(pintype "input")
		)
		(pad "D1" smd circle
			(at -5.199999 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D2" smd circle
			(at -4.399999 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D3" smd circle
			(at -3.6 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D4" smd circle
			(at -2.8 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D5" smd circle
			(at -2 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D6" smd circle
			(at -1.2 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D7" smd circle
			(at -0.4 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 325 "Net-(U2F-MCS+)")
			(pinfunction "MCS+")
			(pintype "input")
		)
		(pad "D8" smd circle
			(at 0.4 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 326 "Net-(U2F-MCS-)")
			(pinfunction "MCS-")
			(pintype "input")
		)
		(pad "D9" smd circle
			(at 1.2 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D10" smd circle
			(at 2 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D11" smd circle
			(at 2.8 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D12" smd circle
			(at 3.6 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D13" smd circle
			(at 4.4 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "D14" smd circle
			(at 5.199999 -2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "E1" smd circle
			(at -5.199999 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 231 "Net-(U2G-VRX2LO_1P0)")
			(pinfunction "VRX2LO_1P0")
			(pintype "power_in")
		)
		(pad "E2" smd circle
			(at -4.399999 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "VRX2LO_1P3")
			(pintype "power_in")
		)
		(pad "E3" smd circle
			(at -3.6 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 395 "/AG_02")
			(pinfunction "AGPIO_02")
			(pintype "passive")
		)
		(pad "E4" smd circle
			(at -2.8 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "VRFSYN2_1P3")
			(pintype "power_in")
		)
		(pad "E5" smd circle
			(at -2 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "VCLKSYN_1P3")
			(pintype "power_in")
		)
		(pad "E6" smd circle
			(at -1.2 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "E7" smd circle
			(at -0.4 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 313 "Net-(U2F-DEV_CLK_IN+)")
			(pinfunction "DEV_CLK_IN+")
			(pintype "input")
		)
		(pad "E8" smd circle
			(at 0.4 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "Net-(U2F-DEV_CLK_IN-)")
			(pinfunction "DEV_CLK_IN-")
			(pintype "input")
		)
		(pad "E9" smd circle
			(at 1.2 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "E10" smd circle
			(at 2 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "VAUXSYN_1P3")
			(pintype "power_in")
		)
		(pad "E11" smd circle
			(at 2.8 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "VRFSYN1_1P3")
			(pintype "power_in")
		)
		(pad "E12" smd circle
			(at 3.6 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 405 "/AG_00")
			(pinfunction "AGPIO_00")
			(pintype "passive")
		)
		(pad "E13" smd circle
			(at 4.4 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "VRX1LO_1P3")
			(pintype "power_in")
		)
		(pad "E14" smd circle
			(at 5.199999 -2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 230 "Net-(U2G-VRX1LO_1P0)")
			(pinfunction "VRX1LO_1P0")
			(pintype "power_in")
		)
		(pad "F1" smd circle
			(at -5.199999 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F2" smd circle
			(at -4.399999 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F3" smd circle
			(at -3.6 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F4" smd circle
			(at -2.8 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 424 "/AG_04")
			(pinfunction "AGPIO_04")
			(pintype "passive")
		)
		(pad "F5" smd circle
			(at -2 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 347 "/AG_03")
			(pinfunction "AGPIO_03")
			(pintype "passive")
		)
		(pad "F6" smd circle
			(at -1.2 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F7" smd circle
			(at -0.4 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F8" smd circle
			(at 0.4 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F9" smd circle
			(at 1.2 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F10" smd circle
			(at 2 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 425 "/AG_01")
			(pinfunction "AGPIO_01")
			(pintype "passive")
		)
		(pad "F11" smd circle
			(at 2.8 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 406 "/AG_10")
			(pinfunction "AGPIO_10")
			(pintype "passive")
		)
		(pad "F12" smd circle
			(at 3.6 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F13" smd circle
			(at 4.4 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "F14" smd circle
			(at 5.199999 -1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "G1" smd circle
			(at -5.199999 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 319 "Net-(U2E-TX2+)")
			(pinfunction "TX2+")
			(pintype "output")
		)
		(pad "G2" smd circle
			(at -4.399999 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "G3" smd circle
			(at -3.6 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "VTX2LO_1P3")
			(pintype "power_in")
		)
		(pad "G4" smd circle
			(at -2.8 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 423 "/AG_05")
			(pinfunction "AGPIO_05")
			(pintype "passive")
		)
		(pad "G5" smd circle
			(at -2 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "VCLKVCO_1P3")
			(pintype "power_in")
		)
		(pad "G6" smd circle
			(at -1.2 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 407 "/AG_06")
			(pinfunction "AGPIO_06")
			(pintype "passive")
		)
		(pad "G7" smd circle
			(at -0.4 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "VCONV_1P8")
			(pintype "power_in")
		)
		(pad "G8" smd circle
			(at 0.4 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "VAGPIO_1P8")
			(pintype "power_in")
		)
		(pad "G9" smd circle
			(at 1.2 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 408 "/AG_08")
			(pinfunction "AGPIO_08")
			(pintype "passive")
		)
		(pad "G10" smd circle
			(at 2 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "VAUXVCO_1P3")
			(pintype "power_in")
		)
		(pad "G11" smd circle
			(at 2.8 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 409 "/AG_11")
			(pinfunction "AGPIO_11")
			(pintype "passive")
		)
		(pad "G12" smd circle
			(at 3.6 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "VTX1LO_1P3")
			(pintype "power_in")
		)
		(pad "G13" smd circle
			(at 4.4 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "G14" smd circle
			(at 5.199999 -0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 317 "Net-(U2D-TX1+)")
			(pinfunction "TX1+")
			(pintype "output")
		)
		(pad "H1" smd circle
			(at -5.199999 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 320 "Net-(U2E-TX2-)")
			(pinfunction "TX2-")
			(pintype "output")
		)
		(pad "H2" smd circle
			(at -4.399999 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "VANA2_1P8")
			(pintype "power_in")
		)
		(pad "H3" smd circle
			(at -3.6 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 220 "unconnected-(U2G-VTX2LO_1P0-PadH3)")
			(pinfunction "VTX2LO_1P0")
			(pintype "power_in+no_connect")
		)
		(pad "H4" smd circle
			(at -2.8 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 412 "/ADC_3")
			(pinfunction "AUXADC_3")
			(pintype "input")
		)
		(pad "H5" smd circle
			(at -2 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 228 "Net-(U2G-VCLKVCO_1P0)")
			(pinfunction "VCLKVCO_1P0")
			(pintype "power_in")
		)
		(pad "H6" smd circle
			(at -1.2 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 410 "/AG_07")
			(pinfunction "AGPIO_07")
			(pintype "passive")
		)
		(pad "H7" smd circle
			(at -0.4 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 233 "Net-(U2G-VCONV_1P0)")
			(pinfunction "VCONV_1P0")
			(pintype "power_in")
		)
		(pad "H8" smd circle
			(at 0.4 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "VCONV_1P3")
			(pintype "power_in")
		)
		(pad "H9" smd circle
			(at 1.2 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 411 "/AG_09")
			(pinfunction "AGPIO_09")
			(pintype "passive")
		)
		(pad "H10" smd circle
			(at 2 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 229 "Net-(U2G-VAUXVCO_1P0)")
			(pinfunction "VAUXVCO_1P0")
			(pintype "power_in")
		)
		(pad "H11" smd circle
			(at 2.8 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 413 "/ADC_0")
			(pinfunction "AUXADC_0")
			(pintype "input")
		)
		(pad "H12" smd circle
			(at 3.6 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 217 "unconnected-(U2G-VTX1LO_1P0-PadH12)")
			(pinfunction "VTX1LO_1P0")
			(pintype "power_in+no_connect")
		)
		(pad "H13" smd circle
			(at 4.4 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "VANA1_1P8")
			(pintype "power_in")
		)
		(pad "H14" smd circle
			(at 5.199999 0.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 318 "Net-(U2D-TX1-)")
			(pinfunction "TX1-")
			(pintype "output")
		)
		(pad "J1" smd circle
			(at -5.199999 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J2" smd circle
			(at -4.399999 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J3" smd circle
			(at -3.6 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J4" smd circle
			(at -2.8 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J5" smd circle
			(at -2 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J6" smd circle
			(at -1.2 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J7" smd circle
			(at -0.4 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J8" smd circle
			(at 0.4 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J9" smd circle
			(at 1.2 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J10" smd circle
			(at 2 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J11" smd circle
			(at 2.8 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J12" smd circle
			(at 3.6 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J13" smd circle
			(at 4.4 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "J14" smd circle
			(at 5.199999 1.2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "passive")
		)
		(pad "K1" smd circle
			(at -5.199999 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 467 "Net-(U2A-SPI_CLK)")
			(pinfunction "SPI_CLK")
			(pintype "input")
		)
		(pad "K2" smd circle
			(at -4.399999 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 468 "Net-(U2A-SPI_DIO)")
			(pinfunction "SPI_DIO")
			(pintype "bidirectional")
		)
		(pad "K3" smd circle
			(at -3.6 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 184 "/RX2_EN")
			(pinfunction "RX2_EN")
			(pintype "input")
		)
		(pad "K4" smd circle
			(at -2.8 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA/TESTCK+")
			(pintype "input")
		)
		(pad "K5" smd circle
			(at -2 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSA/TESTCK-")
			(pintype "input")
		)
		(pad "K6" smd circle
			(at -1.2 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 418 "/DG_00")
			(pinfunction "DGPIO_00")
			(pintype "passive")
		)
		(pad "K7" smd circle
			(at -0.4 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 416 "/DG_01")
			(pinfunction "DGPIO_01")
			(pintype "passive")
		)
		(pad "K8" smd circle
			(at 0.4 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 417 "/DG_02")
			(pinfunction "DGPIO_02")
			(pintype "passive")
		)
		(pad "K9" smd circle
			(at 1.2 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 188 "/AD_TDO")
			(pinfunction "DGPIO_03")
			(pintype "passive")
		)
		(pad "K10" smd circle
			(at 2 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 210 "/AD_~{RST}")
			(pinfunction "DGPIO_04")
			(pintype "passive")
		)
		(pad "K11" smd circle
			(at 2.8 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 181 "/AD_TDI")
			(pinfunction "DGPIO_05")
			(pintype "passive")
		)
		(pad "K12" smd circle
			(at 3.6 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "/RX1_EN")
			(pinfunction "RX1_EN")
			(pintype "input")
		)
		(pad "K13" smd circle
			(at 4.4 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 493 "/NDB_RESET_1P8")
			(pinfunction "RESETB")
			(pintype "input")
		)
		(pad "K14" smd circle
			(at 5.199999 2 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 494 "/NDB_FMC_INT_1P8")
			(pinfunction "GP_INT")
			(pintype "output")
		)
		(pad "L1" smd circle
			(at -5.199999 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 470 "Net-(U2A-SPI_EN)")
			(pinfunction "SPI_EN")
			(pintype "bidirectional")
		)
		(pad "L2" smd circle
			(at -4.399999 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 469 "Net-(U2A-SPI_DO)")
			(pinfunction "SPI_DO")
			(pintype "output")
		)
		(pad "L3" smd circle
			(at -3.6 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 271 "/TX2_EN")
			(pinfunction "TX2_EN")
			(pintype "input")
		)
		(pad "L4" smd circle
			(at -2.8 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "/AD_TMS")
			(pinfunction "DGPIO_06")
			(pintype "passive")
		)
		(pad "L5" smd circle
			(at -2 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/AD_TCLK")
			(pinfunction "DGPIO_07")
			(pintype "passive")
		)
		(pad "L6" smd circle
			(at -1.2 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 422 "/DG_08")
			(pinfunction "DGPIO_08")
			(pintype "passive")
		)
		(pad "L7" smd circle
			(at -0.4 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 277 "/VDIG_1P0_F")
			(pinfunction "VDIG_1P0")
			(pintype "power_in")
		)
		(pad "L8" smd circle
			(at 0.4 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 277 "/VDIG_1P0_F")
			(pinfunction "VDIG_1P0")
			(pintype "power_in")
		)
		(pad "L9" smd circle
			(at 1.2 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 419 "/DG_09")
			(pinfunction "DGPIO_09")
			(pintype "passive")
		)
		(pad "L10" smd circle
			(at 2 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 420 "/DG_10")
			(pinfunction "DGPIO_10")
			(pintype "passive")
		)
		(pad "L11" smd circle
			(at 2.8 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 421 "/DG_11")
			(pinfunction "DGPIO_11")
			(pintype "passive")
		)
		(pad "L12" smd circle
			(at 3.6 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 263 "/TX1_EN")
			(pinfunction "TX1_EN")
			(pintype "input")
		)
		(pad "L13" smd circle
			(at 4.4 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 396 "Net-(U2A-MODE)")
			(pinfunction "MODE")
			(pintype "input")
		)
		(pad "L14" smd circle
			(at 5.199999 2.8 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 331 "Net-(U2F-DEV_CLK_OUT)")
			(pinfunction "DEV_CLK_OUT")
			(pintype "output")
		)
		(pad "M1" smd circle
			(at -5.199999 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 180 "/RX2_ID-")
			(pinfunction "RX2_IDATA_OUT-")
			(pintype "output")
		)
		(pad "M2" smd circle
			(at -4.399999 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 209 "/RX2_ID+")
			(pinfunction "RX2_IDATA_OUT+")
			(pintype "output")
		)
		(pad "M3" smd circle
			(at -3.6 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 218 "/RX2_DCLK-")
			(pinfunction "RX2_DCLK_OUT-")
			(pintype "output")
		)
		(pad "M4" smd circle
			(at -2.8 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 226 "/RX2_DCLK+")
			(pinfunction "RX2_DCLK_OUT+")
			(pintype "output")
		)
		(pad "M5" smd circle
			(at -2 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 269 "/TX2_CLK_O+")
			(pinfunction "TX2_DCLK_OUT+")
			(pintype "output")
		)
		(pad "M6" smd circle
			(at -1.2 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 260 "/TX2_CLK_O-")
			(pinfunction "TX2_DCLK_OUT-")
			(pintype "output")
		)
		(pad "M7" smd circle
			(at -0.4 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 163 "/VDIGIO_1P8_F")
			(pinfunction "VDIGIO_1P8")
			(pintype "power_in")
		)
		(pad "M8" smd circle
			(at 0.4 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 221 "Net-(U2G-VDIG_0P9)")
			(pinfunction "VDIG_0P9")
			(pintype "power_in")
		)
		(pad "M9" smd circle
			(at 1.2 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 270 "/TX1_CLK_O-")
			(pinfunction "TX1_DCLK_OUT-")
			(pintype "output")
		)
		(pad "M10" smd circle
			(at 2 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 227 "/TX1_CLK_O+")
			(pinfunction "TX1_DCLK_OUT+")
			(pintype "output")
		)
		(pad "M11" smd circle
			(at 2.8 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 203 "/RX1_DCLK+")
			(pinfunction "RX1_DCLK_OUT+")
			(pintype "output")
		)
		(pad "M12" smd circle
			(at 3.6 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 186 "/RX1_DCLK-")
			(pinfunction "RX1_DCLK_OUT-")
			(pintype "output")
		)
		(pad "M13" smd circle
			(at 4.4 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 200 "/RX1_ID+")
			(pinfunction "RX1_IDATA_OUT+")
			(pintype "output")
		)
		(pad "M14" smd circle
			(at 5.199999 3.6 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 178 "/RX1_ID-")
			(pinfunction "RX1_IDATA_OUT-")
			(pintype "output")
		)
		(pad "N1" smd circle
			(at -5.199999 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 224 "/RX2_ST-")
			(pinfunction "RX2_STROBE_OUT-")
			(pintype "output")
		)
		(pad "N2" smd circle
			(at -4.399999 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 207 "/RX2_ST+")
			(pinfunction "RX2_STROBE_OUT+")
			(pintype "output")
		)
		(pad "N3" smd circle
			(at -3.6 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 189 "/RX2_QD-")
			(pinfunction "RX2_QDATA_OUT-")
			(pintype "output")
		)
		(pad "N4" smd circle
			(at -2.8 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 175 "/RX2_QD+")
			(pinfunction "RX2_QDATA_OUT+")
			(pintype "output")
		)
		(pad "N5" smd circle
			(at -2 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 266 "/TX2_CLK_I+")
			(pinfunction "TX2_DCLK_IN+")
			(pintype "input")
		)
		(pad "N6" smd circle
			(at -1.2 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 262 "/TX2_CLK_I-")
			(pinfunction "TX1_DCLK_IN-")
			(pintype "input")
		)
		(pad "N7" smd circle
			(at -0.4 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSD")
			(pintype "power_in")
		)
		(pad "N8" smd circle
			(at 0.4 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSD")
			(pintype "power_in")
		)
		(pad "N9" smd circle
			(at 1.2 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 268 "/TX1_CLK_I-")
			(pinfunction "TX1_DCLK_IN-")
			(pintype "input")
		)
		(pad "N10" smd circle
			(at 2 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 258 "/TX1_CLK_I+")
			(pinfunction "TX1_DCLK_IN+")
			(pintype "input")
		)
		(pad "N11" smd circle
			(at 2.8 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 169 "/RX1_QD+")
			(pinfunction "RX1_QDATA_OUT+")
			(pintype "output")
		)
		(pad "N12" smd circle
			(at 3.6 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 214 "/RX1_QD-")
			(pinfunction "RX1_QDATA_OUT-")
			(pintype "output")
		)
		(pad "N13" smd circle
			(at 4.4 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "/RX1_ST+")
			(pinfunction "RX1_STROBE_OUT+")
			(pintype "output")
		)
		(pad "N14" smd circle
			(at 5.199999 4.4 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 215 "/RX1_ST-")
			(pinfunction "RX1_STROBE_OUT-")
			(pintype "output")
		)
		(pad "P1" smd circle
			(at -5.199999 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSD")
			(pintype "power_in")
		)
		(pad "P2" smd circle
			(at -4.399999 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 255 "/TX2_ST+")
			(pinfunction "TX2_STROBE_IN+")
			(pintype "input")
		)
		(pad "P3" smd circle
			(at -3.6 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 275 "/TX2_ST-")
			(pinfunction "TX2_STROBE_IN-")
			(pintype "input")
		)
		(pad "P4" smd circle
			(at -2.8 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 274 "/TX2_QD-")
			(pinfunction "TX2_QDATA_IN-")
			(pintype "input")
		)
		(pad "P5" smd circle
			(at -2 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 267 "/TX2_QD+")
			(pinfunction "TX2_QDATA_IN+")
			(pintype "input")
		)
		(pad "P6" smd circle
			(at -1.2 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 265 "/TX2_ID+")
			(pinfunction "TX2_IDATA_IN+")
			(pintype "input")
		)
		(pad "P7" smd circle
			(at -0.4 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 259 "/TX2_ID-")
			(pinfunction "TX2_IDATA_IN-")
			(pintype "input")
		)
		(pad "P8" smd circle
			(at 0.4 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 261 "/TX1_ID-")
			(pinfunction "TX1_IDATA_IN-")
			(pintype "input")
		)
		(pad "P9" smd circle
			(at 1.2 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 272 "/TX1_ID+")
			(pinfunction "TX1_IDATA_IN+")
			(pintype "input")
		)
		(pad "P10" smd circle
			(at 2 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 256 "/TX1_QD+")
			(pinfunction "TX1_QDATA_IN+")
			(pintype "input")
		)
		(pad "P11" smd circle
			(at 2.8 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 264 "/TX1_QD-")
			(pinfunction "TX1_QDATA_IN-")
			(pintype "input")
		)
		(pad "P12" smd circle
			(at 3.6 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 257 "/TX1_ST-")
			(pinfunction "TX1_STROBE_IN-")
			(pintype "input")
		)
		(pad "P13" smd circle
			(at 4.4 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 273 "/TX1_ST+")
			(pinfunction "TX1_STROBE_IN+")
			(pintype "input")
		)
		(pad "P14" smd circle
			(at 5.199999 5.199999 270)
			(size 0.4064 0.4064)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSD")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_BGA/BC-196-16_ADI.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 92.71 72.353)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J15"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 433 "/FPGA/PR47B")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 438 "/FPGA/PR38A")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 443 "/FPGA/PR32C")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 449 "/FPGA/PR17B")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 454 "/FPGA/PR8C")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 107.0102 88.3042)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R41"
			(at -0.1524 -1.1176 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 339 "Net-(Q4-C)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 346 "Net-(D1-BK)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:sot-23"
		(layer "F.Cu")
		(at 109.728 91.03216 180)
		(descr "SOT-23")
		(property "Reference" "Q3"
			(at -2.3622 -0.04064 180)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904"
			(at 0 0.0762 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 337 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 338 "Net-(Q3-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-3.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 115.7478 53.7856 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R2"
			(at -0.2286 1.27 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "/FPGA/FLASH.CLK")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 169.926 83.021 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C50"
			(at 0 -1.016 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 153.5176 65.0036 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C82"
			(at -2.328 -0.1778 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 219 "Net-(C82-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 225 "Net-(C82-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_RF_conn:CONN1_5-1814832-2_TEC"
		(layer "F.Cu")
		(at 176.657 98.896)
		(tags "5-1814832-2 ")
		(property "Reference" "J4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SMA_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_RF_conn:CONN1_5-1814832-2_TEC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1-1773725-8_RF_COAX_QRG&DocType=Data+Sheet&DocLang=English&DocFormat=pdf&PartCntxt=5-1814832-2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.0066 2.0066)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 334 "Net-(J4-RF)")
			(pinfunction "RF")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 2.54 2.54)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_RF_conn/c-5-1814832-2-c-3d.stp"
			(offset
				(xyz 0 0 10)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 152.6032 65.0036 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C83"
			(at -2.2264 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 312 "Net-(C83-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 311 "Net-(C83-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 138.1506 66.13 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C46"
			(at -0.127 -1.2192 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:ind_0402PA"
		(layer "F.Cu")
		(at 152.6032 67.0832 -90)
		(descr "SMT Inductor, 0402")
		(property "Reference" "L7"
			(at 1.6122 0.127 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.2nH"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:ind_0402PA"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 320 "Net-(U2E-TX2-)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 312 "Net-(C83-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-0402PA.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 150.495 56.0208 90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "P7"
			(at -0.0762 -2.667 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X04"
			(at 0 9.95 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X04 Pin_Header_Angled_1X04 Socket_Strip_Straight_1X04 Socket_Strip_Angled_1X04")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 423 "/AG_05")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 407 "/AG_06")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 410 "/AG_07")
			(pinfunction "P4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_smd_transistors:POWER56"
		(layer "F.Cu")
		(at 75.0034 89.6758 90)
		(descr "PSOP-8")
		(property "Reference" "Q6"
			(at 3.2258 -1.1402 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMP6023LFG"
			(at 0 1.016 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_smd_transistors:POWER56"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/DMP6023LFG.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "P-Channel MOSFET POWERDI 0.025 RDS"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.905 3 90)
			(size 0.59944 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "+5.0V")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.635 3 90)
			(size 0.59944 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "+5.0V")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.635 3 90)
			(size 0.59944 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "+5.0V")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.905 3 90)
			(size 0.59944 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 430 "Net-(Q6-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 1.905 -3 90)
			(size 0.59944 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 428 "Net-(Z1-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.635 -3 90)
			(size 0.59944 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 428 "Net-(Z1-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -0.635 -3 90)
			(size 0.59944 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 428 "Net-(Z1-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -1.905 -3 90)
			(size 0.59944 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 428 "Net-(Z1-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0 -0.5 90)
			(size 4 3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 428 "Net-(Z1-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_transistors/Power 56.stp"
			(offset
				(xyz 0 0 0.999999985)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
	)
	(footprint "t_sot:SSOP-8_TEX"
		(layer "F.Cu")
		(at 125.9078 55.97 90)
		(tags "TCA9406")
		(property "Reference" "U17"
			(at 0.127 2.5146 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCA9406"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_sot:SSOP-8_TEX"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9406.pdf?ts=1710769372418&ref_url=https%253A%252F%252Fwww.google.com%252F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "I2C Level Translator"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.2 -1.55 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.2 -1.55 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 -0.974999 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 288 "/FPGA/sJTAG2_CLK")
			(pinfunction "SDA_B")
			(pintype "open_collector")
		)
		(pad "2" smd rect
			(at -1.7 -0.325001 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.7 0.325001 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.7 0.974999 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 151 "/FPGA/JTAG2.TCK")
			(pinfunction "SDA_A")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at 1.7 0.974999 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "/FPGA/JTAG2.TDO")
			(pinfunction "SCL_A")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.7 0.325001 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 285 "Net-(U17-OE)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 1.7 -0.325001 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 1.7 -0.974999 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 286 "/FPGA/sJTAG2_TDO")
			(pinfunction "SCL_B")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.3 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 174.244 77.56 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R34"
			(at -0.296 -1.016 90)
			(layer "F.SilkS")
		)
		(property "Value" "13k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(U21-TTL_IN)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 126.1922 50.5852 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J11"
			(at 1.397 5.1866 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x1"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 281 "+1.8V")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 285 "Net-(U17-OE)")
			(pinfunction "2")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 129.3368 100.8176 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R52"
			(at -2.117 0.0508 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 396 "Net-(U2A-MODE)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 163 "/VDIGIO_1P8_F")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 157.7594 66.8324 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C77"
			(at -2.0232 -0.254 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 193 "Net-(U2C-RX2A-)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 190 "Net-(T2-SECONDARY)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 132.715 101.7408 90)
		(descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 2.54mm double row")
		(property "Reference" "J7"
			(at 3.0988 -2.5654 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x5"
			(at 1.27 12.49 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 163 "/VDIGIO_1P8_F")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/AD_TMS")
			(pinfunction "2")
			(pintype "power_out")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "3")
			(pintype "power_out")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/AD_TCLK")
			(pinfunction "4")
			(pintype "power_out")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "5")
			(pintype "power_out")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 188 "/AD_TDO")
			(pinfunction "6")
			(pintype "power_out")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "unconnected-(J7-Pad7)")
			(pinfunction "7")
			(pintype "power_out+no_connect")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 181 "/AD_TDI")
			(pinfunction "8")
			(pintype "power_out")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "9")
			(pintype "power_out")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 210 "/AD_~{RST}")
			(pinfunction "10")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 153.6954 89.105 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C84"
			(at 1.917 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:SMT_PAD_40"
		(layer "F.Cu")
		(at 119.3038 54.446)
		(property "Reference" "TP3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEST_POINT"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_misc:SMT_PAD_40"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 252 "/FPGA/D_UART2_RX")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_coilcraft:ind_0603cs"
		(layer "F.Cu")
		(at 150.368 86.7936 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "L4"
			(at 0.0896 -1.2446 -90)
			(layer "F.SilkS")
		)
		(property "Value" "220nH"
			(at 0 0.6096 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:ind_0603cs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 318 "Net-(U2D-TX1-)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-0603CS.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "t_BGA:TF-BGA54 8x8mm"
		(layer "F.Cu")
		(at 114.008 76.7726 -90)
		(property "Reference" "U4"
			(at -5.7658 4.2546 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "IS42VM16160K-6BLI"
			(at 0.4 -6.1 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_BGA:TF-BGA54 8x8mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/198/42_45SM_RM_VM16160K-268434.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SDRAM 32Mb 2Mx16"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "3"
			(at -1.9 -4.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -3.5 -4.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "J"
			(at -5 3.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "9"
			(at 2.9 -4.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "7"
			(at 1.3 -4.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B"
			(at -5 -2.1 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D"
			(at -5 -0.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A"
			(at -5 -2.9 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "F"
			(at -5 1.1 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "C"
			(at -5 -1.3 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -2.7 -4.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "8"
			(at 2.1 -4.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "H"
			(at -5 2.7 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "E"
			(at -5 0.3 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "G"
			(at -5 1.9 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "8"
			(at 2.1 -4.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "G"
			(at -5 1.9 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "C"
			(at -5 -1.3 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "A"
			(at -5 -2.9 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "E"
			(at -5 0.3 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at -3.5 -4.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "H"
			(at -5 2.7 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "7"
			(at 1.3 -4.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "F"
			(at -5 1.1 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "2"
			(at -2.7 -4.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "B"
			(at -5 -2.1 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "D"
			(at -5 -0.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "3"
			(at -1.9 -4.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "9"
			(at 2.9 -4.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "J"
			(at -5 3.5 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -3.2 -3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "A2" smd circle
			(at -2.4 -3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 240 "/FPGA/SDRAM_DQ15")
			(pinfunction "DQ15")
			(pintype "bidirectional")
		)
		(pad "A3" smd circle
			(at -1.6 -3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "A7" smd circle
			(at 1.6 -3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "A8" smd circle
			(at 2.4 -3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 244 "/FPGA/SDRAM_DQ0")
			(pinfunction "DQ0")
			(pintype "bidirectional")
		)
		(pad "A9" smd circle
			(at 3.2 -3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/FPGA/FM_1P8")
			(pinfunction "VDD")
			(pintype "bidirectional")
		)
		(pad "B1" smd circle
			(at -3.2 -2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 121 "/FPGA/SDRAM_DQ14")
			(pinfunction "DQ14")
			(pintype "bidirectional")
		)
		(pad "B2" smd circle
			(at -2.4 -2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 238 "/FPGA/SDRAM_DQ13")
			(pinfunction "DQ13")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at -1.6 -2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "B7" smd circle
			(at 1.6 -2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "B8" smd circle
			(at 2.4 -2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "/FPGA/SDRAM_DQ2")
			(pinfunction "DQ2")
			(pintype "bidirectional")
		)
		(pad "B9" smd circle
			(at 3.2 -2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "/FPGA/SDRAM_DQ1")
			(pinfunction "DQ1")
			(pintype "power_in")
		)
		(pad "C1" smd circle
			(at -3.2 -1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "/FPGA/SDRAM_DQ12")
			(pinfunction "DQ12")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -2.4 -1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 104 "/FPGA/SDRAM_DQ11")
			(pinfunction "DQ11")
			(pintype "bidirectional")
		)
		(pad "C3" smd circle
			(at -1.6 -1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "C7" smd circle
			(at 1.6 -1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "C8" smd circle
			(at 2.4 -1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "/FPGA/SDRAM_DQ4")
			(pinfunction "DQ4")
			(pintype "bidirectional")
		)
		(pad "C9" smd circle
			(at 3.2 -1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "/FPGA/SDRAM_DQ3")
			(pinfunction "DQ3")
			(pintype "bidirectional")
		)
		(pad "D1" smd circle
			(at -3.2 -0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 123 "/FPGA/SDRAM_DQ10")
			(pinfunction "DQ10")
			(pintype "bidirectional")
		)
		(pad "D2" smd circle
			(at -2.4 -0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "/FPGA/SDRAM_DQ9")
			(pinfunction "DQ9")
			(pintype "bidirectional")
		)
		(pad "D3" smd circle
			(at -1.6 -0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VDDQ")
			(pintype "power_in")
		)
		(pad "D7" smd circle
			(at 1.6 -0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSSQ")
			(pintype "power_in")
		)
		(pad "D8" smd circle
			(at 2.4 -0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 247 "/FPGA/SDRAM_DQ6")
			(pinfunction "DQ6")
			(pintype "bidirectional")
		)
		(pad "D9" smd circle
			(at 3.2 -0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "/FPGA/SDRAM_DQ5")
			(pinfunction "DQ5")
			(pintype "bidirectional")
		)
		(pad "E1" smd circle
			(at -3.2 0 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 157 "/FPGA/SDRAM_DQ8")
			(pinfunction "DQ8")
			(pintype "bidirectional")
		)
		(pad "E2" smd circle
			(at -2.4 0 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 234 "unconnected-(U4-NC-PadE2)")
			(pinfunction "NC")
			(pintype "bidirectional")
		)
		(pad "E3" smd circle
			(at -1.6 0 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "E7" smd circle
			(at 1.6 0 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/FPGA/FM_1P8")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "E8" smd circle
			(at 2.4 0 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 130 "/FPGA/SDRAM_DQM0")
			(pinfunction "DQML")
			(pintype "input")
		)
		(pad "E9" smd circle
			(at 3.2 0 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 119 "/FPGA/SDRAM_DQ7")
			(pinfunction "DQ7")
			(pintype "bidirectional")
		)
		(pad "F1" smd circle
			(at -3.2 0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 248 "/FPGA/SDRAM_DQM1")
			(pinfunction "DQMH")
			(pintype "input")
		)
		(pad "F2" smd circle
			(at -2.4 0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 132 "/FPGA/SDRAM_x.CLK")
			(pinfunction "CLK")
			(pintype "bidirectional")
		)
		(pad "F3" smd circle
			(at -1.6 0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "/FPGA/SDRAM_x.CKE")
			(pinfunction "CKE")
			(pintype "input")
		)
		(pad "F7" smd circle
			(at 1.6 0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 249 "/FPGA/SDRAM_x.nCAS")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "F8" smd circle
			(at 2.4 0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "/FPGA/SDRAM_x.nRAS")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "F9" smd circle
			(at 3.2 0.8 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "/FPGA/SDRAM_x.nWE")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "G1" smd circle
			(at -3.2 1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "/FPGA/SDRAM_A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "G2" smd circle
			(at -2.4 1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 246 "/FPGA/SDRAM_A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "G3" smd circle
			(at -1.6 1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 156 "/FPGA/SDRAM_A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "G7" smd circle
			(at 1.6 1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 133 "/FPGA/SDRAM_BA0")
			(pinfunction "BA0")
			(pintype "input")
		)
		(pad "G8" smd circle
			(at 2.4 1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 245 "/FPGA/SDRAM_BA1")
			(pinfunction "BA1")
			(pintype "input")
		)
		(pad "G9" smd circle
			(at 3.2 1.6 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "/FPGA/SDRAM_x.mCS")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "H1" smd circle
			(at -3.2 2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 153 "/FPGA/SDRAM_A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "H2" smd circle
			(at -2.4 2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 106 "/FPGA/SDRAM_A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "H3" smd circle
			(at -1.6 2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "/FPGA/SDRAM_A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "H7" smd circle
			(at 1.6 2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "/FPGA/SDRAM_A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "H8" smd circle
			(at 2.4 2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 152 "/FPGA/SDRAM_A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "H9" smd circle
			(at 3.2 2.4 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 237 "/FPGA/SDRAM_A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "J1" smd circle
			(at -3.2 3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "J2" smd circle
			(at -2.4 3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 242 "/FPGA/SDRAM_A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "J3" smd circle
			(at -1.6 3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 241 "/FPGA/SDRAM_A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "J7" smd circle
			(at 1.6 3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 137 "/FPGA/SDRAM_A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "J8" smd circle
			(at 2.4 3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "/FPGA/SDRAM_A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "J9" smd circle
			(at 3.2 3.2 270)
			(size 0.35 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/FPGA/FM_1P8")
			(pinfunction "VDD")
			(pintype "power_in")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 96.7144 59.5768 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R59"
			(at -0.212 -1.1176 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 399 "Net-(Q5-B)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 254 "/FPGA/USB_ENUM")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 95.25 67.273 90)
		(descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 2.54mm double row")
		(property "Reference" "J8"
			(at 2.6416 12.5222 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x5"
			(at 1.27 12.49 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "/FPGA/JTAG1.TMS")
			(pinfunction "2")
			(pintype "power_out")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "3")
			(pintype "power_out")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/FPGA/JTAG1.TCK")
			(pinfunction "4")
			(pintype "power_out")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "5")
			(pintype "power_out")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/FPGA/JTAG1.TDO")
			(pinfunction "6")
			(pintype "power_out")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "unconnected-(J8-Pad7)")
			(pinfunction "7")
			(pintype "power_out+no_connect")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/FPGA/JTAG1.TDI")
			(pinfunction "8")
			(pintype "power_out")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "9")
			(pintype "power_out")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(J8-Pad10)")
			(pinfunction "10")
			(pintype "power_out+no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 210.82 151.474)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R105"
			(at 2.413 0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 533 "/SCLK_TX_BOARD_1V8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 543 "Net-(K1B-P6_2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 173.010337 90.26)
		(property "Reference" "TP7"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 151.892 142.457)
		(property "Reference" "TP22"
			(at 0.127 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 513 "/RF_RX_SPI_CS_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 96.266 157.951)
		(property "Reference" "TP12"
			(at 0 2.413 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 536 "/+12V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 100.33 72.353)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J21"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 436 "/FPGA/PR44D")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 441 "/FPGA/PR35C")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 446 "/FPGA/PR29B")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 452 "/FPGA/PR11B")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 457 "/FPGA/PR5C")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 161.6202 77.6616 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R30"
			(at -1.9812 -0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.99K"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 327 "Net-(U2A-RBIAS)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 164.9476 72.2768 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R53"
			(at -0.5334 -1.143 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 397 "Net-(U2A-MODEA)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 163 "/VDIGIO_1P8_F")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_Mini_Circuits:DB1627_MNC"
		(layer "F.Cu")
		(at 157.8483 91.7332)
		(tags "TCM2-33X+ ")
		(property "Reference" "T3"
			(at 3.5687 1.7018 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TC1-1-13MX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_Mini_Circuits:DB1627_MNC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -3.302 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5875 1.27)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 216 "Net-(C81-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.5875 0)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 332 "unconnected-(T3-Pad2)")
			(pinfunction "2")
			(pintype "input+no_connect")
		)
		(pad "3" smd rect
			(at -1.5875 -1.27)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 205 "Net-(C80-Pad2)")
			(pinfunction "3")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 1.5875 -1.27)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "4")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 1.5875 0)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 426 "unconnected-(T3-Pad5)")
			(pinfunction "5")
			(pintype "no_connect")
		)
		(pad "6" smd rect
			(at 1.5875 1.27)
			(size 1.651 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 334 "Net-(J4-RF)")
			(pinfunction "6")
			(pintype "input")
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "F.Cu")
		(at 87.3252 86.6786 90)
		(tags "INA236AIDDFR ")
		(property "Reference" "U15"
			(at 0.0508 2.921 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "INA236"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina236.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.0574 -1.6764 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.0574 -1.7018 -90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 -90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "+5.0V")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 432 "/Power Supply/Vin")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 296 "Net-(U13-A0)")
			(pinfunction "SCL")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 295 "Net-(U13-SDA)")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "7" smd rect
			(at 1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 306 "unconnected-(U15-ALERT-Pad8)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 130.2766 65.4696 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R4"
			(at -2.3876 0.2794 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "Net-(U1H-INITN)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 154.7114 64.3266 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C87"
			(at -0.0762 1.0922 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 123.5202 58.087 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R57"
			(at 2.0916 -0.1524 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 288 "/FPGA/sJTAG2_CLK")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 77.47 58.5608 90)
		(descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 2.54mm double row")
		(property "Reference" "J12"
			(at 2.8448 -3.175 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x5"
			(at 1.27 12.49 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 287 "/FPGA/sJTAG2_TMS")
			(pinfunction "2")
			(pintype "power_out")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "3")
			(pintype "power_out")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 288 "/FPGA/sJTAG2_CLK")
			(pinfunction "4")
			(pintype "power_out")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "5")
			(pintype "power_out")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/FPGA/JTAG1.TDO")
			(pinfunction "6")
			(pintype "power_out")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "unconnected-(J12-Pad7)")
			(pinfunction "7")
			(pintype "power_out+no_connect")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 236 "/FPGA/FPGA_DONE")
			(pinfunction "8")
			(pintype "power_out")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "9")
			(pintype "power_out")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/FPGA/STM_~{RST}")
			(pinfunction "10")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 150.495 96.6608 90)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "P4"
			(at -0.2286 20.3708 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X08"
			(at 0 20.11 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X08 Pin_Header_Angled_1X08 Socket_Strip_Straight_1X08 Socket_Strip_Angled_1X08")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 405 "/AG_00")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 425 "/AG_01")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 417 "/DG_02")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 408 "/AG_08")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 409 "/AG_11")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 411 "/AG_09")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 159.639 157.57)
		(property "Reference" "TP21"
			(at 0.127 2.413 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 508 "/RF_TX_SPI_DO_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "F.Cu")
		(at 109.728 56.0208 -90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C44"
			(at -1.778 -0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 0.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "+1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 270)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 109.474 50.763 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J13"
			(at -1.2446 -3.0988 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x1"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 281 "+1.8V")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "Net-(U18-OE)")
			(pinfunction "2")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 76.7754 53.1506)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R56"
			(at -2.201 0.0254 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 287 "/FPGA/sJTAG2_TMS")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 213.233 82.513)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R101"
			(at -2.413 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/SCLK_HARM_FLT_1V8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 543 "Net-(K1B-P6_2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:ind_0603cs"
		(layer "F.Cu")
		(at 151.511 66.7442 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "L8"
			(at -0.0046 1.1938 90)
			(layer "F.SilkS")
		)
		(property "Value" "220nH"
			(at 0 0.6096 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:ind_0603cs"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 320 "Net-(U2E-TX2-)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-0603CS.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 161.6202 80.6588)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R27"
			(at 2.032 0.0254 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 324 "Net-(U2F-EXT_LO1-)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SSOP-8_TEX"
		(layer "F.Cu")
		(at 114.71275 102.715799)
		(tags "TCA9406")
		(property "Reference" "U20"
			(at -0.05715 -2.397399 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCA9406"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_sot:SSOP-8_TEX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9406.pdf?ts=1710769372418&ref_url=https%253A%252F%252Fwww.google.com%252F"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "I2C Level Translator"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.2 -1.55 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.2 -1.55 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 -0.974999)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 292 "Net-(U10-A0)")
			(pinfunction "SDA_B")
			(pintype "open_collector")
		)
		(pad "2" smd rect
			(at -1.7 -0.325001)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.7 0.325001)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.7 0.974999)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 199 "/I2C_SDA")
			(pinfunction "SDA_A")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at 1.7 0.974999)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 276 "/I2C_SCL")
			(pinfunction "SCL_A")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.7 0.325001)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 291 "Net-(Q1-C)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 1.7 -0.325001)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 1.7 -0.974999)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 290 "Net-(U10-SCL)")
			(pinfunction "SCL_B")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.3 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "hornet phase 2:SULLINS_SBH11-PBPC-D10-ST-BK"
		(layer "F.Cu")
		(at 185.039 72.861 90)
		(property "Reference" "JSDB1"
			(at -18.161 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "SBH11-PBPC-D10-ST-BK"
			(at 1.08 6.115 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "hornet phase 2:SULLINS_SBH11-PBPC-D10-ST-BK"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "J"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "9.4mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Sullins Connector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -11.43 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -11.43 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -8.89 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 491 "/SCLK_RX_PATH_1V8")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -8.89 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 524 "/MOSI_RX_PATH_1V8")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at -6.35 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 503 "/MISO_BPFS_1V8")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at -6.35 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 431 "/{slash}CS_EXPANDER_1V8")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at -3.81 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 496 "/MUX{slash}CS_1V8")
			(pinfunction "7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -3.81 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 281 "+1.8V")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at -1.27 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 490 "/DGPIO_0_1P8_THRU")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at -1.27 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at 1.27 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/SFL_BPFS_1V8")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at 1.27 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 506 "/RX{slash}RESET_1V8")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at 3.81 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 487 "/AGPIO_1")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 3.81 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/RX_PATH_DISABLE_1V8")
			(pinfunction "14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 6.35 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 512 "/DGPIO_1_1P8_THRU")
			(pinfunction "15")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 6.35 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 500 "/DGPIO_2_1P8_THRU")
			(pinfunction "16")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at 8.89 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 516 "/DGPIO_3_1P8_THRU")
			(pinfunction "17")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at 8.89 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 523 "/DGPIO_4_1P8_THRU")
			(pinfunction "18")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at 11.43 1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 475 "/RX_ATTEN_LE_1V8")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at 11.43 -1.27 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "C:/Users/yh5034/Desktop/hornet phase 2/SBH11-PBPC-D10-ST-BK.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 211.963 156.173 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R103"
			(at 0.254 1.016 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 540 "Net-(K1B-P6_0)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 525 "/MOSI_HARM_FLT_1V8")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 62.23 113.628)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J23"
			(at -0.0762 -3.0988 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J23-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J23-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J23-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(J23-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 80.01 50.763 90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "P6"
			(at 0.0508 10.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X04"
			(at 0 9.95 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X04 Pin_Header_Angled_1X04 Socket_Strip_Straight_1X04 Socket_Strip_Angled_1X04")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "+3.3V")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 287 "/FPGA/sJTAG2_TMS")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 288 "/FPGA/sJTAG2_CLK")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 140.8684 58.7386 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R3"
			(at -1.778 -0.2286 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "/FPGA/FLASH.IO2")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 182.753 51.906)
		(property "Reference" "TP6"
			(at -2.032 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_BGA:caBGA256_LAT-M"
		(layer "F.Cu")
		(at 130.823 76.8668 180)
		(tags "LFE5U-25F-6BG256I ")
		(property "Reference" "U1"
			(at -8.3944 -8.0846 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LFE5U-25F-6BG256C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_BGA:caBGA256_LAT-M"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "16"
			(at 6.1598 -8.1608 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "A"
			(at -7.7848 -6.0272 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "T"
			(at -7.6327 5.999999 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "1"
			(at -6.1338 -8.4656 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "16"
			(at 6.2614 -8.1608 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -6.0576 -7.9576 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "T"
			(at -8.0642 6.2156 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A"
			(at -8.0388 -6.0272 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A"
			(at -7.6327 -6 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "16"
			(at 5.999999 -7.6327 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at -6 -7.6327 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "T"
			(at -7.6327 5.999999 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -6 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "A2" smd circle
			(at -5.2 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 108 "unconnected-(U1G-PT4A{slash}+-PadA2)")
			(pinfunction "PT4A/+")
			(pintype "bidirectional")
		)
		(pad "A3" smd circle
			(at -4.4 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 465 "/FP_05")
			(pinfunction "PT6A/+")
			(pintype "bidirectional")
		)
		(pad "A4" smd circle
			(at -3.6 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 192 "/FP_57")
			(pinfunction "PT6B/-")
			(pintype "bidirectional")
		)
		(pad "A5" smd circle
			(at -2.8 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/FP_55")
			(pinfunction "PT18A/+")
			(pintype "bidirectional")
		)
		(pad "A6" smd circle
			(at -2 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 194 "/FP_53")
			(pinfunction "PT18B/-")
			(pintype "bidirectional")
		)
		(pad "A7" smd circle
			(at -1.2 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/FP_51")
			(pinfunction "PT29A/PCLKT0_0/+")
			(pintype "bidirectional")
		)
		(pad "A8" smd circle
			(at -0.4 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "/FP_50")
			(pinfunction "PT29B/PCLKC0_0/-")
			(pintype "bidirectional")
		)
		(pad "A9" smd circle
			(at 0.4 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 279 "/FPGA/UART1_TX_FPGA")
			(pinfunction "PT42A/+")
			(pintype "bidirectional")
		)
		(pad "A10" smd circle
			(at 1.199999 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/QSPI.~{CE}")
			(pinfunction "PT42B/-")
			(pintype "bidirectional")
		)
		(pad "A11" smd circle
			(at 1.999999 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 342 "/FPGA/F_LED_G")
			(pinfunction "PT53A/+")
			(pintype "bidirectional")
		)
		(pad "A12" smd circle
			(at 2.799999 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 341 "/FPGA/F_LED_B")
			(pinfunction "PT53B/-")
			(pintype "bidirectional")
		)
		(pad "A13" smd circle
			(at 3.599999 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 237 "/FPGA/SDRAM_A10")
			(pinfunction "PT65A/+")
			(pintype "bidirectional")
		)
		(pad "A14" smd circle
			(at 4.399999 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 127 "/FPGA/SDRAM_x.mCS")
			(pinfunction "PT65B/-")
			(pintype "bidirectional")
		)
		(pad "A15" smd circle
			(at 5.199999 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 162 "/FPGA/SDRAM_x.nWE")
			(pinfunction "PT67B/-")
			(pintype "bidirectional")
		)
		(pad "A16" smd circle
			(at 5.999999 -6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "B1" smd circle
			(at -6 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 273 "/TX1_ST+")
			(pinfunction "PL2A/HS+/LDQ8")
			(pintype "bidirectional")
		)
		(pad "B2" smd circle
			(at -5.2 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 257 "/TX1_ST-")
			(pinfunction "PL2B/HS-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "B3" smd circle
			(at -4.4 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 74 "unconnected-(U1G-PT4B{slash}--PadB3)")
			(pinfunction "PT4B/-")
			(pintype "bidirectional")
		)
		(pad "B4" smd circle
			(at -3.6 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 466 "/FP_123")
			(pinfunction "PT11B/-")
			(pintype "bidirectional")
		)
		(pad "B5" smd circle
			(at -2.8 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "/FP_56")
			(pinfunction "PT15B/-")
			(pintype "bidirectional")
		)
		(pad "B6" smd circle
			(at -2 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "/FP_54")
			(pinfunction "PT22B/-")
			(pintype "bidirectional")
		)
		(pad "B7" smd circle
			(at -1.2 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "/FP_52")
			(pinfunction "PT27B/PCLKC0_1/-")
			(pintype "bidirectional")
		)
		(pad "B8" smd circle
			(at -0.4 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 464 "/FP_120")
			(pinfunction "PT35B/PCLKC1_0/-")
			(pintype "bidirectional")
		)
		(pad "B9" smd circle
			(at 0.4 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 280 "/FPGA/UART1_RX_FPGA")
			(pinfunction "PT38A/GR_PCLK1_0/+")
			(pintype "bidirectional")
		)
		(pad "B10" smd circle
			(at 1.199999 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/QSPI.I3")
			(pinfunction "PT44A/+")
			(pintype "bidirectional")
		)
		(pad "B11" smd circle
			(at 1.999999 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 343 "/FPGA/F_LED_R")
			(pinfunction "PT49A/+")
			(pintype "bidirectional")
		)
		(pad "B12" smd circle
			(at 2.799999 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 109 "/FPGA/SDRAM_A2")
			(pinfunction "PT56A/+")
			(pintype "bidirectional")
		)
		(pad "B13" smd circle
			(at 3.599999 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 152 "/FPGA/SDRAM_A1")
			(pinfunction "PT60A/+")
			(pintype "bidirectional")
		)
		(pad "B14" smd circle
			(at 4.399999 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 245 "/FPGA/SDRAM_BA1")
			(pinfunction "PT67A/+")
			(pintype "bidirectional")
		)
		(pad "B15" smd circle
			(at 5.199999 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 119 "/FPGA/SDRAM_DQ7")
			(pinfunction "PR2B/S0_IN/HS-/RDQ8")
			(pintype "bidirectional")
		)
		(pad "B16" smd circle
			(at 5.999999 -5.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 110 "/FPGA/SDRAM_x.nRAS")
			(pinfunction "PR2A/HS+/RDQ8")
			(pintype "bidirectional")
		)
		(pad "C1" smd circle
			(at -6 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 272 "/TX1_ID+")
			(pinfunction "PL5A/HS+/LDQ8")
			(pintype "bidirectional")
		)
		(pad "C2" smd circle
			(at -5.2 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 261 "/TX1_ID-")
			(pinfunction "PL5B/HS-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "C3" smd circle
			(at -4.4 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 200 "/RX1_ID+")
			(pinfunction "PL2C/+/LDQ8")
			(pintype "bidirectional")
		)
		(pad "C4" smd circle
			(at -3.6 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/FP_80")
			(pinfunction "PT11A/+")
			(pintype "bidirectional")
		)
		(pad "C5" smd circle
			(at -2.8 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/FP_83")
			(pinfunction "PT15A/+")
			(pintype "bidirectional")
		)
		(pad "C6" smd circle
			(at -2 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "/FP_86")
			(pinfunction "PT22A/+")
			(pintype "bidirectional")
		)
		(pad "C7" smd circle
			(at -1.2 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "/FP_82")
			(pinfunction "PT27A/PCLKT0_1/+")
			(pintype "bidirectional")
		)
		(pad "C8" smd circle
			(at -0.4 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 459 "/FP_121")
			(pinfunction "PT35A/PCLKT1_0/+")
			(pintype "bidirectional")
		)
		(pad "C9" smd circle
			(at 0.4 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/QSPI.I0")
			(pinfunction "PT38B/GR_PCLK1_1/-")
			(pintype "bidirectional")
		)
		(pad "C10" smd circle
			(at 1.199999 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/QSPI.I2")
			(pinfunction "PT44B/-")
			(pintype "bidirectional")
		)
		(pad "C11" smd circle
			(at 1.999999 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 202 "/FP_124")
			(pinfunction "PT49B/-")
			(pintype "bidirectional")
		)
		(pad "C12" smd circle
			(at 2.799999 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 206 "/FP_132")
			(pinfunction "PT56B/-")
			(pintype "bidirectional")
		)
		(pad "C13" smd circle
			(at 3.599999 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 460 "/FP_133")
			(pinfunction "PT60B/-")
			(pintype "bidirectional")
		)
		(pad "C14" smd circle
			(at 4.399999 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 140 "unconnected-(U1E-PR2C{slash}+{slash}RDQ8-PadC14)")
			(pinfunction "PR2C/+/RDQ8")
			(pintype "bidirectional")
		)
		(pad "C15" smd circle
			(at 5.199999 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 138 "/FPGA/SDRAM_DQ5")
			(pinfunction "PR5B/HS-/RDQ8")
			(pintype "bidirectional")
		)
		(pad "C16" smd circle
			(at 5.999999 -4.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 130 "/FPGA/SDRAM_DQM0")
			(pinfunction "PR5A/HS+/RDQ8")
			(pintype "bidirectional")
		)
		(pad "D1" smd circle
			(at -6 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 103 "unconnected-(U1A-PL8A{slash}HS+{slash}LDQS8-PadD1)")
			(pinfunction "PL8A/HS+/LDQS8")
			(pintype "bidirectional")
		)
		(pad "D2" smd circle
			(at -5.2 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "D3" smd circle
			(at -4.4 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 178 "/RX1_ID-")
			(pinfunction "PL2D/-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "D4" smd circle
			(at -3.6 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/FP_87")
			(pinfunction "PT9B/-")
			(pintype "bidirectional")
		)
		(pad "D5" smd circle
			(at -2.8 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "/FP_84")
			(pinfunction "PT13B/-")
			(pintype "bidirectional")
		)
		(pad "D6" smd circle
			(at -2 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/FP_81")
			(pinfunction "PT20B/-")
			(pintype "bidirectional")
		)
		(pad "D7" smd circle
			(at -1.2 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "/FP_85")
			(pinfunction "PT24B/GR_PCLK0_0/-")
			(pintype "bidirectional")
		)
		(pad "D8" smd circle
			(at -0.4 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 461 "/FP_125")
			(pinfunction "PT33B/PCLKC1_1/-")
			(pintype "bidirectional")
		)
		(pad "D9" smd circle
			(at 0.4 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/QSPI.I1")
			(pinfunction "PT40A/+")
			(pintype "bidirectional")
		)
		(pad "D10" smd circle
			(at 1.199999 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 86 "unconnected-(U1F-PT47A{slash}+-PadD10)")
			(pinfunction "PT47A/+")
			(pintype "bidirectional")
		)
		(pad "D11" smd circle
			(at 1.999999 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 463 "/FP_131")
			(pinfunction "PT51A/+")
			(pintype "bidirectional")
		)
		(pad "D12" smd circle
			(at 2.799999 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 462 "/FP_130")
			(pinfunction "PT58A/+")
			(pintype "bidirectional")
		)
		(pad "D13" smd circle
			(at 3.599999 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "unconnected-(U1F-PT62A{slash}+-PadD13)")
			(pinfunction "PT62A/+")
			(pintype "bidirectional")
		)
		(pad "D14" smd circle
			(at 4.399999 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 139 "/FPGA/SDRAM_DQ3")
			(pinfunction "PR2D/-/RDQ8")
			(pintype "bidirectional")
		)
		(pad "D15" smd circle
			(at 5.199999 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "D16" smd circle
			(at 5.999999 -3.6 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 247 "/FPGA/SDRAM_DQ6")
			(pinfunction "PR8A/HS+/RDQS8")
			(pintype "bidirectional")
		)
		(pad "E1" smd circle
			(at -6 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 101 "unconnected-(U1A-PL11D{slash}-{slash}LDQ8-PadE1)")
			(pinfunction "PL11D/-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "E2" smd circle
			(at -5.2 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 105 "unconnected-(U1A-PL8B{slash}HS-{slash}LDQSN8-PadE2)")
			(pinfunction "PL8B/HS-/LDQSN8")
			(pintype "bidirectional")
		)
		(pad "E3" smd circle
			(at -4.4 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 169 "/RX1_QD+")
			(pinfunction "PL5C/-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "E4" smd circle
			(at -3.6 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 160 "unconnected-(U1G-PT9A{slash}+-PadE4)")
			(pinfunction "PT9A/+")
			(pintype "bidirectional")
		)
		(pad "E5" smd circle
			(at -2.8 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 149 "unconnected-(U1G-PT13A{slash}+-PadE5)")
			(pinfunction "PT13A/+")
			(pintype "bidirectional")
		)
		(pad "E6" smd circle
			(at -2 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 131 "unconnected-(U1G-PT20A{slash}+-PadE6)")
			(pinfunction "PT20A/+")
			(pintype "bidirectional")
		)
		(pad "E7" smd circle
			(at -1.2 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 143 "unconnected-(U1G-PT24A{slash}GR_PCLK0_1{slash}+-PadE7)")
			(pinfunction "PT24A/GR_PCLK0_1/+")
			(pintype "bidirectional")
		)
		(pad "E8" smd circle
			(at -0.4 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/QSPI.SCLK")
			(pinfunction "PT33A/PCLKT1_1/+")
			(pintype "bidirectional")
		)
		(pad "E9" smd circle
			(at 0.4 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 90 "unconnected-(U1F-PT40B{slash}--PadE9)")
			(pinfunction "PT40B/-")
			(pintype "bidirectional")
		)
		(pad "E10" smd circle
			(at 1.199999 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 95 "unconnected-(U1F-PT47B{slash}--PadE10)")
			(pinfunction "PT47B/-")
			(pintype "bidirectional")
		)
		(pad "E11" smd circle
			(at 1.999999 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 129 "unconnected-(U1F-PT51B{slash}--PadE11)")
			(pinfunction "PT51B/-")
			(pintype "bidirectional")
		)
		(pad "E12" smd circle
			(at 2.799999 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 83 "unconnected-(U1F-PT58B{slash}--PadE12)")
			(pinfunction "PT58B/-")
			(pintype "bidirectional")
		)
		(pad "E13" smd circle
			(at 3.599999 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 99 "unconnected-(U1F-PT62B{slash}--PadE13)")
			(pinfunction "PT62B/-")
			(pintype "bidirectional")
		)
		(pad "E14" smd circle
			(at 4.399999 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 457 "/FPGA/PR5C")
			(pinfunction "PR5C/+/RDQ8")
			(pintype "bidirectional")
		)
		(pad "E15" smd circle
			(at 5.199999 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 158 "/FPGA/SDRAM_DQ1")
			(pinfunction "PR8B/HS-/RDQSN8")
			(pintype "bidirectional")
		)
		(pad "E16" smd circle
			(at 5.999999 -2.8 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 120 "/FPGA/SDRAM_DQ4")
			(pinfunction "PR11D/-/RDQ8")
			(pintype "bidirectional")
		)
		(pad "F1" smd circle
			(at -6 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 256 "/TX1_QD+")
			(pinfunction "PL14A/HS+/LDQ20")
			(pintype "bidirectional")
		)
		(pad "F2" smd circle
			(at -5.2 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "unconnected-(U1A-PL11C{slash}-{slash}LDQ8-PadF2)")
			(pinfunction "PL11C/-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "F3" smd circle
			(at -4.4 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 214 "/RX1_QD-")
			(pinfunction "PL5D/-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "F4" smd circle
			(at -3.6 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 263 "/TX1_EN")
			(pinfunction "PL8C/+/LDQ8")
			(pintype "bidirectional")
		)
		(pad "F5" smd circle
			(at -2.8 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 151 "/FPGA/JTAG2.TCK")
			(pinfunction "PL8D/-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "F6" smd circle
			(at -2 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VCCIO0")
			(pintype "power_in")
		)
		(pad "F7" smd circle
			(at -1.2 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VCCIO0")
			(pintype "power_in")
		)
		(pad "F8" smd circle
			(at -0.4 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "F9" smd circle
			(at 0.4 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "F10" smd circle
			(at 1.199999 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VCCIO1")
			(pintype "power_in")
		)
		(pad "F11" smd circle
			(at 1.999999 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VCCIO1")
			(pintype "power_in")
		)
		(pad "F12" smd circle
			(at 2.799999 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 458 "/FPGA/PR8D")
			(pinfunction "PR8D/-/RDQ8")
			(pintype "bidirectional")
		)
		(pad "F13" smd circle
			(at 3.599999 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 454 "/FPGA/PR8C")
			(pinfunction "PR8C/+/RDQ8")
			(pintype "bidirectional")
		)
		(pad "F14" smd circle
			(at 4.399999 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 456 "/FPGA/PR5D")
			(pinfunction "PR5D/-/RDQ8")
			(pintype "bidirectional")
		)
		(pad "F15" smd circle
			(at 5.199999 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 161 "/FPGA/SDRAM_DQ2")
			(pinfunction "PR11C/+/RDQ8")
			(pintype "bidirectional")
		)
		(pad "F16" smd circle
			(at 5.999999 -2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 244 "/FPGA/SDRAM_DQ0")
			(pinfunction "PR14A/HS+/RDQ20")
			(pintype "bidirectional")
		)
		(pad "G1" smd circle
			(at -6 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 203 "/RX1_DCLK+")
			(pinfunction "PL20A/GR_PCLK7_1/HX+/LDQS20")
			(pintype "bidirectional")
		)
		(pad "G2" smd circle
			(at -5.2 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 264 "/TX1_QD-")
			(pinfunction "PL14B/HS-/LDQ20")
			(pintype "bidirectional")
		)
		(pad "G3" smd circle
			(at -4.4 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 168 "/RX1_ST+")
			(pinfunction "PL14C/VREF1_7/+/LDQ20")
			(pintype "bidirectional")
		)
		(pad "G4" smd circle
			(at -3.6 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 268 "/TX1_CLK_I-")
			(pinfunction "PL11B/HS-/LDQ8")
			(pintype "bidirectional")
		)
		(pad "G5" smd circle
			(at -2.8 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 258 "/TX1_CLK_I+")
			(pinfunction "PL11A/HS+/LDQ8")
			(pintype "bidirectional")
		)
		(pad "G6" smd circle
			(at -2 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "+1.1V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "G7" smd circle
			(at -1.2 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "+1.1V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "G8" smd circle
			(at -0.4 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "G9" smd circle
			(at 0.4 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "+1.1V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "G10" smd circle
			(at 1.199999 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "G11" smd circle
			(at 1.999999 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "+2.5V")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "G12" smd circle
			(at 2.799999 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 455 "/FPGA/PR11A")
			(pinfunction "PR11A/HS+/RDQ8")
			(pintype "bidirectional")
		)
		(pad "G13" smd circle
			(at 3.599999 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 452 "/FPGA/PR11B")
			(pinfunction "PR11B/HS-/RDQ8")
			(pintype "bidirectional")
		)
		(pad "G14" smd circle
			(at 4.399999 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 453 "/FPGA/PR14C")
			(pinfunction "PR14C/VREF1_2/+/RDQ20")
			(pintype "bidirectional")
		)
		(pad "G15" smd circle
			(at 5.199999 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 133 "/FPGA/SDRAM_BA0")
			(pinfunction "PR14B/HS-/RDQ20")
			(pintype "bidirectional")
		)
		(pad "G16" smd circle
			(at 5.999999 -1.2 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 249 "/FPGA/SDRAM_x.nCAS")
			(pinfunction "PR20A/GR_PCLK2_1/HS+/RDQS2")
			(pintype "bidirectional")
		)
		(pad "H1" smd circle
			(at -6 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "H2" smd circle
			(at -5.2 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 186 "/RX1_DCLK-")
			(pinfunction "PL20B/HS-/LDQSN20")
			(pintype "bidirectional")
		)
		(pad "H3" smd circle
			(at -4.4 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 215 "/RX1_ST-")
			(pinfunction "PL14D/-/LDQ20")
			(pintype "bidirectional")
		)
		(pad "H4" smd circle
			(at -3.6 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 211 "/RX1_EN")
			(pinfunction "PL17B/HS-/LDQ20")
			(pintype "bidirectional")
		)
		(pad "H5" smd circle
			(at -2.8 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 239 "/FPGA/JTAG2.TMS")
			(pinfunction "PL17A/HS+/LDQ20")
			(pintype "bidirectional")
		)
		(pad "H6" smd circle
			(at -2 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/FPGA/N_1P8")
			(pinfunction "VCCIO7")
			(pintype "power_in")
		)
		(pad "H7" smd circle
			(at -1.2 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/FPGA/N_1P8")
			(pinfunction "VCCIO7")
			(pintype "power_in")
		)
		(pad "H8" smd circle
			(at -0.4 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "H9" smd circle
			(at 0.4 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "H10" smd circle
			(at 1.199999 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "H11" smd circle
			(at 1.999999 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VCCIO2")
			(pintype "power_in")
		)
		(pad "H12" smd circle
			(at 2.799999 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 451 "/FPGA/PR17A")
			(pinfunction "PR17A/HS+/RDQ20")
			(pintype "bidirectional")
		)
		(pad "H13" smd circle
			(at 3.599999 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 449 "/FPGA/PR17B")
			(pinfunction "PR17B/HS-/RDQ20")
			(pintype "bidirectional")
		)
		(pad "H14" smd circle
			(at 4.399999 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 450 "/FPGA/PR14D")
			(pinfunction "PR14D/-/RDQ20")
			(pintype "bidirectional")
		)
		(pad "H15" smd circle
			(at 5.199999 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 117 "/FPGA/SDRAM_A0")
			(pinfunction "PR20B/HS/RDQSN20")
			(pintype "bidirectional")
		)
		(pad "H16" smd circle
			(at 5.999999 -0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "J1" smd circle
			(at -6 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 227 "/TX1_CLK_O+")
			(pinfunction "PL23A/PCLKT7_1/HS+/LDQ20")
			(pintype "bidirectional")
		)
		(pad "J2" smd circle
			(at -5.2 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 270 "/TX1_CLK_O-")
			(pinfunction "PL23B/PCLKC7_1/HS-/LDQ20")
			(pintype "bidirectional")
		)
		(pad "J3" smd circle
			(at -4.4 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "unconnected-(U1A-PL20C{slash}GR_PCLK7_0{slash}+{slash}LDQ20-PadJ3)")
			(pinfunction "PL20C/GR_PCLK7_0/+/LDQ20")
			(pintype "bidirectional")
		)
		(pad "J4" smd circle
			(at -3.6 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 145 "unconnected-(U1A-PL117C{slash}+{slash}LDQ20-PadJ4)")
			(pinfunction "PL117C/+/LDQ20")
			(pintype "bidirectional")
		)
		(pad "J5" smd circle
			(at -2.8 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 135 "/FPGA/JTAG2.TDO")
			(pinfunction "PL17D/-/LDQ20")
			(pintype "bidirectional")
		)
		(pad "J6" smd circle
			(at -2 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/FPGA/N_1P8")
			(pinfunction "VCCIO6")
			(pintype "power_in")
		)
		(pad "J7" smd circle
			(at -1.2 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/FPGA/N_1P8")
			(pinfunction "VCCIO6")
			(pintype "power_in")
		)
		(pad "J8" smd circle
			(at -0.4 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "J9" smd circle
			(at 0.4 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "J10" smd circle
			(at 1.199999 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "J11" smd circle
			(at 1.999999 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VCCIO2")
			(pintype "power_in")
		)
		(pad "J12" smd circle
			(at 2.799999 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 118 "unconnected-(U1E-PR17D{slash}-{slash}RDQ20-PadJ12)")
			(pinfunction "PR17D/-/RDQ20")
			(pintype "bidirectional")
		)
		(pad "J13" smd circle
			(at 3.599999 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 111 "unconnected-(U1E-PR17C{slash}+{slash}RDQ20-PadJ13)")
			(pinfunction "PR17C/+/RDQ20")
			(pintype "bidirectional")
		)
		(pad "J14" smd circle
			(at 4.399999 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "unconnected-(U1E-PR20C{slash}GR_PCLK2_0{slash}+{slash}RDQ20-PadJ14)")
			(pinfunction "PR20C/GR_PCLK2_0/+/RDQ20")
			(pintype "bidirectional")
		)
		(pad "J15" smd circle
			(at 5.199999 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 241 "/FPGA/SDRAM_A4")
			(pinfunction "PR23B/PCLKC2_1/HS-/RDQ20")
			(pintype "bidirectional")
		)
		(pad "J16" smd circle
			(at 5.999999 0.4 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 137 "/FPGA/SDRAM_A3")
			(pinfunction "PR23A/PCLKT2_1/HS+/RDQ20")
			(pintype "bidirectional")
		)
		(pad "K1" smd circle
			(at -6 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 125 "unconnected-(U1A-PL23C{slash}PCLKT7_0{slash}+{slash}LDQ20-PadK1)")
			(pinfunction "PL23C/PCLKT7_0/+/LDQ20")
			(pintype "bidirectional")
		)
		(pad "K2" smd circle
			(at -5.2 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 148 "unconnected-(U1A-PL23D{slash}PCLKC7_0{slash}-{slash}LDQ20-PadK2)")
			(pinfunction "PL23D/PCLKC7_0/-/LDQ20")
			(pintype "bidirectional")
		)
		(pad "K3" smd circle
			(at -4.4 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 112 "unconnected-(U1A-PL20D{slash}-{slash}LDQ20-PadK3)")
			(pinfunction "PL20D/-/LDQ20")
			(pintype "bidirectional")
		)
		(pad "K4" smd circle
			(at -3.6 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 265 "/TX2_ID+")
			(pinfunction "PL29A/GR_PCLK6_0/HS+/LDQ32")
			(pintype "bidirectional")
		)
		(pad "K5" smd circle
			(at -2.8 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 259 "/TX2_ID-")
			(pinfunction "PL29B/HS-/LDQ32")
			(pintype "bidirectional")
		)
		(pad "K6" smd circle
			(at -2 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "K7" smd circle
			(at -1.2 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "K8" smd circle
			(at -0.4 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "K9" smd circle
			(at 0.4 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "K10" smd circle
			(at 1.199999 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "K11" smd circle
			(at 1.999999 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VCCIO3")
			(pintype "power_in")
		)
		(pad "K12" smd circle
			(at 2.799999 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 446 "/FPGA/PR29B")
			(pinfunction "PR29B/HS-/RDQ32")
			(pintype "bidirectional")
		)
		(pad "K13" smd circle
			(at 3.599999 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 447 "/FPGA/PR29A")
			(pinfunction "PR29A/GR_PCLK3_0/HS+/RDQ32")
			(pintype "bidirectional")
		)
		(pad "K14" smd circle
			(at 4.399999 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "unconnected-(U1E-PR20D{slash}-{slash}RDQ20-PadK14)")
			(pinfunction "PR20D/-/RDQ20")
			(pintype "bidirectional")
		)
		(pad "K15" smd circle
			(at 5.199999 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 156 "/FPGA/SDRAM_A9")
			(pinfunction "PR23D/PCLKC2_0/-/RDQ20")
			(pintype "bidirectional")
		)
		(pad "K16" smd circle
			(at 5.999999 1.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 146 "/FPGA/SDRAM_A6")
			(pinfunction "PR23C/PCLKT2_0/+/RDQ20")
			(pintype "bidirectional")
		)
		(pad "L1" smd circle
			(at -6 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 269 "/TX2_CLK_O+")
			(pinfunction "PL26A/PLCKT6_1/HS+/LDQ32")
			(pintype "bidirectional")
		)
		(pad "L2" smd circle
			(at -5.2 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 260 "/TX2_CLK_O-")
			(pinfunction "PL26B/PCLKC6_1/HS-/LDQ32")
			(pintype "bidirectional")
		)
		(pad "L3" smd circle
			(at -4.4 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "unconnected-(U1B-PL32C{slash}+{slash}LDQ32-PadL3)")
			(pinfunction "PL32C/+/LDQ32")
			(pintype "bidirectional")
		)
		(pad "L4" smd circle
			(at -3.6 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 93 "unconnected-(U1B-PL29C{slash}GR_PCLK6_1{slash}+{slash}LDQ32-PadL4)")
			(pinfunction "PL29C/GR_PCLK6_1/+/LDQ32")
			(pintype "bidirectional")
		)
		(pad "L5" smd circle
			(at -2.8 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "unconnected-(U1B-PL29D{slash}-{slash}LDQ32-PadL5)")
			(pinfunction "PL29D/-/LDQ32")
			(pintype "bidirectional")
		)
		(pad "L6" smd circle
			(at -2 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VCCIO8")
			(pintype "power_in")
		)
		(pad "L7" smd circle
			(at -1.2 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 88 "+2.5V")
			(pinfunction "VCCAUX")
			(pintype "power_in")
		)
		(pad "L8" smd circle
			(at -0.4 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "+1.1V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "L9" smd circle
			(at 0.4 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "+1.1V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "L10" smd circle
			(at 1.199999 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 107 "+1.1V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "L11" smd circle
			(at 1.999999 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "VCCIO3")
			(pintype "power_in")
		)
		(pad "L12" smd circle
			(at 2.799999 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 445 "/FPGA/PR29D")
			(pinfunction "PR29D/-/RDQ32")
			(pintype "bidirectional")
		)
		(pad "L13" smd circle
			(at 3.599999 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 444 "/FPGA/PR29C")
			(pinfunction "PR29C/GR_PCLK3_1/+/RDQ32")
			(pintype "bidirectional")
		)
		(pad "L14" smd circle
			(at 4.399999 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 443 "/FPGA/PR32C")
			(pinfunction "PR32C/+/RDQ32")
			(pintype "bidirectional")
		)
		(pad "L15" smd circle
			(at 5.199999 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 240 "/FPGA/SDRAM_DQ15")
			(pinfunction "PR26B/PCLKC3_1/HS-/RDQ32")
			(pintype "bidirectional")
		)
		(pad "L16" smd circle
			(at 5.999999 1.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "/FPGA/SDRAM_x.CKE")
			(pinfunction "PR26A/PCLKT3_1/HS+/RDQ32")
			(pintype "bidirectional")
		)
		(pad "M1" smd circle
			(at -6 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 226 "/RX2_DCLK+")
			(pinfunction "PL26C/PCLKT6_0/+/LDQ32")
			(pintype "bidirectional")
		)
		(pad "M2" smd circle
			(at -5.2 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 218 "/RX2_DCLK-")
			(pinfunction "PL26D/PCLKC6_0/-/LDQ32")
			(pintype "bidirectional")
		)
		(pad "M3" smd circle
			(at -4.4 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "unconnected-(U1B-PL23D{slash}-{slash}LDQ32-PadM3)")
			(pinfunction "PL23D/-/LDQ32")
			(pintype "bidirectional")
		)
		(pad "M4" smd circle
			(at -3.6 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 122 "unconnected-(U1B-PL35C{slash}+{slash}LDQ32-PadM4)")
			(pinfunction "PL35C/+/LDQ32")
			(pintype "bidirectional")
		)
		(pad "M5" smd circle
			(at -2.8 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 473 "/SPI2x.MISO")
			(pinfunction "PL44C/+/LDQ44")
			(pintype "bidirectional")
		)
		(pad "M6" smd circle
			(at -2 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 266 "/TX2_CLK_I+")
			(pinfunction "PL447A/HS+/LDQSN44")
			(pintype "bidirectional")
		)
		(pad "M7" smd circle
			(at -1.2 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 128 "/FPGA/FLASH.IO2")
			(pinfunction "PB9B/D2/IO2/-")
			(pintype "bidirectional")
		)
		(pad "M8" smd circle
			(at -0.4 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 299 "Net-(U1C-PB15B{slash}DOUT{slash}CS0N{slash}-)")
			(pinfunction "PB15B/DOUT/CS0N/-")
			(pintype "bidirectional")
		)
		(pad "M9" smd circle
			(at 0.4 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 212 "Net-(U1C-PB18A{slash}WRITEN)")
			(pinfunction "PB18A/WRITEN")
			(pintype "bidirectional")
		)
		(pad "M10" smd circle
			(at 1.199999 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 100 "/FPGA/JTAG1.TDO")
			(pinfunction "TDO")
			(pintype "bidirectional")
		)
		(pad "M11" smd circle
			(at 1.999999 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 448 "unconnected-(U1D-PR47A{slash}HS+{slash}RDQ44-PadM11)")
			(pinfunction "PR47A/HS+/RDQ44")
			(pintype "bidirectional")
		)
		(pad "M12" smd circle
			(at 2.799999 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 439 "/FPGA/PR44C")
			(pinfunction "PR44C/+/RDQ44")
			(pintype "bidirectional")
		)
		(pad "M13" smd circle
			(at 3.599999 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 441 "/FPGA/PR35C")
			(pinfunction "PR35C/+/RDQ32")
			(pintype "bidirectional")
		)
		(pad "M14" smd circle
			(at 4.399999 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 442 "/FPGA/PR32D")
			(pinfunction "PR32D/-/RDQ32")
			(pintype "bidirectional")
		)
		(pad "M15" smd circle
			(at 5.199999 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 121 "/FPGA/SDRAM_DQ14")
			(pinfunction "PR26D/PCLKC3_0/-/RDQ32")
			(pintype "bidirectional")
		)
		(pad "M16" smd circle
			(at 5.999999 2.799999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 238 "/FPGA/SDRAM_DQ13")
			(pinfunction "PR26C/PCLKT3_0/+/RDQ32")
			(pintype "bidirectional")
		)
		(pad "N1" smd circle
			(at -6 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 175 "/RX2_QD+")
			(pinfunction "PL32A/HS+/LDQS32")
			(pintype "bidirectional")
		)
		(pad "N2" smd circle
			(at -5.2 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "N3" smd circle
			(at -4.4 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 271 "/TX2_EN")
			(pinfunction "PL35D/-/LDQ32")
			(pintype "bidirectional")
		)
		(pad "N4" smd circle
			(at -3.6 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "/FPGA/JTAG2.TDI")
			(pinfunction "PL38A/HS+/LDQ44")
			(pintype "bidirectional")
		)
		(pad "N5" smd circle
			(at -2.8 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 474 "/SPI2x.CE")
			(pinfunction "PL44D/-/LDQ44")
			(pintype "bidirectional")
		)
		(pad "N6" smd circle
			(at -2 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 262 "/TX2_CLK_I-")
			(pinfunction "PL47B/HS-/LDQ44")
			(pintype "bidirectional")
		)
		(pad "N7" smd circle
			(at -1.2 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "/FPGA/FLASH.IO3")
			(pinfunction "PB9A/D3/IO3/+")
			(pintype "bidirectional")
		)
		(pad "N8" smd circle
			(at -0.4 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 134 "/FPGA/FLASH.CS")
			(pinfunction "PB15A/HOLDN/DI/BUSY/CSSPIN/CEN/+")
			(pintype "bidirectional")
		)
		(pad "N9" smd circle
			(at 0.4 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 85 "/FPGA/FLASH.CLK")
			(pinfunction "CCLK/MCLK/SCK")
			(pintype "bidirectional")
		)
		(pad "N10" smd circle
			(at 1.199999 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 401 "Net-(U1H-CFG_0)")
			(pinfunction "CFG_0")
			(pintype "bidirectional")
		)
		(pad "N11" smd circle
			(at 1.999999 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 433 "/FPGA/PR47B")
			(pinfunction "PR47B/HS-/RDQ44")
			(pintype "bidirectional")
		)
		(pad "N12" smd circle
			(at 2.799999 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 436 "/FPGA/PR44D")
			(pinfunction "PR44D/-/RDQ44")
			(pintype "bidirectional")
		)
		(pad "N13" smd circle
			(at 3.599999 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 438 "/FPGA/PR38A")
			(pinfunction "PR38A/HS+/RDQ44")
			(pintype "bidirectional")
		)
		(pad "N14" smd circle
			(at 4.399999 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "/FPGA/SDRAM_DQ12")
			(pinfunction "PR35D/-/RDQ32")
			(pintype "bidirectional")
		)
		(pad "N15" smd circle
			(at 5.199999 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "N16" smd circle
			(at 5.999999 3.599999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 104 "/FPGA/SDRAM_DQ11")
			(pinfunction "PR32A/HS+/RDQS32")
			(pintype "bidirectional")
		)
		(pad "P1" smd circle
			(at -6 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 267 "/TX2_QD+")
			(pinfunction "PL35A/HS+/LDQ32")
			(pintype "bidirectional")
		)
		(pad "P2" smd circle
			(at -5.2 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 189 "/RX2_QD-")
			(pinfunction "PL32B/HS-/LDQSN32")
			(pintype "bidirectional")
		)
		(pad "P3" smd circle
			(at -4.4 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 150 "unconnected-(U1B-PL38B{slash}HS-{slash}LDQ44-PadP3)")
			(pinfunction "PL38B/HS-/LDQ44")
			(pintype "bidirectional")
		)
		(pad "P4" smd circle
			(at -3.6 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 255 "/TX2_ST+")
			(pinfunction "PL41A/HS+/LDQ44")
			(pintype "bidirectional")
		)
		(pad "P5" smd circle
			(at -2.8 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 472 "/SPI2x.MOSI")
			(pinfunction "PL47D/LLC_GPLL0C_IN/-/LDQSN44")
			(pintype "bidirectional")
		)
		(pad "P6" smd circle
			(at -2 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 283 "/FPGA/CLK_25MHz")
			(pinfunction "PL447C/LLC_GPLLT_IN/+/LDQSN44")
			(pintype "bidirectional")
		)
		(pad "P7" smd circle
			(at -1.2 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 144 "Net-(U1C-PB6B{slash}D4{slash}MOSI2{slash}IO4{slash}-)")
			(pinfunction "PB6B/D4/MOSI2/IO4/-")
			(pintype "bidirectional")
		)
		(pad "P8" smd circle
			(at -0.4 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 183 "Net-(U1C-PB13B{slash}CS1N{slash}-)")
			(pinfunction "PB13B/CS1N/-")
			(pintype "bidirectional")
		)
		(pad "P9" smd circle
			(at 0.4 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 236 "/FPGA/FPGA_DONE")
			(pinfunction "DONE")
			(pintype "bidirectional")
		)
		(pad "P10" smd circle
			(at 1.199999 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "Net-(U1H-CFG_1)")
			(pinfunction "CFG_1")
			(pintype "bidirectional")
		)
		(pad "P11" smd circle
			(at 1.999999 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 435 "/FPGA/PR47C")
			(pinfunction "PR47C/LRC_GPLL0T_IN/+/RDQ44")
			(pintype "bidirectional")
		)
		(pad "P12" smd circle
			(at 2.799999 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 434 "/FPGA/PR47D")
			(pinfunction "PR47D/LRC_GPLL0C_IN/-/RDQ44")
			(pintype "bidirectional")
		)
		(pad "P13" smd circle
			(at 3.599999 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 437 "/FPGA/PR41A")
			(pinfunction "PR41A/HS+/RDQ44")
			(pintype "bidirectional")
		)
		(pad "P14" smd circle
			(at 4.399999 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 440 "/FPGA/PR38B")
			(pinfunction "PR38B/HS/RDQ44")
			(pintype "bidirectional")
		)
		(pad "P15" smd circle
			(at 5.199999 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 123 "/FPGA/SDRAM_DQ10")
			(pinfunction "PR32B/HS-/RDQSN32")
			(pintype "bidirectional")
		)
		(pad "P16" smd circle
			(at 5.999999 4.399999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 124 "/FPGA/SDRAM_DQ9")
			(pinfunction "PR35A/HS+/RDQ32")
			(pintype "bidirectional")
		)
		(pad "R1" smd circle
			(at -6 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 274 "/TX2_QD-")
			(pinfunction "PL35B/VREF1_6/HS-/LDQ32")
			(pintype "bidirectional")
		)
		(pad "R2" smd circle
			(at -5.2 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 207 "/RX2_ST+")
			(pinfunction "PL38C/+/LDQ44")
			(pintype "bidirectional")
		)
		(pad "R3" smd circle
			(at -4.4 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 275 "/TX2_ST-")
			(pinfunction "PL41B/HS-/LDQ44")
			(pintype "bidirectional")
		)
		(pad "R4" smd circle
			(at -3.6 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 209 "/RX2_ID+")
			(pinfunction "PL41C/+/LDQ44")
			(pintype "bidirectional")
		)
		(pad "R5" smd circle
			(at -2.8 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 471 "/SPI2x.CLK")
			(pinfunction "PL44A/HS+/LDQS44")
			(pintype "bidirectional")
		)
		(pad "R6" smd circle
			(at -2 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 154 "Net-(U1C-PB4B{slash}D6{slash}IO6{slash}-)")
			(pinfunction "PB4B/D6/IO6/-")
			(pintype "bidirectional")
		)
		(pad "R7" smd circle
			(at -1.2 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 302 "Net-(U1C-PB6A{slash}D5{slash}MISO2{slash}IO5{slash}+)")
			(pinfunction "PB6A/D5/MISO2/IO5/+")
			(pintype "bidirectional")
		)
		(pad "R8" smd circle
			(at -0.4 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 308 "Net-(U1C-PB13A{slash}SN{slash}CSN{slash}+)")
			(pinfunction "PB13A/SN/CSN/+")
			(pintype "bidirectional")
		)
		(pad "R9" smd circle
			(at 0.4 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "/FPGA/FPGA_nPROG")
			(pinfunction "PROGRAMN")
			(pintype "bidirectional")
		)
		(pad "R10" smd circle
			(at 1.199999 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 400 "Net-(U1H-CFG_2)")
			(pinfunction "CFG_2")
			(pintype "bidirectional")
		)
		(pad "R11" smd circle
			(at 1.999999 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "/FPGA/JTAG1.TDI")
			(pinfunction "TDI")
			(pintype "bidirectional")
		)
		(pad "R12" smd circle
			(at 2.799999 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 242 "/FPGA/SDRAM_A5")
			(pinfunction "PR44A/HS+/RDQS44")
			(pintype "bidirectional")
		)
		(pad "R13" smd circle
			(at 3.599999 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 106 "/FPGA/SDRAM_A7")
			(pinfunction "PR41C/+/RDQ44")
			(pintype "bidirectional")
		)
		(pad "R14" smd circle
			(at 4.399999 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 246 "/FPGA/SDRAM_A11")
			(pinfunction "PR41B/HS-/RDQ44")
			(pintype "bidirectional")
		)
		(pad "R15" smd circle
			(at 5.199999 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 132 "/FPGA/SDRAM_x.CLK")
			(pinfunction "PR38C/+/RDQ44")
			(pintype "bidirectional")
		)
		(pad "R16" smd circle
			(at 5.999999 5.199999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 157 "/FPGA/SDRAM_DQ8")
			(pinfunction "PR35B/VREF1_3/HS-/RDQ32")
			(pintype "bidirectional")
		)
		(pad "T1" smd circle
			(at -6 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "T2" smd circle
			(at -5.2 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 224 "/RX2_ST-")
			(pinfunction "PL38D/-/LDQ44")
			(pintype "bidirectional")
		)
		(pad "T3" smd circle
			(at -4.4 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 180 "/RX2_ID-")
			(pinfunction "PL41D/-/LDQ44")
			(pintype "bidirectional")
		)
		(pad "T4" smd circle
			(at -3.6 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 184 "/RX2_EN")
			(pinfunction "PL44B/HS-/LDQSN44")
			(pintype "bidirectional")
		)
		(pad "T5" smd circle
			(at -2.8 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "T6" smd circle
			(at -2 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 309 "Net-(U1C-PB4A{slash}D7{slash}IO7{slash}+)")
			(pinfunction "PB4A/D7/IO7/+")
			(pintype "bidirectional")
		)
		(pad "T7" smd circle
			(at -1.2 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 235 "/FPGA/FLASH.MISO")
			(pinfunction "PB11A/D1/MISO/IO1/+")
			(pintype "bidirectional")
		)
		(pad "T8" smd circle
			(at -0.4 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 159 "/FPGA/FLASH.MOSI")
			(pinfunction "PB11B/D0/MOSI/IO0/-")
			(pintype "bidirectional")
		)
		(pad "T9" smd circle
			(at 0.4 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "Net-(U1H-INITN)")
			(pinfunction "INITN")
			(pintype "bidirectional")
		)
		(pad "T10" smd circle
			(at 1.199999 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "/FPGA/JTAG1.TCK")
			(pinfunction "TCK")
			(pintype "bidirectional")
		)
		(pad "T11" smd circle
			(at 1.999999 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 126 "/FPGA/JTAG1.TMS")
			(pinfunction "TMS")
			(pintype "bidirectional")
		)
		(pad "T12" smd circle
			(at 2.799999 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "T13" smd circle
			(at 3.599999 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 153 "/FPGA/SDRAM_A8")
			(pinfunction "PR44B/HS-/RDQSN44")
			(pintype "bidirectional")
		)
		(pad "T14" smd circle
			(at 4.399999 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 147 "/FPGA/SDRAM_A12")
			(pinfunction "PR41D/-/RDQ44")
			(pintype "bidirectional")
		)
		(pad "T15" smd circle
			(at 5.199999 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 248 "/FPGA/SDRAM_DQM1")
			(pinfunction "PR38D/-/RDQ44")
			(pintype "bidirectional")
		)
		(pad "T16" smd circle
			(at 5.999999 5.999999 180)
			(size 0.3556 0.3556)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(model ":T_LIBS:3d/t_BGA/caBGA256_LAT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 161.6964 75.0454 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C79"
			(at -1.8796 -0.1016 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 201 "Net-(U2C-RX2B-)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 198 "unconnected-(C79-Pad2)")
			(pintype "passive+no_connect")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 212.386 80.1)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R102"
			(at 0.212 1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 526 "/MISO_HARM_FLT_1V8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 541 "Net-(K1B-P6_1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_logos:Thales_15x2_Cu"
		(layer "F.Cu")
		(at 182.88 155.792)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_logos:Thales_15x2_Cu"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(locked yes)
		(layer "F.Cu")
		(at 196.85 52.033)
		(property "Reference" "REF**"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MTG_250_D125"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 154.559 142.457)
		(property "Reference" "TP23"
			(at 0 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 510 "/RF_RX_SPI_CLK_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_connectors:Banana_Horiz_Blk"
		(layer "F.Cu")
		(at 69.27 98.603 180)
		(property "Reference" "J17"
			(at 8.3608 -6.389 180)
			(layer "F.SilkS")
		)
		(property "Value" "BANANA_JACK"
			(at 0 -0.5 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_connectors:Banana_Horiz_Blk"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 7.6454 0 180)
			(size 3.048 3.048)
			(drill 2.032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -7.6454 0 180)
			(size 3.048 3.048)
			(drill 2.032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_connectors/AB2_90DEG_4MM_JACK_PTH-BLK.wrl"
			(hide yes)
			(offset
				(xyz -11.049 -4.826 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${T_LIBS}/3d/t_connectors/DELTRON_BLACK.STEP"
			(offset
				(xyz 7.8 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 151.511 88.5716 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C81"
			(at -2.3488 -0.1016 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "Net-(C81-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 216 "Net-(C81-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(locked yes)
		(layer "F.Cu")
		(at 196.85 133.35)
		(property "Reference" "REF**"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MTG_250_D125"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "t_sot:SSOP-8_TEX"
		(layer "F.Cu")
		(at 106.78795 56.087201 180)
		(tags "TCA9406")
		(property "Reference" "U18"
			(at 0 2.327001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCA9406"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_sot:SSOP-8_TEX"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9406.pdf?ts=1710769372418&ref_url=https%253A%252F%252Fwww.google.com%252F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "I2C Level Translator"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.2 -1.55 180)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.2 -1.55 180)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 -0.974999 180)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 155 "/FPGA/UART1_RX")
			(pinfunction "SDA_B")
			(pintype "open_collector")
		)
		(pad "2" smd rect
			(at -1.7 -0.325001 180)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.7 0.325001 180)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.7 0.974999 180)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 280 "/FPGA/UART1_RX_FPGA")
			(pinfunction "SDA_A")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at 1.7 0.974999 180)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 279 "/FPGA/UART1_TX_FPGA")
			(pinfunction "SCL_A")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.7 0.325001 180)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 310 "Net-(U18-OE)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 1.7 -0.325001 180)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 1.7 -0.974999 180)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 243 "/FPGA/UART1_TX")
			(pinfunction "SCL_B")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.3 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_crystal:FC-135"
		(layer "F.Cu")
		(at 120.4468 61.4364 -90)
		(property "Reference" "X1"
			(at 2.6616 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "12.000 MHz"
			(at 0 -0.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_crystal:FC-135"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.kyocera-crystal.jp/eng/wp-content/uploads/2014/09/cx2520db_e.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CX2520 SMT Crystal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1 0.1 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.25 0 270)
			(size 1 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-(U5-PD1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.25 0 270)
			(size 1 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U5-PD0)")
			(pinfunction "3")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 152.527 88.5462 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C80"
			(at -2.3996 0.0254 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 208 "Net-(C80-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 205 "Net-(C80-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 156.7942 66.8236 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C76"
			(at -1.9636 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 177 "Net-(U2C-RX2A+)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 182 "Net-(T2-SECONDARY_DOT)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 151.6126 64.352 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C85"
			(at 2.1336 -0.2286 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 157.099 157.57)
		(property "Reference" "TP20"
			(at 0 2.667 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 507 "/RF_TX_SPI_DI_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 136.779 142.457)
		(property "Reference" "TP9"
			(at 0.254 -2.159 -90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 539 "/DGPIO_7_1P8_THRU")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_Mech_Switch:OS10201"
		(layer "F.Cu")
		(at 70.195 50.834 180)
		(descr "SPDP Slide Switch - Through Hole Side Switch")
		(property "Reference" "SW2"
			(at 0.345 -3.358 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SWITCH_2P_1C"
			(at 1.234 -4.501 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_Mech_Switch:OS10201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "1825232-1_TEC")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2 0 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 545 "unconnected-(SW2-Pad1)")
			(pinfunction "1")
			(pintype "unspecified+no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 0 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/FPGA/STM_~{RST}")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 2 0 180)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at -4.1 0 180)
			(size 2.1 2.1)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "m")
			(pintype "unspecified")
		)
		(pad "5" thru_hole circle
			(at 4.1 0 180)
			(size 2.1 2.1)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "m")
			(pintype "unspecified")
		)
		(model "${T_LIBS}/3d/t_Mech_Switch/OS102011MA1QN1.stp"
			(offset
				(xyz 0 0 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "F.Cu")
		(at 125.9332 64.1996 180)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C47"
			(at -1.8542 0.2794 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 0.5 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 180)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "+1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 180)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 112.649 53.8022 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R9"
			(at 0.0166 -0.9906 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 94 "Net-(U5-PB2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 86.106 157.951)
		(property "Reference" "TP14"
			(at -0.127 2.413 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 504 "/NDB_FMCA_SDA_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 166.497 90.768)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R98"
			(at -0.127 -1.143 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 520 "Net-(X3-OE)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 161.6368 82.6146 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C74"
			(at -2.0408 -0.3302 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 173 "Net-(U2B-RX1B+)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 172 "unconnected-(C74-Pad2)")
			(pintype "passive+no_connect")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 161.6114 79.6936 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C75"
			(at -1.99 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 176 "Net-(U2B-RX1B-)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 174 "unconnected-(C75-Pad2)")
			(pintype "passive+no_connect")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 83.566 142.584)
		(property "Reference" "TP17"
			(at 0.127 -2.413 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 535 "/NDB_FMCA_SCL_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_do:DO-214AC"
		(layer "F.Cu")
		(at 65.913 91.022 180)
		(descr "Diode SMA")
		(tags "Diode SMA")
		(property "Reference" "Z1"
			(at 5.2324 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "TVS-BI"
			(at 0 4.3 180)
			(layer "F.Fab")
		)
		(property "Footprint" "t_do:DO-214AC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 428 "Net-(Z1-K)")
			(pinfunction "K")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 2 0 180)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "A")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_do/DO-214AC(SMA).step"
			(offset
				(xyz 0 0 1.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_connectors:SAMTEC-HTST-115-01-X-DV"
		(locked yes)
		(layer "F.Cu")
		(at 144.399 149.823)
		(descr "translated Allegro footprint")
		(property "Reference" "JSDB5"
			(at -25.3785 6.7495 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x15_HTST_115_01_L"
			(at 0 0.5725 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:SAMTEC-HTST-115-01-X-DV"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x15, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "30"
			(at 23.651 -2.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "29"
			(at 23.651 4.254 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -24.68 4.254 0)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -24.68 -2.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "9.271"
			(at -26.744 0.127 0)
			(layer "Dwgs.User")
		)
		(fp_text user "45.720"
			(at -0.8 9.512 0)
			(layer "Dwgs.User")
		)
		(fp_text user "6.858"
			(at -24.917 0.127 0)
			(layer "Dwgs.User")
		)
		(fp_text user "43.180"
			(at -0.8 -8.877 0)
			(layer "Dwgs.User")
		)
		(fp_text user "2.540"
			(at -20.409 -7.112 0)
			(layer "Dwgs.User")
		)
		(fp_text user "35.560"
			(at -0.8 -8.001 0)
			(layer "Dwgs.User")
		)
		(fp_text user "2"
			(at -24.68 -2.604 0)
			(layer "F.Fab")
		)
		(fp_text user "30"
			(at 23.651 -2.604 0)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at -24.68 4.254 0)
			(layer "F.Fab")
		)
		(fp_text user "29"
			(at 23.651 4.254 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -17.78 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -17.78 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -15.24 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 490 "/DGPIO_0_1P8_THRU")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -15.24 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 512 "/DGPIO_1_1P8_THRU")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -12.7 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 500 "/DGPIO_2_1P8_THRU")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -12.7 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 516 "/DGPIO_3_1P8_THRU")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -10.16 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 523 "/DGPIO_4_1P8_THRU")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -10.16 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 538 "/DGPIO_5_1P8_THRU")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -7.62 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 537 "/DGPIO_6_1P8_THRU")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -7.62 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 539 "/DGPIO_7_1P8_THRU")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -5.08 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 534 "/DGPIO_8_1P8_THRU")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -5.08 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 529 "/DGPIO_9_1P8_THRU")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -2.54 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 532 "/DGPIO_10_1P8_THRU")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -2.54 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 531 "/DGPIO_11_1P8_THRU")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 0 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 0 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 2.54 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 2.54 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 5.08 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 5.08 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 7.62 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 514 "/RF_TX_SPI_CS_1P8")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 7.62 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 513 "/RF_RX_SPI_CS_1P8")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 10.16 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 518 "/RF_TX_SPI_CLK_1P8")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 10.16 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 510 "/RF_RX_SPI_CLK_1P8")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 12.7 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 507 "/RF_TX_SPI_DI_1P8")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at 12.7 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 511 "/RF_RX_SPI_DI_1P8")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 15.24 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 508 "/RF_TX_SPI_DO_1P8")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 15.24 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 517 "/RF_RX_SPI_DO_1P8")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 17.78 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 515 "unconnected-(JSDB5-Pin_29-Pad29)")
			(pinfunction "Pin_29")
			(pintype "passive+no_connect")
		)
		(pad "30" smd rect
			(at 17.78 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 509 "/RF_READY")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_connectors/HTST-115-01-L-DV.stp"
			(offset
				(xyz 0 0 1.27)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 120.5904 57.7226 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R8"
			(at 0.0596 0.9906 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "/FPGA/STM_~{RST}")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 126.9492 65.5204 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R54"
			(at -2.0574 0.0508 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 400 "Net-(U1H-CFG_2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_crystal:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm"
		(layer "F.Cu")
		(at 172.847 86.493)
		(descr "SMD Crystal Oscillator Seiko Epson SG-8002LB https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC, 5.0x3.2mm^2 package")
		(tags "SMD SMT crystal oscillator")
		(property "Reference" "X3"
			(at 3.175 0.211 -90)
			(layer "F.SilkS")
		)
		(property "Value" "SG-5032CCN"
			(at 0 2.85 180)
			(layer "F.Fab")
		)
		(property "Footprint" "t_crystal:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG5032CCN&lang=en"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CMOS Clock Oscillator 2.5 to 50 MHz"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Oscillator*SMD*SeikoEpson*SG8002LB*5.0x3.2mm*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.27 1.1)
			(size 1.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 520 "Net-(X3-OE)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.27 1.1)
			(size 1.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 1.27 -1.1)
			(size 1.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 519 "Net-(X3-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -1.27 -1.1)
			(size 1.6 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 136.4068 63.6154 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R18"
			(at -1.9978 0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 282 "Net-(U6-Standby)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SSOP-8_TEX"
		(layer "F.Cu")
		(at 125.9332 61.3294 90)
		(tags "TCA9406")
		(property "Reference" "U19"
			(at 0 2.4384 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCA9406"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_sot:SSOP-8_TEX"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9406.pdf?ts=1710769372418&ref_url=https%253A%252F%252Fwww.google.com%252F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "I2C Level Translator"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.2 -1.55 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.2 -1.55 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 -0.974999 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 287 "/FPGA/sJTAG2_TMS")
			(pinfunction "SDA_B")
			(pintype "open_collector")
		)
		(pad "2" smd rect
			(at -1.7 -0.325001 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.7 0.325001 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.7 0.974999 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 239 "/FPGA/JTAG2.TMS")
			(pinfunction "SDA_A")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at 1.7 0.974999 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 141 "/FPGA/JTAG2.TDI")
			(pinfunction "SCL_A")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.7 0.325001 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 285 "Net-(U17-OE)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 1.7 -0.325001 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 1.7 -0.974999 90)
			(size 1.1 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 289 "/FPGA/sJTAG2_TDI")
			(pinfunction "SCL_B")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1.3 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Oscillator:Oscillator_SMD_Abracon_ASDMB-4Pin_2.5x2.0mm"
		(layer "F.Cu")
		(at 135.8016 65.7272 180)
		(descr "Miniature Crystal Clock Oscillator Abracon ASDMB series, 2.5x2.0mm package, http://www.abracon.com/Oscillators/ASDMB.pdf")
		(tags "SMD SMT crystal oscillator")
		(property "Reference" "U6"
			(at 1.5118 2.1372 180)
			(layer "F.SilkS")
		)
		(property "Value" "ASDMB-25.00MHz"
			(at 0 2.45 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Oscillator:Oscillator_SMD_Abracon_ASDMB-4Pin_2.5x2.0mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://abracon.com/Oscillators/ASDMB.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1.8-3.3V SMD Ultra Miniature Crystal Clock Oscillator, Abracon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Oscillator*SMD*Abracon*ASDMB*2.5x2.0mm*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0.775 180)
			(size 0.65 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 282 "Net-(U6-Standby)")
			(pinfunction "Standby")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.825 0.775 180)
			(size 0.65 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 0.825 -0.775 180)
			(size 0.65 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 283 "/FPGA/CLK_25MHz")
			(pinfunction "Out")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -0.825 -0.775 180)
			(size 0.65 0.85)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 281 "+1.8V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_Abracon_ASDMB-4Pin_2.5x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(locked yes)
		(layer "F.Cu")
		(at 61.595 52.033)
		(property "Reference" "REF**"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MTG_250_D125"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 174.244 83.234 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R67"
			(at 0 -0.9144 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 519 "Net-(X3-OUT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(C90-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:ind_0402PA"
		(layer "F.Cu")
		(at 152.5016 86.5142 90)
		(descr "SMT Inductor, 0402")
		(property "Reference" "L2"
			(at 1.7152 0.1524 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1.2nH"
			(at 0 0.4826 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:ind_0402PA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 317 "Net-(U2D-TX1+)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 208 "Net-(C80-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-0402PA.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 161.6202 81.624)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R26"
			(at 2.0828 0.1016 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 323 "Net-(U2F-EXT_LO1+)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 150.495 50.9408 90)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "P1"
			(at -0.127 -2.7432 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X08"
			(at 0 20.11 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X08 Pin_Header_Angled_1X08 Socket_Strip_Straight_1X08 Socket_Strip_Angled_1X08")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 422 "/DG_08")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 418 "/DG_00")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 416 "/DG_01")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 424 "/AG_04")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 347 "/AG_03")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 395 "/AG_02")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 136.779 157.57)
		(property "Reference" "TP11"
			(at 0 2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 537 "/DGPIO_6_1P8_THRU")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 134.239 142.457)
		(property "Reference" "TP10"
			(at 0 -2.413 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 538 "/DGPIO_5_1P8_THRU")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 132.715 53.303 90)
		(descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 2.54mm double row")
		(property "Reference" "J14"
			(at 2.5654 -2.8956 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_2x5"
			(at 1.27 12.49 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "Net-(U1C-PB4A{slash}D7{slash}IO7{slash}+)")
			(pinfunction "1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "Net-(U1C-PB4B{slash}D6{slash}IO6{slash}-)")
			(pinfunction "2")
			(pintype "power_out")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 302 "Net-(U1C-PB6A{slash}D5{slash}MISO2{slash}IO5{slash}+)")
			(pinfunction "3")
			(pintype "power_out")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 144 "Net-(U1C-PB6B{slash}D4{slash}MOSI2{slash}IO4{slash}-)")
			(pinfunction "4")
			(pintype "power_out")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "Net-(U1C-PB13A{slash}SN{slash}CSN{slash}+)")
			(pinfunction "5")
			(pintype "power_out")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 183 "Net-(U1C-PB13B{slash}CS1N{slash}-)")
			(pinfunction "6")
			(pintype "power_out")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 299 "Net-(U1C-PB15B{slash}DOUT{slash}CS0N{slash}-)")
			(pinfunction "7")
			(pintype "power_out")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 212 "Net-(U1C-PB18A{slash}WRITEN)")
			(pinfunction "8")
			(pintype "power_out")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "9")
			(pintype "power_out")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "10")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 157.099 142.457)
		(property "Reference" "TP24"
			(at 0 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 511 "/RF_RX_SPI_DI_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 104.14 72.353)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "J22"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 12.49 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 437 "/FPGA/PR41A")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 442 "/FPGA/PR32D")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 447 "/FPGA/PR29A")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 453 "/FPGA/PR14C")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 458 "/FPGA/PR8D")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:ind_0603cs"
		(layer "F.Cu")
		(at 153.6954 86.7682 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "L1"
			(at -0.1658 -1.3208 90)
			(layer "F.SilkS")
		)
		(property "Value" "220nH"
			(at 0 0.6096 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:ind_0603cs"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 317 "Net-(U2D-TX1+)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-0603CS.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -90)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 211.709 150.458)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R106"
			(at -2.032 -0.889 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 528 "/TX_ATTEN_LE_1V8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 542 "Net-(K1B-P6_5)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 212.09 83.656 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R110"
			(at 2.159 -0.508 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 491 "/SCLK_RX_PATH_1V8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 543 "Net-(K1B-P6_2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 125.6792 65.5204 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R55"
			(at -2.0828 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 401 "Net-(U1H-CFG_0)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 150.368 89.063 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C86"
			(at 0.054 1.143 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "F.Cu")
		(at 111.76 102.7314 90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 1.905 -0.0508 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 0.5 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 281 "+1.8V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 90)
			(size 0.4 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 211.074 152.998 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R107"
			(at 2.413 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 540 "Net-(K1B-P6_0)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 530 "/MOSI_TX_BOARD_1V8")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:SAMTEC-HTST-115-01-X-DV"
		(locked yes)
		(layer "F.Cu")
		(at 91.186 149.759)
		(descr "translated Allegro footprint")
		(property "Reference" "JSDB4"
			(at -25.3785 6.7495 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x15_HTST_115_01_L"
			(at 0 0.5725 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:SAMTEC-HTST-115-01-X-DV"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x15, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "29"
			(at 23.651 4.254 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -24.68 4.254 0)
			(layer "F.SilkS")
		)
		(fp_text user "30"
			(at 23.651 -2.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -24.68 -2.604 0)
			(layer "F.SilkS")
		)
		(fp_text user "6.858"
			(at -24.917 0.127 0)
			(layer "Dwgs.User")
		)
		(fp_text user "45.720"
			(at -0.8 9.512 0)
			(layer "Dwgs.User")
		)
		(fp_text user "9.271"
			(at -26.744 0.127 0)
			(layer "Dwgs.User")
		)
		(fp_text user "2.540"
			(at -20.409 -7.112 0)
			(layer "Dwgs.User")
		)
		(fp_text user "43.180"
			(at -0.8 -8.877 0)
			(layer "Dwgs.User")
		)
		(fp_text user "35.560"
			(at -0.8 -8.001 0)
			(layer "Dwgs.User")
		)
		(fp_text user "30"
			(at 23.651 -2.604 0)
			(layer "F.Fab")
		)
		(fp_text user "29"
			(at 23.651 4.254 0)
			(layer "F.Fab")
		)
		(fp_text user "1"
			(at -24.68 4.254 0)
			(layer "F.Fab")
		)
		(fp_text user "2"
			(at -24.68 -2.604 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -17.78 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -17.78 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -15.24 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 45 "/SPI2.CLK")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -15.24 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 42 "/SPI2.MOSI")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -12.7 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 23 "/SPI2.MISO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -12.7 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 43 "/SPI2.CE")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -10.16 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 9 "/FP_83")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -10.16 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 33 "/FP_82")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -7.62 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 493 "/NDB_RESET_1P8")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -7.62 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 535 "/NDB_FMCA_SCL_1P8")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -5.08 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 504 "/NDB_FMCA_SDA_1P8")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -5.08 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 487 "/AGPIO_1")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -2.54 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 494 "/NDB_FMC_INT_1P8")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -2.54 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 499 "/nTOP_PTT_1P8")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 0 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 0 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 2.54 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 536 "/+12V")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 2.54 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 536 "/+12V")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 5.08 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 536 "/+12V")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 5.08 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 536 "/+12V")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 7.62 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 7.62 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 10.16 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 10.16 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 232 "GND")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 12.7 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 501 "unconnected-(JSDB4-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
		)
		(pad "26" smd rect
			(at 12.7 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 495 "unconnected-(JSDB4-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
		)
		(pad "27" smd rect
			(at 15.24 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 502 "unconnected-(JSDB4-Pin_27-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive+no_connect")
		)
		(pad "28" smd rect
			(at 15.24 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 505 "unconnected-(JSDB4-Pin_28-Pad28)")
			(pinfunction "Pin_28")
			(pintype "passive+no_connect")
		)
		(pad "29" smd rect
			(at 17.78 3.62)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 497 "unconnected-(JSDB4-Pin_29-Pad29)")
			(pinfunction "Pin_29")
			(pintype "passive+no_connect")
		)
		(pad "30" smd rect
			(at 17.78 -3.238)
			(size 1.27 5.08)
			(layers "F.Cu" "F.Paste")
			(net 498 "unconnected-(JSDB4-Pin_30-Pad30)")
			(pinfunction "Pin_30")
			(pintype "passive+no_connect")
		)
		(model "${T_LIBS}/3d/t_connectors/HTST-115-01-L-DV.stp"
			(offset
				(xyz 0 0 1.27)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 165.5572 77.2044 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R33"
			(at 0 -0.9144 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "Net-(U2F-DEV_CLK_IN-)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 313 "Net-(U2F-DEV_CLK_IN+)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 94.3356 57.2654)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R11"
			(at -2.3368 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 87 "Net-(J1-CC1_B)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 99.7712 57.24 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R10"
			(at -2.2098 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 89 "Net-(J1-CC1_A)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 122.0724 62.5374 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C2"
			(at 0.1128 -1.143 90)
			(layer "F.SilkS")
		)
		(property "Value" "20pF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U5-PD0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 165.5318 79.2618 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C89"
			(at 2.0574 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U21-OUT+)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 315 "Net-(U2F-DEV_CLK_IN-)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:TENSILITY_54-00164"
		(layer "F.Cu")
		(at 64.48 65.583 -90)
		(property "Reference" "J18"
			(at -6.4888 -0.5948 180)
			(layer "F.SilkS")
		)
		(property "Value" "54-00164"
			(at 6.985 -8.8625 90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:TENSILITY_54-00164"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://tensility.s3.amazonaws.com/uploads/pdffiles/54-00164.pdf?X-Amz-Expires=600&X-Amz-Date=20240331T163449Z&X-Amz-Algorithm=AWS4-HMAC-SHA256&X-Amz-Credential=AKIAIS2S4WRDQDSWDRZQ%2F20240331%2Fus-west-2%2Fs3%2Faws4_request&X-Amz-SignedHeaders=host&X-Amz-Signature=dd187ecc808e980761eec5cc10a40fa574f70948ad1b5e55d355e12e2c7dea64"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5.5mm Power Connector"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "54-00164"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "11.3mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "TENSILITY"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(pad "" np_thru_hole circle
			(at 0 -2.25 270)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 2.25 270)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -5.5 2.25 270)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(F1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "A2" smd rect
			(at -5.5 -3.95 270)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(F1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "B" smd rect
			(at 5.5 2.25 270)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "C" smd rect
			(at 5.5 -3.95 270)
			(size 2 2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(model "${T_LIBS}/3d/t_connectors/54-00164.step"
			(offset
				(xyz 0 0 0.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_1210_3225Metric"
		(layer "F.Cu")
		(at 65.659 87.339)
		(descr "Fuse SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "F1"
			(at 3.3274 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "FUSE"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Fuse:Fuse_1210_3225Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0)
			(size 1.25 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2)
			(net 72 "Net-(F1-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at 1.4 0)
			(size 1.25 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2)
			(net 428 "Net-(Z1-K)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${KICAD8_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 99.949 102.6678 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R22"
			(at -2.4002 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 278 "/I2C_SEL")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 284 "Net-(Q1-B)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_do:DO-214AC"
		(layer "F.Cu")
		(at 83.0326 86.9646 90)
		(descr "Diode SMA")
		(tags "Diode SMA")
		(property "Reference" "D3"
			(at -4.3368 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "DIODESCH"
			(at 0 4.3 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "t_do:DO-214AC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D? S*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "+5.0V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 429 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_do/DO-214AC(SMA).step"
			(offset
				(xyz 0 0 1.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 157.48 86.5992 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C73"
			(at -1.8828 0.0762 -90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 171 "Net-(U2B-RX1A-)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 167 "Net-(T1-SECONDARY_DOT)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 210.185 80.1 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R32"
			(at 0 -1.016 180)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 503 "/MISO_BPFS_1V8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 541 "Net-(K1B-P6_1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:sot-23"
		(layer "F.Cu")
		(at 93.7514 59.5006)
		(descr "SOT-23")
		(property "Reference" "Q5"
			(at -2.4638 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3906"
			(at 0 0.0762 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_sot:sot-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3906-D.PDF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -0.9525 1.05664)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 399 "Net-(Q5-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.9525 1.05664)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1.05664)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 398 "Net-(Q5-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-3.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
		(layer "F.Cu")
		(at 114.7272 59.4563 180)
		(descr "QFN, 36 Pin (www.st.com/resource/en/datasheet/stm32f101t6.pdf#page=72), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U5"
			(at 2.764 -4.5147 180)
			(layer "F.SilkS")
		)
		(property "Value" "STM32F103T8Ux"
			(at 0 4.33 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32f103t8.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M3 MCU, 64KB flash, 20KB RAM, 72 MHz, 2.0-3.6V, 26 GPIO, VFQFPN36"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*6x6mm*P0.5mm*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -1.37 -1.37 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "" smd roundrect
			(at -1.37 0 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "" smd roundrect
			(at -1.37 1.37 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "" smd roundrect
			(at 0 -1.37 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "" smd roundrect
			(at 0 0 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "" smd roundrect
			(at 0 1.37 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "" smd roundrect
			(at 1.37 -1.37 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "" smd roundrect
			(at 1.37 0 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "" smd roundrect
			(at 1.37 1.37 180)
			(size 1.1 1.1)
			(layers "F.Paste")
			(roundrect_rratio 0.227273)
		)
		(pad "1" smd roundrect
			(at -2.8375 -2 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8375 -1.5 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U5-PD0)")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.8375 -1 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "Net-(U5-PD1)")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.8375 -0.5 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "/FPGA/STM_~{RST}")
			(pinfunction "NRST")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.8375 0 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pinfunction "VSSA")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -2.8375 0.5 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -2.8375 1 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 289 "/FPGA/sJTAG2_TDI")
			(pinfunction "PA0")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -2.8375 1.5 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 286 "/FPGA/sJTAG2_TDO")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -2.8375 2 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 253 "/FPGA/D_UART2_TX")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -2 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 252 "/FPGA/D_UART2_RX")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -1.5 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 134 "/FPGA/FLASH.CS")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -1 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 85 "/FPGA/FLASH.CLK")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -0.5 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 235 "/FPGA/FLASH.MISO")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 0 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 159 "/FPGA/FLASH.MOSI")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 0.5 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 254 "/FPGA/USB_ENUM")
			(pinfunction "PB0")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 1 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 250 "/FPGA/LED_RUN")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 1.5 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 94 "Net-(U5-PB2)")
			(pinfunction "PB2")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 2 2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at 2.8375 2 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at 2.8375 1.5 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 251 "/FPGA/MCO")
			(pinfunction "PA8")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 2.8375 1 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 243 "/FPGA/UART1_TX")
			(pinfunction "PA9")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 2.8375 0.5 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 155 "/FPGA/UART1_RX")
			(pinfunction "PA10")
			(pintype "bidirectional")
		)
		(pad "23" smd roundrect
			(at 2.8375 0 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 71 "/FPGA/USB_N")
			(pinfunction "PA11")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at 2.8375 -0.5 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "/FPGA/USB_P")
			(pinfunction "PA12")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at 2.8375 -1 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 287 "/FPGA/sJTAG2_TMS")
			(pinfunction "PA13")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 2.8375 -1.5 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "27" smd roundrect
			(at 2.8375 -2 180)
			(size 1.075 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at 2 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 288 "/FPGA/sJTAG2_CLK")
			(pinfunction "PA14")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at 1.5 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 236 "/FPGA/FPGA_DONE")
			(pinfunction "PA15")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 1 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 100 "/FPGA/JTAG1.TDO")
			(pinfunction "PB3")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 0.5 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "/FPGA/JTAG1.TMS")
			(pinfunction "PB4")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 0 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 115 "/FPGA/JTAG1.TDI")
			(pinfunction "PB5")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at -0.5 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 78 "/FPGA/JTAG1.TCK")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at -1 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "/FPGA/FPGA_nPROG")
			(pinfunction "PB7")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at -1.5 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 92 "Net-(U5-BOOT0)")
			(pinfunction "BOOT0")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at -2 -2.8375 180)
			(size 0.25 1.075)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at 0 0 180)
			(size 4.1 4.1)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 232 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-36-1EP_6x6mm_P0.5mm_EP4.1x4.1mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:ind_0402PA"
		(layer "F.Cu")
		(at 153.4922 67.0832 -90)
		(descr "SMT Inductor, 0402")
		(property "Reference" "L6"
			(at 1.536 -0.2032 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.2nH"
			(at 0 0.4826 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:ind_0402PA"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 319 "Net-(U2E-TX2+)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 219 "Net-(C82-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-0402PA.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_coilcraft:ind_0402PA"
		(layer "F.Cu")
		(at 151.5364 86.5142 90)
		(descr "SMT Inductor, 0402")
		(property "Reference" "L3"
			(at 1.7152 -0.1778 -90)
			(layer "F.SilkS")
		)
		(property "Value" "1.2nH"
			(at 0 0.4826 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:ind_0402PA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 318 "Net-(U2D-TX1-)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 213 "Net-(C81-Pad1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-0402PA.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 96.6978 58.5354)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R58"
			(at 0.0762 -1.0668 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "/FPGA/USB_P")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 398 "Net-(Q5-C)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 161.6964 73.0134)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R25"
			(at 1.905 0.0254 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 322 "Net-(U2F-EXT_LO2+)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 161.6202 78.6268)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R29"
			(at 2.032 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 326 "Net-(U2F-MCS-)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_RF_conn:CONN1_5-1814832-2_TEC"
		(layer "F.Cu")
		(at 166.37 58.51)
		(tags "5-1814832-2 ")
		(property "Reference" "J3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SMA_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_RF_conn:CONN1_5-1814832-2_TEC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1-1773725-8_RF_COAX_QRG&DocType=Data+Sheet&DocLang=English&DocFormat=pdf&PartCntxt=5-1814832-2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.0066 2.0066)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 330 "Net-(J3-RF)")
			(pinfunction "RF")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 2.54 2.54)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_RF_conn/c-5-1814832-2-c-3d.stp"
			(offset
				(xyz 0 0 10)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_MtgHoles:MTG_250_D125"
		(locked yes)
		(layer "F.Cu")
		(at 61.595 133.35)
		(property "Reference" "REF**"
			(at 0 0.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MTG_250_D125"
			(at 0 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_MtgHoles:MTG_250_D125"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
	)
	(footprint "Cy8CMod_062_4343W:CY8CPROTO-062-4343W"
		(locked yes)
		(layer "F.Cu")
		(at 124.079 108.966 180)
		(property "Reference" "K1"
			(at 0 2.4 180)
			(layer "F.SilkS")
		)
		(property "Value" "CY8CPROTO-062-4343W"
			(at 0 -2.4 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Cy8CMod_062_4343W:CY8CPROTO-062-4343W"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PSOC6 eval board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${VALUE}"
			(at 0.254 -5.08 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -49.53 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at -46.99 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(K1A-VTARG-Pad2)")
			(pinfunction "VTARG")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at -44.45 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/SFL_BPFS_1V8")
			(pinfunction "P10_0")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at -41.91 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(K1A-P10_3-Pad4)")
			(pinfunction "P10_3")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at -39.37 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(K1A-P10_4-Pad5)")
			(pinfunction "P10_4")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at -36.83 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(K1A-P10_2-Pad6)")
			(pinfunction "P10_2")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at -34.29 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 487 "/AGPIO_1")
			(pinfunction "P10_1")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at -31.75 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(K1A-P10_5-Pad8)")
			(pinfunction "P10_5")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at -29.21 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 465 "/FP_05")
			(pinfunction "P0_5")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at -26.67 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 466 "/FP_123")
			(pinfunction "P12_3")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at -24.13 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/QSPI.I2")
			(pinfunction "P11_4")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at -21.59 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/QSPI.I3")
			(pinfunction "P11_3")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at -19.05 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/QSPI.~{CE}")
			(pinfunction "P11_2")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at -16.51 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/QSPI.SCLK")
			(pinfunction "P11_7")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at -13.97 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/QSPI.I1")
			(pinfunction "P11_5")
			(pintype "input")
		)
		(pad "16" thru_hole oval
			(at -11.43 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/QSPI.I0")
			(pinfunction "P11_6")
			(pintype "input")
		)
		(pad "17" thru_hole oval
			(at -8.89 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 461 "/FP_125")
			(pinfunction "P12_5")
			(pintype "input")
		)
		(pad "18" thru_hole oval
			(at -6.35 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 464 "/FP_120")
			(pinfunction "P12_0")
			(pintype "input")
		)
		(pad "19" thru_hole oval
			(at -3.81 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 459 "/FP_121")
			(pinfunction "P12_1")
			(pintype "input")
		)
		(pad "20" thru_hole oval
			(at -1.27 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 202 "/FP_124")
			(pinfunction "P12_4")
			(pintype "input")
		)
		(pad "21" thru_hole oval
			(at 1.27 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(K1A-VDDIO_0-Pad21)")
			(pinfunction "VDDIO_0")
			(pintype "input")
		)
		(pad "22" thru_hole oval
			(at 3.81 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 463 "/FP_131")
			(pinfunction "P13_1")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 6.35 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 206 "/FP_132")
			(pinfunction "P13_2")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 8.89 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 460 "/FP_133")
			(pinfunction "P13_3")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 11.43 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 462 "/FP_130")
			(pinfunction "P13_0")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 13.97 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 276 "/I2C_SCL")
			(pinfunction "P13_4")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 16.51 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 199 "/I2C_SDA")
			(pinfunction "P13_5")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 19.05 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "29" thru_hole oval
			(at 21.59 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(K1A-P13_7-Pad29)")
			(pinfunction "P13_7")
			(pintype "input")
		)
		(pad "30" thru_hole oval
			(at 24.13 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 278 "/I2C_SEL")
			(pinfunction "P13_6")
			(pintype "input")
		)
		(pad "31" thru_hole oval
			(at 26.67 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(K1A-P0_4-Pad31)")
			(pinfunction "P0_4")
			(pintype "input")
		)
		(pad "32" thru_hole oval
			(at 29.21 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J23-Pin_1)")
			(pinfunction "VTARG")
			(pintype "input")
		)
		(pad "33" thru_hole oval
			(at 31.75 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "34" thru_hole oval
			(at 34.29 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J23-Pin_3)")
			(pinfunction "XRES")
			(pintype "input")
		)
		(pad "35" thru_hole oval
			(at 36.83 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J23-Pin_4)")
			(pinfunction "P6_7")
			(pintype "input")
		)
		(pad "36" thru_hole oval
			(at 39.37 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(J23-Pin_5)")
			(pinfunction "P6_6")
			(pintype "input")
		)
		(pad "37" thru_hole oval
			(at 41.91 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(K1A-BT_UART_RXD-Pad37)")
			(pinfunction "BT_UART_RXD")
			(pintype "input")
		)
		(pad "38" thru_hole oval
			(at 44.45 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(K1A-BT_UART_CTS-Pad38)")
			(pinfunction "BT_UART_CTS")
			(pintype "input")
		)
		(pad "39" thru_hole oval
			(at 46.99 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(K1A-BT_UART_RTS-Pad39)")
			(pinfunction "BT_UART_RTS")
			(pintype "input")
		)
		(pad "40" thru_hole oval
			(at 49.53 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(K1A-BT_UART_TXD-Pad40)")
			(pinfunction "BT_UART_TXD")
			(pintype "input")
		)
		(pad "41" thru_hole rect
			(at -49.53 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(K1B-Vref-Pad41)")
			(pinfunction "Vref")
			(pintype "input")
		)
		(pad "42" thru_hole oval
			(at -46.99 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "43" thru_hole oval
			(at -44.45 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(K1B-VBACKUP-Pad43)")
			(pinfunction "VBACKUP")
			(pintype "input")
		)
		(pad "44" thru_hole oval
			(at -41.91 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 316 "/RX_PATH_DISABLE_1V8")
			(pinfunction "P9_6")
			(pintype "input")
		)
		(pad "45" thru_hole oval
			(at -39.37 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 506 "/RX{slash}RESET_1V8")
			(pinfunction "P9_7")
			(pintype "input")
		)
		(pad "46" thru_hole oval
			(at -36.83 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 494 "/NDB_FMC_INT_1P8")
			(pinfunction "P9_4")
			(pintype "input")
		)
		(pad "47" thru_hole oval
			(at -34.29 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/SPI2.MISO")
			(pinfunction "P9_1")
			(pintype "input")
		)
		(pad "48" thru_hole oval
			(at -31.75 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/SPI2.CLK")
			(pinfunction "P9_2")
			(pintype "input")
		)
		(pad "49" thru_hole oval
			(at -29.21 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/FP_80")
			(pinfunction "P8_0")
			(pintype "input")
		)
		(pad "50" thru_hole oval
			(at -26.67 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "51" thru_hole oval
			(at -24.13 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/FP_87")
			(pinfunction "P8_7")
			(pintype "input")
		)
		(pad "52" thru_hole oval
			(at -21.59 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/FP_83")
			(pinfunction "P8_3")
			(pintype "input")
		)
		(pad "53" thru_hole oval
			(at -19.05 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/FP_84")
			(pinfunction "P8_4")
			(pintype "input")
		)
		(pad "54" thru_hole oval
			(at -16.51 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/FP_86")
			(pinfunction "P8_6")
			(pintype "input")
		)
		(pad "55" thru_hole oval
			(at -13.97 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/FP_81")
			(pinfunction "P8_1")
			(pintype "input")
		)
		(pad "56" thru_hole oval
			(at -11.43 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 544 "Net-(K1B-P6_3)")
			(pinfunction "P6_3")
			(pintype "input")
		)
		(pad "57" thru_hole oval
			(at -8.89 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(K1B-P1_0-Pad57)")
			(pinfunction "P1_0")
			(pintype "input")
		)
		(pad "58" thru_hole oval
			(at -6.35 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/FP_82")
			(pinfunction "P8_2")
			(pintype "input")
		)
		(pad "59" thru_hole oval
			(at -3.81 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/FP_85")
			(pinfunction "P8_5")
			(pintype "input")
		)
		(pad "60" thru_hole oval
			(at -1.27 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/SPI2.CE")
			(pinfunction "P9_3")
			(pintype "input")
		)
		(pad "61" thru_hole oval
			(at 1.27 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 493 "/NDB_RESET_1P8")
			(pinfunction "P9_5")
			(pintype "input")
		)
		(pad "62" thru_hole oval
			(at 3.81 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/SPI2.MOSI")
			(pinfunction "P9_0")
			(pintype "input")
		)
		(pad "63" thru_hole oval
			(at 6.35 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "64" thru_hole oval
			(at 8.89 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(K1B-P6_VDD-Pad64)")
			(pinfunction "P6_VDD")
			(pintype "input")
		)
		(pad "65" thru_hole oval
			(at 11.43 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 542 "Net-(K1B-P6_5)")
			(pinfunction "P6_5")
			(pintype "input")
		)
		(pad "66" thru_hole oval
			(at 13.97 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(K1B-P6_4-Pad66)")
			(pinfunction "P6_4")
			(pintype "input")
		)
		(pad "67" thru_hole oval
			(at 16.51 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 543 "Net-(K1B-P6_2)")
			(pinfunction "P6_2")
			(pintype "input")
		)
		(pad "68" thru_hole oval
			(at 19.05 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 541 "Net-(K1B-P6_1)")
			(pinfunction "P6_1")
			(pintype "input")
		)
		(pad "69" thru_hole oval
			(at 21.59 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 540 "Net-(K1B-P6_0)")
			(pinfunction "P6_0")
			(pintype "input")
		)
		(pad "70" thru_hole oval
			(at 24.13 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(K1B-VDD_USB-Pad70)")
			(pinfunction "VDD_USB")
			(pintype "input")
		)
		(pad "71" thru_hole oval
			(at 26.67 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "72" thru_hole oval
			(at 29.21 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(K1B-VTARG-Pad72)")
			(pinfunction "VTARG")
			(pintype "input")
		)
		(pad "73" thru_hole oval
			(at 31.75 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 192 "/FP_57")
			(pinfunction "P5_7")
			(pintype "input")
		)
		(pad "74" thru_hole oval
			(at 34.29 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/FP_56")
			(pinfunction "P5_6")
			(pintype "input")
		)
		(pad "75" thru_hole oval
			(at 36.83 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/FP_55")
			(pinfunction "P5_5")
			(pintype "input")
		)
		(pad "76" thru_hole oval
			(at 39.37 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/FP_54")
			(pinfunction "P5_4")
			(pintype "input")
		)
		(pad "77" thru_hole oval
			(at 41.91 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 194 "/FP_53")
			(pinfunction "P5_3")
			(pintype "input")
		)
		(pad "78" thru_hole oval
			(at 44.45 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/FP_52")
			(pinfunction "P5_2")
			(pintype "input")
		)
		(pad "79" thru_hole oval
			(at 46.99 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/FP_51")
			(pinfunction "P5_1")
			(pintype "input")
		)
		(pad "80" thru_hole oval
			(at 49.53 -22.86 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/FP_50")
			(pinfunction "P5_0")
			(pintype "input")
		)
		(pad "81" thru_hole rect
			(at -59.309 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "+5.0V")
			(pinfunction "VCC_5V")
			(pintype "input")
		)
		(pad "82" thru_hole oval
			(at -56.769 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "83" thru_hole oval
			(at -54.229 0 180)
			(size 1.3 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(K1C-VCC_3V6-Pad83)")
			(pinfunction "VCC_3V6")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_Cypress/Cy8CProto_062_4343W Pins.step"
			(offset
				(xyz -157.5 91.5 4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 209 155.665 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R111"
			(at -1.651 -0.339 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 540 "Net-(K1B-P6_0)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 524 "/MOSI_RX_PATH_1V8")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 142.990678 60.8214 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R91"
			(at -2.0066 0.0028 90)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 467 "Net-(U2A-SPI_CLK)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 471 "/SPI2x.CLK")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 120.354 50.5852 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R12"
			(at 0.0088 1.143 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 285 "Net-(U17-OE)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 159.639 142.457)
		(property "Reference" "TP25"
			(at -0.127 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 517 "/RF_RX_SPI_DO_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 112.7164 86.2468 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R38"
			(at -2.0916 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 0.8128 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 340 "Net-(Q4-B)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 343 "/FPGA/F_LED_R")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_misc:TP60"
		(layer "F.Cu")
		(at 96.266 142.33)
		(property "Reference" "TP13"
			(at 0.127 -2.413 90)
			(layer "F.SilkS")
		)
		(property "Value" "TEST_POINT"
			(at 0.05 -1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_misc:TP60"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 536 "/+12V")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 175.133 51.017)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "P3"
			(at 2.7686 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X08"
			(at 0 20.11 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X08 Pin_Header_Angled_1X08 Socket_Strip_Straight_1X08 Socket_Strip_Angled_1X08")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.921 -0.127 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 412 "/ADC_3")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 414 "/ADC_2")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 415 "/ADC_1")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 413 "/ADC_0")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "GND")
			(pinfunction "P8")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 130.0988 60.034 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R1"
			(at -1.778 -0.0254 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 97 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "/FPGA/FLASH.IO3")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "B.Cu")
		(at 159.953599 67.27935 90)
		(tags "INA236AIDDFR ")
		(property "Reference" "U11"
			(at 2.03835 2.631801 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "INA236"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina236.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.58115 2.5498 -90)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -1.58115 2.5498 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 294 "/Power Supply/V_1P3")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 187 "/VSYN_1P3")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 290 "Net-(U10-SCL)")
			(pinfunction "SCL")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 292 "Net-(U10-A0)")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "7" smd rect
			(at 1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 290 "Net-(U10-SCL)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 301 "unconnected-(U11-ALERT-Pad8)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 113.9564 89.9806 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C173"
			(at 0.3422 4.3688 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 370 "/Power Supply/ALT_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 131.5974 78.8808 180)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0.25 0.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 103.505 91.6658 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C119"
			(at -2.3026 -0.002901 -90)
			(layer "B.SilkS")
		)
		(property "Value" "22pF"
			(at 0 -0.8636 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/Power Supply/ap3445_3P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 351 "Net-(U22-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 151.6232 80.5572 -135)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 1.695783 0.115258 -135)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 225)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 225)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 225)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 185 "/VANA_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 225)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 112.141 91.9618 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C172"
			(at -4.2672 0.5588 -90)
			(layer "B.SilkS")
		)
		(property "Value" "22pF"
			(at 0 -0.8636 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 370 "/Power Supply/ALT_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 369 "Net-(U23-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 153.178468 78.178532 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C106"
			(at 0.066513 0.053882 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 197 "/VSYN_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "B.Cu")
		(at 125.8062 88.3804)
		(property "Reference" "L13"
			(at 0.2794 -3.1496 180)
			(layer "B.SilkS")
		)
		(property "Value" "1uH"
			(at 0 0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/6adcb47d-8b55-416c-976e-1e22e0d2848c/xal4000.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Coilcraft XAL 4020 Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 373 "Net-(U24-LX)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "+1.1V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 131.0767 92.0762 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R42"
			(at 2.4764 -0.0381 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 348 "Net-(U24-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 131.953 76.0106 90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0.25 0.5 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/FPGA/N_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 123.7742 76.6202 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C13"
			(at -0.0254 1.0668 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -0.0508 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 105.6004 94.1716 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R45"
			(at 0.0126 -3.9624 180)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -0.9652 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 351 "Net-(U22-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 126.8172 114.1342 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C132"
			(at -2.7414 -0.0304 90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 114.935 92.2158 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R46"
			(at 4.8006 -0.1524 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 369 "Net-(U23-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 129.286 77.9664)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0.25 0.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 88 "+2.5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 121.7168 86.9834 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C142"
			(at -0.0508 3.4036 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.0508 0.0254 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 88 "+2.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 150.9268 76.544 45)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C68"
			(at 1.867893 -0.251447 45)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.863599 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 45)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 45)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 233 "Net-(U2G-VCONV_1P0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 45)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 124.3838 84.037 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C34"
			(at -0.9652 -1.1176 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 88 "+2.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 155.3464 83.9228 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R69"
			(at 0.038 -1.1684 -90)
			(layer "B.SilkS")
		)
		(property "Value" "11k"
			(at 0 -0.8128 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 366 "Net-(U25-FB1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 119.4904 80.7096 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C4"
			(at 1.7614 -0.1016 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "/FPGA/FM_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 129.3622 76.417)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0.25 0.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 100.8634 97.4482 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C116"
			(at -0.127 -1.9304 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 131.6482 74.9184 180)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0.25 0.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 88 "+2.5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 149.987 77.3822 -45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C70"
			(at 0.25 0.5 135)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 315)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 315)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 315)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 277 "/VDIG_1P0_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 315)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 137.668 80.5192 -135)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB3"
			(at -0.080893 -1.284106 -135)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -0.965199 -135)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -135)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.799999 0 225)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 281 "+1.8V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.799999 0 225)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 55 "/FPGA/N_1P8")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "B.Cu")
		(at 104.8512 119.3557 -90)
		(property "Reference" "L17"
			(at -2.9083 1.0414 180)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 0.5 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/6adcb47d-8b55-416c-976e-1e22e0d2848c/xal4000.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Coilcraft XAL 4020 Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0 270)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 364 "Net-(U25-SW3)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0 270)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 139.446 78.2712 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C16"
			(at -0.1016 0.9906 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 55 "/FPGA/N_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 129.4257 90.0568 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C115"
			(at -2.7051 -0.0254 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "B.Cu")
		(at 153.0858 61.8374 90)
		(tags "INA236AIDDFR ")
		(property "Reference" "U10"
			(at 2.032 2.6924 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "INA236"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina236.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.58115 2.5498 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "*"
			(at -1.58115 2.5498 -90)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 294 "/Power Supply/V_1P3")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 179 "/VANA_1P3")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 290 "Net-(U10-SCL)")
			(pinfunction "SCL")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 292 "Net-(U10-A0)")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "7" smd rect
			(at 1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 292 "Net-(U10-A0)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 300 "unconnected-(U10-ALERT-Pad8)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 152.2056 70.575 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C92"
			(at 1.9646 -0.0254 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 161.036 73.5214)
		(descr "SMT resistor, 0603")
		(property "Reference" "R19"
			(at 2.4384 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.02 Ohms"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.1396 0.0206 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 294 "/Power Supply/V_1P3")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 187 "/VSYN_1P3")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 147.7264 54.5476 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R90"
			(at -2.1082 -0.1524 90)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 -0.8128 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 470 "Net-(U2A-SPI_EN)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 43 "/SPI2.CE")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 153.8986 69.2884 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C67"
			(at -2.1678 -0.0254 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 231 "Net-(U2G-VRX2LO_1P0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 123.2358 95.3908)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C124"
			(at -0.0204 3.7592 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 143.4338 80.8112 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R15"
			(at 2.3876 0.0254 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.02 Ohms"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 297 "/Power Supply/V_1P8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 96 "/VDIGIO_1P8")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT-23-6"
		(layer "B.Cu")
		(at 109.66196 92.8 90)
		(descr "SOT-23")
		(property "Reference" "U23"
			(at 0.0254 0.25 -90)
			(layer "Eco1.User")
			(hide yes)
		)
		(property "Value" "AP3445LW6-7"
			(at 0 -0.3302 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_sot:SOT-23-6"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3445-L.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Buck Regulator 1MHz 2A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT26_AP3445_DIO SOT26_AP3445_DIO-M SOT26_AP3445_DIO-L")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0084 -0.019201 -90)
			(layer "B.SilkS")
		)
		(pad "1" smd rect
			(at -0.9525 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at 0.9525 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 374 "Net-(U23-LX)")
			(pinfunction "LX")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0.9525 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 0 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 392 "unconnected-(U23-PG-Pad5)")
			(pinfunction "PG")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -0.9525 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 369 "Net-(U23-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-6-4.stp"
			(offset
				(xyz -0.07499999887 0 0.0799999988)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 152.9842 74.0294 90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C112"
			(at 0.25 0.5 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 197 "/VSYN_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 118.0288 114.7446 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R80"
			(at 2.5898 -0.0204 -90)
			(layer "B.SilkS")
		)
		(property "Value" "200k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 387 "Net-(U25-CFG1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 116.5302 126.6062 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R72"
			(at 3.7858 -0.3098 90)
			(layer "B.SilkS")
		)
		(property "Value" "3.92k"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 357 "Net-(C158-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 379 "Net-(U25-COMP1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 153.1874 83.402)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C66"
			(at 0.0254 2.1844 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 230 "Net-(U2G-VRX1LO_1P0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 152.3492 64.5044)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C30"
			(at -0.0508 0.9144 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "B.Cu")
		(at 138.4554 86.0944 90)
		(tags "INA236AIDDFR ")
		(property "Reference" "U12"
			(at -3.0734 0.1778 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "INA236"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina236.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.5146 2.1336 -90)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -1.8542 1.9304 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 297 "/Power Supply/V_1P8")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 96 "/VDIGIO_1P8")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 290 "Net-(U10-SCL)")
			(pinfunction "SCL")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 292 "Net-(U10-A0)")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "7" smd rect
			(at 1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 303 "unconnected-(U12-ALERT-Pad8)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 122.2706 124.0942 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C137"
			(at 3.024 -0.6554 -90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 109.9566 126.2416 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C139"
			(at -3.0074 -0.2286 -90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "B.Cu")
		(at 127.7874 117.8952 90)
		(property "Reference" "L16"
			(at 0.0254 3.5052 0)
			(layer "B.SilkS")
		)
		(property "Value" "3.3uH"
			(at 0 0.5 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/6adcb47d-8b55-416c-976e-1e22e0d2848c/xal4000.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Coilcraft XAL 4020 Inductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0 90)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 363 "Net-(C162-Pad1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0 90)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 123.2612 113.8174)
		(descr "SMT resistor, 0603")
		(property "Reference" "R84"
			(at 0.6146 -1.8404 -90)
			(layer "B.SilkS")
		)
		(property "Value" "2.21k"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 403 "Net-(C146-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 130.0226 78.9316)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0.25 0.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 117.9018 126.6316 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R71"
			(at 3.735 -0.2082 90)
			(layer "B.SilkS")
		)
		(property "Value" "499k"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 378 "Net-(U25-RAMP1)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 152.5778 76.5948 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C96"
			(at 0.025401 0 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 129.6924 92.0888 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R48"
			(at -2.4892 0.0508 -90)
			(layer "B.SilkS")
		)
		(property "Value" "82.5k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "+1.1V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 348 "Net-(U24-FB)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 129.3368 77.179)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0.25 0.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 132.6642 76.163 90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0.25 0.5 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/FPGA/N_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 101.0666 122.7314 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C150"
			(at -3.114 -0.0508 -90)
			(layer "B.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -1.3462 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 154.4066 81.6494)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C99"
			(at 1.8542 -0.2032 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 185 "/VANA_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_qfn:CC-43-1_ADI"
		(layer "B.Cu")
		(at 115.297399 120.6892 90)
		(tags "ADP5056ACCZ-R7 ")
		(property "Reference" "U25"
			(at -3.7338 2.228401 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "ADP5056ACCZ-R7"
			(at 0.0508 -0.0494 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_qfn:CC-43-1_ADI"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adp5056.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Triple Buck Regulator"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CC-43-1_ADI")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.843601 2.25 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -1.843601 2.25 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.250001 2.370001)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "2" smd rect
			(at -2.250001 1.87)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at -2.250001 1.370001)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 378 "Net-(U25-RAMP1)")
			(pinfunction "RAMP1")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -2.250001 0.869999)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 366 "Net-(U25-FB1)")
			(pinfunction "FB1")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -2.250001 0.37)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 379 "Net-(U25-COMP1)")
			(pinfunction "COMP1")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -2.250001 -0.129999)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 389 "Net-(U25-RT)")
			(pinfunction "RT")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at -2.250001 -0.630001)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 384 "Net-(U25-EN1)")
			(pinfunction "EN1")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -2.250001 -1.13)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "9" smd rect
			(at -2.250001 -1.630001)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 355 "Net-(U25-VREG)")
			(pinfunction "VREG")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at -2.25 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "VBIAS")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at -1.75 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 394 "unconnected-(U25-SYNC{slash}MODE-Pad11)")
			(pinfunction "SYNC/MODE")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -1.25 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 360 "Net-(U25-BST1)")
			(pinfunction "BST1")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at -0.75 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 365 "Net-(U25-BST3)")
			(pinfunction "BST3")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -0.25 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "PGND")
			(pintype "power_out")
		)
		(pad "15" smd rect
			(at 0.25 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 364 "Net-(U25-SW3)")
			(pinfunction "SW3")
			(pintype "output")
		)
		(pad "16" smd rect
			(at 0.75 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "PVIN3")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 1.25 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 362 "Net-(U25-BST2)")
			(pinfunction "BST2")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 1.75 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 386 "Net-(U25-EN3)")
			(pinfunction "EN3")
			(pintype "input")
		)
		(pad "19" smd rect
			(at 2.25 -2.335001 90)
			(size 0.254 0.6604)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 382 "Net-(U25-RAMP3)")
			(pinfunction "RAMP3")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at 2.250001 -1.630001)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 368 "Net-(U25-FB3)")
			(pinfunction "FB3")
			(pintype "input")
		)
		(pad "21" smd rect
			(at 2.250001 -1.13)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 383 "Net-(U25-COMP3)")
			(pinfunction "COMP3")
			(pintype "output")
		)
		(pad "22" smd rect
			(at 2.250001 -0.630001)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 377 "/Power Supply/PGOOD")
			(pinfunction "PWRGD")
			(pintype "output")
		)
		(pad "23" smd rect
			(at 2.250001 -0.129999)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 385 "Net-(U25-EN2)")
			(pinfunction "EN2")
			(pintype "input")
		)
		(pad "24" smd rect
			(at 2.250001 0.37)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 381 "Net-(U25-COMP2)")
			(pinfunction "COMP2")
			(pintype "output")
		)
		(pad "25" smd rect
			(at 2.250001 0.869999)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 367 "Net-(U25-FB2)")
			(pinfunction "FB2")
			(pintype "input")
		)
		(pad "26" smd rect
			(at 2.250001 1.370001)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 380 "Net-(U25-RAMP2)")
			(pinfunction "RAMP2")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 2.250001 1.87)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 388 "Net-(U25-CFG2)")
			(pinfunction "CFG2")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 2.250001 2.370001)
			(size 0.254 0.3048)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 387 "Net-(U25-CFG1)")
			(pinfunction "CFG1")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at 1.675 2.210001 90)
			(size 0.254 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "PVIN2")
			(pintype "power_in")
		)
		(pad "30" smd rect
			(at 1.675 1.145001 90)
			(size 0.254 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "PVIN2")
			(pintype "power_in")
		)
		(pad "31" smd rect
			(at 1.675 0.080001 90)
			(size 0.254 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "PVIN2")
			(pintype "power_in")
		)
		(pad "32" smd rect
			(at 0.925 2.210001 90)
			(size 0.508 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 363 "Net-(C162-Pad1)")
			(pinfunction "SW2")
			(pintype "output")
		)
		(pad "33" smd rect
			(at 0.925 1.145001 90)
			(size 0.508 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 363 "Net-(C162-Pad1)")
			(pinfunction "SW2")
			(pintype "output")
		)
		(pad "34" smd rect
			(at 0.925 0.080001 90)
			(size 0.508 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 363 "Net-(C162-Pad1)")
			(pinfunction "SW2")
			(pintype "output")
		)
		(pad "35" smd rect
			(at 0 2.210001 90)
			(size 0.6096 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "PGND")
			(pintype "power_out")
		)
		(pad "36" smd rect
			(at 0 1.145001 90)
			(size 0.6096 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "PGND")
			(pintype "power_out")
		)
		(pad "37" smd rect
			(at 0 0.080001 90)
			(size 0.6096 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "PGND")
			(pintype "power_out")
		)
		(pad "38" smd rect
			(at -0.925 2.210001 90)
			(size 0.508 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 361 "Net-(C161-Pad2)")
			(pinfunction "SW1")
			(pintype "output")
		)
		(pad "39" smd rect
			(at -0.925 1.145001 90)
			(size 0.508 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 361 "Net-(C161-Pad2)")
			(pinfunction "SW1")
			(pintype "output")
		)
		(pad "40" smd rect
			(at -0.925 0.080001 90)
			(size 0.508 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 361 "Net-(C161-Pad2)")
			(pinfunction "SW1")
			(pintype "output")
		)
		(pad "41" smd rect
			(at -1.675 2.210001 90)
			(size 0.254 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "PVIN1")
			(pintype "power_in")
		)
		(pad "42" smd rect
			(at -1.675 1.145001 90)
			(size 0.254 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "PVIN1")
			(pintype "power_in")
		)
		(pad "43" smd rect
			(at -1.675 0.080001 90)
			(size 0.254 0.8382)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "PVIN1")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_qfn/ADP5056 v2.step"
			(offset
				(xyz -2.5 -2.75 0.05)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 146.2532 56.7662 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R88"
			(at -0.0088 -1.1938 90)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 -0.8128 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 468 "Net-(U2A-SPI_DIO)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 42 "/SPI2.MOSI")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 114.3 78.3728)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0.0254 -1.0922 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/FPGA/FM_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 110.1852 97.6768 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C171"
			(at 0.0254 -3.0734 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 130.4798 77.7632 90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0.25 0.5 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "B.Cu")
		(at 117.983 88.3804)
		(property "Reference" "L9"
			(at -1.7526 -2.8702 180)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/6adcb47d-8b55-416c-976e-1e22e0d2848c/xal4000.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Coilcraft XAL 4020 Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 371 "Net-(U8-LX)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 88 "+2.5V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 101.6508 115.1394 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R86"
			(at 3.2132 0.0254 -90)
			(layer "B.SilkS")
		)
		(property "Value" "2.21k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 404 "Net-(C147-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0805"
		(layer "B.Cu")
		(at 119.7864 117.3516 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "FB16"
			(at -2.9312 0.7112 -90)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -1.3462 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1 -0.1 -90)
			(layer "B.CrtYd")
		)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 432 "/Power Supply/Vin")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 154.3558 78.9316 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C108"
			(at 0 -0.076201 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 197 "/VSYN_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 140.9954 56.3764 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R93"
			(at -2.0574 0.127 90)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 -0.8128 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 469 "Net-(U2A-SPI_DO)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 473 "/SPI2x.MISO")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 132.842 79.2618 -90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0.25 0.5 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 270)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 270)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 129.7178 86.2722 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C37"
			(at -2.3368 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.863599 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 132.969 74.8168 -90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C33"
			(at -0.0018 0.0188 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 270)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 270)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 147.6502 77.306 -45)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C61"
			(at 0 1.077631 135)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.863599 135)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 135)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 315)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 221 "Net-(U2G-VDIG_0P9)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 315)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 129.3622 75.6804)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0.25 0.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 159.4358 74.8676 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB10"
			(at -2.7686 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -0.9652 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 197 "/VSYN_1P3_F")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 187 "/VSYN_1P3")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 152.4254 81.3192 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C95"
			(at -1.724209 -0.107763 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 100.8634 95.2638 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C9"
			(at -2.54 -0.8382 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 107.0356 123.0754 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C114"
			(at -2.7446 -0.0254 -90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 144.1958 73.623 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C69"
			(at -2.0066 0.0254 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 277 "/VDIG_1P0_F")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 121.7288 90.006 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C128"
			(at -0.1912 4.318 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 88 "+2.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 116.6572 114.7446 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R81"
			(at 2.5898 0.1066 -90)
			(layer "B.SilkS")
		)
		(property "Value" "16.2k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 388 "Net-(U25-CFG2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_logos:Thales_26x3_Cu"
		(layer "B.Cu")
		(at 170.307 115.279 180)
		(property "Reference" "G***"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_logos:Thales_26x3_Cu"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 123.7742 78.0426 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C19"
			(at 0 -1.0668 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 116.8098 75.1724)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 1.9606 0.127 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0805"
		(layer "B.Cu")
		(at 100.9904 119.0534 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "FB12"
			(at -0.0152 2.032 90)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -1.3462 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1 -0.1 90)
			(layer "B.CrtYd")
		)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 297 "/Power Supply/V_1P8")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "B.Cu")
		(at 107.9754 78.6268 180)
		(tags "INA236AIDDFR ")
		(property "Reference" "U14"
			(at 0.2032 2.5908 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "INA236"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina236.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.9812 1.905 180)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -1.58115 2.5498 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "*"
			(at -0.4445 1.397 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4445 1.397 180)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 0.974999 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 63 "/Power Supply/FV_1P8")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.32715 0.325001 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 281 "+1.8V")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.32715 -0.325001 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.32715 -0.974999 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.32715 -0.974999 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 296 "Net-(U13-A0)")
			(pinfunction "SCL")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 -0.325001 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 295 "Net-(U13-SDA)")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "7" smd rect
			(at 1.32715 0.325001 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 295 "Net-(U13-SDA)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.32715 0.974999 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 305 "unconnected-(U14-ALERT-Pad8)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 119.0752 97.4228 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C126"
			(at -0.0508 -3.2766 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0805"
		(layer "B.Cu")
		(at 134.3254 126.074 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "FB11"
			(at -3.495 0.2032 180)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1 -0.1 180)
			(layer "B.CrtYd")
		)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 294 "/Power Supply/V_1P3")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 154.432 72.2006)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C100"
			(at 0.4826 -0.9398 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 185 "/VANA_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 159.1476 70.067 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C31"
			(at -2.0408 -0.2794 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 100.584 84.9768)
		(descr "SMT resistor, 0603")
		(property "Reference" "R21"
			(at -2.413 -0.9398 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.02 Ohms"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/Power Supply/ap3445_3P3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 131.6482 77.306 180)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0.25 0.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/FPGA/N_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 155.5496 75.782 135)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C101"
			(at -0.125724 0.880065 -45)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 135)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 135)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 135)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 185 "/VANA_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 135)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 104.2289 86.45 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C143"
			(at -2.4511 4.191 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/Power Supply/ap3445_3P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 128.2396 114.1342 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C133"
			(at -2.7922 -0.005 90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 145.1356 77.2894 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C91"
			(at -2.0486 0.1524 -90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 163 "/VDIGIO_1P8_F")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 120.4036 113.8174 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R85"
			(at 0.1346 1.7642 -90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -0.9652 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 367 "Net-(U25-FB2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 154.7622 74.1818 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C105"
			(at 2.065459 0.772302 45)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 197 "/VSYN_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 152.8318 72.988)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C98"
			(at 1.5494 -0.8382 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 185 "/VANA_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 129.8956 74.766)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0.25 0.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 121.92 77.4966 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB2"
			(at -2.4258 -0.0508 90)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 281 "+1.8V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "/FPGA/F_1P8")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 119.2276 128.7156)
		(descr "SMT resistor, 0603")
		(property "Reference" "R62"
			(at 0.5334 1.5494 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.21k"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 402 "Net-(C145-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 120.429 127)
		(descr "SMT resistor, 0603")
		(property "Reference" "R83"
			(at 2.4562 -0.0116 0)
			(layer "B.SilkS")
		)
		(property "Value" "9.09k"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 366 "Net-(U25-FB1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 104.2035 89.6504 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C122"
			(at -2.2225 4.9784 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/Power Supply/ap3445_3P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 154.7876 79.7444 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C107"
			(at 0.050801 0.0254 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 197 "/VSYN_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 151.4602 84.291 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R64"
			(at -2.1082 0.127 -90)
			(layer "B.SilkS")
		)
		(property "Value" "20k"
			(at 0 -0.8128 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 368 "Net-(U25-FB3)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0805"
		(layer "B.Cu")
		(at 134.3558 114.3646 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "FB6"
			(at -0.061 1.5494 180)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1 -0.1 180)
			(layer "B.CrtYd")
		)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 298 "/Power Supply/V_1P0")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 102.8446 123.0888 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C123"
			(at -2.7058 -0.0762 -90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 115.812 128.7526 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C158"
			(at -0.52 -4.8144 180)
			(layer "B.SilkS")
		)
		(property "Value" "47nF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 357 "Net-(C158-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 123.2358 97.4228)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C125"
			(at 0.0558 3.2004 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 122.0304 111.469 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C146"
			(at 0.593 5.715 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 367 "Net-(U25-FB2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 403 "Net-(C146-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 110.1598 95.6448 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C170"
			(at -0.0254 -3.8354 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 109.0626 112.5982 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C160"
			(at 0.1474 6.0568 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 359 "Net-(C160-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0805"
		(layer "B.Cu")
		(at 116.6774 82.7162 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "FB14"
			(at 1.717 1.6256 180)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1 -0.1 180)
			(layer "B.CrtYd")
		)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 297 "/Power Supply/V_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 63 "/Power Supply/FV_1P8")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0805"
		(layer "B.Cu")
		(at 97.2922 95.2638 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "FB15"
			(at 3.1344 -0.0508 180)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0864 0.0254 180)
			(layer "B.CrtYd")
		)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 432 "/Power Supply/Vin")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 152.0444 72.2006)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C110"
			(at -2.0828 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 105.6132 123.0888 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C117"
			(at -2.7058 0 -90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "B.Cu")
		(at 110.1598 88.3804)
		(property "Reference" "L18"
			(at -0.3302 -3.048 180)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/6adcb47d-8b55-416c-976e-1e22e0d2848c/xal4000.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Coilcraft XAL 4020 Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 374 "Net-(U23-LX)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 370 "/Power Supply/ALT_1P8")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 142.4052 75.02)
		(descr "SMT resistor, 0603")
		(property "Reference" "R16"
			(at -2.4512 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.02 Ohms"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 298 "/Power Supply/V_1P0")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 82 "/VDIG_1P0")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 117.1702 74.2072 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C10"
			(at -0.0084 1.143 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 142.367 73.6484)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB5"
			(at -2.4892 -0.0508 0)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 277 "/VDIG_1P0_F")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 82 "/VDIG_1P0")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 158.0388 77.7632 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C63"
			(at -2.2606 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 223 "Net-(U2G-VRFLO1_1P0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 146.7358 54.5222 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R94"
			(at -2.0828 0.1016 90)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 -0.8128 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 470 "Net-(U2A-SPI_EN)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 474 "/SPI2x.CE")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 120.3032 77.3822)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C43"
			(at -2.0154 -0.3556 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 281 "+1.8V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 128.3462 127.3948 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C168"
			(at -2.6162 0.0508 -90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 115.1346 126.6062 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R82"
			(at -3.7858 -0.9616 -90)
			(layer "B.SilkS")
		)
		(property "Value" "110k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 389 "Net-(U25-RT)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 158.5468 76.3408 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C62"
			(at -2.286 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 222 "Net-(U2G-VRFLO2_1P0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 143.9164 77.649 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB7"
			(at -0.1396 -1.397 -90)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 163 "/VDIGIO_1P8_F")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 96 "/VDIGIO_1P8")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 114.676 112.5348)
		(descr "SMT resistor, 0603")
		(property "Reference" "C159"
			(at -0.503 -5.8918 0)
			(layer "B.SilkS")
		)
		(property "Value" "33nF"
			(at 0 -1.016 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 358 "Net-(C159-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 155.1686 68.6828 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB9"
			(at -0.089 -1.3716 90)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 185 "/VANA_1P3_F")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 179 "/VANA_1P3")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 125.4202 114.1208 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C131"
			(at -2.7026 -0.005 90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 110.9218 122.5332 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C157"
			(at -3.0632 -0.0254 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 104.1908 114.8218 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C166"
			(at -2.6162 0.015899 90)
			(layer "B.SilkS")
		)
		(property "Value" "180pF"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 368 "Net-(U25-FB3)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 105.537 91.2506 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R44"
			(at -0.127 -4.5974 180)
			(layer "B.SilkS")
		)
		(property "Value" "332k"
			(at 0 -0.9652 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/Power Supply/ap3445_3P3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 375 "Net-(R44-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 121.7118 128.6256)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C145"
			(at 0.2336 1.1568 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 366 "Net-(U25-FB1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 402 "Net-(C145-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 124.4092 117.3262 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C156"
			(at 2.9566 -0.6096 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 121.5136 92.1268 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R43"
			(at -0.0701 0.009799 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "475k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 88 "+2.5V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 352 "Net-(U8-FB)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 151.003 79.3888 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C65"
			(at -0.0508 -1.0668 -90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 229 "Net-(U2G-VAUXVCO_1P0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 104.2035 88.0502 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C130"
			(at -2.3495 4.6482 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/Power Supply/ap3445_3P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 119.8498 78.5252)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB1"
			(at -2.5272 -0.381 0)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 281 "+1.8V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "/FPGA/FM_1P8")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 126.8934 127.3948 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C135"
			(at -2.5146 -0.0712 -90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "B.Cu")
		(at 100.3427 88.0248)
		(property "Reference" "L10"
			(at -3.2639 2.2098 180)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/6adcb47d-8b55-416c-976e-1e22e0d2848c/xal4000.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Coilcraft XAL 4020 Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 372 "Net-(U22-LX)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/Power Supply/ap3445_3P3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 122.3518 117.3262 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C155"
			(at 2.9566 -0.4826 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 129.413 87.5166 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C141"
			(at -2.6416 -0.0002 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 117.221 79.5666 90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.0414 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/FPGA/FM_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 152.4508 75.7566 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C109"
			(at 0.35921 0.071842 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 153.2128 82.386)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C97"
			(at -0.1524 2.159 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 185 "/VANA_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_coilcraft:Coilcraft_XAL4020"
		(layer "B.Cu")
		(at 127.7316 123.5583 -90)
		(property "Reference" "L15"
			(at -1.2181 -3.307 180)
			(layer "B.SilkS")
		)
		(property "Value" "3.3uH"
			(at 0 0.5 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_coilcraft:Coilcraft_XAL4020"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/6adcb47d-8b55-416c-976e-1e22e0d2848c/xal4000.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Coilcraft XAL 4020 Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.1811 0 270)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 361 "Net-(C161-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 1.1811 0 270)
			(size 0.9652 3.4036)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_coilcraft/Coilcraft-XEL4020.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 148.4376 76.4932 -135)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C93"
			(at -0.502894 1.005789 -135)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 225)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 225)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 225)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 163 "/VDIGIO_1P8_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 225)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 111.1962 114.719 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R70"
			(at -2.7166 -0.005 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 377 "/Power Supply/PGOOD")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 355 "Net-(U25-VREG)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 108.326 114.6936 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R87"
			(at 3.7834 -0.122 -90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 368 "Net-(U25-FB3)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 120.2436 92.3682 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C127"
			(at 0.0143 0.006499 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22pF"
			(at 0 -0.8636 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 88 "+2.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 352 "Net-(U8-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 121.7295 88.5074 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C129"
			(at -0.1143 3.8862 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1676 -0.0508 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 88 "+2.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 113.9564 88.5074 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C174"
			(at 0.3422 4.0132 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 370 "/Power Supply/ALT_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 133.2738 77.306)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0.25 0.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/FPGA/N_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 145.2372 56.7662 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R92"
			(at 0.0166 1.143 90)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 -0.8128 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 468 "Net-(U2A-SPI_DIO)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 472 "/SPI2x.MOSI")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 142.0114 56.3686 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R89"
			(at -2.0242 -0.381 90)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 0 -0.8128 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 469 "Net-(U2A-SPI_DO)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "/SPI2.MISO")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "B.Cu")
		(at 147.2946 60.3388 90)
		(tags "INA236AIDDFR ")
		(property "Reference" "U7"
			(at 1.6764 2.4384 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "INA236"
			(at -0.2032 -1.4732 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina236.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.58115 2.5498 -90)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -1.58115 2.5498 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 297 "/Power Supply/V_1P8")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 166 "/VANA_1P8")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 290 "Net-(U10-SCL)")
			(pinfunction "SCL")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 292 "Net-(U10-A0)")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "7" smd rect
			(at 1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 293 "unconnected-(U7-ALERT-Pad8)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "B.Cu")
		(at 140.8176 67.2476 90)
		(tags "INA236AIDDFR ")
		(property "Reference" "U13"
			(at 3.3528 -1.4224 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "INA236"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina236.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.58115 2.5498 -90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "*"
			(at -1.58115 2.5498 -90)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4445 1.397 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 298 "/Power Supply/V_1P0")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 82 "/VDIG_1P0")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 296 "Net-(U13-A0)")
			(pinfunction "SCL")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 295 "Net-(U13-SDA)")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "7" smd rect
			(at 1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 296 "Net-(U13-A0)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 304 "unconnected-(U13-ALERT-Pad8)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 158.2166 79.1602 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C103"
			(at -2.5146 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0342 -0.0254 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 197 "/VSYN_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 131.5974 78.068 180)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0.25 0.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 124.328 124.0942 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C136"
			(at 2.9732 -0.4014 -90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT-23-6"
		(layer "B.Cu")
		(at 117.856 92.5714 90)
		(descr "SOT-23")
		(property "Reference" "U8"
			(at 0.0254 0.25 -90)
			(layer "Eco1.User")
			(hide yes)
		)
		(property "Value" "AP3445LW6-7"
			(at 0 -0.9525 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_sot:SOT-23-6"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3445-L.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Buck Regulator 1MHz 2A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT26_AP3445_DIO SOT26_AP3445_DIO-M SOT26_AP3445_DIO-L")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.0254 -0.0508 -90)
			(layer "B.SilkS")
		)
		(pad "1" smd rect
			(at -0.9525 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at 0.9525 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 371 "Net-(U8-LX)")
			(pinfunction "LX")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0.9525 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 0 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 390 "unconnected-(U8-PG-Pad5)")
			(pinfunction "PG")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -0.9525 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 352 "Net-(U8-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-6-4.stp"
			(offset
				(xyz -0.07499999887 0 0.0799999988)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 122.9106 92.1524 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R49"
			(at 0.0254 -0.0254 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "150k"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 352 "Net-(U8-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 133.2738 78.0426)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0.25 0.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 146.5834 62.828)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C29"
			(at -1.8034 0.127 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 108.8644 122.5282 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C140"
			(at -3.1598 0.0254 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 131.44 113.7158 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C149"
			(at -3.0088 -0.2082 90)
			(layer "B.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -1.3462 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 129.794 127.3948 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C169"
			(at -2.667 -0.254 -90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 149.995932 75.773068 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C71"
			(at -0.066513 -0.017961 45)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 277 "/VDIG_1P0_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 120.2132 124.0942 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C138"
			(at 3.024 -0.9856 -90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 155.1686 65.9522 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R13"
			(at 0 1.3208 -90)
			(layer "B.SilkS")
		)
		(property "Value" "0.02 Ohms"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 294 "/Power Supply/V_1P3")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 179 "/VANA_1P3")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 119.0752 95.3908 180)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C121"
			(at 0 -3.7338 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.3462 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 180)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT-23-6"
		(layer "B.Cu")
		(at 100.8507 92.3936 90)
		(descr "SOT-23")
		(property "Reference" "U22"
			(at 0.0254 0.25 -90)
			(layer "Eco1.User")
			(hide yes)
		)
		(property "Value" "AP3445LW6-7"
			(at 0 -0.3302 -90)
			(layer "B.Fab")
		)
		(property "Footprint" "t_sot:SOT-23-6"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3445-L.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Buck Regulator 1MHz 2A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT26_AP3445_DIO SOT26_AP3445_DIO-M SOT26_AP3445_DIO-L")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.0254 -2.6797 -90)
			(layer "B.SilkS")
		)
		(pad "1" smd rect
			(at -0.9525 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at 0.9525 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 372 "Net-(U22-LX)")
			(pinfunction "LX")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0.9525 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 0 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 391 "unconnected-(U22-PG-Pad5)")
			(pinfunction "PG")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -0.9525 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 351 "Net-(U22-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-6-4.stp"
			(offset
				(xyz -0.07499999887 0 0.0799999988)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 112.0358 126.2278 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C154"
			(at 3.0212 0.4028 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.3462 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 355 "Net-(U25-VREG)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 129.662 114.1088 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C134"
			(at -2.716 -0.0304 90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 104.2162 123.0634 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C120"
			(at -2.7312 0 -90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 350 "/Power Supply/adp5056_1P8V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 114.2238 94.3494)
		(descr "SMT resistor, 0603")
		(property "Reference" "R47"
			(at -0.0508 4.4196 0)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -0.9652 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 369 "Net-(U23-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 376 "Net-(R47-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 145.3642 81.5858 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R63"
			(at -1.994 0.0254 -90)
			(layer "B.SilkS")
		)
		(property "Value" "6.81k"
			(at 0 -0.8128 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 277 "/VDIG_1P0_F")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 367 "Net-(U25-FB2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 105.6004 92.7238 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "R50"
			(at 0.0126 -4.2672 180)
			(layer "B.SilkS")
		)
		(property "Value" "121k"
			(at 0 -0.9652 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 351 "Net-(U22-FB)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 375 "Net-(R44-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 114.0714 74.1056)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C25"
			(at 0 -1.0668 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 113.411 92.2286 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R51"
			(at -4.7116 0.4826 -90)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 370 "/Power Supply/ALT_1P8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 376 "Net-(R47-Pad2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 129.4257 88.8122 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C118"
			(at -2.6543 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 102.9716 114.8052 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C147"
			(at 2.5996 -0.0508 -90)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -0.8636 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 368 "Net-(U25-FB3)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 404 "Net-(C147-Pad2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 123.6588 128.651 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C164"
			(at 0.037 -4.9668 180)
			(layer "B.SilkS")
		)
		(property "Value" "180pF"
			(at 0 -0.8636 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 366 "Net-(U25-FB1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 150.791 74.5374)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C64"
			(at -0.1182 -0.9906 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 228 "Net-(U2G-VCLKVCO_1P0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 115.2856 114.7446 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R73"
			(at 3.7836 0.4114 -90)
			(layer "B.SilkS")
		)
		(property "Value" "150k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 380 "Net-(U25-RAMP2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 140.208 69.8384)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C32"
			(at -1.8288 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 97 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 122.0304 112.5866)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C165"
			(at -0.6438 -5.6642 0)
			(layer "B.SilkS")
		)
		(property "Value" "180pF"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 353 "/Power Supply/adp5056_1P0V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 367 "Net-(U25-FB2)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 154.6606 73.2928 45)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C104"
			(at 2.245064 0.413092 45)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 45)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -135)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 45)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 197 "/VSYN_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 45)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 113.9698 87.0088 180)
		(descr "SMT resistor, 0603")
		(property "Reference" "C144"
			(at 0.3556 3.6068 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 180)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 370 "/Power Supply/ALT_1P8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 180)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0805"
		(layer "B.Cu")
		(at 119.5324 83.3614 -90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "FB13"
			(at 1.5138 1.4732 -90)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -1.3462 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1 -0.1 90)
			(layer "B.CrtYd")
		)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 370 "/Power Supply/ALT_1P8")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 63 "/Power Supply/FV_1P8")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 113.7376 126.581 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R77"
			(at -2.414 -0.4536 -90)
			(layer "B.SilkS")
		)
		(property "Value" "10"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 384 "Net-(U25-EN1)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 151.257 77.6362 -135)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C102"
			(at 0.112 0.0128 -135)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 45)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -135)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 225)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 225)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 225)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 185 "/VANA_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 225)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 148.7424 64.2504 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R14"
			(at -0.3556 -1.3716 -90)
			(layer "B.SilkS")
		)
		(property "Value" "0.02 Ohms"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 297 "/Power Supply/V_1P8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 166 "/VANA_1P8")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 106.9544 114.681 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R75"
			(at 2.831 -0.2744 -90)
			(layer "B.SilkS")
		)
		(property "Value" "150k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 382 "Net-(U25-RAMP3)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 128.524 92.3174 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C7"
			(at -1.9558 0.1524 -90)
			(layer "B.SilkS")
		)
		(property "Value" "22pF"
			(at 0 -0.8636 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 348 "Net-(U24-FB)")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 115.189 75.147)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -1.778 0.3556 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 38 "/FPGA/F_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0805"
		(layer "B.Cu")
		(at 131.567 127.066 90)
		(descr "SMT capacitor, 0805")
		(property "Reference" "C148"
			(at -2.8688 0.3098 -90)
			(layer "B.SilkS")
		)
		(property "Value" "100uF"
			(at 0 -1.3462 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0805"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 90)
			(size 1 1.5)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0805.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "B.Cu")
		(at 95.06585 87.583201 180)
		(tags "INA236AIDDFR ")
		(property "Reference" "U16"
			(at 0.73025 2.454001 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "INA236"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ina236.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.70815 1.844401 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -1.58115 2.5498 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(fp_text user "*"
			(at -0.4445 1.397 180)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.4445 1.397 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 0.974999 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/Power Supply/ap3445_3P3V")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.32715 0.325001 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.32715 -0.325001 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.32715 -0.974999 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 97 "+3.3V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.32715 -0.974999 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 296 "Net-(U13-A0)")
			(pinfunction "SCL")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 -0.325001 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 295 "Net-(U13-SDA)")
			(pinfunction "SDA")
			(pintype "open_collector")
		)
		(pad "7" smd rect
			(at 1.32715 0.325001 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 1.32715 0.974999 180)
			(size 1.0033 0.4318)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 307 "unconnected-(U16-ALERT-Pad8)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 125.4456 127.393 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C167"
			(at -2.4656 -0.2236 -90)
			(layer "B.SilkS")
		)
		(property "Value" "47uf"
			(at 0 -1.016 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 354 "/Power Supply/adp5056_1P3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 121.3358 81.535 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R17"
			(at -0.0634 -1.3716 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.02 Ohms"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 63 "/Power Supply/FV_1P8")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 281 "+1.8V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 112.5932 114.7318 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R78"
			(at -2.7548 0.1982 90)
			(layer "B.SilkS")
		)
		(property "Value" "10"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 385 "Net-(U25-EN2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 130.4946 74.131 180)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C113"
			(at 0.25 0.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 107 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 180)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 150.0378 67.3238 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C94"
			(at 0.2286 -1.1684 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF 4V"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 165 "/VANA_1P8_F")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 148.7424 67.0316 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB8"
			(at 0.089 1.3208 90)
			(layer "B.SilkS")
		)
		(property "Value" "FB"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1016 0.0508 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 165 "/VANA_1P8_F")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 166 "/VANA_1P8")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 110.7948 79.5666 90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 1.6002 0.2032 -90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "FPGA")
		(sheetfile "Nav1_FPGA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/FPGA/FM_1P8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 90)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 113.9394 114.7446 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R74"
			(at 3.8598 -0.4014 -90)
			(layer "B.SilkS")
		)
		(property "Value" "4.75k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 358 "Net-(C159-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 381 "Net-(U25-COMP2)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0201"
		(layer "B.Cu")
		(at 155.8544 77.7378 -90)
		(descr "Capacitor SMD 0201 (0603 Metric),")
		(tags "capacitor")
		(property "Reference" "C111"
			(at 0.25 0.5 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at -0.05 -0.5 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0201"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Nav1.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.3 0 270)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 185 "/VANA_1P3_F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.3 0 270)
			(size 0.4 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 232 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 109.723 114.7064 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R76"
			(at 3.7962 0.259 -90)
			(layer "B.SilkS")
		)
		(property "Value" "6.18k"
			(at 0 -0.9652 -90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 -90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 359 "Net-(C160-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 383 "Net-(U25-COMP3)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "B.Cu")
		(at 105.5116 114.6174 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "R79"
			(at -2.742 0.1016 90)
			(layer "B.SilkS")
		)
		(property "Value" "10"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 386 "Net-(U25-EN3)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 356 "Net-(U25-PVIN3)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT-23-6"
		(layer "B.Cu")
		(at 126.1999 92.5714 90)
		(descr "SOT-23")
		(property "Reference" "U24"
			(at 0.0254 0.25 -90)
			(layer "Eco1.User")
			(hide yes)
		)
		(property "Value" "AP3445LW6-7"
			(at 0 -0.3302 -90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "t_sot:SOT-23-6"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP3445-L.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Buck Regulator 1MHz 2A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT26_AP3445_DIO SOT26_AP3445_DIO-M SOT26_AP3445_DIO-L")
		(sheetname "Power Supply")
		(sheetfile "Nav1_PowerSupply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.4384 0.3937 180)
			(layer "B.SilkS")
		)
		(pad "1" smd rect
			(at -0.9525 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 232 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at 0.9525 -1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 373 "Net-(U24-LX)")
			(pinfunction "LX")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0.9525 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 349 "Net-(U22-EN)")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 0 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 393 "unconnected-(U24-PG-Pad5)")
			(pinfunction "PG")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -0.9525 1.05664 90)
			(size 0.59944 1.00076)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 348 "Net-(U24-FB)")
			(pinfunction "FB")
			(pintype "unspecified")
		)
		(model "${T_LIBS}/3d/t_sot/SOT23-6-4.stp"
			(offset
				(xyz -0.07499999887 0 0.0799999988)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 57.785 48.223)
		(end 225.66 162.123)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "ADRV FPGA PSOC6 SDB\nSK1708\nYTH August 21, 2024"
		(at 183.6928 127.6234 0)
		(layer "B.Cu")
	)
	(gr_text "STLink"
		(at 88.265 54.192 -0)
		(layer "B.SilkS")
	)
	(gr_text "D6"
		(at 153.7208 104.865 90)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 138.1506 97.7276 90)
		(layer "F.SilkS")
	)
	(gr_text "SWD"
		(at 81.4578 49.366 0)
		(layer "F.SilkS")
	)
	(gr_text "CY8CPROTO-062-4343W"
		(at 190.1698 135.2688 90)
		(layer "F.SilkS")
	)
	(gr_text "4Mx16"
		(at 110.998 70.956 0)
		(layer "F.SilkS")
	)
	(gr_text "D2"
		(at 158.6484 99.8358 90)
		(layer "F.SilkS")
	)
	(gr_text "TCK\n"
		(at 135.8392 97.753 90)
		(layer "F.SilkS")
	)
	(gr_text "D8"
		(at 153.4922 53.9888 90)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 79.0702 54.6238 90)
		(layer "F.SilkS")
	)
	(gr_text "A9\n"
		(at 166.243 99.785 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 86.868 49.3152 0)
		(layer "F.SilkS")
	)
	(gr_text "ADC 0"
		(at 169.164 64.352 0)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 132.8674 97.7784 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 64.6684 105.9826 0)
		(layer "F.SilkS")
	)
	(gr_text "VTARG"
		(at 64.4144 114.1614 0)
		(layer "F.SilkS")
	)
	(gr_text "A3"
		(at 163.703 53.9888 90)
		(layer "F.SilkS")
	)
	(gr_text "SWDCLK"
		(at 63.8048 121.8322 0)
		(layer "F.SilkS")
	)
	(gr_text "D5"
		(at 161.1884 104.9158 90)
		(layer "F.SilkS")
	)
	(gr_text "ADC 1"
		(at 168.91 61.812 0)
		(layer "F.SilkS")
	)
	(gr_text "CK"
		(at 84.3788 49.3406 0)
		(layer "F.SilkS")
	)
	(gr_text "TCK\n"
		(at 80.9752 54.5984 90)
		(layer "F.SilkS")
	)
	(gr_text "CLK OUT"
		(at 147.5232 94.0192 0)
		(layer "F.SilkS")
	)
	(gr_text "STM32\nJTAG"
		(at 78.2828 64.9362 0)
		(layer "F.SilkS")
	)
	(gr_text "SWDIO"
		(at 64.389 124.2198 0)
		(layer "F.SilkS")
	)
	(gr_text "MODE A"
		(at 166.8526 69.6352 0)
		(layer "F.SilkS")
	)
	(gr_text "TDI"
		(at 140.8684 97.753 90)
		(layer "F.SilkS")
	)
	(gr_text "VCC"
		(at 78.5622 49.3914 0)
		(layer "F.SilkS")
	)
	(gr_text "ECP5 FPGA"
		(at 122.936 83.402 90)
		(layer "F.SilkS")
	)
	(gr_text "ADRV9002"
		(at 144.78 83.021 90)
		(layer "F.SilkS")
	)
	(gr_text "TX\n"
		(at 180.869336 100.855862 0)
		(layer "F.SilkS")
	)
	(gr_text "D9\n"
		(at 141.0208 92.292 90)
		(layer "F.SilkS")
	)
	(gr_text "A0"
		(at 153.543 99.658 90)
		(layer "F.SilkS")
	)
	(gr_text "D10"
		(at 143.4592 92.3174 90)
		(layer "F.SilkS")
	)
	(gr_text "FPGA GPIO"
		(at 107.95 82.513 90)
		(layer "F.SilkS")
	)
	(gr_text "!! +5.5V MAX !!"
		(at 64.897 73.75 0)
		(layer "F.SilkS")
	)
	(gr_text "D1"
		(at 158.6992 54.0142 90)
		(layer "F.SilkS")
	)
	(gr_text "ADC 2"
		(at 169.037 59.526 0)
		(layer "F.SilkS")
	)
	(gr_text "KitProg3"
		(at 59.2328 128.0806 0)
		(layer "F.SilkS")
	)
	(gr_text "A8"
		(at 161.29 99.8104 90)
		(layer "F.SilkS")
	)
	(gr_text "A2"
		(at 166.243 53.9888 90)
		(layer "F.SilkS")
	)
	(gr_text "A11"
		(at 163.703 100.293 90)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 99.4156 62.9296 0)
		(layer "F.SilkS")
	)
	(gr_text "D7"
		(at 156.083 104.8396 90)
		(layer "F.SilkS")
	)
	(gr_text "TDI"
		(at 86.0044 54.5984 90)
		(layer "F.SilkS")
	)
	(gr_text "iCELink"
		(at 100.6348 60.3134 0)
		(layer "F.SilkS")
	)
	(gr_text "TDI"
		(at 102.2604 62.9042 0)
		(layer "F.SilkS")
	)
	(gr_text "D11"
		(at 166.116 105.246 90)
		(layer "F.SilkS")
	)
	(gr_text "ADRV\nJTAG"
		(at 148.1074 102.96 90)
		(layer "F.SilkS")
	)
	(gr_text "D3"
		(at 158.6738 104.8904 90)
		(layer "F.SilkS")
	)
	(gr_text "3.3V IO"
		(at 145.8976 54.0142 90)
		(layer "F.SilkS")
	)
	(gr_text "D0"
		(at 156.1338 53.9888 90)
		(layer "F.SilkS")
	)
	(gr_text "~{RST}"
		(at 64.4144 119.3684 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 83.947 82.7924 0)
		(layer "F.SilkS")
	)
	(gr_text "FPGA\nJTAG"
		(at 87.5284 68.035 0)
		(layer "F.SilkS")
	)
	(gr_text "A7"
		(at 158.6992 58.9164 90)
		(layer "F.SilkS")
	)
	(gr_text "RX\n\n"
		(at 170.053 58.002 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 64.389 116.9046 0)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 83.2866 54.573 90)
		(layer "F.SilkS")
	)
	(gr_text "D4"
		(at 163.8046 104.9412 90)
		(layer "F.SilkS")
	)
	(gr_text "ADC 3"
		(at 169.291 56.859 0)
		(layer "F.SilkS")
	)
	(gr_text "~{RST}"
		(at 88.265 54.4714 90)
		(layer "F.SilkS")
	)
	(gr_text "A4"
		(at 161.163 53.938 90)
		(layer "F.SilkS")
	)
	(gr_text "A5"
		(at 153.4922 58.9926 90)
		(layer "F.SilkS")
	)
	(gr_text "A6"
		(at 156.0322 59.018 90)
		(layer "F.SilkS")
	)
	(gr_text "TCK\n"
		(at 96.7486 62.955 0)
		(layer "F.SilkS")
	)
	(gr_text "A10"
		(at 138.3284 92.3174 90)
		(layer "F.SilkS")
	)
	(gr_text "~{RST}\n"
		(at 143.4592 97.753 90)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 93.726 62.955 0)
		(layer "F.SilkS")
	)
	(gr_text "MODE"
		(at 124.0282 100.674 90)
		(layer "F.SilkS")
	)
	(gr_text "A1"
		(at 156.083 99.7088 90)
		(layer "F.SilkS")
	)
	(gr_text_box "SK1708\nYTH 21/8/2024\n"
		(start 198.882 104.357)
		(end 219.837 112.866)
		(layer "F.Cu")
		(border yes)
	)
	(zone
		(net 21)
		(net_name "+5.0V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 77.216 92.419) (xy 84.6836 92.419) (xy 85.598 91.5046) (xy 85.598 88.736) (xy 84.7344 87.8724)
				(xy 79.9338 87.8724) (xy 79.3496 88.4566) (xy 77.216 88.4566)
			)
		)
	)
	(zone
		(net 428)
		(net_name "Net-(Z1-K)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 66.3956 92.673) (xy 75.8952 92.673) (xy 75.8952 87.3136) (xy 74.4474 85.8658) (xy 66.421 85.8658)
			)
		)
	)
	(zone
		(net 232)
		(net_name "GND")
		(layers "In1.Cu" "In4.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 58.42 48.858) (xy 225.025 48.858) (xy 225.025 161.488) (xy 58.42 161.488)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/FPGA/F_1P8")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.159 78.3474) (xy 129.0066 78.576) (xy 129.0066 79.0332) (xy 129.4892 79.4904) (xy 132.4864 79.4904)
				(xy 132.6896 79.2872) (xy 132.6896 78.7792) (xy 132.1816 78.3474)
			)
		)
	)
	(zone
		(net 88)
		(net_name "+2.5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.143 78.5252) (xy 128.143 77.687) (xy 131.6482 74.1818) (xy 132.461 74.1818) (xy 132.7404 74.4612)
				(xy 132.7404 75.5788) (xy 130.1242 78.195) (xy 129.0828 78.195) (xy 128.5748 78.703) (xy 128.3208 78.703)
			)
		)
	)
	(zone
		(net 294)
		(net_name "/Power Supply/V_1P3")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 154.4828 64.3266) (xy 155.2448 63.4884) (xy 160.8328 63.4884) (xy 165.4556 68.035) (xy 165.5826 119.4192)
				(xy 157.9626 127.1408) (xy 135.0518 126.9884) (xy 135.0772 124.677) (xy 140.0556 119.6986) (xy 149.733 119.6986)
				(xy 152.8572 116.5236) (xy 152.8826 105.1698) (xy 152.9334 84.1894) (xy 158.4198 79.4142) (xy 158.3182 70.4226)
				(xy 154.5336 67.0698)
			)
		)
	)
	(zone
		(net 107)
		(net_name "+1.1V")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.1336 74.7406) (xy 129.4638 75.0708) (xy 129.4638 79.1094) (xy 127.2032 81.37) (xy 127.2032 85.434)
				(xy 127.6604 85.9166) (xy 129.2098 85.9166) (xy 132.1308 82.9956) (xy 132.1308 79.084) (xy 132.6388 78.576)
				(xy 132.6388 77.5854) (xy 132.4356 77.3822) (xy 131.5974 77.3822) (xy 131.2672 77.052) (xy 131.2672 74.639)
				(xy 130.7592 74.131) (xy 129.413 74.131) (xy 129.1336 74.4104)
			)
		)
	)
	(zone
		(net 165)
		(net_name "/VANA_1P8_F")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.9014 68.162) (xy 152.0444 69.2796) (xy 152.0444 72.48) (xy 151.765 72.6832) (xy 151.765 73.1404)
				(xy 152.0444 73.369) (xy 152.0444 73.9024) (xy 151.8412 74.1056) (xy 151.8412 75.0708) (xy 152.0444 75.274)
				(xy 152.0444 75.6042) (xy 152.2222 75.782) (xy 152.2222 76.036) (xy 152.2222 77.0012) (xy 152.1206 77.1282)
				(xy 151.8666 77.1282) (xy 151.765 77.052) (xy 151.765 76.9504) (xy 151.5872 76.7726) (xy 151.2316 76.7726)
				(xy 151.0538 76.9504) (xy 151.0538 79.9984) (xy 152.273 81.0652) (xy 152.2476 81.9288) (xy 152.0952 82.0558)
				(xy 151.2316 82.0558) (xy 149.6314 80.4302) (xy 149.6314 77.7307) (xy 149.8092 77.5854) (xy 149.8092 76.671)
				(xy 150.1648 76.3154) (xy 150.1648 74.8676) (xy 148.4122 73.115) (xy 148.4122 68.162)
			)
		)
	)
	(zone
		(net 432)
		(net_name "/Power Supply/Vin")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.285 116.1426) (xy 121.539 116.3966) (xy 121.539 117.565) (xy 120.9548 118.1492) (xy 117.5258 118.1492)
				(xy 115.7224 119.978) (xy 111.4806 119.9526) (xy 110.4392 120.994) (xy 104.5718 126.9376) (xy 85.6488 126.8868)
				(xy 84.6582 125.9216) (xy 84.6836 91.8348) (xy 86.8934 88.9392) (xy 92.837 88.9392) (xy 96.5962 92.673)
				(xy 96.6216 117.692) (xy 97.1296 118.2762) (xy 98.2218 119.3938) (xy 101.3206 119.3684) (xy 104.5718 116.1172)
			)
		)
	)
	(zone
		(net 197)
		(net_name "/VSYN_1P3_F")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.988 78.6014) (xy 156.2862 80.3032) (xy 154.2288 80.3032) (xy 154.1018 80.1254) (xy 154.1018 79.8714)
				(xy 154.051 79.7444) (xy 152.5778 78.7538) (xy 152.5778 78.1696) (xy 152.7302 78.0172) (xy 155.8036 78.0172)
				(xy 156.1338 77.687) (xy 156.1338 75.5534) (xy 155.7782 75.1978) (xy 154.0256 75.1978) (xy 153.1874 75.1978)
				(xy 152.8572 74.9438) (xy 152.6032 74.7406) (xy 152.6032 74.3342) (xy 153.0096 73.9278) (xy 153.9748 73.9278)
				(xy 154.305 73.5722) (xy 154.9908 72.9118) (xy 157.7594 72.9118) (xy 157.988 73.1404) (xy 157.988 74.512)
			)
		)
	)
	(zone
		(net 97)
		(net_name "+3.3V")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 86.868 88.609) (xy 92.9386 88.609) (xy 96.9772 92.6222) (xy 96.9772 102.7568) (xy 97.8408 103.6458)
				(xy 116.9162 103.6458) (xy 117.4242 103.1378) (xy 117.4242 100.166) (xy 116.9162 99.658) (xy 101.2698 99.658)
				(xy 99.8728 98.2356) (xy 99.8982 93.1556) (xy 101.4476 91.6062) (xy 108.3564 91.6062) (xy 109.7534 90.2092)
				(xy 109.7788 80.0492) (xy 113.9698 75.8836) (xy 113.9698 74.8168) (xy 114.427 74.385) (xy 118.364 74.385)
				(xy 118.7196 74.7406) (xy 128.4986 74.7406) (xy 129.1844 73.9786) (xy 131.2672 73.9786) (xy 132.9182 75.8074)
				(xy 136.9568 75.8074) (xy 136.9568 72.4038) (xy 140.4874 68.8986) (xy 148.0058 61.8882) (xy 149.9362 61.9136)
				(xy 151.2316 63.4884) (xy 154.2796 63.4884) (xy 154.686 62.9804) (xy 160.9852 63.0058) (xy 166.1414 67.8826)
				(xy 166.1668 94.9336) (xy 189.5094 94.9336) (xy 192.1002 91.9364) (xy 192.1764 50.0518) (xy 105.460334 50.106961)
				(xy 104.013 51.525) (xy 104.013 57.494) (xy 102.3112 59.1958) (xy 96.7994 59.1958) (xy 94.234 61.7612)
				(xy 94.2086 75.782) (xy 86.106 82.9956) (xy 86.0806 87.847)
			)
		)
	)
	(zone
		(net 297)
		(net_name "/Power Supply/V_1P8")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 148.0058 62.2692) (xy 149.7076 62.2946) (xy 150.4442 63.1582) (xy 150.4442 67.8064) (xy 148.3106 67.8318)
				(xy 148.0566 68.162) (xy 148.0566 73.623) (xy 143.7132 73.623) (xy 142.0368 75.3502) (xy 142.0368 76.8742)
				(xy 144.1704 79.0078) (xy 144.1196 103.4934) (xy 134.0866 113.5518) (xy 134.0866 115.7362) (xy 104.1908 115.7362)
				(xy 100.965 118.9874) (xy 98.552 118.9874) (xy 97.8408 118.2762) (xy 97.8408 114.5678) (xy 106.9086 104.4332)
				(xy 131.5212 104.4332) (xy 133.5278 102.325) (xy 133.5278 93.308) (xy 131.7752 91.53) (xy 116.205 91.5046)
				(xy 111.1504 86.4754) (xy 111.1504 83.1734) (xy 111.6584 82.4622) (xy 115.4684 82.4622) (xy 116.3066 83.2496)
				(xy 116.3066 86.2976) (xy 117.6528 87.593) (xy 132.3594 87.593) (xy 133.4262 86.5262) (xy 135.8646 86.5262)
				(xy 136.398 85.9928) (xy 136.414424 83.977066) (xy 138.938 81.497) (xy 139.6492 80.7604) (xy 139.6492 77.9664)
				(xy 138.43 76.7472) (xy 138.43 71.5148) (xy 148.0312 62.2438)
			)
		)
	)
	(zone
		(net 429)
		(net_name "Net-(D3-A)")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100.076 55.6398) (xy 100.4824 56.0462) (xy 100.4824 58.5608) (xy 100.076 58.9418) (xy 96.5708 58.9418)
				(xy 93.9038 61.6088) (xy 93.8784 75.274) (xy 85.2424 82.894) (xy 85.2424 84.4434) (xy 84.5058 85.18)
				(xy 82.1182 85.1546) (xy 81.3816 84.418) (xy 81.3816 66.2824) (xy 92.0242 55.6398)
			)
		)
	)
	(zone
		(net 298)
		(net_name "/Power Supply/V_1P0")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 136.3472 116.2188) (xy 148.7678 116.2188) (xy 151.9428 112.993) (xy 151.9428 82.4114) (xy 150.9522 82.4114)
				(xy 149.0472 80.5064) (xy 149.0472 77.8902) (xy 148.0312 77.2044) (xy 145.6182 77.2298) (xy 143.6878 75.3248)
				(xy 142.5956 75.3248) (xy 142.2654 75.6804) (xy 142.2654 76.8234) (xy 144.0434 78.6014) (xy 144.8054 79.3634)
				(xy 144.8308 103.9506) (xy 135.8138 112.8152) (xy 135.8138 115.6854)
			)
		)
	)
	(zone
		(net 281)
		(net_name "+1.8V")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.4976 79.338) (xy 121.6152 79.338) (xy 122.3264 80.0492) (xy 122.3264 82.767) (xy 121.285 83.8084)
				(xy 120.4468 83.8084) (xy 118.8466 85.4086) (xy 118.8466 86.2468) (xy 119.1514 86.5262) (xy 124.0536 86.5262)
				(xy 124.5108 86.069) (xy 129.3368 86.069) (xy 130.7846 84.6212) (xy 135.2804 84.6212) (xy 135.9408 84.6212)
				(xy 136.2202 84.9006) (xy 136.2202 85.8658) (xy 135.8138 86.2722) (xy 133.3246 86.2722) (xy 132.2324 87.3644)
				(xy 117.6782 87.4406) (xy 116.4844 86.2468) (xy 116.4844 82.9194) (xy 120.0912 79.338)
			)
		)
	)
	(zone
		(net 72)
		(net_name "Net-(F1-Pad1)")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 65.786 89.371) (xy 71.5518 83.6306) (xy 77.5462 83.6306) (xy 79.3242 82.4622) (xy 79.3242 63.7678)
				(xy 73.1774 57.6718) (xy 60.2234 57.6718) (xy 59.0296 58.891) (xy 59.0296 88.5074) (xy 59.8424 89.371)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/FPGA/FM_1P8")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110.2868 80.5826) (xy 118.4402 80.608) (xy 118.9228 80.608) (xy 119.253 80.3794) (xy 119.253 79.6428)
				(xy 118.9228 79.3126) (xy 116.7638 79.3126) (xy 115.2144 77.7632) (xy 112.5474 77.7886) (xy 110.2868 80.0492)
			)
		)
	)
	(zone
		(net 163)
		(net_name "/VDIGIO_1P8_F")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.3736 75.6296) (xy 144.5768 75.4264) (xy 147.8534 75.4264) (xy 148.463 75.4264) (xy 148.9456 76.0106)
				(xy 148.9456 76.3154) (xy 148.3106 76.9504) (xy 145.4912 76.925) (xy 144.3736 75.8074)
			)
		)
	)
	(zone
		(net 277)
		(net_name "/VDIG_1P0_F")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.7038 74.1564) (xy 144.9324 73.9278) (xy 146.2532 73.9278) (xy 148.9964 73.9278) (xy 150.1648 75.0708)
				(xy 150.1648 76.2646) (xy 149.7838 76.6456) (xy 149.7838 77.2552) (xy 149.6314 77.4076) (xy 149.3012 77.4076)
				(xy 149.0726 77.179) (xy 149.0726 76.036) (xy 148.4884 75.3248) (xy 148.3868 75.3248) (xy 144.9324 75.3248)
				(xy 144.7038 75.0962)
			)
		)
	)
	(zone
		(net 185)
		(net_name "/VANA_1P3_F")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 154.813 69.7622) (xy 154.6352 70.0162) (xy 153.9748 70.0162) (xy 153.4922 70.5242) (xy 153.4922 71.7942)
				(xy 152.9334 72.4038) (xy 152.2984 72.4038) (xy 151.8412 72.734) (xy 151.8412 73.0896) (xy 152.1714 73.3436)
				(xy 152.1714 73.9532) (xy 151.9682 74.1564) (xy 151.9682 74.9946) (xy 152.1714 75.1978) (xy 152.1714 75.6296)
				(xy 152.4508 75.8582) (xy 152.4508 76.9758) (xy 152.146 77.2806) (xy 151.7904 77.2806) (xy 151.638 77.1282)
				(xy 151.638 76.9504) (xy 151.5364 76.8488) (xy 151.257 76.8488) (xy 151.13 76.9758) (xy 151.13 79.8714)
				(xy 153.5176 81.9034) (xy 153.8224 81.9034) (xy 154.2542 81.3192) (xy 154.2542 80.3794) (xy 153.92196 80.153805)
				(xy 153.924 79.7698) (xy 152.5016 78.8046) (xy 152.5016 78.1442) (xy 152.7302 77.9156) (xy 155.7274 77.9156)
				(xy 156.0068 77.5854) (xy 156.0068 77.3822) (xy 156.1846 77.179) (xy 156.1846 75.7566) (xy 155.702 75.274)
				(xy 153.0858 75.274) (xy 152.527 74.7152) (xy 152.527 74.3088) (xy 153.035 73.8008) (xy 153.924 73.8008)
				(xy 154.7114 73.0134) (xy 155.0162 72.7086) (xy 155.0162 71.2862) (xy 155.194 71.083) (xy 155.3972 71.083)
				(xy 155.6258 70.8544) (xy 155.6258 69.9654) (xy 155.4226 69.7622)
			)
		)
	)
	(zone
		(net 356)
		(net_name "Net-(U25-PVIN3)")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.5268 117.057) (xy 125.5268 124.4992) (xy 116.9924 124.4738) (xy 114.4524 127.0138) (xy 113.4618 127.0138)
				(xy 112.2172 125.7184) (xy 109.2454 125.7184) (xy 108.1024 124.042) (xy 108.1024 123.3562) (xy 109.1692 122.2894)
				(xy 114.935 122.264) (xy 114.935 121.0448) (xy 117.348 118.6318) (xy 118.8212 118.6318) (xy 119.1006 118.3524)
				(xy 121.2342 118.3778) (xy 121.793 117.7936) (xy 121.793 117.057)
			)
		)
	)
	(zone
		(net 88)
		(net_name "+2.5V")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.27 78.195) (xy 128.651 78.195) (xy 128.778 78.322) (xy 128.778 79.5666) (xy 126.9492 81.3954)
				(xy 126.9492 83.2496) (xy 123.8504 86.3484) (xy 119.2022 86.3484) (xy 119.0244 86.196) (xy 119.0244 85.4594)
				(xy 120.396 84.0878) (xy 121.3612 84.0878) (xy 126.1872 79.2618) (xy 127.2032 79.2618)
			)
		)
	)
	(zone
		(net 349)
		(net_name "Net-(U22-EN)")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 101.4222 99.3278) (xy 124.714 99.3786) (xy 125.603 98.4896) (xy 125.603 93.4858) (xy 124.714 92.5968)
				(xy 101.3968 92.5714) (xy 100.33 93.6382) (xy 100.33 98.2102)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/FPGA/N_1P8")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.4196 76.9758) (xy 131.6482 77.2298) (xy 132.4864 77.2298) (xy 135.1534 79.9476) (xy 138.6332 79.9476)
				(xy 139.1666 79.4142) (xy 139.1666 78.7284) (xy 138.4554 78.0172) (xy 137.0584 78.0172) (xy 135.1534 76.1122)
				(xy 131.699 76.1122) (xy 131.4196 76.3916)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/FPGA/F_1P8")
		(layer "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.2794 79.0332) (xy 128.1938 78.1188) (xy 128.6764 78.1188) (xy 128.8542 78.2966) (xy 128.8542 78.6522)
				(xy 129.032 78.8808) (xy 129.2606 78.8808) (xy 129.413 78.7284) (xy 129.413 77.7632) (xy 129.3622 77.687)
				(xy 129.3622 75.1216) (xy 129.2098 74.9692) (xy 118.4148 74.9692) (xy 118.0592 74.6136) (xy 114.5032 74.6136)
				(xy 114.2238 74.893) (xy 114.2238 76.5694) (xy 116.713 79.0586)
			)
		)
	)
	(zone
		(net 350)
		(net_name "/Power Supply/adp5056_1P8V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 107.442 122.6704) (xy 107.3912 120.867) (xy 106.553 120.0034) (xy 100.3046 120.0288) (xy 100.3046 121.2734)
				(xy 100.3046 122.2894) (xy 100.6602 122.645)
			)
		)
	)
	(zone
		(net 353)
		(net_name "/Power Supply/adp5056_1P0V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.8316 117.2094) (xy 129.6416 117.2094) (xy 133.9342 115.1012) (xy 133.9342 114.0598) (xy 130.3528 114.0598)
				(xy 129.9464 114.4154) (xy 125.8316 114.4154)
			)
		)
	)
	(zone
		(net 370)
		(net_name "/Power Supply/ALT_1P8")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.3198 83.91) (xy 120.3198 85.307) (xy 119.761 85.8658) (xy 114.3508 85.8658) (xy 113.6904 86.5262)
				(xy 113.6904 90.6664) (xy 113.7158 91.7586) (xy 111.8616 91.7332) (xy 111.8616 91.1236) (xy 110.8964 90.1076)
				(xy 110.8456 86.45) (xy 113.4364 83.8592)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/Power Supply/ap3445_3P3V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 101.0412 89.8028) (xy 102.2858 89.8028) (xy 102.9716 90.4886) (xy 102.9716 91.403) (xy 103.2256 91.657)
				(xy 105.1052 91.657) (xy 105.1052 90.6156) (xy 104.4194 90.6156) (xy 104.0638 90.26) (xy 104.0638 86.069)
				(xy 102.6414 84.6212) (xy 101.3206 84.6212) (xy 101.0412 84.9006)
			)
		)
	)
	(zone
		(net 363)
		(net_name "Net-(C162-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.3826 118.6434) (xy 125.979 118.6434) (xy 125.5218 119.1006) (xy 115.3872 119.1006) (xy 114.9808 119.4308)
				(xy 114.9808 120.015) (xy 118.0846 120.015) (xy 118.6688 120.3336) (xy 129.413 120.359)
			)
		)
	)
	(zone
		(net 364)
		(net_name "Net-(U25-SW3)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.284 120.5622) (xy 109.2708 120.5622) (xy 107.9754 119.5716) (xy 103.7082 119.597) (xy 103.1748 119.0636)
				(xy 103.1748 117.819) (xy 108.6612 117.819) (xy 110.2106 119.3938) (xy 111.5314 119.3938) (xy 112.4712 120.232)
				(xy 113.284 120.232)
			)
		)
	)
	(zone
		(net 361)
		(net_name "Net-(C161-Pad2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.9604 121.3496) (xy 118.0846 121.3496) (xy 118.6688 120.9686) (xy 129.3876 120.9686) (xy 129.3876 122.8482)
				(xy 125.9586 122.8736) (xy 125.4252 122.3402) (xy 118.6434 122.3402) (xy 118.0338 122.0354) (xy 115.0112 122.0354)
			)
		)
	)
	(zone
		(net 107)
		(net_name "+1.1V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.8702 91.784) (xy 129.8702 90.9458) (xy 129.159 90.2346) (xy 129.159 85.7642) (xy 128.7018 85.307)
				(xy 127.6604 85.307) (xy 127.3429 85.7134) (xy 127.3429 86.3992) (xy 127.0127 86.9326) (xy 126.9873 90.1076)
				(xy 128.198128 91.271497) (xy 128.1938 91.784)
			)
		)
	)
	(zone
		(net 354)
		(net_name "/Power Supply/adp5056_1P3V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.984 124.2452) (xy 125.984 125.3628) (xy 125.0188 126.328) (xy 124.968 127.1662) (xy 133.9088 127.217)
				(xy 133.9342 125.2104) (xy 130.5814 125.2104) (xy 129.667 124.296)
			)
		)
	)
	(zone
		(net 88)
		(net_name "+2.5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.1524)
		)
		(min_thickness 0.0762)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.6942 85.9674) (xy 121.3866 85.9674) (xy 121.3866 90.387) (xy 121.92 90.9204) (xy 121.92 91.8602)
				(xy 119.9134 91.8602) (xy 119.9134 91.149) (xy 118.7196 89.9552)
			)
		)
	)
)