<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="60.96" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="0" x2="50.8" y2="0" width="0" layer="20"/>
<wire x1="50.8" y1="0" x2="50.8" y2="60.96" width="0" layer="20"/>
<wire x1="50.8" y1="60.96" x2="0" y2="60.96" width="0" layer="20"/>
<text>Colorsound One-Knob Fuzz Clone</text>
<hole x="5.715" y="12.7" drill="3.302"/>
<hole x="45.085" y="12.7" drill="3.302"/>
</plain>
<libraries>
<library name="zth_eteknet">
<packages>
<package name="RESISTOR-0.5W">
<description>Resistor - 1/2 Watt</description>
</package>
<package name="POT16RAR">
<description>16mm single-gang potentiometer, right-angle PCB mount, smaller trace</description>
</package>
<package name="C050-025X075WW-S">
<description>Capacitor - grid 5 mm (2x wide)</description>
</package>
<package name="PAD-LARGE-N">
<description>Through-hole pad, large size, "narrow"</description>
</package>
<package name="DIODE-1N40XX">
<description>1N400X diode</description>
</package>
<package name="CMX-L01">
<description>Capacitor - electrolytic, polar, large</description>
</package>
<package name="CMX-M01">
<description>Capacitor - electrolytic, polar, medium</description>
</package>
<package name="NPN-SOCK2">
</package>
<package name="LED-RL-N">
<description>LED (remote), Large, smaller hole size</description>
</package>
</packages>
</library>
<library name="zth_tubeamps">
<description>Components for valve-based circuits</description>
<packages>
<package name="CN-MOJOD-100N">
<description>Mojo Dijon capacitor, 100n/220n</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="VS" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="G" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="C5" library="zth_eteknet" package="CMX-L01" value="47u\">
<attribute name="NAME"/>
</element>
<element name="D2" library="zth_eteknet" package="DIODE-1N40XX" value="4002">
<attribute name="NAME"/>
</element>
<element name="YG" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="Q1" library="zth_eteknet" package="NPN-SOCK2" value="BC109">
<attribute name="NAME"/>
</element>
<element name="Q2" library="zth_eteknet" package="NPN-SOCK2" value="BC108">
<attribute name="NAME"/>
</element>
<element name="C3" library="zth_eteknet" package="CMX-M01" value="10u">
<attribute name="NAME"/>
</element>
<element name="R4" library="zth_eteknet" package="RESISTOR-0.5W" value="82">
<attribute name="NAME"/>
</element>
<element name="R2" library="zth_eteknet" package="RESISTOR-0.5W" value="10k">
<attribute name="NAME"/>
</element>
<element name="R1" library="zth_eteknet" package="RESISTOR-0.5W" value="1M">
<attribute name="NAME"/>
</element>
<element name="R3" library="zth_eteknet" package="RESISTOR-0.5W" value="150k">
<attribute name="NAME"/>
</element>
<element name="C4" library="zth_tubeamps" package="CN-MOJOD-100N" value="220n">
<attribute name="NAME"/>
</element>
<element name="LEVEL" library="zth_eteknet" package="POT16RAR" value="B500k"/>
<element name="R5" library="zth_eteknet" package="RESISTOR-0.5W" value="2k2">
<attribute name="NAME"/>
</element>
<element name="C1" library="zth_tubeamps" package="CN-MOJOD-100N" value="100n">
<attribute name="NAME"/>
</element>
<element name="R6" library="zth_eteknet" package="RESISTOR-0.5W" value="1k">
<attribute name="NAME"/>
</element>
<element name="C2" library="zth_eteknet" package="C050-025X075WW-S" value="220p">
<attribute name="NAME"/>
</element>
<element name="R7" library="zth_eteknet" package="RESISTOR-0.5W" value="18k">
<attribute name="NAME"/>
</element>
<element name="D1" library="zth_eteknet" package="LED-RL-N" value="red">
<attribute name="NAME"/>
</element>
<element name="Y" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="X" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
<element name="XG" library="zth_eteknet" package="PAD-LARGE-N" value=" ">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="V+">
<contactref element="C5" pad="+"/>
<contactref element="D2" pad="C"/>
<contactref element="R7" pad="2"/>
<contactref element="VS" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C5" pad="-"/>
<contactref element="D2" pad="A"/>
<contactref element="Q1" pad="E"/>
<contactref element="LEVEL" pad="P0"/>
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="G" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="YG" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="XG" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="LEVEL" pad="W"/>
<contactref element="Y" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="Q2" pad="E"/>
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="+"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="Q2" pad="B"/>
<contactref element="Q1" pad="C"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="R5" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="B"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="Q2" pad="C"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="LEVEL" pad="P1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="D1" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="C1" pad="1"/>
<contactref element="X" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
