<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="60.63" y2="0" width="0" layer="20"/>
<wire x1="60.63" y1="0" x2="60.63" y2="30.47" width="0" layer="20"/>
<wire x1="60.63" y1="30.47" x2="0" y2="30.47" width="0" layer="20"/>
<wire x1="0" y1="30.47" x2="0" y2="0" width="0" layer="20"/>
<text>SCART Breakout</text>
<text>Audio OUT (R)</text>
<text>Audio IN (R)</text>
<text>Audio OUT</text>
<text>Audio GND</text>
<text>GND (7)</text>
<text>Audio IN (L/Mono)</text>
<text>RGB Blue OUT</text>
<text>0-2V OFF</text>
<text>GND (11)</text>
<text>Clock / Data 2</text>
<text>RGB Green OUT</text>
<text>Reserved / Data 1</text>
<text>GND (15)</text>
<text>GND (8, 10 &amp; 12)</text>
<text>RGB Red OUT</text>
<text>0-0.4V Composite</text>
<text>GND (19, 20)</text>
<text>GND (16)</text>
<text>Composite OUT</text>
<text>Composite IN</text>
<text>Shell / Chassis</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>16</text>
<text>17</text>
<text>18</text>
<text>19</text>
<text>20</text>
<text>21</text>
<text>S-Video C IN</text>
<text>YPbPr Pb OUT</text>
<text>5-8V ON (16:9)</text>
<text>9.5-12V ON (4:3)</text>
<text>Control bus</text>
<text>YPbPr Y OUT</text>
<text>S-Video C OUT</text>
<text>YPbPr Pr OUT</text>
<text>1-3V RGB</text>
<text>S-Video Y OUT</text>
<text>S-Video Y IN</text>
<text>(L/Mono)</text>
<text>(AV.link)</text>
</plain>
<libraries>
<library name="con-hirschmann">
<description>&lt;b&gt;Hirschmann Connectors&lt;/b&gt;&lt;p&gt;
Audio, scart, microphone, headphone&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SCART-F">
<description>TV SCART &lt;B&gt;CONNECTOR&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="1X21">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="con-hirschmann" package="SCART-F" value="SCART-F">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="JP1" library="pinhead" package="1X21" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="X1" pad="10"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="X1" pad="12"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="8"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="X1" pad="6"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="X1" pad="4"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="X1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="X1" pad="14"/>
<contactref element="JP1" pad="14"/>
</signal>
<signal name="N$8">
<contactref element="X1" pad="16"/>
<contactref element="JP1" pad="16"/>
</signal>
<signal name="N$9">
<contactref element="X1" pad="18"/>
<contactref element="JP1" pad="18"/>
</signal>
<signal name="N$10">
<contactref element="X1" pad="20"/>
<contactref element="JP1" pad="20"/>
</signal>
<signal name="N$11">
<contactref element="X1" pad="21"/>
<contactref element="JP1" pad="21"/>
</signal>
<signal name="N$12">
<contactref element="X1" pad="19"/>
<contactref element="JP1" pad="19"/>
</signal>
<signal name="N$13">
<contactref element="X1" pad="17"/>
<contactref element="JP1" pad="17"/>
</signal>
<signal name="N$14">
<contactref element="X1" pad="15"/>
<contactref element="JP1" pad="15"/>
</signal>
<signal name="N$15">
<contactref element="X1" pad="13"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="N$16">
<contactref element="X1" pad="11"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="N$17">
<contactref element="X1" pad="9"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$18">
<contactref element="X1" pad="7"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="X1" pad="5"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$20">
<contactref element="X1" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="X1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
