(kicad_pcb (version 20171130) (host pcbnew 5.1.6)
  (general
    (thickness 1.6)
    (drawings 37)
    (tracks 29)
    (zones 0)
    (modules 4)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VBUS)
  (net 2 GND)
  (net 3 /D6)
  (net 4 /D5)
  (net 5 /D7)
  (net 6 /D4)
  (net 7 /D0)
  (net 8 /D3)
  (net 9 /D1)
  (net 10 /D2)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net GND)
    (add_net VBUS)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Horizontal (layer F.Cu) (tedit 5F3B4F64)
    (at 141.605 97.79)
    (descr "Through hole angled pin header, 1x08, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 4.385 -2.27) (layer F.SilkS) hide)
    (fp_text value Conn_01x08_Female (at 4.385 20.05) (layer F.Fab))
    (fp_text user %R (at 2.77 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D0))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /D1))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /D2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /D3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D4))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /D7))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5F3B4DCA)
    (at 137.16 97.79)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5F3B4A93)
    (at 137.16 115.57)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VBUS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 137.16 109.22 180)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference J1 (at 0.635 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_02x05_Odd_Even (at 0.635 6.775) (layer F.Fab))
    (fp_text user %R (at 0.635 2.54 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 1.27 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /D6))
    (pad 9 thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /D5))
    (pad 8 thru_hole oval (at 1.27 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 /D7))
    (pad 7 thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /D4))
    (pad 6 thru_hole oval (at 1.27 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 /D0))
    (pad 5 thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 /D3))
    (pad 4 thru_hole oval (at 1.27 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 /D1))
    (pad 3 thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /D2))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 VBUS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text +V (at 137.16 113.284 270) (layer B.SilkS))
  (gr_text GND (at 137.16 100.838 270) (layer B.SilkS))
  (gr_text GND (at 137.16 100.838 270) (layer F.SilkS))
  (gr_text +V (at 137.16 113.284 270) (layer F.SilkS))
  (gr_text 0 (at 139.446 115.57 270) (layer B.SilkS))
  (gr_text 1 (at 139.446 113.03 270) (layer B.SilkS))
  (gr_text 2 (at 139.446 110.49 270) (layer B.SilkS))
  (gr_text 3 (at 139.446 107.95 270) (layer B.SilkS))
  (gr_text 4 (at 139.446 105.41 270) (layer B.SilkS))
  (gr_text 5 (at 139.446 102.87 270) (layer B.SilkS))
  (gr_text 6 (at 139.446 100.33 270) (layer B.SilkS))
  (gr_text 7 (at 139.446 97.79 270) (layer B.SilkS))
  (gr_text 0 (at 139.446 115.57 270) (layer F.SilkS))
  (gr_text 1 (at 139.446 113.03 270) (layer F.SilkS))
  (gr_text 2 (at 139.446 110.49 270) (layer F.SilkS))
  (gr_text 3 (at 139.446 107.95 270) (layer F.SilkS))
  (gr_text 6 (at 139.446 100.33 270) (layer F.SilkS))
  (gr_text 4 (at 139.446 105.41 270) (layer F.SilkS))
  (gr_text 5 (at 139.446 102.87 270) (layer F.SilkS))
  (gr_text 7 (at 139.446 97.79 270) (layer F.SilkS))
  (gr_arc (start 142.24 116.205) (end 142.24 116.84) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 136.525 116.205) (end 135.89 116.205) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 136.525 97.155) (end 136.525 96.52) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 142.24 97.155) (end 142.875 97.155) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 136.525 96.52) (end 142.24 96.52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.62 103.505) (end 135.89 97.155) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.62 109.855) (end 134.62 103.505) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.89 116.205) (end 134.62 109.855) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.24 116.84) (end 136.525 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.875 97.155) (end 142.875 116.205) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.875 116.84) (xy 135.89 116.84) (xy 134.62 109.855) (xy 134.62 103.505) (xy 135.89 96.52)
        (xy 142.875 96.52)
      )
    )
  )
)
