(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(I+1-Pad1)")
  (net 2 "Net-(I-1-Pad1)")
  (footprint "_es_Mechanical:13.8 mil hole" (layer "F.Cu")
    (at 135.89 111.125)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "13.8 mil hole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.35052 0.35052) (drill 0.35052) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "_es_Mechanical:10 mil hole" (layer "F.Cu")
    (at 144.145 104.14)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10 mil hole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.254) (layers "*.Cu" "*.Mask"))
  )
  (footprint "_es_Mechanical:10 mil hole" (layer "F.Cu")
    (at 141.605 104.14)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10 mil hole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.254) (layers "*.Cu" "*.Mask"))
  )
  (footprint "_es_Mechanical:13.8 mil hole" (layer "F.Cu")
    (at 149.86 111.125)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "13.8 mil hole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.35052 0.35052) (drill 0.35052) (layers "F&B.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder" (layer "F.Cu")
    (at 142.875 111.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Alohossenini Resistor Holder 2.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.17) (layer "F.SilkS"))
    (fp_text value "R_Small_US" (at 0 1.17) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(I+1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.5975 0) (size 0.715 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(I-1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "_es_Mechanical:10 mil hole" (layer "F.Cu")
    (at 144.145 118.11)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10 mil hole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.254) (layers "*.Cu" "*.Mask"))
  )
  (footprint "_es_Mechanical:10 mil hole" (layer "F.Cu")
    (at 141.605 118.11)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10 mil hole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.254) (layers "*.Cu" "*.Mask"))
  )
  (footprint "_es_Mechanical:10 mil hole" (layer "F.Cu")
    (at 142.875 104.14)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10 mil hole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.254) (layers "*.Cu" "*.Mask"))
  )
  (footprint "_es_Mechanical:10 mil hole" (layer "F.Cu")
    (at 142.875 118.11)
    (attr smd)
    (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS") hide)
    (fp_text value "10 mil hole" (at 0 1 unlocked) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.254 0.254) (drill 0.254) (layers "*.Cu" "*.Mask"))
  )
  (gr_line (start 156.21 95.25) (end 129.54 95.25)
    (layer "Edge.Cuts"))
  (gr_line (start 127 97.79) (end 127 124.46)
    (layer "Edge.Cuts"))
  (gr_arc (start 129.54 125.73) (mid 128.27 124.46) (end 129.54 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 129.54 96.52) (end 137.16 96.52)
    (layer "Edge.Cuts"))
  (gr_arc (start 129.54 99.06) (mid 128.27 97.79) (end 129.54 96.52)
    (layer "Edge.Cuts"))
  (gr_line (start 156.21 99.06) (end 148.59 99.06)
    (layer "Edge.Cuts"))
  (gr_arc (start 158.75 124.46) (mid 158.006051 126.256051) (end 156.21 127)
    (layer "Edge.Cuts"))
  (gr_line (start 148.59 123.19) (end 156.21 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 129.54 123.19) (end 137.16 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 158.75 124.46) (end 158.75 97.79)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.59 99.06) (mid 147.32 97.79) (end 148.59 96.52)
    (layer "Edge.Cuts"))
  (gr_arc (start 156.21 96.52) (mid 157.48 97.79) (end 156.21 99.06)
    (layer "Edge.Cuts"))
  (gr_arc (start 127 97.79) (mid 127.743949 95.993949) (end 129.54 95.25)
    (layer "Edge.Cuts"))
  (gr_line (start 156.21 125.73) (end 148.59 125.73)
    (layer "Edge.Cuts"))
  (gr_arc (start 137.16 96.52) (mid 138.43 97.79) (end 137.16 99.06)
    (layer "Edge.Cuts"))
  (gr_arc (start 129.54 127) (mid 127.743949 126.256051) (end 127 124.46)
    (layer "Edge.Cuts"))
  (gr_arc (start 156.21 123.19) (mid 157.48 124.46) (end 156.21 125.73)
    (layer "Edge.Cuts"))
  (gr_arc (start 148.59 125.73) (mid 147.32 124.46) (end 148.59 123.19)
    (layer "Edge.Cuts"))
  (gr_line (start 137.16 125.73) (end 129.54 125.73)
    (layer "Edge.Cuts"))
  (gr_line (start 137.16 99.06) (end 129.54 99.06)
    (layer "Edge.Cuts"))
  (gr_arc (start 137.16 123.19) (mid 138.43 124.46) (end 137.16 125.73)
    (layer "Edge.Cuts"))
  (gr_line (start 148.59 96.52) (end 156.21 96.52)
    (layer "Edge.Cuts"))
  (gr_arc (start 156.21 95.25) (mid 158.006051 95.993949) (end 158.75 97.79)
    (layer "Edge.Cuts"))
  (gr_line (start 129.54 127) (end 156.21 127)
    (layer "Edge.Cuts"))
  (gr_text "246 Alihosseini Resistor Holder v2" (at 129.794 121.92) (layer "F.SilkS"))
  (gr_text "Cut Out" (at 133.35 97.79) (layer "F.SilkS"))
  (gr_text "Cut Out" (at 152.4 97.79) (layer "F.SilkS"))
  (gr_text "Cut Out" (at 133.35 124.46) (layer "F.SilkS"))
  (gr_text "Cut Out" (at 152.4 124.46) (layer "F.SilkS"))
)
