(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "alexglow-footprints:2-pin-power" (layer "F.Cu")
    (at 172.54 48.4 180)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference " " (at 0 -2.032) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.032) (layer "F.SilkS"))
    (fp_text user "+" (at 4.54 -0.1) (layer "F.SilkS"))
    (fp_text user "-" (at -1.96 -0.1) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -0.1016 180) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 2.54 -0.1 180) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:hlogoTiny" (layer "F.Cu")
    (at 149.75 97.75)
    (attr through_hole)
    (fp_text reference " " (at 0 0) (layer "F.SilkS") hide)
    (fp_text value " " (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004" (layer "F.Cu")
    (at 177.48 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference " " (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.032 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "9" thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "10" thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "11" thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "12" thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004" (layer "F.Cu")
    (at 169.85 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference " " (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.032 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "9" thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "10" thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "11" thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "12" thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004" (layer "F.Cu")
    (at 174.94 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference " " (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.032 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "9" thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "10" thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "11" thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "12" thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004" (layer "F.Cu")
    (at 129.21 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference " " (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.032 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "9" thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "10" thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "11" thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "12" thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004" (layer "F.Cu")
    (at 172.4 81.275 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference " " (at 0 -2.032 90) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.032 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "2" thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "3" thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "4" thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "5" thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "6" thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "7" thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "8" thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "9" thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "10" thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "11" thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
    (pad "12" thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers "*.Cu" "*.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "cbot-breadboard:coretext-520" (layer "B.Cu")
    (at 149.87036 94.5 180)
    (attr through_hole)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 76.2)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 76.2)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 78.74)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 53.34)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 55.88)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 53.34)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "cbot-breadboard:herz-whole-mask-neg-520" (layer "B.Cu")
    (at 141.91 68.707 180)
    (attr through_hole)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "cbot-breadboard:bow-smol-neg-385" (layer "B.Cu")
    (at 149.59096 71.5772 180)
    (attr through_hole)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 55.88)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 78.74)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 58.42)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 81.28)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 81.28)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 58.42)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 60.96)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 60.96)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 63.5)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 63.5)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 66.04)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 66.04)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 68.58)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 68.58)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 71.12)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 71.12)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 150.8 73.66)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:round-pad" (layer "B.Cu")
    (at 148.26 73.66)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer "B.SilkS"))
    (fp_text value " " (at 0 -1.27) (layer "B.SilkS"))
    (pad "P$1" smd circle (at 0 0) (size 1.27 1.27) (layers "B.Cu" "B.Paste" "B.Mask")
      (solder_mask_margin 0.1016))
  )
  (footprint "alexglow-footprints:pn2222a" (layer "B.Cu")
    (at 173 97.5 180)
    (attr through_hole)
    (fp_text reference " " (at 0 1.5) (layer "B.SilkS"))
    (fp_text value "PN2222A" (at 0 -1.5) (layer "B.Fab"))
    (pad "1" thru_hole circle (at -3 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 3 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "alexglow-footprints:pn2222a" (layer "B.Cu")
    (at 128.5 88 90)
    (attr through_hole)
    (fp_text reference " " (at 0 1.5 90) (layer "B.SilkS"))
    (fp_text value "PN2222A" (at 0 -1.5 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at -3 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 3 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "alexglow-footprints:pn2222a" (layer "B.Cu")
    (at 137.25 48.5)
    (attr through_hole)
    (fp_text reference " " (at 0 1.5) (layer "B.SilkS"))
    (fp_text value "PN2222A" (at 0 -1.5) (layer "B.Fab"))
    (pad "1" thru_hole circle (at -3 0) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 3 0) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (footprint "alexglow-footprints:pn2222a" (layer "B.Cu")
    (at 173 91 180)
    (attr through_hole)
    (fp_text reference " " (at 0 1.5) (layer "B.SilkS"))
    (fp_text value "PN2222A" (at 0 -1.5) (layer "B.Fab"))
    (pad "1" thru_hole circle (at -3 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "2" thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
    (pad "3" thru_hole circle (at 3 0 180) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask"))
  )
  (gr_circle (center 178 48.75) (end 179.5 48.75)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 178 100.5) (end 179.5 100.5)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 126 48.15) (end 126 100.4)
    (layer "Edge.Cuts"))
  (gr_line (start 126 100.4) (end 126 100.9)
    (layer "Edge.Cuts"))
  (gr_line (start 180.75 48.25) (end 180.75 100.5)
    (layer "Edge.Cuts"))
  (gr_line (start 180.75 100.5) (end 180.75 101)
    (layer "Edge.Cuts"))
  (gr_circle (center 128.7 48.65) (end 130.2 48.65)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 128.7 100.4) (end 130.2 100.4)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 178.5 46) (end 128.2 46)
    (layer "Edge.Cuts"))
  (gr_line (start 178.5 103.25) (end 128.25 103.25)
    (layer "Edge.Cuts"))
  (gr_line (start 126 47.5) (end 127.5 46)
    (layer "Edge.Cuts"))
  (gr_line (start 179.25 103.25) (end 180.75 101.75)
    (layer "Edge.Cuts"))
  (gr_line (start 180.75 48.25) (end 180.75 47.5)
    (layer "Edge.Cuts"))
  (gr_line (start 180.75 101.75) (end 180.75 101)
    (layer "Edge.Cuts"))
  (gr_line (start 126 100.9) (end 126 101.75)
    (layer "Edge.Cuts"))
  (gr_line (start 127.5 103.25) (end 128.25 103.25)
    (layer "Edge.Cuts"))
  (gr_line (start 180.75 47.5) (end 179.25 46)
    (layer "Edge.Cuts"))
  (gr_line (start 178.5 103.25) (end 179.25 103.25)
    (layer "Edge.Cuts"))
  (gr_line (start 126 48.15) (end 126 47.5)
    (layer "Edge.Cuts"))
  (gr_line (start 127.5 46) (end 128.2 46)
    (layer "Edge.Cuts"))
  (gr_line (start 179.25 46) (end 178.5 46)
    (layer "Edge.Cuts"))
  (gr_line (start 126 101.75) (end 127.5 103.25)
    (layer "Edge.Cuts"))
  (gr_text "“MITTLER ZWISCHEN HIRN UND HANDEN MUSS DAS HERZ SEIN!”" (at 154 100.7) (layer "B.SilkS"))
  (gr_text "v4\nalex glow\n@glowascii" (at 149.55 86) (layer "B.SilkS"))
  (gr_text "gnd" (at 177.5 84.282 90) (layer "F.SilkS"))
  (gr_text "5v" (at 174.94 83.901 90) (layer "F.SilkS"))
  (gr_text "USB" (at 165.5 48.6) (layer "F.SilkS"))
  (gr_text "Companion Bot core: designed for use with\nTeensy and Arduino Nano 33 BLE Sense.\n\nStick a mini breadboard in this box,\naligned with the breakout header rows.\nSolder M/F headers on (as labeled).\n\n^ Install board with USB jack UP ^\nConnect breadboard GPIO pins to\nbreakout header rows with M/M wires.\n\nSolder a stripped USB cable for power in.\nConnect “gnd” row to the controller’s GND.\n\n<—— Need to use one of these pins?    \nUse the pads on the back to connect\n    to an unused header over here. ——>\n\nUse transistors for switching motors,\nheaters, etc. Attach device to +/- pins.\n\nCheck the pins of your transistor!\nCheck the pins of your NeoPixels!\nHACK ON!" (at 149.5 72.5) (layer "F.SilkS"))
  (gr_text "gpio" (at 169.85 82.885 90) (layer "F.SilkS"))
  (gr_text "-" (at 176 96) (layer "F.SilkS"))
  (gr_text "M" (at 177.5 51) (layer "F.SilkS"))
  (gr_text "-" (at 130 91 270) (layer "F.SilkS"))
  (gr_text "D" (at 130 88 270) (layer "F.SilkS"))
  (gr_text "+" (at 130 85 270) (layer "F.SilkS"))
  (gr_text "-" (at 134.25 50 180) (layer "F.SilkS"))
  (gr_text "D" (at 137.25 50) (layer "F.SilkS"))
  (gr_text "+" (at 140.25 50 180) (layer "F.SilkS"))
  (gr_text "M" (at 172.5 51) (layer "F.SilkS"))
  (gr_text "F" (at 170 51) (layer "F.SilkS"))
  (gr_text "M" (at 175 51) (layer "F.SilkS"))
  (gr_text "05/2023" (at 138.75 94.75) (layer "F.SilkS"))
  (gr_text "+" (at 170 89.5) (layer "F.SilkS"))
  (gr_text "D" (at 173 89.5) (layer "F.SilkS"))
  (gr_text "-" (at 176 89.5) (layer "F.SilkS"))
  (gr_text "+" (at 170 96) (layer "F.SilkS"))
  (gr_text "<3, alex" (at 160.25 94.75) (layer "F.SilkS"))
  (gr_text "F" (at 129.25 51.25) (layer "F.SilkS"))
  (gr_text "D" (at 173 96) (layer "F.SilkS"))
  (gr_text "M3" (at 128.75 98) (layer "F.SilkS"))
)
