(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 114)
    (zones 0)
    (modules 17)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D1-Pad3)")
  (net 4 "Net-(D1-Pad4)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 "Net-(D4-Pad1)")
  (net 10 "Net-(D4-Pad2)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad3)")
  (net 13 "Net-(J1-Pad4)")
  (net 14 "Net-(J1-Pad5)")
  (net 15 "Net-(J1-Pad6)")
  (net 16 "Net-(J1-Pad7)")
  (net 17 "Net-(J1-Pad8)")
  (net 18 "Net-(J1-Pad9)")
  (net 19 "Net-(J1-Pad10)")
  (net 20 "Net-(J1-Pad11)")
  (net 21 "Net-(J1-Pad12)")
  (net 22 "Net-(J1-Pad13)")
  (net 23 "Net-(J1-Pad14)")
  (net 24 "Net-(J1-Pad15)")
  (net 25 "Net-(J1-Pad16)")
  (net 26 "Net-(J1-Pad17)")
  (net 27 "Net-(J1-Pad18)")
  (net 28 "Net-(J1-Pad19)")
  (net 29 "Net-(J1-Pad20)")
  (net 30 "Net-(J1-Pad23)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
  )
  (module LED_THT:LED_D5.0mm-4_RGB (layer F.Cu) (tedit 5F301843)
    (at 90.09 96.79 90)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins RGB RGBLED")
    (fp_text reference D1 (at 1.905 -3.96 90) (layer F.SilkS))
    (fp_text value LED_ABRG (at 1.905 3.96 90) (layer F.Fab))
    (fp_text user %R (at 1.905 -3.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 2.54 0 90) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 0 0 90) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 4 thru_hole oval (at 1.27 0 90) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5A1EC915)
    (at 152.5 78 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference SW6 (at 2.49 -3.02 90) (layer F.SilkS))
    (fp_text value SW_DPDT_x2 (at 2.11 3.14 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x12_P2.54mm_Vertical (layer F.Cu) (tedit 5F2EFFCA)
    (at 125 62.5 90)
    (descr "Through hole straight pin header, 2x12, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x12 2.54mm double row")
    (fp_text reference J1 (at -1.27 -2.77 90) (layer F.SilkS))
    (fp_text value Conn_02x12_Counter_Clockwise (at -1.27 30.71 90) (layer F.Fab) hide)
    (fp_text user %R (at -1.27 13.97 180) (layer F.Fab))
    (pad 24 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(D4-Pad2)"))
    (pad 23 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad23)"))
    (pad 22 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 21 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (pad 20 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad20)"))
    (pad 19 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5A1EC915)
    (at 119 78 90)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference SW5 (at 3.99 -2.99 90) (layer F.SilkS))
    (fp_text value SW_DPDT_x2 (at 2 3 90) (layer F.Fab))
    (fp_text user %R (at 3.99 -2.99 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad14)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 88.82 71.46 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -3.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 97 71.5 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -3.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 105 71.5 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -3.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 107.41 90.44 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.37) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 107.41 95.52 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.37) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 107.355001 100.6 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 -2.37) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.37) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 88.82 75.58 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 97 75.5 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 105 75.5 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 -2.37 90) (layer F.SilkS))
    (fp_text value 220 (at 5.08 2.37 90) (layer F.Fab) hide)
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5D160D14)
    (at 147.5 100 90)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW1 (at 6.08 -4.66 90) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 90) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5 90) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 2 thru_hole oval (at 12.5 5 90) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad11)"))
    (pad 1 thru_hole oval (at 12.5 0 90) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5D160D14)
    (at 123 87.5 270)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW2 (at 6.08 -4.66 90) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 90) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0 270) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 2 thru_hole oval (at 12.5 5 270) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)"))
    (pad 1 thru_hole oval (at 0 0 270) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 2 thru_hole oval (at 0 5 270) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5D160D14)
    (at 137.5 87.5 270)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW3 (at 6.08 -4.66 90) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 90) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 5 270) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)"))
    (pad 1 thru_hole oval (at 0 0 270) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 2 thru_hole oval (at 12.5 5 270) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad9)"))
    (pad 1 thru_hole oval (at 12.5 0 270) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH-12mm (layer F.Cu) (tedit 5D160D14)
    (at 132.08 82.55 90)
    (descr "SW PUSH 12mm https://www.e-switch.com/system/asset/product_line/data_sheet/143/TL1100.pdf")
    (tags "tact sw push 12mm")
    (fp_text reference SW4 (at 6.08 -4.66 90) (layer F.SilkS))
    (fp_text value SW_Push (at 6.62 9.93 90) (layer F.Fab))
    (fp_text user %R (at 6.35 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 12.5 0 90) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 2 thru_hole oval (at 12.5 5 90) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad10)"))
    (pad 1 thru_hole oval (at 0 0 90) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad12)"))
    (pad 2 thru_hole oval (at 0 5 90) (size 3.048 1.85) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad10)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 121 58) (end 121 55) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 115 60.5) (end 115 63.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 85.5 66.5) (end 85.5 63.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 85.5 102) (end 82.5 102) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 157 102) (end 157 105) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 157 58) (end 160 58) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 115 63.5) (end 85.5 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118 58) (end 118 60.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 82.5 55) (end 82.5 55) (layer Edge.Cuts) (width 0.1))
  (gr_text GPIO20 (at 122.5 78.5 90) (layer F.SilkS))
  (gr_text GPIO21 (at 155.5 79 90) (layer F.SilkS))
  (gr_text GPIO19 (at 142 81.5 90) (layer F.SilkS))
  (gr_text GPIO26 (at 146 103) (layer F.SilkS))
  (gr_text GPIO13 (at 131 103) (layer F.SilkS))
  (gr_text GPIO6 (at 116.5 103) (layer F.SilkS))
  (gr_text GPIO8 (at 86.5 77 90) (layer F.SilkS))
  (gr_text GPIO25 (at 94.5 77 90) (layer F.SilkS))
  (gr_text GPIO24 (at 102.5 77 90) (layer F.SilkS))
  (gr_text GPIO11 (at 107 103) (layer F.SilkS))
  (gr_text GPIO9 (at 106.5 98) (layer F.SilkS))
  (gr_text GPIO10 (at 107 93) (layer F.SilkS))
  (gr_text BLUE (at 98 103) (layer F.SilkS))
  (gr_text GREEN (at 98.5 98) (layer F.SilkS))
  (gr_text RED (at 97.5 93) (layer F.SilkS))
  (gr_text BLUE (at 102.5 84 90) (layer F.SilkS))
  (gr_text GREEN (at 94 83.5 90) (layer F.SilkS))
  (gr_text RED (at 86.5 84.5 90) (layer F.SilkS))
  (gr_line (start 160 58) (end 160 102) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121 55) (end 157 55) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 82.5 102) (end 82.5 66.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157 105) (end 85.5 105) (layer Edge.Cuts) (width 0.1))
  (zone (net 21) (net_name "Net-(J1-Pad12)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159 104) (xy 83.5 104) (xy 83.5 65.5) (xy 84.5 64.5) (xy 117 64.5)
        (xy 120.5 61.5) (xy 159 61.5)
      )
    )
  )
  (zone (net 21) (net_name "Net-(J1-Pad12)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159 104) (xy 83.5 104) (xy 83.5 65.5) (xy 85 64) (xy 117 64)
        (xy 121.5 56) (xy 159 56)
      )
    )
  )
)
