<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.8" y2="0" width="0" layer="20"/>
<wire x1="50.8" y1="0" x2="50.8" y2="41.91" width="0" layer="20"/>
<wire x1="50.8" y1="41.91" x2="0" y2="41.91" width="0" layer="20"/>
<wire x1="0" y1="41.91" x2="0" y2="0" width="0" layer="20"/>
<text>Arduino Mother Board v1.0</text>
<text>A. Suliman</text>
<hole x="2.8575" y="39.0525" drill="3.175"/>
<hole x="47.78375" y="2.8575" drill="3.175"/>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
</plain>
<libraries>
<library name="cederna">
<packages>
<package name="TP5000OR5001">
</package>
</packages>
</library>
<library name="bedsensorV5">
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="0603">
<description>&lt;b&gt;0603 package&lt;/b&gt;
Modified from stock (rcl) C0603 to permit placing on standard EAGLE layout grid; only modified keepout lines.</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="TRI-CON-SMD">
<description>&lt;b&gt;0402 SMD package&lt;/b&gt;&lt;p&gt;
Copied from stock (tested libraries) - only keepout zone has been modified to allow spacing on standard EAGLE grid.</description>
</package>
<package name="MXR9500MZ">
<description>&lt;b&gt;3D accelerometer through hole&lt;/b&gt;</description>
</package>
<package name="ARDUINO_PRO">
<description>&lt;b&gt;3D accelerometer through hole&lt;/b&gt;</description>
</package>
<package name="TACTILE_SPST-NO_ARDUINO">
<description>&lt;b&gt;TACTILE_SPST-NO&lt;/b&gt;</description>
</package>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
</packages>
</library>
<library name="Battery Holder">
<description>&lt;h3&gt; PCBLayout.com - Frequently Used &lt;i&gt;Battery Holder&lt;/i&gt;&lt;/h3&gt;

Visit us at &lt;a href="http://www.PCBLayout.com"&gt;PCBLayout.com&lt;/a&gt; for quick and hassle-free PCB Layout/Manufacturing ordering experience.
&lt;BR&gt;
&lt;BR&gt;
This library has been generated by our experienced pcb layout engineers using current IPC and/or industry standards. We &lt;b&gt;believe&lt;/b&gt; the content to be accurate, complete and current. But, this content is provided as a courtesy and &lt;u&gt;user assumes all risk and responsiblity of it's usage&lt;/u&gt;.
&lt;BR&gt;
&lt;BR&gt;
Feel free to contact us at &lt;a href="mailto:Support@PCBLayout.com"&gt;Support@PCBLayout.com&lt;/a&gt; if you have any questions/concerns regarding any of our content or services.</description>
<packages>
<package name="79573231">
</package>
</packages>
</library>
<library name="on-semiconductor">
<description>&lt;b&gt;ON Semiconductor&lt;/b&gt;&lt;p&gt;
&lt;a href="http://onsemi.com"&gt; Home page &lt;/a&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SC-74">
<description>&lt;b&gt;Small Outline Transistor; 6 leads&lt;/b&gt; SC-74 CASE 318F-05 ISSUE M&lt;p&gt;
Source: U6 OnSemi Inductive Load Driver MDC3105-D.PDF</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="3.3V" library="cederna" package="TP5000OR5001" value="TPTP5001">
<attribute name="NAME"/>
</element>
<element name="D" library="bedsensorV5" package="1206" value="A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="bedsensorV5" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="bedsensorV5" package="0603" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="bedsensorV5" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="bedsensorV5" package="SOT223" value="VREG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="bedsensorV5" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DG" library="cederna" package="TP5000OR5001" value="TPTP5001">
<attribute name="NAME"/>
</element>
<element name="DG1" library="cederna" package="TP5000OR5001" value="TPTP5001">
<attribute name="NAME"/>
</element>
<element name="BT1" library="Battery Holder" package="79573231" value="79573231">
<attribute name="CREATED_BY" value="PCBLayout.com"/>
<attribute name="DIGIKEY_PART_NO" value="732-12329-ND"/>
<attribute name="MANUFACTURER" value="Wurth Electronics Inc."/>
<attribute name="MPN" value="79573231"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="on-semiconductor" package="SC-74" value="MDC3105DMT1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MDC3105DMT1G"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="04R7836"/>
</element>
<element name="J2" library="bedsensorV5" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT/REG" library="bedsensorV5" package="TRI-CON-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PW1" library="bedsensorV5" package="TRI-CON-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PW2" library="bedsensorV5" package="TRI-CON-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="on-semiconductor" package="SC-74" value="MDC3105DMT1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MDC3105DMT1G"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="04R7836"/>
</element>
<element name="J1" library="bedsensorV5" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PW3" library="bedsensorV5" package="TRI-CON-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PW4" library="bedsensorV5" package="TRI-CON-SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ACCEL" library="bedsensorV5" package="MXR9500MZ" value="MXR9500DEV">
<attribute name="ACCELEROMETER" value="MXR9500MZ"/>
<attribute name="NAME"/>
</element>
<element name="PWM1" library="cederna" package="TP5000OR5001" value="TPTP5001"/>
<element name="PWM3" library="cederna" package="TP5000OR5001" value="TPTP5001">
<attribute name="NAME"/>
</element>
<element name="PWM4" library="cederna" package="TP5000OR5001" value="TPTP5001">
<attribute name="NAME"/>
</element>
<element name="PWM2" library="cederna" package="TP5000OR5001" value="TPTP5001">
<attribute name="NAME"/>
</element>
<element name="B1" library="bedsensorV5" package="ARDUINO_PRO" value="ARDUINO_PRO_MINI">
<attribute name="NAME"/>
</element>
<element name="BAL" library="bedsensorV5" package="TACTILE_SPST-NO_ARDUINO" value="TACTILE_SPST-NO-ARD">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="3.3VD">
<contactref element="3.3V" pad="P$1"/>
<contactref element="BAT/REG" pad="3"/>
<contactref element="PW1" pad="1"/>
<contactref element="PW2" pad="2"/>
<contactref element="PW3" pad="1"/>
<contactref element="PW4" pad="2"/>
<contactref element="ACCEL" pad="1-1"/>
</signal>
<signal name="DGND">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="DG" pad="P$1"/>
<contactref element="DG1" pad="P$1"/>
<contactref element="BT1" pad="N"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="ACCEL" pad="1-4"/>
<contactref element="ACCEL" pad="2-4"/>
<contactref element="B1" pad="7-9"/>
<contactref element="B1" pad="6-2"/>
<contactref element="BAL" pad="P$2"/>
<contactref element="BAL" pad="P$1"/>
</signal>
<signal name="N$35">
<contactref element="D" pad="C"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SW1">
<contactref element="B1" pad="7-6"/>
<contactref element="BAL" pad="P$4"/>
<contactref element="BAL" pad="P$3"/>
</signal>
<signal name="GND1">
</signal>
<signal name="PWR_D">
<contactref element="C1" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="J3" pad="2"/>
<contactref element="B1" pad="6-1"/>
</signal>
<signal name="N$14">
<contactref element="U3" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="BAT/REG" pad="1"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="1-TDO">
</signal>
<signal name="19">
</signal>
<signal name="BATT">
<contactref element="BT1" pad="P2"/>
<contactref element="BT1" pad="P1"/>
<contactref element="BAT/REG" pad="2"/>
<contactref element="B1" pad="6-4"/>
</signal>
<signal name="N$12">
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="PW1" pad="3"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="PWM3">
<contactref element="PW3" pad="2"/>
<contactref element="U2" pad="5"/>
<contactref element="PWM3" pad="P$1"/>
<contactref element="B1" pad="7-4"/>
</signal>
<signal name="PWM4">
<contactref element="PW4" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="PWM4" pad="P$1"/>
<contactref element="B1" pad="7-1"/>
</signal>
<signal name="PWM2">
<contactref element="U1" pad="2"/>
<contactref element="PW2" pad="1"/>
<contactref element="PWM2" pad="P$1"/>
<contactref element="B1" pad="7-5"/>
</signal>
<signal name="PWM1">
<contactref element="U1" pad="5"/>
<contactref element="PW1" pad="2"/>
<contactref element="PWM1" pad="P$1"/>
<contactref element="B1" pad="7-7"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="3"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="PW3" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="XOUT">
<contactref element="ACCEL" pad="2-1"/>
<contactref element="B1" pad="6-8"/>
</signal>
<signal name="YOUT">
<contactref element="ACCEL" pad="2-2"/>
<contactref element="B1" pad="6-7"/>
</signal>
<signal name="ZOUT">
<contactref element="ACCEL" pad="2-3"/>
<contactref element="B1" pad="6-6"/>
</signal>
<signal name="DI2">
<contactref element="ACCEL" pad="1-2"/>
<contactref element="B1" pad="6-12"/>
</signal>
<signal name="DI1">
<contactref element="ACCEL" pad="1-3"/>
<contactref element="B1" pad="6-11"/>
</signal>
<signal name="N$6">
<contactref element="PW4" pad="3"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="PW2" pad="3"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="B1" pad="7-8"/>
<contactref element="D" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
