(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 8)
    (no_connects 0)
    (area 134.569999 95.199999 167.690001 116.890001)
    (thickness 1.6)
    (drawings 9)
    (tracks 53)
    (zones 0)
    (modules 6)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 E-)
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P2-Pad1)")
  (net 5 S-)
  (net 6 E+)
  (net 7 "Net-(P3-Pad3)")
  (net 8 S+)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class thic ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net E+)
    (add_net E-)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad3)")
    (add_net S+)
    (add_net S-)
  )
  (module Connectors_Molex:Molex_PicoBlade_53261-0371_03x1.25mm_Angled (layer F.Cu) (tedit 5B07AE9D)
    (at 161.29 111.76)
    (descr "Molex PicoBlade, single row, side entry type, surface mount, PN:53261-0371")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference P1 (at 0 2.54) (layer F.SilkS))
    (fp_text value "" (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 -1.45) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 0 -1.45) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 E-))
    (pad 3 smd rect (at 1.25 -1.45) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad "" smd rect (at -3.75 1.45) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.75 1.45) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53261-0371_03x1.25mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53261-0371_03x1.25mm_Angled (layer F.Cu) (tedit 5B07AEA3)
    (at 140.97 111.76)
    (descr "Molex PicoBlade, single row, side entry type, surface mount, PN:53261-0371")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference P2 (at 0 2.54) (layer F.SilkS))
    (fp_text value "" (at 0 5) (layer F.Fab))
    (fp_text user %R (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 -1.45) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P2-Pad1)"))
    (pad 2 smd rect (at 0 -1.45) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 S-))
    (pad 3 smd rect (at 1.25 -1.45) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad "" smd rect (at -3.75 1.45) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.75 1.45) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53261-0371_03x1.25mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53261-0371_03x1.25mm_Angled (layer F.Cu) (tedit 5B07AE80)
    (at 139.7 101.6 270)
    (descr "Molex PicoBlade, single row, side entry type, surface mount, PN:53261-0371")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference P3 (at 0 2.54 360) (layer F.SilkS))
    (fp_text value "" (at 0 5 270) (layer F.Fab))
    (fp_text user %R (at 0 2.5 360) (layer F.Fab))
    (pad 1 smd rect (at -1.25 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P2-Pad1)"))
    (pad 2 smd rect (at 0 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 E+))
    (pad 3 smd rect (at 1.25 -1.45 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P3-Pad3)"))
    (pad "" smd rect (at -3.75 1.45 270) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.75 1.45 270) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53261-0371_03x1.25mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53261-0371_03x1.25mm_Angled (layer F.Cu) (tedit 5B07AE8F)
    (at 162.56 101.6 90)
    (descr "Molex PicoBlade, single row, side entry type, surface mount, PN:53261-0371")
    (tags "connector molex picoblade smt")
    (attr smd)
    (fp_text reference P4 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value "" (at 0 5 90) (layer F.Fab))
    (fp_text user %R (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 0 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 S+))
    (pad 3 smd rect (at 1.25 -1.45 90) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P3-Pad3)"))
    (pad "" smd rect (at -3.75 1.45 90) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.75 1.45 90) (size 2.2 3.1) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53261-0371_03x1.25mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_FFC-FPC:TE_84952-4_1x04-1MP_P1.0mm_Horizontal (layer F.Cu) (tedit 5B07AE6B)
    (at 151.13 104.14 180)
    (descr "TE FPC connector, 04 bottom-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84952&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84952-4")
    (tags "te fpc 84952")
    (attr smd)
    (fp_text reference P5 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value "" (at 0 7.7 180) (layer F.Fab))
    (fp_text user %R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.8 180) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 6 E+))
    (pad 2 smd rect (at -0.5 -1.8 180) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 E-))
    (pad 3 smd rect (at 0.5 -1.8 180) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 5 S-))
    (pad 4 smd rect (at 1.5 -1.8 180) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 8 S+))
    (pad MP smd rect (at -4.49 1 180) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad MP smd rect (at 4.49 1 180) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/TE_84952-4_1x04-1MP_P1.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:cutelab_1cm (layer F.Cu) (tedit 5B07AD3E)
    (at 151.13 111.76)
    (descr "Imported from cutelab_inverti_path.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference svg2mod (at 0 -7.477367) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 7.477367) (layer F.SilkS) hide)
  )
  (gr_text "IKA pad\nLoad Cell Full Bridge 1.0" (at 151.13 97.155) (layer F.SilkS))
  (gr_arc (start 137.16 97.79) (end 134.62 97.79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 137.16 114.3) (end 137.16 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 165.1 114.3) (end 167.64 114.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 165.1 97.79) (end 165.1 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.62 114.3) (end 134.62 97.79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.1 116.84) (end 137.16 116.84) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.64 97.79) (end 167.64 114.3) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 95.25) (end 165.1 95.25) (angle 90) (layer Edge.Cuts) (width 0.1))
)
