(kicad_pcb (version 4) (host pcbnew 4.0.3-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 129.180074 89.315469 150.847005 110.684532)
    (thickness 1.6)
    (drawings 1)
    (tracks 4)
    (zones 0)
    (modules 8)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P2-Pad1)")
  (net 3 "Net-(P3-Pad3)")
  (net 4 "Net-(P3-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad4)")
  )
  (module TO18Breakout:AYB_Cu-INV (layer F.Cu) (tedit 0)
    (at 140 100)
    (fp_text reference G*** (at 0 0) (layer F.Cu) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Cu) hide)
  )
  (module TO18Breakout:LDPAD (layer B.Cu) (tedit 5B596CF8)
    (at 136 100)
    (fp_text reference P1 (at 0 2.032) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.556) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )
  (module TO18Breakout:LDPAD (layer B.Cu) (tedit 5B596CF4)
    (at 140 104)
    (fp_text reference P2 (at 0 2.032) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.556) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(P2-Pad1)"))
  )
  (module TO18Breakout:TO18SOCKET (layer F.Cu) (tedit 5B596CAE)
    (at 140 100)
    (fp_text reference P3 (at 0 -4.064) (layer F.SilkS) hide)
    (fp_text value TO18SOCKET (at 0 -5.588) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1 0) (size 1 1) (drill 0.55) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)") (solder_mask_margin 0.1))
    (pad 2 thru_hole circle (at 0 1) (size 1 1) (drill 0.55) (layers *.Cu *.Mask)
      (net 2 "Net-(P2-Pad1)") (solder_mask_margin 0.1))
    (pad 3 thru_hole circle (at 1 0) (size 1 1) (drill 0.55) (layers *.Cu *.Mask)
      (net 3 "Net-(P3-Pad3)") (solder_mask_margin 0.1))
    (pad 4 thru_hole circle (at 0 -1) (size 1 1) (drill 0.55) (layers *.Cu *.Mask)
      (net 4 "Net-(P3-Pad4)") (solder_mask_margin 0.1))
  )
  (module TO18Breakout:LDPAD (layer B.Cu) (tedit 5B596CEF)
    (at 144 100)
    (fp_text reference P4 (at 0 2.032) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.556) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(P3-Pad3)"))
  )
  (module TO18Breakout:LDPAD (layer B.Cu) (tedit 5B596F40)
    (at 140 96)
    (fp_text reference P5 (at 0 2.032) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.556) (layer B.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 2 2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(P3-Pad4)"))
  )
  (module TO18Breakout:AYB_Mask (layer F.Cu) (tedit 0)
    (at 140 100)
    (fp_text reference G*** (at 0 0) (layer F.Mask) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Mask) hide)
  )
  (module TO18Breakout:AYB_Silk (layer B.Cu) (tedit 0)
    (at 140 100 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_circle (center 140 100) (end 150.25 100) (layer Edge.Cuts) (width 0.15))
)
