(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0509)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "VCC")
  (net 4 "/LED1")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "/LED0")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "/LED2")
  (net 9 "Net-(D3-Pad2)")
  (net 10 "/LED3")
  (net 11 "Net-(D4-Pad2)")
  (net 12 "/LED4")
  (net 13 "Net-(D5-Pad2)")
  (net 14 "/LED5")
  (net 15 "Net-(D6-Pad2)")
  (net 16 "/LED6")
  (net 17 "Net-(D7-Pad2)")
  (net 18 "/LED7")
  (net 19 "Net-(D8-Pad2)")
  (net 20 "/LED8")
  (net 21 "Net-(D9-Pad2)")
  (net 22 "/LED9")
  (net 23 "Net-(D10-Pad2)")
  (net 24 "/LED10")
  (net 25 "Net-(D11-Pad2)")
  (net 26 "/LED11")
  (net 27 "Net-(D12-Pad2)")
  (net 28 "/LED12")
  (net 29 "Net-(D13-Pad2)")
  (net 30 "/LED13")
  (net 31 "Net-(D14-Pad2)")
  (net 32 "/LED14")
  (net 33 "Net-(D15-Pad2)")
  (net 34 "/LED15")
  (net 35 "Net-(D16-Pad2)")
  (net 36 "/SDI")
  (net 37 "/SCK")
  (net 38 "/SDO")
  (net 39 "/RESET")
  (net 40 "unconnected-(J2-Pad2)")
  (net 41 "unconnected-(J2-Pad3)")
  (net 42 "unconnected-(J2-Pad4)")
  (net 43 "unconnected-(J2-Pad6)")
  (net 44 "/ADC0")
  (net 45 "/ADC1")
  (net 46 "unconnected-(U1-Pad14)")
  (net 47 "/RX")
  (net 48 "/TX")
  (net 49 "Net-(U1-Pad7)")
  (net 50 "unconnected-(U1-Pad8)")
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 113.152901 80.069027 105)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED6")
    (attr smd)
    (fp_text reference "D7" (at -1.484216 1.84171 105) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 105) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 105) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 105) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 16 "/LED6") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 105) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 17 "Net-(D7-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-64037CBD" (layer "F.Cu")
    (tedit 64037CBD)
    (at 127.254 108.458 -90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPCIsICJDYXBSaWdodENob2ljZSI6ICIvIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkb2thT25lIiwgIkhlaWdodEN0cmwiOiAiMC43IiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIjEiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiOCIsICJQYWRkaW5nTGVmdEN0cmwiOiAiNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjUiLCAiUGFkZGluZ1RvcEN0cmwiOiAiOCIsICJXaWR0aEN0cmwiOiAiIn0=")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-64037CBD" (at 0 -3.827357 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 3.827357 90) (layer "F.SilkS") hide)
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 128.819735 80.069026 75)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED9")
    (attr smd)
    (fp_text reference "D10" (at -1.276763 1.876661 75) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 75) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 75) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 22 "/LED9") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 75) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 23 "Net-(D10-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91.023655 88.234305 -35)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED2")
    (attr smd)
    (fp_text reference "R4" (at 2.793999 -1.523999 145) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.777999 145) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 145) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 325) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 325) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 9 "Net-(D3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-64037C19" (layer "F.Cu")
    (tedit 64037C19)
    (at 122.428 95.504)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiIiwgIkNhcFJpZ2h0Q2hvaWNlIjogIiIsICJGb250Q29tYm9Cb3giOiAiRnJlZG9rYU9uZSIsICJIZWlnaHRDdHJsIjogIjEiLCAiTGF5ZXJDb21ib0JveCI6ICJGLlNpbGtTIiwgIk11bHRpTGluZVRleHQiOiAiQVRNZWdhNDhcbm1pY3JvY29udHJvbGxlciIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICI4IiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICI1IiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiNSIsICJQYWRkaW5nVG9wQ3RybCI6ICI4IiwgIldpZHRoQ3RybCI6ICIifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-64037C19" (at 0 -4.644079) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.644079) (layer "F.SilkS") hide)
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 144.213243 98.624621 -65)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED14")
    (attr exclude_from_pos_files)
    (fp_text reference "TP15" (at 2.032 0.762001 25) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.050001 115) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.999999 115) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 295) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 32 "/LED14") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 87.63 110.744 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 2.54 -2.54 90) (layer "F.SilkS"))
    (fp_text value "AVR-ISP-6" (at 1.27 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/SDI") (pinfunction "MISO") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "VCC") (pinfunction "VCC") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "/SCK") (pinfunction "SCK") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/SDO") (pinfunction "MOSI") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/RESET") (pinfunction "~{RST}") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-64037C58" (layer "F.Cu")
    (tedit 64037C58)
    (at 88.392 104.648)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiIiwgIkNhcFJpZ2h0Q2hvaWNlIjogIiIsICJGb250Q29tYm9Cb3giOiAiRnJlZG9rYU9uZSIsICJIZWlnaHRDdHJsIjogIjEiLCAiTGF5ZXJDb21ib0JveCI6ICJGLlNpbGtTIiwgIk11bHRpTGluZVRleHQiOiAiQVZSSVNQXG5oZWFkZXIiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiOCIsICJQYWRkaW5nTGVmdEN0cmwiOiAiNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjUiLCAiUGFkZGluZ1RvcEN0cmwiOiAiOCIsICJXaWR0aEN0cmwiOiAiIn0=")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-64037C58" (at 0 -4.641698) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.641698) (layer "F.SilkS") hide)
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 142.387612 87.902444 45)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED12")
    (attr smd)
    (fp_text reference "D13" (at -0.989361 1.858237 45) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 45) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 28 "/LED12") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 45) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 29 "Net-(D13-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 123.624173 79.152909 85)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED8")
    (attr smd)
    (fp_text reference "D9" (at -1.220637 1.710722 85) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 85) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 85) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 20 "/LED8") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 85) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 21 "Net-(D9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.362395 88.234305 -145)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED13")
    (attr smd)
    (fp_text reference "R15" (at 2.794 -1.524 35) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524001 -1.778 35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 35) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 215) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 215) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 31 "Net-(D14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 114.619022 84.824609 15)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED6")
    (attr exclude_from_pos_files)
    (fp_text reference "TP7" (at 2.031999 0.762 105) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.050001 15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.999999 15) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 15) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 16 "/LED6") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 123.406781 84.05578 -5)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED8")
    (attr exclude_from_pos_files)
    (fp_text reference "TP9" (at 2.032 0.762001 85) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at -0.000001 2.05 175) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.000001 -2 175) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 355) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 20 "/LED8") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.150283 83.316382 -45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED3")
    (attr smd)
    (fp_text reference "R5" (at 2.794 -1.523999 135) (layer "F.SilkS"))
    (fp_text value "R" (at 1.523999 -1.777999 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 11 "Net-(D4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.627995 75.97981 -65)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED5")
    (attr smd)
    (fp_text reference "R7" (at 2.794 -1.524 115) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.777999 115) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 115) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 295) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 295) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 15 "Net-(D6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-6403760C" (layer "F.Cu")
    (tedit 6403760C)
    (at 105.41 104.394 90)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiIiwgIkNhcFJpZ2h0Q2hvaWNlIjogIiIsICJGb250Q29tYm9Cb3giOiAiRnJlZG9rYU9uZSIsICJIZWlnaHRDdHJsIjogIjEuMyIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJWQ0NcbkFuYWxvZyAwXG5BbmFsb2cgMVxuR05EIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjgiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjUiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICI1IiwgIlBhZGRpbmdUb3BDdHJsIjogIjgiLCAiV2lkdGhDdHJsIjogIiJ9")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-6403760C" (at 0 -7.690993 90) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 7.690993 90) (layer "F.SilkS") hide)
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 96.193862 91.943874 145)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED2")
    (attr smd)
    (fp_text reference "D3" (at -1.143222 2.035763 145) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 145) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 145) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 145) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 8 "/LED2") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 145) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 9 "Net-(D3-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 96.65851 102.785121 75)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED1")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 2.032 0.762 165) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05 75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 75) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 75) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 4 "/LED1") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.235769 83.316383 -135)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED12")
    (attr smd)
    (fp_text reference "R14" (at 2.794 -1.523999 45) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.778 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 225) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 225) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 29 "Net-(D13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 103.232513 91.398612 45)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED3")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at 2.031999 0.762 135) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 45) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 45) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 10 "/LED3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.572341 93.794095 -155)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED14")
    (attr smd)
    (fp_text reference "R16" (at 2.794001 -1.524 25) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524001 -1.778 25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 25) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 205) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 205) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 33 "Net-(D15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.81371 93.794094 -25)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED0")
    (attr smd)
    (fp_text reference "R3" (at 2.793999 -1.524 155) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.778 155) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 155) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 335) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 335) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 7 "Net-(D2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 156.768074 99.826819 -165)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED15")
    (attr smd)
    (fp_text reference "R17" (at 2.794 -1.524 15) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524001 -1.778001 15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 15) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 195) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 195) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 35 "Net-(D16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_Micro-B_Amphenol_10118194_Horizontal" (layer "F.Cu")
    (tedit 5F2142B6)
    (at 155.194 109.728)
    (descr "USB Micro-B receptacle, horizontal, SMD, 10118194, https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/10118194.pdf")
    (tags "USB Micro B horizontal SMD")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 0 -3.5) (layer "F.SilkS") hide)
    (fp_text value "USB_B_Micro" (at 0 4.75) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 0 2.75) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 -0.05) (layer "F.Fab"))
    (pad "" smd oval (at -3.5 1.3) (size 0.89 1.55) (layers "F.Paste"))
    (pad "" smd oval (at 3.5 1.3) (size 0.89 1.55) (layers "F.Paste"))
    (pad "" smd oval (at 2.5 -1.4) (size 1.25 0.95) (layers "F.Paste"))
    (pad "" smd oval (at -2.5 -1.4) (size 1.25 0.95) (layers "F.Paste"))
    (pad "1" smd rect (at -1.3 -1.4) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VCC") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at -0.65 -1.4) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(J2-Pad2)") (pinfunction "D-") (pintype "bidirectional+no_connect"))
    (pad "3" smd rect (at 0 -1.4) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "unconnected-(J2-Pad3)") (pinfunction "D+") (pintype "bidirectional+no_connect"))
    (pad "4" smd rect (at 0.65 -1.4) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "unconnected-(J2-Pad4)") (pinfunction "ID") (pintype "passive+no_connect"))
    (pad "5" smd rect (at 1.3 -1.4) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "6" smd rect (at -1 1.3) (size 1.5 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(J2-Pad6)") (pinfunction "Shield") (pintype "passive+no_connect"))
    (pad "6" smd rect (at 2.9 1.3) (size 1.2 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(J2-Pad6)") (pinfunction "Shield") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at -3.5 1.3) (size 0.89 1.55) (drill oval 0.5 1.15) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J2-Pad6)") (pinfunction "Shield") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 3.5 1.3) (size 0.89 1.55) (drill oval 0.5 1.15) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J2-Pad6)") (pinfunction "Shield") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 2.5 -1.4) (size 1.25 0.95) (drill oval 0.85 0.55) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J2-Pad6)") (pinfunction "Shield") (pintype "passive+no_connect"))
    (pad "6" smd rect (at -2.9 1.3) (size 1.2 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(J2-Pad6)") (pinfunction "Shield") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at -2.5 -1.4) (size 1.25 0.95) (drill oval 0.85 0.55) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J2-Pad6)") (pinfunction "Shield") (pintype "passive+no_connect"))
    (pad "6" smd rect (at 1 1.3) (size 1.5 1.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(J2-Pad6)") (pinfunction "Shield") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_Micro-B_Amphenol_10118194_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 138.346182 84.511282 55)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED11")
    (attr smd)
    (fp_text reference "D12" (at -1.237304 1.898923 55) (layer "F.SilkS"))
    (fp_text value "LED" (at -0.000001 1.649999 55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 55) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 55) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 26 "/LED11") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 55) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 27 "Net-(D12-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 100.386564 94.790284 55)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED2")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 2.032 0.761999 145) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at -0.000001 2.049999 55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.000001 -2.000001 55) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 55) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 8 "/LED2") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 135.128 102.87 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 1.778 90) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 131.572 102.87 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 3 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 141.999488 94.790284 -55)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED13")
    (attr exclude_from_pos_files)
    (fp_text reference "TP14" (at 2.032 0.762001 35) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.050001 125) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.999999 125) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 305) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 30 "/LED13") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 118.97927 84.05578 5)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED7")
    (attr exclude_from_pos_files)
    (fp_text reference "TP8" (at 2.031999 0.762 95) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05 5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.000001 -2 5) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 5) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 18 "/LED7") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 112.776 101.854 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 150.221028 101.47032 15)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED15")
    (attr smd)
    (fp_text reference "D16" (at -1.503613 1.86134 15) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 15) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 15) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 34 "/LED15") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 15) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 35 "Net-(D16-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 118.348462 79.152909 95)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED7")
    (attr smd)
    (fp_text reference "D8" (at -1.285318 1.942909 95) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 95) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 95) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 18 "/LED7") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 95) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 19 "Net-(D8-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 101.6 110.744 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/ADC0") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/ADC1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 139.153538 91.398613 -45)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED12")
    (attr exclude_from_pos_files)
    (fp_text reference "TP13" (at 2.032 0.762001 45) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.050001 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.999999 135) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 315) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 28 "/LED12") (pinfunction "1") (pintype "passive"))
  )
  (footprint "kibuzzard-641A1732" (layer "F.Cu")
    (tedit 641A1732)
    (at 145.0086 109.5248)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPCIsICJDYXBSaWdodENob2ljZSI6ICJdIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkb2thT25lIiwgIkhlaWdodEN0cmwiOiAiMS4yIiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIk1vZGUiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiOCIsICJQYWRkaW5nTGVmdEN0cmwiOiAiNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjUiLCAiUGFkZGluZ1RvcEN0cmwiOiAiOCIsICJXaWR0aEN0cmwiOiAiIn0=")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-641A1732" (at 0 -4.431665) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.431665) (layer "F.SilkS") hide)
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.068206 79.189756 -55)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED4")
    (attr smd)
    (fp_text reference "R6" (at 2.794 -1.524 125) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.777999 125) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 125) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 305) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 305) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 13 "Net-(D5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 145.778773 91.943873 35)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED13")
    (attr smd)
    (fp_text reference "D14" (at -0.945698 1.823467 35) (layer "F.SilkS"))
    (fp_text value "LED" (at -0.000001 1.65 35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 35) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 35) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 30 "/LED13") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 35) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 31 "Net-(D14-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 131.927529 86.338908 -25)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED10")
    (attr exclude_from_pos_files)
    (fp_text reference "TP11" (at 2.032 0.762 65) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05 155) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.999999 155) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 335) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 24 "/LED10") (pinfunction "1") (pintype "passive"))
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 108.195353 81.873426 115)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED5")
    (attr smd)
    (fp_text reference "D6" (at -1.690289 2.023926 115) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 115) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 115) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 115) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 14 "/LED5") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 115) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 15 "Net-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.98308 72.669274 -85)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED7")
    (attr smd)
    (fp_text reference "R9" (at 2.794 -1.523999 95) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.778 95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 95) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 275) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 275) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 19 "Net-(D8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 127.76703 84.824609 -15)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED9")
    (attr exclude_from_pos_files)
    (fp_text reference "TP10" (at 2.032 0.762 75) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05 165) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 165) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 345) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 22 "/LED9") (pinfunction "1") (pintype "passive"))
  )
  (footprint "kibuzzard-64037C81" (layer "F.Cu")
    (tedit 64037C81)
    (at 155.2702 105.2576)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiIiwgIkNhcFJpZ2h0Q2hvaWNlIjogIiIsICJGb250Q29tYm9Cb3giOiAiRnJlZG9rYU9uZSIsICJIZWlnaHRDdHJsIjogIjAuOSIsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTXVsdGlMaW5lVGV4dCI6ICJVU0ItQiBtaWNyb1xuKFBvd2VyIE9ubHkpIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogIjgiLCAiUGFkZGluZ0xlZnRDdHJsIjogIjUiLCAiUGFkZGluZ1JpZ2h0Q3RybCI6ICI1IiwgIlBhZGRpbmdUb3BDdHJsIjogIjgiLCAiV2lkdGhDdHJsIjogIiJ9")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-64037C81" (at 0 -4.659282) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 4.659282) (layer "F.SilkS") hide)
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.402971 72.669274 -95)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED8")
    (attr smd)
    (fp_text reference "R10" (at 2.794001 -1.524 85) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.778 85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 85) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 265) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 265) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 21 "Net-(D9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 98.172808 98.624622 65)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED0")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 2.031999 0.761999 155) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.049999 65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 65) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 6 "/LED0") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136.758056 75.979809 -115)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED10")
    (attr smd)
    (fp_text reference "R12" (at 2.794 -1.524 65) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524001 -1.778 65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 65) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 245) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 245) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 25 "Net-(D11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T-SH_NO_CK_KMR2xxG" (layer "F.Cu")
    (tedit 5D8D2A01)
    (at 137.922 110.081 180)
    (descr "CK components KMR2 tactile switch with ground pin http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at 4.826 0.254) (layer "F.SilkS") hide)
    (fp_text value "SW_Push" (at 0 2.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.45) (layer "F.Fab"))
    (pad "1" smd rect (at -2.05 -0.8 180) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 2.05 -0.8 180) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.05 0.8 180) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(U1-Pad7)") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 0.8 180) (size 0.9 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(U1-Pad7)") (pinfunction "2") (pintype "passive"))
    (pad "SH" smd rect (at 0 -1.425 180) (size 1.7 0.55) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T-SH_NO_CK_KMR2xxG.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 103.626452 84.511282 125)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED4")
    (attr smd)
    (fp_text reference "D5" (at -1.517995 2.044629 125) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 125) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 125) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 125) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 12 "/LED4") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 125) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 13 "Net-(D5-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.317845 79.189755 -125)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED11")
    (attr smd)
    (fp_text reference "R13" (at 2.794 -1.524 55) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524001 -1.777999 55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 55) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 235) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 235) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 27 "Net-(D12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm" (layer "F.Cu")
    (tedit 5A02F146)
    (at 122.130339 103.754561 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -6.05) (layer "F.SilkS"))
    (fp_text value "ATmega48PB-A" (at 0 6.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.25 -2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/LED15") (pinfunction "PD3") (pintype "bidirectional"))
    (pad "2" smd rect (at -4.25 -2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/LED14") (pinfunction "PD4") (pintype "bidirectional"))
    (pad "3" smd rect (at -4.25 -1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/LED13") (pinfunction "PE0") (pintype "bidirectional"))
    (pad "4" smd rect (at -4.25 -0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd rect (at -4.25 0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd rect (at -4.25 1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/LED12") (pinfunction "PE1") (pintype "bidirectional"))
    (pad "7" smd rect (at -4.25 2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(U1-Pad7)") (pinfunction "XTAL1/PB6") (pintype "bidirectional"))
    (pad "8" smd rect (at -4.25 2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "unconnected-(U1-Pad8)") (pinfunction "XTAL2/PB7") (pintype "bidirectional+no_connect"))
    (pad "9" smd rect (at -2.8 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/LED11") (pinfunction "PD5") (pintype "bidirectional"))
    (pad "10" smd rect (at -2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "/LED10") (pinfunction "PD6") (pintype "bidirectional"))
    (pad "11" smd rect (at -1.2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/LED9") (pinfunction "PD7") (pintype "bidirectional"))
    (pad "12" smd rect (at -0.4 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/LED8") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "13" smd rect (at 0.4 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/LED7") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd rect (at 1.2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "unconnected-(U1-Pad14)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "15" smd rect (at 2 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "/SDO") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "16" smd rect (at 2.8 4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/SDI") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "17" smd rect (at 4.25 2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/SCK") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "18" smd rect (at 4.25 2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "VCC") (pinfunction "AVCC") (pintype "power_in"))
    (pad "19" smd rect (at 4.25 1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/LED6") (pinfunction "PE2") (pintype "bidirectional"))
    (pad "20" smd rect (at 4.25 0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(C1-Pad2)") (pinfunction "AREF") (pintype "passive"))
    (pad "21" smd rect (at 4.25 -0.4 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "22" smd rect (at 4.25 -1.2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/LED5") (pinfunction "PE3") (pintype "bidirectional"))
    (pad "23" smd rect (at 4.25 -2 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/ADC0") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "24" smd rect (at 4.25 -2.8 180) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/ADC1") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "25" smd rect (at 2.8 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/LED4") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "26" smd rect (at 2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/LED3") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "27" smd rect (at 1.2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/LED2") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "28" smd rect (at 0.4 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/LED0") (pinfunction "PC5") (pintype "bidirectional"))
    (pad "29" smd rect (at -0.4 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/RESET") (pinfunction "~{RESET}/PC6") (pintype "bidirectional"))
    (pad "30" smd rect (at -1.2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/RX") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "31" smd rect (at -2 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/TX") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "32" smd rect (at -2.8 -4.25 270) (size 1.6 0.55) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/LED1") (pinfunction "PD2") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.725332 73.784077 -105)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED9")
    (attr smd)
    (fp_text reference "R11" (at 2.794 -1.524 75) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.778 75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 75) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 255) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 255) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 23 "Net-(D10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 93.556006 96.512774 155)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED0")
    (attr smd)
    (fp_text reference "D2" (at -1.231811 1.96772 155) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 155) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 155) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 155) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 6 "/LED0") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 155) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 7 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 148.416629 96.512774 25)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED14")
    (attr smd)
    (fp_text reference "D15" (at -0.934889 1.814091 25) (layer "F.SilkS"))
    (fp_text value "LED" (at -0.000001 1.65 25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 25) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 25) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 32 "/LED14") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 25) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 33 "Net-(D15-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 131.572 107.95)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "SMT_Soldering_class.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "4.8K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 39 "/RESET") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 91.751607 101.47032 165)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED1")
    (attr smd)
    (fp_text reference "D1" (at -1.235155 2.037425 165) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 165) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 165) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 165) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 4 "/LED1") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 165) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 5 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 135.761867 88.552663 -35)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED11")
    (attr exclude_from_pos_files)
    (fp_text reference "TP12" (at 2.032 0.762 55) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at -0.000001 2.05 145) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 145) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 325) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 26 "/LED11") (pinfunction "1") (pintype "passive"))
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 133.777281 81.873426 65)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED10")
    (attr smd)
    (fp_text reference "D11" (at -1.300702 1.816623 65) (layer "F.SilkS"))
    (fp_text value "LED" (at -0.000001 1.649999 65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 65) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 65) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 24 "/LED10") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 65) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 25 "Net-(D11-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.617978 99.826819 -15)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED1")
    (attr smd)
    (fp_text reference "R2" (at 2.794 -1.524 165) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.778 165) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 165) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 345) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 345) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 5 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 99.585024 87.902444 135)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED3")
    (attr smd)
    (fp_text reference "D4" (at -1.232156 1.97666 135) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.649999 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 135) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 10 "/LED3") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 135) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 11 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 145.727542 102.785121 -75)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED15")
    (attr exclude_from_pos_files)
    (fp_text reference "TP16" (at 2.032 0.762001 15) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.050001 105) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.999999 105) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 285) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 34 "/LED15") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 110.458521 86.338908 25)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED5")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 2.031999 0.762 115) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at -0.000001 2.05 25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.000001 -2 25) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 25) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 14 "/LED5") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D2.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 106.624184 88.552663 35)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED4")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 2.032 0.762 125) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 2.05 35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 35) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0 35) (size 2 2) (layers "F.Cu" "F.Mask")
      (net 12 "/LED4") (pinfunction "1") (pintype "passive"))
  )
  (footprint "kibuzzard-64037CBD" (layer "F.Cu")
    (tedit 64037CBD)
    (at 85.09 110.49 180)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPCIsICJDYXBSaWdodENob2ljZSI6ICIvIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkb2thT25lIiwgIkhlaWdodEN0cmwiOiAiMC43IiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIjEiLCAiUGFkZGluZ0JvdHRvbUN0cmwiOiAiOCIsICJQYWRkaW5nTGVmdEN0cmwiOiAiNSIsICJQYWRkaW5nUmlnaHRDdHJsIjogIjUiLCAiUGFkZGluZ1RvcEN0cmwiOiAiOCIsICJXaWR0aEN0cmwiOiAiIn0=")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-64037CBD" (at 0 -3.827357) (layer "F.SilkS") hide)
    (fp_text value "G***" (at 0 3.827357) (layer "F.SilkS") hide)
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.66072 73.784077 -75)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "led.kicad_sch")
    (property "Sheetname" "LED6")
    (attr smd)
    (fp_text reference "R8" (at 2.794 -1.523999 105) (layer "F.SilkS"))
    (fp_text value "R" (at 1.524 -1.778 105) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 105) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 285) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 3 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 285) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 17 "Net-(D7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "kibuzzard-6419EFEB" (layer "B.Cu")
    (tedit 6419EFEB)
    (at 121.666 94.234 180)
    (descr "Generated with KiBuzzard")
    (tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiPCIsICJDYXBSaWdodENob2ljZSI6ICIvIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkb2thT25lIiwgIkhlaWdodEN0cmwiOiAiMS44IiwgIkxheWVyQ29tYm9Cb3giOiAiRi5TaWxrUyIsICJNdWx0aUxpbmVUZXh0IjogIlZlcnNpb24gMlxuQXByaWwgMjAyMyIsICJQYWRkaW5nQm90dG9tQ3RybCI6ICI4IiwgIlBhZGRpbmdMZWZ0Q3RybCI6ICI1IiwgIlBhZGRpbmdSaWdodEN0cmwiOiAiNSIsICJQYWRkaW5nVG9wQ3RybCI6ICI4IiwgIldpZHRoQ3RybCI6ICIifQ==")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "kibuzzard-6419EFEB" (at 0 7.211802) (layer "B.SilkS") hide)
    (fp_text value "G***" (at 0 -7.211802) (layer "B.SilkS") hide)
  )
  (gr_line (start 160.711903 102.447071) (end 160.711903 112.522) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 81.534001 102.87) (mid 120.943651 69.090985) (end 160.711903 102.447071) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 81.534001 112.522) (end 81.534001 102.87) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 160.711903 112.522) (end 81.534001 112.522) (layer "Edge.Cuts") (width 0.1))
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.462 104.902)
        (xy 160.02 104.902)
        (xy 160.02 111.506)
        (xy 91.948 111.506)
        (xy 91.948 107.188)
        (xy 93.472 107.188)
        (xy 95.504 109.22)
        (xy 106.172 98.552)
        (xy 134.112 98.552)
      )
    )
  )
)
