<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17" y2="0" width="0" layer="20"/>
<wire x1="17" y1="0" x2="17" y2="17" width="0" layer="20"/>
<wire x1="17" y1="17" x2="0" y2="17" width="0" layer="20"/>
<wire x1="0" y1="17" x2="0" y2="0" width="0" layer="20"/>
<text>FLYANDI.NET</text>
<text>BitsyLED</text>
<text>DT 5V GND</text>
<text>DT 5V GND</text>
<text>DT 5V GND</text>
</plain>
<libraries>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO14">
<description>SOIC, 0.15 inch width</description>
</package>
</packages>
</library>
<library name="FPVTools">
<packages>
<package name="SMDPAD_TB_3X3">
</package>
</packages>
</library>
<library name="Seeed-Connector">
<packages>
<package name="H3-2.54">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOD-123">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SLAVECTRL" library="SparkFun-IC-Microcontroller" package="SO14" value="ATTINY84">
<attribute name="BGA"/>
<attribute name="PROD_ID" value="IC-11285"/>
<attribute name="VALUE" value="ATTINY84"/>
</element>
<element name="PRG" library="FPVTools" package="SMDPAD_TB_3X3" value="SMDPAD_TB_3X3"/>
<element name="RC" library="Seeed-Connector" package="H3-2.54" value="3p-2.54">
<attribute name="NAME"/>
</element>
<element name="LEFT" library="Seeed-Connector" package="H3-2.54" value="3p-2.54">
<attribute name="NAME"/>
</element>
<element name="RIGHT" library="Seeed-Connector" package="H3-2.54" value="3p-2.54">
<attribute name="NAME"/>
</element>
<element name="OTHER" library="Seeed-Connector" package="H3-2.54" value="3p-2.54">
<attribute name="NAME"/>
</element>
<element name="C1" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="SOD-123" value=""/>
</elements>
<signals>
<signal name="RC">
<contactref element="SLAVECTRL" pad="13"/>
<contactref element="RC" pad="1"/>
</signal>
<signal name="GND">
<contactref element="PRG" pad="1"/>
<contactref element="LEFT" pad="3"/>
<contactref element="RC" pad="3"/>
<contactref element="RIGHT" pad="3"/>
<contactref element="OTHER" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="SLAVECTRL" pad="14"/>
</signal>
<signal name="5V">
<contactref element="PRG" pad="2"/>
<contactref element="OTHER" pad="2"/>
<contactref element="RIGHT" pad="2"/>
<contactref element="LEFT" pad="2"/>
<contactref element="RC" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="SCL">
<contactref element="SLAVECTRL" pad="9"/>
<contactref element="PRG" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="SLAVECTRL" pad="7"/>
<contactref element="PRG" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="SLAVECTRL" pad="4"/>
<contactref element="PRG" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="SLAVECTRL" pad="8"/>
<contactref element="PRG" pad="3"/>
</signal>
<signal name="LD0">
<contactref element="SLAVECTRL" pad="12"/>
<contactref element="OTHER" pad="1"/>
</signal>
<signal name="LD1">
<contactref element="SLAVECTRL" pad="11"/>
<contactref element="LEFT" pad="1"/>
</signal>
<signal name="LD2">
<contactref element="SLAVECTRL" pad="10"/>
<contactref element="RIGHT" pad="1"/>
</signal>
<signal name="VR">
<contactref element="SLAVECTRL" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
