(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(U2-VOUT)")
	(net 3 "Net-(U1-OSCO)")
	(net 4 "Net-(U1-OSCI)")
	(net 5 "Net-(U1-VPHY)")
	(net 6 "Net-(U1-VPLL)")
	(net 7 "Net-(D1-A)")
	(net 8 "Net-(J1-Pad2)")
	(net 9 "Net-(J1-Pad3)")
	(net 10 "Net-(D2-K)")
	(net 11 "/TMS")
	(net 12 "/TCK")
	(net 13 "/TDI")
	(net 14 "/TDO")
	(net 15 "unconnected-(P3-P4-Pad4)")
	(net 16 "unconnected-(P3-P5-Pad5)")
	(net 17 "Net-(P4-P1)")
	(net 18 "Net-(P4-P2)")
	(net 19 "Net-(P4-P3)")
	(net 20 "Net-(P4-P4)")
	(net 21 "Net-(P4-P5)")
	(net 22 "Net-(P4-P6)")
	(net 23 "Net-(P4-P7)")
	(net 24 "Net-(P4-P8)")
	(net 25 "Net-(U1-DM)")
	(net 26 "Net-(U1-DP)")
	(net 27 "Net-(U1-~{RESET})")
	(net 28 "Net-(U3-DO)")
	(net 29 "Net-(U1-EECLK)")
	(net 30 "Net-(U1-EECS)")
	(net 31 "Net-(U1-EEDATA)")
	(net 32 "Net-(U1-REF)")
	(net 33 "Net-(U1-ADBUS0)")
	(net 34 "Net-(U1-ADBUS1)")
	(net 35 "Net-(U1-ADBUS2)")
	(net 36 "Net-(U1-ADBUS3)")
	(net 37 "unconnected-(U1-ADBUS4-Pad21)")
	(net 38 "unconnected-(U1-ADBUS5-Pad22)")
	(net 39 "unconnected-(U1-ADBUS6-Pad23)")
	(net 40 "unconnected-(U1-ADBUS7-Pad24)")
	(net 41 "unconnected-(U1-ACBUS0-Pad26)")
	(net 42 "unconnected-(U1-ACBUS1-Pad27)")
	(net 43 "unconnected-(U1-ACBUS2-Pad28)")
	(net 44 "unconnected-(U1-ACBUS3-Pad29)")
	(net 45 "unconnected-(U1-ACBUS4-Pad30)")
	(net 46 "unconnected-(U1-ACBUS5-Pad32)")
	(net 47 "unconnected-(U1-ACBUS6-Pad33)")
	(net 48 "unconnected-(U1-ACBUS7-Pad34)")
	(net 49 "unconnected-(U1-~{SUSPEND}-Pad36)")
	(net 50 "unconnected-(U1-BCBUS0-Pad48)")
	(net 51 "unconnected-(U1-BCBUS1-Pad52)")
	(net 52 "unconnected-(U1-BCBUS2-Pad53)")
	(net 53 "unconnected-(U1-BCBUS3-Pad54)")
	(net 54 "unconnected-(U1-BCBUS4-Pad55)")
	(net 55 "unconnected-(U1-BCBUS5-Pad57)")
	(net 56 "unconnected-(U1-BCBUS6-Pad58)")
	(net 57 "unconnected-(U1-BCBUS7-Pad59)")
	(net 58 "unconnected-(U1-~{PWREN}-Pad60)")
	(net 59 "unconnected-(U2-NC-Pad2)")
	(net 60 "unconnected-(U2-NC-Pad5)")
	(net 61 "unconnected-(U3-NC-Pad6)")
	(net 62 "unconnected-(U3-NC-Pad7)")
	(net 63 "/+5V0")
	(net 64 "+3.3V")
	(net 65 "/+1V8")
	(net 66 "/VUSB")
	(net 67 "Net-(D2-A)")
	(net 68 "Net-(D3-K)")
	(net 69 "Net-(D3-A)")
	(net 70 "Net-(J1-Pad4)")
	(net 71 "Net-(P3-P1)")
	(net 72 "Net-(Q1-G)")
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 125.603 96.381 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C2"
			(at -2.2994 -0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/+5V0")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 135.001 96.012 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R5"
			(at -1.7526 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U3-DO)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 135.001 98.552 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R7"
			(at -1.8542 -0.0508 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(U1-EECS)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 146.685 113.665 180)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "P4"
			(at 0.0254 20.193 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X08"
			(at -0.127 21.126 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X08 Pin_Header_Angled_1X08 Socket_Strip_Straight_1X08 Socket_Strip_Angled_1X08")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(P4-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(P4-P2)")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(P4-P3)")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(P4-P4)")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(P4-P5)")
			(pinfunction "P5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(P4-P6)")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(P4-P7)")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(P4-P8)")
			(pinfunction "P8")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_Mech_Switch:1825232-1"
		(layer "F.Cu")
		(at 146.5707 123.92 90)
		(property "Reference" "SW1"
			(at 7.6896 0.0889 180)
			(layer "F.SilkS")
		)
		(property "Value" "SWITCH_2P_1C"
			(at 2 -1.6002 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_Mech_Switch:1825232-1"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "1825232-1_TEC")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at -0.3368 -1.5367 0)
			(layer "F.SilkS")
		)
		(fp_text user "Copyright 2016 Accelerated Designs. All rights reserved."
			(at 0 0 90)
			(layer "Cmts.User")
		)
		(fp_text user "*"
			(at -1 -3.1115 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(P3-P1)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(Q1-G)")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 4.000001 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "+3.3V")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at -2 0 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "m")
			(pintype "unspecified")
		)
		(pad "5" thru_hole circle
			(at 6 0 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "m")
			(pintype "unspecified")
		)
		(model "${T_LIBS}/3d/t_Mech_Switch/c-1825232-1-b-3d.stp"
			(offset
				(xyz 2 -2.2 2.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 130.344 100.584 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C9"
			(at -1.863 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "18pF"
			(at 0 0.8636 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U1-OSCI)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 127 125.857)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C17"
			(at 2.032 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(Q1-G)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 137.9855 121.97464 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0.40256 1.6383 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED_GREEN_SMD"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 270)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 270)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 67 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 138.176 124.968 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R11"
			(at 0.127 -1.143 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "Net-(D2-A)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 125.095 103.364 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at -2.3 -0.0762 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED_GREEN_SMD"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.8 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.35x4.35mm"
		(layer "F.Cu")
		(at 138.307 109.352)
		(descr "QFN, 64 Pin (https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT2232H.pdf#page=57), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U1"
			(at 0 -6.1264 0)
			(layer "F.SilkS")
		)
		(property "Value" "FT2232HQ"
			(at 0 5.81 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.35x4.35mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT2232H.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Hi Speed Double Channel USB UART/FIFO, QFN-64"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*9x9mm*P0.5mm*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -1.45 -1.45)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at -1.45 0)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at -1.45 1.45)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at 0 -1.45)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at 0 0)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at 0 1.45)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at 1.45 -1.45)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at 1.45 0)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "" smd roundrect
			(at 1.45 1.45)
			(size 1.17 1.17)
			(layers "F.Paste")
			(roundrect_rratio 0.213675)
		)
		(pad "1" smd roundrect
			(at -4.45 -3.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -4.45 -3.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(U1-OSCI)")
			(pinfunction "OSCI")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -4.45 -2.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-OSCO)")
			(pinfunction "OSCO")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -4.45 -2.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-VPHY)")
			(pinfunction "VPHY")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -4.45 -1.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -4.45 -1.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U1-REF)")
			(pinfunction "REF")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -4.45 -0.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U1-DM)")
			(pinfunction "DM")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -4.45 -0.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U1-DP)")
			(pinfunction "DP")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -4.45 0.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-VPLL)")
			(pinfunction "VPLL")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -4.45 0.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -4.45 1.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -4.45 1.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/+1V8")
			(pinfunction "VCORE")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at -4.45 2.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "TEST")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at -4.45 2.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U1-~{RESET})")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -4.45 3.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -4.45 3.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U1-ADBUS0)")
			(pinfunction "ADBUS0")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -3.75 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(U1-ADBUS1)")
			(pinfunction "ADBUS1")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -3.25 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U1-ADBUS2)")
			(pinfunction "ADBUS2")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -2.75 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U1-ADBUS3)")
			(pinfunction "ADBUS3")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -2.25 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "+3.3V")
			(pinfunction "VCCIO")
			(pintype "power_in")
		)
		(pad "21" smd roundrect
			(at -1.75 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "unconnected-(U1-ADBUS4-Pad21)")
			(pinfunction "ADBUS4")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" smd roundrect
			(at -1.25 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "unconnected-(U1-ADBUS5-Pad22)")
			(pinfunction "ADBUS5")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" smd roundrect
			(at -0.75 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(U1-ADBUS6-Pad23)")
			(pinfunction "ADBUS6")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" smd roundrect
			(at -0.25 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "unconnected-(U1-ADBUS7-Pad24)")
			(pinfunction "ADBUS7")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" smd roundrect
			(at 0.25 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "26" smd roundrect
			(at 0.75 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "unconnected-(U1-ACBUS0-Pad26)")
			(pinfunction "ACBUS0")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" smd roundrect
			(at 1.25 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "unconnected-(U1-ACBUS1-Pad27)")
			(pinfunction "ACBUS1")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" smd roundrect
			(at 1.75 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "unconnected-(U1-ACBUS2-Pad28)")
			(pinfunction "ACBUS2")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" smd roundrect
			(at 2.25 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(U1-ACBUS3-Pad29)")
			(pinfunction "ACBUS3")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" smd roundrect
			(at 2.75 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "unconnected-(U1-ACBUS4-Pad30)")
			(pinfunction "ACBUS4")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" smd roundrect
			(at 3.25 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "+3.3V")
			(pinfunction "VCCIO")
			(pintype "power_in")
		)
		(pad "32" smd roundrect
			(at 3.75 4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(U1-ACBUS5-Pad32)")
			(pinfunction "ACBUS5")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" smd roundrect
			(at 4.45 3.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "unconnected-(U1-ACBUS6-Pad33)")
			(pinfunction "ACBUS6")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" smd roundrect
			(at 4.45 3.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(U1-ACBUS7-Pad34)")
			(pinfunction "ACBUS7")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" smd roundrect
			(at 4.45 2.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "36" smd roundrect
			(at 4.45 2.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U1-~{SUSPEND}-Pad36)")
			(pinfunction "~{SUSPEND}")
			(pintype "output+no_connect")
		)
		(pad "37" smd roundrect
			(at 4.45 1.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/+1V8")
			(pinfunction "VCORE")
			(pintype "power_in")
		)
		(pad "38" smd roundrect
			(at 4.45 1.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(P4-P1)")
			(pinfunction "BDBUS0")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 4.45 0.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(P4-P2)")
			(pinfunction "BDBUS1")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at 4.45 0.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(P4-P3)")
			(pinfunction "BDBUS2")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 4.45 -0.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(P4-P4)")
			(pinfunction "BDBUS3")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at 4.45 -0.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "+3.3V")
			(pinfunction "VCCIO")
			(pintype "power_in")
		)
		(pad "43" smd roundrect
			(at 4.45 -1.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(P4-P5)")
			(pinfunction "BDBUS4")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at 4.45 -1.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(P4-P6)")
			(pinfunction "BDBUS5")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at 4.45 -2.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(P4-P7)")
			(pinfunction "BDBUS6")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at 4.45 -2.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "Net-(P4-P8)")
			(pinfunction "BDBUS7")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 4.45 -3.25)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "48" smd roundrect
			(at 4.45 -3.75)
			(size 0.8 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "unconnected-(U1-BCBUS0-Pad48)")
			(pinfunction "BCBUS0")
			(pintype "bidirectional+no_connect")
		)
		(pad "49" smd roundrect
			(at 3.75 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/+1V8")
			(pinfunction "VREGOUT")
			(pintype "power_out")
		)
		(pad "50" smd roundrect
			(at 3.25 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "+3.3V")
			(pinfunction "VREGIN")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at 2.75 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "52" smd roundrect
			(at 2.25 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "unconnected-(U1-BCBUS1-Pad52)")
			(pinfunction "BCBUS1")
			(pintype "bidirectional+no_connect")
		)
		(pad "53" smd roundrect
			(at 1.75 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(U1-BCBUS2-Pad53)")
			(pinfunction "BCBUS2")
			(pintype "bidirectional+no_connect")
		)
		(pad "54" smd roundrect
			(at 1.25 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U1-BCBUS3-Pad54)")
			(pinfunction "BCBUS3")
			(pintype "bidirectional+no_connect")
		)
		(pad "55" smd roundrect
			(at 0.75 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U1-BCBUS4-Pad55)")
			(pinfunction "BCBUS4")
			(pintype "bidirectional+no_connect")
		)
		(pad "56" smd roundrect
			(at 0.25 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "+3.3V")
			(pinfunction "VCCIO")
			(pintype "power_in")
		)
		(pad "57" smd roundrect
			(at -0.25 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "unconnected-(U1-BCBUS5-Pad57)")
			(pinfunction "BCBUS5")
			(pintype "bidirectional+no_connect")
		)
		(pad "58" smd roundrect
			(at -0.75 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "unconnected-(U1-BCBUS6-Pad58)")
			(pinfunction "BCBUS6")
			(pintype "bidirectional+no_connect")
		)
		(pad "59" smd roundrect
			(at -1.25 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(U1-BCBUS7-Pad59)")
			(pinfunction "BCBUS7")
			(pintype "bidirectional+no_connect")
		)
		(pad "60" smd roundrect
			(at -1.75 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U1-~{PWREN}-Pad60)")
			(pinfunction "~{PWREN}")
			(pintype "output+no_connect")
		)
		(pad "61" smd roundrect
			(at -2.25 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U1-EEDATA)")
			(pinfunction "EEDATA")
			(pintype "bidirectional")
		)
		(pad "62" smd roundrect
			(at -2.75 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U1-EECLK)")
			(pinfunction "EECLK")
			(pintype "output")
		)
		(pad "63" smd roundrect
			(at -3.25 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U1-EECS)")
			(pinfunction "EECS")
			(pintype "output")
		)
		(pad "64" smd roundrect
			(at -3.75 -4.45)
			(size 0.25 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/+1V8")
			(pinfunction "VCORE")
			(pintype "power_in")
		)
		(pad "65" smd rect
			(at 0 0)
			(size 4.35 4.35)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-64-1EP_9x9mm_P0.5mm_EP4.35x4.35mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0603"
		(layer "F.Cu")
		(at 141.77 102.108)
		(descr "SMT resistor, 0603")
		(property "Reference" "R8"
			(at -2.1208 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U3-DO)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(U1-EEDATA)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 125.688 100.584 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R3"
			(at -1.82 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(D1-A)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/+5V0")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 136.4488 120.5396 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R13"
			(at -0.0596 -1.0668 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(D2-K)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 129.738001 123.656 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R14"
			(at 2.3964 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/TCK")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 132.588 118.872 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C19"
			(at 0.0508 1.1176 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_so:SOIC-8"
		(layer "F.Cu")
		(at 140.462 97.536 90)
		(property "Reference" "U3"
			(at 4.318 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "93LCxxA"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_so:SOIC-8"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001749K.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x4.9mm*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "Copyright 2016 Accelerated Designs. All rights reserved."
			(at 0 0 90)
			(layer "Cmts.User")
		)
		(pad "1" smd rect
			(at -2.72415 -1.905 90)
			(size 1.4605 0.5334)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(U1-EECS)")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.72415 -0.635 90)
			(size 1.4605 0.5334)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U1-EECLK)")
			(pinfunction "SCLK")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.72415 0.635 90)
			(size 1.4605 0.5334)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(U1-EEDATA)")
			(pinfunction "DI")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.72415 1.905 90)
			(size 1.4605 0.5334)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U3-DO)")
			(pinfunction "DO")
			(pintype "tri_state")
		)
		(pad "5" smd rect
			(at 2.72415 1.905 90)
			(size 1.4605 0.5334)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at 2.72415 0.635 90)
			(size 1.4605 0.5334)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "unconnected-(U3-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd rect
			(at 2.72415 -0.635 90)
			(size 1.4605 0.5334)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "unconnected-(U3-NC-Pad7)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "8" smd rect
			(at 2.72415 -1.905 90)
			(size 1.4605 0.5334)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${T_LIBS}/3d/t_so/SOIC-8.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "F.Cu")
		(at 126.619 103.035 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB1"
			(at -2.3242 0.0254 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 0.9652 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/+5V0")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "/VUSB")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 131.403 108.585 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R1"
			(at 1.6598 0.0254 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(J1-Pad2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U1-DM)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:Header_5x100"
		(layer "F.Cu")
		(at 135.89 133.35 180)
		(property "Reference" "P1"
			(at -8.128 0.508 180)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X05"
			(at 0 -0.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:Header_5x100"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X05 Pin_Header_Angled_1X05 Socket_Strip_Straight_1X05 Socket_Strip_Angled_1X05")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.127 1.016 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at -5.08 0 180)
			(size 1.905 2.159)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15)
			(net 11 "/TMS")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -2.54 0 180)
			(size 1.905 2.159)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/TCK")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 0 180)
			(size 1.905 2.159)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/TDI")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 0 180)
			(size 1.905 2.159)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 5.08 0 180)
			(size 1.905 2.159)
			(drill 1.27)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/TDO")
			(pinfunction "P5")
			(pintype "passive")
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 132.715 125.857)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C18"
			(at 2.032 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(Q1-G)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_crystal:Crystal_5x3_2"
		(layer "F.Cu")
		(at 130.299 103.70415 -90)
		(property "Reference" "Y1"
			(at -1.72315 -2.797 180)
			(layer "F.SilkS")
		)
		(property "Value" "Crystal_GND24"
			(at 0.1115 2.624 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "t_crystal:Crystal_5x3_2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.27 1.1 270)
			(size 1.6 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U1-OSCI)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 1.1 270)
			(size 1.6 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.27 -1.1 270)
			(size 1.6 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U1-OSCO)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.27 -1.1 270)
			(size 1.6 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "4")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_misc/ASE_3427.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 135.001 97.282 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R6"
			(at -1.8542 -0.0508 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U1-EECLK)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 139.7635 121.97464 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D3"
			(at -0.30864 -1.5621 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED_RED_SMD"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED-3MM LED-5MM LED-10MM LED-0603 LED-0805 LED-1206 LEDV")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 270)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 270)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 134.959 94.742)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C4"
			(at 1.8454 0.0508 360)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 130.852 106.68)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C8"
			(at -1.82 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "18pF"
			(at 0 0.8636 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(U1-OSCO)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 131.445 113.03 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R4"
			(at -1.8288 0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(U1-~{RESET})")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_smd_transistors:SOT-23"
		(layer "F.Cu")
		(at 137.922 118.40464 180)
		(descr "SOT-23")
		(property "Reference" "Q1"
			(at 0 2.32664 180)
			(layer "F.SilkS")
		)
		(property "Value" "BSS123_a"
			(at 0 0.0635 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_smd_transistors:SOT-23"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0.0635 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(D2-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_transistors/sot23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_qfn:LLP-6"
		(layer "F.Cu")
		(at 128.277 96.505 90)
		(property "Reference" "U2"
			(at 2.271 -0.007 180)
			(layer "F.SilkS")
		)
		(property "Value" "LP5900"
			(at 0.127 -1.778 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_qfn:LLP-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://4donline.ihs.com/images/VipMasterIC/IC/NATL/NATLS11477/NATLS11477-1.pdf?hkey=EC6BD57738AE6E33B588C5F9AD3CEFA7"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*WSON*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.127 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.65 1.15 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(U2-VOUT)")
			(pinfunction "VOUT")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 1.15 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "unconnected-(U2-NC-Pad2)")
			(pinfunction "NC")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.65 1.15 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.65 -1.15 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/+5V0")
			(pinfunction "VEN")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 0 -1.15 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "unconnected-(U2-NC-Pad5)")
			(pinfunction "NC")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -0.65 -1.15 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/+5V0")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 0 0 90)
			(size 1.2 0.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_qfn/WSON-6.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 127 118.745 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C20"
			(at -0.127 1.143 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 144.765 129.032 -90)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "P3"
			(at -0.762 -2.428 180)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_01X08"
			(at 0.56715 20.917 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin_Header_Straight_1X08 Pin_Header_Angled_1X08 Socket_Strip_Straight_1X08 Socket_Strip_Angled_1X08")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(P3-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/TDO")
			(pinfunction "P2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/TDI")
			(pinfunction "P3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(P3-P4-Pad4)")
			(pinfunction "P4")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(P3-P5-Pad5)")
			(pinfunction "P5")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/TMS")
			(pinfunction "P6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/TCK")
			(pinfunction "P8")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 131.403 109.728 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R2"
			(at 1.736 0 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(J1-Pad3)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U1-DP)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "F.Cu")
		(at 131.737 97.663)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB2"
			(at 0 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 0.9652 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(U2-VOUT)")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "F.Cu")
		(at 132.588 95.492 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C5"
			(at -2.02 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.016 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 0.0635 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "F.Cu")
		(at 127.254 122.87885 90)
		(tags "INA236AIDDFR ")
		(property "Reference" "U4"
			(at 0.57785 -2.667 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCA9406"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9406.pdf?ts=1710769372418&ref_url=https%253A%252F%252Fwww.google.com%252F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "I2C Level Translator"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.88595 -1.524 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.88595 -1.4732 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "Net-(U1-ADBUS0)")
			(pinfunction "SDA_B")
			(pintype "open_collector")
		)
		(pad "2" smd rect
			(at -1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(Q1-G)")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/TCK")
			(pinfunction "SDA_A")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at 1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/TDI")
			(pinfunction "SCL_A")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(Q1-G)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(U1-ADBUS1)")
			(pinfunction "SCL_B")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_smd_transistors:SOT-23"
		(layer "F.Cu")
		(at 141.2875 118.40464 180)
		(descr "SOT-23")
		(property "Reference" "Q2"
			(at 0.0635 2.32664 180)
			(layer "F.SilkS")
		)
		(property "Value" "BSS123_a"
			(at 0 0.0635 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_smd_transistors:SOT-23"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0.0635 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(D2-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0.9525 1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 -1.05664 180)
			(size 0.59944 1.00076)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "Net-(D3-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_smd_transistors/sot23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 127.762 98.679 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C1"
			(at 1.6764 -0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/+5V0")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 128.651 119.761 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R10"
			(at -0.127 1.016 360)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 360)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(Q1-G)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_USB:conn_usb_B_micro_smd"
		(layer "F.Cu")
		(at 124.841 110.48238 -90)
		(descr "USB B micro SMD connector, Molex P/N 47346-0001")
		(property "Reference" "J1"
			(at 4.93522 -1.651 180)
			(layer "F.SilkS")
		)
		(property "Value" "USB_micro-B"
			(at 0 -4.0005 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_USB:conn_usb_B_micro_smd"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Data+" "D+"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Data-" "D-"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ground" "GND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "VCC" "VCC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(pad "" smd rect
			(at -2.46126 -2.2987 270)
			(size 1.4732 2.10058)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
		)
		(pad "" smd rect
			(at 2.46126 -2.2987 270)
			(size 1.4732 2.10058)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
		)
		(pad "1" smd rect
			(at -1.30048 -2.65938 270)
			(size 0.44958 1.37922)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "/VUSB")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.65024 -2.65938 270)
			(size 0.44958 1.37922)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(J1-Pad2)")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0 -2.65938 270)
			(size 0.44958 1.37922)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(J1-Pad3)")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.65024 -2.65938 270)
			(size 0.44958 1.37922)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "Net-(J1-Pad4)")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 1.30048 -2.65938 270)
			(size 0.44958 1.37922)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.91338 0 270)
			(size 2.3749 1.89738)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -0.8382 0 270)
			(size 1.17348 1.89738)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 0.8382 0 270)
			(size 1.17348 1.89738)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.91338 0 270)
			(size 2.3749 1.89738)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_USB/10118192-002lfc.stp"
			(offset
				(xyz -98 3 -0.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 129.921 111.76 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R18"
			(at 2.032 0.0762 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "Net-(J1-Pad4)")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "F.Cu")
		(at 139.573 124.968 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R12"
			(at 0.127 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "Res6"
			(at 0 0.8128 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "Net-(D3-A)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_sot:SOT23-8_DDF_TEX"
		(layer "F.Cu")
		(at 132.883001 122.936 90)
		(tags "INA236AIDDFR ")
		(property "Reference" "U5"
			(at 3.175 0.974999 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TCA9406"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "t_sot:SOT23-8_DDF_TEX"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9406.pdf?ts=1710769372418&ref_url=https%253A%252F%252Fwww.google.com%252F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "I2C Level Translator"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.9304 -1.412601 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.9304 -1.412601 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.4445 -1.397 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(U1-ADBUS2)")
			(pinfunction "SDA_B")
			(pintype "open_collector")
		)
		(pad "2" smd rect
			(at -1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(Q1-G)")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/TDO")
			(pinfunction "SDA_A")
			(pintype "open_collector")
		)
		(pad "5" smd rect
			(at 1.32715 0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/TMS")
			(pinfunction "SCL_A")
			(pintype "open_collector")
		)
		(pad "6" smd rect
			(at 1.32715 0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(Q1-G)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 1.32715 -0.325001 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "+3.3V")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 1.32715 -0.974999 90)
			(size 1.0033 0.4318)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(U1-ADBUS3)")
			(pinfunction "SCL_B")
			(pintype "open_collector")
		)
		(model "${T_LIBS}/3d/t_sot/DDF0008A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "F.Cu")
		(at 130.81 95.8 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C3"
			(at -2.074 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 0.8636 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(U2-VOUT)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 131.191 108.331 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB4"
			(at 0.127 -1.7018 180)
			(layer "B.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "Net-(U1-VPHY)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 64 "+3.3V")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 132.461 111.379 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C12"
			(at -2.0066 0.0254 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 6 "Net-(U1-VPLL)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 132.588 106.553 -90)
		(descr "SMT resistor, 0603")
		(property "Reference" "C10"
			(at -0.7366 1.7272 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "Net-(U1-VPHY)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0 270)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0603"
		(layer "B.Cu")
		(at 132.969 104.267)
		(descr "SMT resistor, 0603")
		(property "Reference" "C6"
			(at -0.0762 -1.3462 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.016 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.254 -0.0635 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.75 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 65 "/+1V8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 0)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0603.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:fb_0603"
		(layer "B.Cu")
		(at 131.064 111.379 90)
		(descr "SMT resistor, 0603")
		(property "Reference" "FB3"
			(at 0.2794 -1.6764 180)
			(layer "B.SilkS")
		)
		(property "Value" "Ferrite_Bead"
			(at 0 -0.9652 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:fb_0603"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.381 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 6 "Net-(U1-VPLL)")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.8 0 90)
			(size 0.7 0.9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 64 "+3.3V")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/FB_0603.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:res_0402"
		(layer "B.Cu")
		(at 133.858 108.458 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "R9"
			(at -0.2032 -1.8796 180)
			(layer "B.SilkS")
		)
		(property "Value" "Res6"
			(at 0 -0.8128 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:res_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.1905 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 32 "Net-(U1-REF)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_passive_smd/res_0402.stp"
			(offset
				(xyz 0 0 0.02999999955)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 142.875 105.41 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C7"
			(at -1.651 -0.127 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.042 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 65 "/+1V8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 133.731 110.744 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C13"
			(at -0.5588 1.7018 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 6 "Net-(U1-VPLL)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 137.329 113.792 180)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C15"
			(at -0.085 1.1176 360)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -0.8636 360)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 360)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 64 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 180)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 141.266 104.902)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C16"
			(at 0.0088 -1.524 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 64 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 133.858 106.299 -90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C11"
			(at -0.5334 -1.6256 180)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "Net-(U1-VPHY)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 270)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 142.6972 111.7512 90)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C21"
			(at 1.8962 -0.0762 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -0.8636 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 65 "/+1V8")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0 90)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_passive_smd:cap_0402"
		(layer "B.Cu")
		(at 140.758 113.792)
		(descr "SMT capacitor, 0402")
		(property "Reference" "C14"
			(at 0.0088 -1.1684 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 -0.8636 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_passive_smd:cap_0402"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Lattice_FTDI_Programmer.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0635 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 64 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.55 0)
			(size 0.5 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${T_LIBS}/3d/t_passive_smd/cap_0402.stp"
			(offset
				(xyz 0 0 0.04999999925)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 146.899159 92.075)
		(mid 147.287965 92.152338)
		(end 147.617579 92.372579)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.59 127.378849)
		(end 148.59 93.765841)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.899159 92.075)
		(end 124.880841 92.075)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 148.59 127.378849)
		(mid 148.559172 127.627228)
		(end 148.468558 127.860534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.432708 135.355686)
		(end 148.468558 127.860534)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.29242 93.04742)
		(end 147.617579 92.372579)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 148.29242 93.04742)
		(mid 148.512648 93.377037)
		(end 148.59 93.765841)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 128.241851 135.89)
		(mid 127.720841 135.746272)
		(end 127.347292 135.355686)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.16242 92.37258)
		(end 123.487579 93.047421)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.311442 127.860534)
		(mid 123.220829 127.627228)
		(end 123.19 127.378849)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.241851 135.89)
		(end 143.538149 135.89)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.19 93.765841)
		(end 123.19 127.378849)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.432708 135.355686)
		(mid 144.05914 135.746253)
		(end 143.538149 135.89)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.19 93.765841)
		(mid 123.267338 93.377035)
		(end 123.487579 93.047421)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 124.16242 92.37258)
		(mid 124.492037 92.152352)
		(end 124.880841 92.075)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.347292 135.355686)
		(end 123.311442 127.860534)
		(layer "Edge.Cuts")
	)
	(gr_text "TCK\n"
		(at 127.8128 127.4572 -0)
		(layer "B.SilkS")
	)
	(gr_text "D4"
		(at 145.288 104.013 0)
		(layer "B.SilkS")
	)
	(gr_text "X"
		(at 134.9248 127.4572 -0)
		(layer "B.SilkS")
	)
	(gr_text "Ext VCC"
		(at 145.2372 124.3584 0)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 145.796 127.508 -0)
		(layer "B.SilkS")
	)
	(gr_text "D7"
		(at 145.288 96.266 0)
		(layer "B.SilkS")
	)
	(gr_text "D3"
		(at 145.288 106.553 0)
		(layer "B.SilkS")
	)
	(gr_text "D0"
		(at 145.161 114.046 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 134.3152 131.9276 -0)
		(layer "B.SilkS")
	)
	(gr_text "TDI\n"
		(at 140.5636 127.508 -0)
		(layer "B.SilkS")
	)
	(gr_text "D1"
		(at 145.161 111.633 0)
		(layer "B.SilkS")
	)
	(gr_text "TDO"
		(at 131.6736 131.9276 -0)
		(layer "B.SilkS")
	)
	(gr_text "TMS"
		(at 133.1468 127.4572 -0)
		(layer "B.SilkS")
	)
	(gr_text "TCK\n"
		(at 139.446 131.9276 -0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 130.6068 127.4572 -0)
		(layer "B.SilkS")
	)
	(gr_text "D5"
		(at 145.288 101.473 0)
		(layer "B.SilkS")
	)
	(gr_text "TMS"
		(at 141.986 131.9276 -0)
		(layer "B.SilkS")
	)
	(gr_text "D6"
		(at 145.288 98.933 0)
		(layer "B.SilkS")
	)
	(gr_text "DRM 15 June 2024"
		(at 142.0876 98.5012 0)
		(layer "B.SilkS")
	)
	(gr_text "X"
		(at 137.4648 127.4572 -0)
		(layer "B.SilkS")
	)
	(gr_text "Int VCC"
		(at 145.3388 120.5484 0)
		(layer "B.SilkS")
	)
	(gr_text "FTDI 2232H\nJTAG PROGRAMMER"
		(at 142.0876 96.6216 0)
		(layer "B.SilkS")
	)
	(gr_text "D2"
		(at 145.288 109.093 0)
		(layer "B.SilkS")
	)
	(gr_text "TDO"
		(at 143.2052 127.508 -0)
		(layer "B.SilkS")
	)
	(gr_text "TDI\n"
		(at 136.4996 131.9276 -0)
		(layer "B.SilkS")
	)
	(gr_text "D1"
		(at 143.891 111.633 -0)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 140.1064 131.9276 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 128.524 127.4572 0)
		(layer "F.SilkS")
	)
	(gr_text "D3"
		(at 143.891 106.553 -0)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 129.794 131.9276 0)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 131.2672 127.4572 0)
		(layer "F.SilkS")
	)
	(gr_text "D5"
		(at 143.891 101.473 -0)
		(layer "F.SilkS")
	)
	(gr_text "TDI\n"
		(at 139.0904 127.508 0)
		(layer "F.SilkS")
	)
	(gr_text "D2"
		(at 143.891 109.093 -0)
		(layer "F.SilkS")
	)
	(gr_text "TDI\n"
		(at 135.0264 131.9276 0)
		(layer "F.SilkS")
	)
	(gr_text "TCK\n"
		(at 125.984 127.4572 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 132.334 131.9276 0)
		(layer "F.SilkS")
	)
	(gr_text "D0"
		(at 143.764 114.046 -0)
		(layer "F.SilkS")
	)
	(gr_text "D6"
		(at 143.891 98.933 -0)
		(layer "F.SilkS")
	)
	(gr_text "D7"
		(at 143.891 96.266 -0)
		(layer "F.SilkS")
	)
	(gr_text "TCK\n"
		(at 137.6172 131.9276 0)
		(layer "F.SilkS")
	)
	(gr_text "D4"
		(at 143.891 104.013 -0)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 141.3764 127.508 0)
		(layer "F.SilkS")
	)
	(gr_text "X"
		(at 136.7536 127.4572 0)
		(layer "F.SilkS")
	)
	(gr_text "X"
		(at 134.2136 127.4572 0)
		(layer "F.SilkS")
	)
	(gr_text "VCC"
		(at 143.9164 127.508 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.1778)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.095 92.71) (xy 146.685 92.71) (xy 147.955 93.98) (xy 147.955 127.635) (xy 143.51 135.255)
				(xy 128.27 135.255) (xy 123.825 127.635) (xy 123.825 93.98)
			)
		)
	)
)
