(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 155)
    (no_connects 0)
    (area 116.535999 34.493999 171.754001 118.414001)
    (thickness 1.6)
    (drawings 40)
    (tracks 755)
    (zones 0)
    (modules 57)
    (nets 56)
  )
  (page A4)
  (title_block
    (title "Seven segment module")
    (rev 1.0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.22606)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C6-Pad2)")
  (net 4 "Net-(C7-Pad2)")
  (net 5 /RXD0)
  (net 6 /TXD0)
  (net 7 "Net-(IC1-Pad10)")
  (net 8 "Net-(IC1-Pad11)")
  (net 9 "Net-(IC1-Pad12)")
  (net 10 "Net-(IC1-Pad13)")
  (net 11 +24V)
  (net 12 "Net-(R1-Pad2)")
  (net 13 "Net-(R2-Pad2)")
  (net 14 "Net-(R17-Pad2)")
  (net 15 "Net-(R18-Pad2)")
  (net 16 "Net-(U1-Pad17)")
  (net 17 "Net-(U1-Pad18)")
  (net 18 "Net-(U2-Pad17)")
  (net 19 "Net-(U2-Pad18)")
  (net 20 "Net-(U5-Pad17)")
  (net 21 "Net-(U6-Pad17)")
  (net 22 "Net-(U6-Pad18)")
  (net 23 "Net-(U5-Pad18)")
  (net 24 /I_RESET)
  (net 25 /I_MOSI)
  (net 26 /I_MISO)
  (net 27 /I_SCK)
  (net 28 "Net-(Digit1-Pad1)")
  (net 29 "Net-(Digit1-Pad2)")
  (net 30 "Net-(Digit1-Pad3)")
  (net 31 "Net-(Digit1-Pad4)")
  (net 32 "Net-(Digit1-Pad5)")
  (net 33 "Net-(Digit1-Pad6)")
  (net 34 "Net-(Digit1-Pad7)")
  (net 35 "Net-(Digit1-Pad8)")
  (net 36 "Net-(Digit1-Pad9)")
  (net 37 "Net-(Digit1-Pad10)")
  (net 38 "Net-(Digit1-Pad11)")
  (net 39 "Net-(Digit1-Pad12)")
  (net 40 "Net-(Digit1-Pad13)")
  (net 41 "Net-(Digit1-Pad14)")
  (net 42 "Net-(Digit2-Pad1)")
  (net 43 "Net-(Digit2-Pad2)")
  (net 44 "Net-(Digit2-Pad3)")
  (net 45 "Net-(Digit2-Pad4)")
  (net 46 "Net-(Digit2-Pad5)")
  (net 47 "Net-(Digit2-Pad6)")
  (net 48 "Net-(Digit2-Pad7)")
  (net 49 "Net-(Digit2-Pad8)")
  (net 50 "Net-(Digit2-Pad9)")
  (net 51 "Net-(Digit2-Pad10)")
  (net 52 "Net-(Digit2-Pad11)")
  (net 53 "Net-(Digit2-Pad12)")
  (net 54 "Net-(Digit2-Pad13)")
  (net 55 "Net-(Digit2-Pad14)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /I_MISO)
    (add_net /I_MOSI)
    (add_net /I_RESET)
    (add_net /I_SCK)
    (add_net /RXD0)
    (add_net /TXD0)
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(Digit1-Pad1)")
    (add_net "Net-(Digit1-Pad10)")
    (add_net "Net-(Digit1-Pad11)")
    (add_net "Net-(Digit1-Pad12)")
    (add_net "Net-(Digit1-Pad13)")
    (add_net "Net-(Digit1-Pad14)")
    (add_net "Net-(Digit1-Pad2)")
    (add_net "Net-(Digit1-Pad3)")
    (add_net "Net-(Digit1-Pad4)")
    (add_net "Net-(Digit1-Pad5)")
    (add_net "Net-(Digit1-Pad6)")
    (add_net "Net-(Digit1-Pad7)")
    (add_net "Net-(Digit1-Pad8)")
    (add_net "Net-(Digit1-Pad9)")
    (add_net "Net-(Digit2-Pad1)")
    (add_net "Net-(Digit2-Pad10)")
    (add_net "Net-(Digit2-Pad11)")
    (add_net "Net-(Digit2-Pad12)")
    (add_net "Net-(Digit2-Pad13)")
    (add_net "Net-(Digit2-Pad14)")
    (add_net "Net-(Digit2-Pad2)")
    (add_net "Net-(Digit2-Pad3)")
    (add_net "Net-(Digit2-Pad4)")
    (add_net "Net-(Digit2-Pad5)")
    (add_net "Net-(Digit2-Pad6)")
    (add_net "Net-(Digit2-Pad7)")
    (add_net "Net-(Digit2-Pad8)")
    (add_net "Net-(Digit2-Pad9)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U5-Pad17)")
    (add_net "Net-(U5-Pad18)")
    (add_net "Net-(U6-Pad17)")
    (add_net "Net-(U6-Pad18)")
  )
  (net_class "high power" ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net GND)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F57ADC)
    (at 121.539 51.562 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F57AB4)
    (at 147.828 40.894 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.318 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F5771A)
    (at 120.904 91.948 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -4.318 -0.127 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F577C3)
    (at 148.844 91.186 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -4.318 0 270) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F5777C)
    (at 145.288 99.314)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F5767A)
    (at 136.906 109.347)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 22p (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F57673)
    (at 153.67 109.347 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 0 1.778 180) (layer F.SilkS))
    (fp_text value 22p (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58F5776B)
    (at 145.288 106.172)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at -4.953 -3.81) (layer F.SilkS))
    (fp_text value ATTINY841-SSU (at 0 5.375) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C6-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /I_RESET))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /RXD0))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /TXD0))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /I_MOSI))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /I_MISO))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /I_SCK))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 58F57AEE)
    (at 140.716 38.608 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 4.315 -2.27 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 4.315 4.81 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +24V))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 58F4C0D3)
    (at 164.084 114.554 270)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 4.315 -2.27 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 4.315 4.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x03_Pitch2.54mm (layer F.Cu) (tedit 58F4C0B0)
    (at 126.238 114.3 270)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 4.315 -2.27 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 4.315 7.35 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /I_MOSI))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /I_SCK))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x03_Pitch2.54mm (layer F.Cu) (tedit 58F4C0C1)
    (at 136.652 114.3 270)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 4.315 -2.27 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X03 (at 4.315 7.35 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /TXD0))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RXD0))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57ACB)
    (at 121.539 44.831 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57AA7)
    (at 150.622 40.894 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 4.318 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57A0E)
    (at 128.016 53.848)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 4.318 0.762) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(Digit2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57A2A)
    (at 155.702 53.848)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 4.318 0.762) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Digit1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F579F3)
    (at 121.666 61.214)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Digit2-Pad3)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F579C8)
    (at 149.606 61.214)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(Digit1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57944)
    (at 123.698 72.644)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(Digit2-Pad5)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F5790D)
    (at 151.384 72.644)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Digit1-Pad5)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F5789F)
    (at 131.318 80.264)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Digit2-Pad7)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F578C1)
    (at 159.258 80.264)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Digit1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57926)
    (at 138.684 72.644)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(Digit2-Pad9)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F578E9)
    (at 166.37 72.644)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R12 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Digit1-Pad9)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F579DB)
    (at 137.16 61.214)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(Digit2-Pad11)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F579B0)
    (at 165.1 61.214)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Digit1-Pad11)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57962)
    (at 129.286 67.056)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Digit2-Pad13)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F5798F)
    (at 157.226 67.056)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(Digit1-Pad13)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57722)
    (at 123.698 91.948 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R17 (at -4.699 -0.127 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F577D7)
    (at 151.638 91.186 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R18 (at -4.699 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.3 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F579E8)
    (at 129.032 59.69 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R19 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Digit2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F579BB)
    (at 156.972 59.69 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R20 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Digit1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57950)
    (at 121.666 67.31 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R21 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(Digit2-Pad4)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57982)
    (at 149.606 67.31 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R22 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(Digit1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57898)
    (at 123.698 78.74 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R23 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(Digit2-Pad6)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F578B9)
    (at 151.384 78.74 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R24 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Digit1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57881)
    (at 132.588 86.106 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R25 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Digit2-Pad8)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F578CE)
    (at 160.274 86.106 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R26 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Digit1-Pad8)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F578A5)
    (at 138.684 78.74 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R27 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Digit2-Pad10)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F578D6)
    (at 166.624 78.74 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R28 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Digit1-Pad10)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F5796F)
    (at 136.652 67.31 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R29 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Digit2-Pad12)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F5799D)
    (at 164.846 67.31 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R30 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(Digit1-Pad12)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F57935)
    (at 131.318 72.898 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R31 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Digit2-Pad14)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58F578FA)
    (at 159.004 72.898 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R32 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 50R (at 0 2.3 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +24V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(Digit1-Pad14)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58F57A7F)
    (at 130.556 45.212)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -4.953 -7.112) (layer F.SilkS))
    (fp_text value TPIC6B595 (at 0 7.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad12)"))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(Digit2-Pad1)"))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Digit2-Pad3)"))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(Digit2-Pad5)"))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Digit2-Pad7)"))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R1-Pad2)"))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /I_MISO))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(Digit2-Pad9)"))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(Digit2-Pad11)"))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Digit2-Pad13)"))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58F57A87)
    (at 158.242 45.212)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -4.953 -7.112) (layer F.SilkS))
    (fp_text value TPIC6B595 (at 0 7.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad18)"))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Digit1-Pad1)"))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(Digit1-Pad3)"))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(Digit1-Pad5)"))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(Digit1-Pad7)"))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R2-Pad2)"))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /I_MISO))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Digit1-Pad9)"))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Digit1-Pad11)"))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(Digit1-Pad13)"))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module S7S:S7S-display (layer B.Cu) (tedit 58F5BC08)
    (at 130.175 69.85 180)
    (descr "Footprint for 1\" electromechanical seven segment display")
    (fp_text reference Digit2 (at 0 -23.622 180) (layer B.SilkS))
    (fp_text value EM_7SEG (at 0 19.812 180) (layer B.Fab) hide)
    (fp_text user G (at 0 2.032 180) (layer B.SilkS))
    (fp_text user F (at -6.604 8.128 180) (layer B.SilkS))
    (fp_text user E (at -8.382 -3.556 180) (layer B.SilkS))
    (fp_text user D (at -2.286 -11.176 180) (layer B.SilkS))
    (fp_text user C (at 6.604 -3.81 180) (layer B.SilkS))
    (fp_text user B (at 8.636 7.62 180) (layer B.SilkS))
    (fp_text user A (at 2.286 15.494 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0.5334 13.081 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 42 "Net-(Digit2-Pad1)"))
    (pad 2 thru_hole circle (at 4.0894 13.081 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 43 "Net-(Digit2-Pad2)"))
    (pad 3 thru_hole circle (at 6.7056 5.588 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 44 "Net-(Digit2-Pad3)"))
    (pad 4 thru_hole circle (at 10.2616 5.588 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 45 "Net-(Digit2-Pad4)"))
    (pad 5 thru_hole circle (at 4.6736 -5.842 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 46 "Net-(Digit2-Pad5)"))
    (pad 6 thru_hole circle (at 8.2296 -5.842 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 47 "Net-(Digit2-Pad6)"))
    (pad 7 thru_hole circle (at -4.1402 -13.335 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 48 "Net-(Digit2-Pad7)"))
    (pad 8 thru_hole circle (at -0.5842 -13.335 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 49 "Net-(Digit2-Pad8)"))
    (pad 9 thru_hole circle (at -10.3124 -5.842 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 50 "Net-(Digit2-Pad9)"))
    (pad 10 thru_hole circle (at -6.7564 -5.842 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 51 "Net-(Digit2-Pad10)"))
    (pad 11 thru_hole circle (at -8.2804 5.588 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 52 "Net-(Digit2-Pad11)"))
    (pad 12 thru_hole circle (at -4.7244 5.588 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 53 "Net-(Digit2-Pad12)"))
    (pad 13 thru_hole circle (at -1.8034 -0.127 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 54 "Net-(Digit2-Pad13)"))
    (pad 14 thru_hole circle (at 1.7526 -0.127 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 55 "Net-(Digit2-Pad14)"))
  )
  (module S7S:S7S-display (layer B.Cu) (tedit 58F5BBFC)
    (at 157.861 69.85 180)
    (descr "Footprint for 1\" electromechanical seven segment display")
    (fp_text reference Digit1 (at 0 -23.622 180) (layer B.SilkS))
    (fp_text value EM_7SEG (at 0 19.812 180) (layer B.Fab) hide)
    (fp_text user G (at 0 2.032 180) (layer B.SilkS))
    (fp_text user F (at -6.604 8.128 180) (layer B.SilkS))
    (fp_text user E (at -8.382 -3.556 180) (layer B.SilkS))
    (fp_text user D (at -2.286 -11.176 180) (layer B.SilkS))
    (fp_text user C (at 6.604 -3.81 180) (layer B.SilkS))
    (fp_text user B (at 8.636 7.62 180) (layer B.SilkS))
    (fp_text user A (at 2.286 15.494 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0.5334 13.081 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 28 "Net-(Digit1-Pad1)"))
    (pad 2 thru_hole circle (at 4.0894 13.081 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 29 "Net-(Digit1-Pad2)"))
    (pad 3 thru_hole circle (at 6.7056 5.588 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 30 "Net-(Digit1-Pad3)"))
    (pad 4 thru_hole circle (at 10.2616 5.588 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 31 "Net-(Digit1-Pad4)"))
    (pad 5 thru_hole circle (at 4.6736 -5.842 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 32 "Net-(Digit1-Pad5)"))
    (pad 6 thru_hole circle (at 8.2296 -5.842 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 33 "Net-(Digit1-Pad6)"))
    (pad 7 thru_hole circle (at -4.1402 -13.335 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 34 "Net-(Digit1-Pad7)"))
    (pad 8 thru_hole circle (at -0.5842 -13.335 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 35 "Net-(Digit1-Pad8)"))
    (pad 9 thru_hole circle (at -10.3124 -5.842 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 36 "Net-(Digit1-Pad9)"))
    (pad 10 thru_hole circle (at -6.7564 -5.842 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 37 "Net-(Digit1-Pad10)"))
    (pad 11 thru_hole circle (at -8.2804 5.588 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 38 "Net-(Digit1-Pad11)"))
    (pad 12 thru_hole circle (at -4.7244 5.588 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 39 "Net-(Digit1-Pad12)"))
    (pad 13 thru_hole circle (at -1.8034 -0.127 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 40 "Net-(Digit1-Pad13)"))
    (pad 14 thru_hole circle (at 1.7526 -0.127 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 41 "Net-(Digit1-Pad14)"))
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58F57730)
    (at 131.572 96.012)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at -4.953 -7.112) (layer F.SilkS))
    (fp_text value TPIC6B595 (at 0 7.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad18)"))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Digit2-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(Digit2-Pad4)"))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(Digit2-Pad6)"))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Digit2-Pad8)"))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R17-Pad2)"))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /I_MISO))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Digit2-Pad10)"))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Digit2-Pad12)"))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Digit2-Pad14)"))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U5-Pad17)"))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U5-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58F577F1)
    (at 159.512 96.012)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at -4.953 -7.112) (layer F.SilkS))
    (fp_text value TPIC6B595 (at 0 7.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U5-Pad18)"))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Digit1-Pad2)"))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(Digit1-Pad4)"))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(Digit1-Pad6)"))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Digit1-Pad8)"))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R18-Pad2)"))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /I_MISO))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Digit1-Pad10)"))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(Digit1-Pad12)"))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(Digit1-Pad14)"))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U6-Pad17)"))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U6-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 58F57684)
    (at 145.288 113.792)
    (descr "Crystal Quarz HC49/U vertical stehend")
    (tags "Crystal Quarz HC49/U vertical stehend")
    (fp_text reference Y1 (at 6.731 1.651) (layer F.SilkS))
    (fp_text value Crystal (at 0 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 3 "Net-(C6-Pad2)"))
    (pad 2 thru_hole circle (at 2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask)
      (net 4 "Net-(C7-Pad2)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58F4BF01)
    (at 168.275 37.973)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58F4BEE5)
    (at 120.015 37.973)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58F4BF16)
    (at 168.275 109.22)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58F4BF25)
    (at 120.015 109.22)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module interrologo:interrologo-12.7mm (layer B.Cu) (tedit 0)
    (at 163.195 100.33 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module custom-parts:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 58F5B8AB)
    (at 125.603 108.712 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J5 (at 1.27 -2.286 90) (layer F.SilkS) hide)
    (fp_text value CONN_02X03 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /I_MISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /I_SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /I_MOSI))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /I_RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text gnd (at 136.652 112.141) (layer B.SilkS))
  (gr_text gnd (at 136.652 112.141) (layer F.SilkS))
  (gr_text "connect to serial, send \"help\" for usage\n8N1, default speed 9600\nbitbucket.org/pjhardy/vane-display\nPeter Hardy <peter@hardy.dropbear.id.au>" (at 156.083 100.584) (layer B.SilkS))
  (gr_text "electromechanical 7-segment display driver" (at 144.145 43.815) (layer B.SilkS))
  (gr_text ICSP (at 123.19 105.283 90) (layer B.SilkS))
  (gr_text ICSP (at 123.19 105.283 90) (layer F.SilkS))
  (gr_line (start 116.586 116.078) (end 116.586 36.83) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.418 118.364) (end 118.872 118.364) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.704 36.83) (end 171.704 116.078) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.872 34.544) (end 169.418 34.544) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 118.872 116.078) (end 118.872 118.364) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 169.418 116.078) (end 171.704 116.078) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 169.418 36.83) (end 169.418 34.544) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 118.872 36.83) (end 116.586 36.83) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text i2c (at 123.698 111.125) (layer F.SilkS))
  (gr_text serial (at 134.112 111.125) (layer F.SilkS))
  (gr_text scl (at 121.158 112.141) (layer F.SilkS))
  (gr_text sda (at 123.698 112.141) (layer F.SilkS))
  (gr_text gnd (at 126.238 112.141) (layer F.SilkS))
  (gr_text rx (at 131.572 112.141) (layer F.SilkS))
  (gr_text tx (at 134.112 112.141) (layer F.SilkS))
  (gr_text scl (at 121.285 112.141) (layer B.SilkS))
  (gr_text sda (at 123.698 112.141) (layer B.SilkS))
  (gr_text i2c (at 123.698 111.125) (layer B.SilkS))
  (gr_text gnd (at 126.238 112.141) (layer B.SilkS))
  (gr_text tx (at 134.112 112.141) (layer B.SilkS))
  (gr_text rx (at 131.572 112.141) (layer B.SilkS))
  (gr_text serial (at 134.112 111.125) (layer B.SilkS))
  (gr_text - (at 166.878 114.427) (layer B.SilkS))
  (gr_text + (at 158.75 114.427) (layer B.SilkS))
  (gr_text 5V (at 162.941 111.633) (layer B.SilkS))
  (gr_text - (at 166.878 114.427) (layer F.SilkS))
  (gr_text + (at 158.75 114.427) (layer F.SilkS))
  (gr_text 5V (at 162.941 111.633) (layer F.SilkS))
  (gr_text - (at 137.922 38.481) (layer B.SilkS))
  (gr_text + (at 145.923 38.481) (layer B.SilkS))
  (gr_text 19V (at 141.986 41.529) (layer B.SilkS))
  (gr_text - (at 137.922 38.481) (layer F.SilkS))
  (gr_text + (at 145.923 38.481) (layer F.SilkS))
  (gr_text 19V (at 141.986 41.529) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.22606))
    (min_thickness 0.22606)
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 171.704 118.364) (xy 116.586 118.364) (xy 116.586 34.544) (xy 171.704 34.544)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.22606))
    (min_thickness 0.22606)
    (fill yes (arc_segments 16) (thermal_gap 1.016) (thermal_bridge_width 1.016))
    (polygon
      (pts
        (xy 171.704 118.364) (xy 116.586 118.364) (xy 116.586 34.544) (xy 171.704 34.544)
      )
    )
  )
)
