(kicad_pcb (version 20171130) (host pcbnew 5.1.8-db9833491~88~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 71)
    (zones 0)
    (modules 4)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.425 1.75)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 111.379 92.202)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "C:/HotWheels/Hotwheels-Firmware/Documents/PCB_Farbsensor/HotwheelsBoard-Farbsensor/Output/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad6)")
  (net 5 "Net-(J1-Pad7)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 VCC)
  (net 8 "Net-(R1-Pad1)")
  (net 9 "Net-(C1-Pad2)")
  (net 10 "Net-(U1-Pad2)")
  (net 11 "Net-(U1-Pad3)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net VCC)
  )
  (module castellated_pads_bottom:DIP-10_Ver2 (layer F.Cu) (tedit 5FC64B4F)
    (at 101.575 104.175)
    (fp_text reference U1 (at -0.76748 4.04678 90) (layer F.SilkS))
    (fp_text value Castellated_pads_bottom (at 6.1337 13.04854) (layer F.Fab))
    (pad 10 smd roundrect (at 11.4 7.75) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at 11.4 0.05) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(R1-Pad1)"))
    (pad 9 smd roundrect (at 8.95 7.75) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad6)"))
    (pad 2 smd roundrect (at 8.95 0.05) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(U1-Pad2)"))
    (pad 8 smd roundrect (at 6.5 7.75) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad7)"))
    (pad 3 smd roundrect (at 6.5 0.05) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(U1-Pad3)"))
    (pad 7 smd roundrect (at 4.05 7.75) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 smd roundrect (at 4.05 0.05) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C1-Pad2)"))
    (pad 6 smd roundrect (at 1.6 7.75) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad1)"))
    (pad 5 smd roundrect (at 1.6 0.05) (size 1.7 1.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad3)"))
  )
  (module Connector_PinSocket_1.00mm:PinSocket_1x07_P1.00mm_Vertical (layer F.Cu) (tedit 5FBFA7C0)
    (at 105.08 114.478 90)
    (descr "Through hole straight socket strip, 1x07, 1.00mm pitch, single row (https://gct.co/files/drawings/bc065.pdf), script generated")
    (tags "Through hole socket strip THT 1x07 1.00mm single row")
    (fp_text reference J1 (at -0.3046 -1.97378 90) (layer F.SilkS))
    (fp_text value "Main Connector" (at 1.651 3.302 180) (layer Cmts.User))
    (fp_text user %R (at -0.29 3 180) (layer F.Fab))
    (pad 7 thru_hole oval (at 0 6 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 5 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 4 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 3 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 VCC))
    (pad 3 thru_hole oval (at 0 2 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 1 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_1.00mm.3dshapes/PinSocket_1x07_P1.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer B.Cu) (tedit 5FBFFEA6)
    (at 110.795 102.032 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -2.794 1.27 180) (layer B.SilkS))
    (fp_text value 1500R (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217)
      (net 7 VCC))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5FC64C3E)
    (at 106.096 102.032)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -3.429 -1.27 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175)
      (net 9 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175)
      (net 7 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Sotaro v1.0" (at 108.11002 107.7341) (layer B.SilkS))
  (gr_circle (center 114.605 114.425) (end 115.38 114.425) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 101.545 114.425) (end 102.32 114.425) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 114.605 102.075) (end 115.38 102.075) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 101.545 102.075) (end 102.32 102.075) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100 100) (end 116.15 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.15 100) (end 116.15 116.15) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 116.15) (end 116.15 116.15) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 100) (end 100 116.15) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 100) (xy 100 116.129) (xy 116.129 116.129) (xy 116.129 100) (xy 116.129 99.873)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 100) (xy 100 116.129) (xy 116.129 116.129) (xy 116.129 100)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.78668 111.59998) (xy 101.57206 111.59998) (xy 101.57206 109.81944) (xy 106.78668 109.81944)
      )
    )
  )
)
