(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 22)
    (zones 0)
    (modules 6)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.7)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 "Net-(P2-Pad2)")
  (net 3 GND)
  (net 4 "Net-(Q1-Pad2)")
  (net 5 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.7)
    (via_drill 0.4)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net VCC)
  )
  (module Terminal_Blocks:TerminalBlock_bornier-3_P5.08mm (layer F.Cu) (tedit 59FF03B9)
    (at 31.115 27.94)
    (descr "simple 3-pin terminal block, pitch 5.08mm, revamped version of bornier3")
    (tags "terminal block bornier3")
    (fp_text reference P2 (at 5.05 -4.65) (layer F.SilkS))
    (fp_text value "1-Wire Bus" (at 5.08 5.08) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 "Net-(P2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-3_P5.08mm.wrl
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 33.02 38.1 270)
    (descr "TO-92 leads molded, narrow, oval pads, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 3.81) (layer F.SilkS))
    (fp_text value BS170 (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 1.27 3.81) (layer F.Fab))
    (pad 3 thru_hole oval (at 2.54 0 315) (size 1.8 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 315) (size 1.3 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(P2-Pad2)"))
    (pad 2 thru_hole oval (at 1.27 -1.27) (size 1.8 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow_Oval.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 39.925 36.195 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(P2-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 39.925 32.385 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(P2-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 40.72 45.085 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 2.2K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module wemos_d1_mini:wemos-d1-mini-DIL-only (layer B.Cu) (tedit 5C0440C4)
    (at 36.195 40.64 90)
    (fp_text reference U1 (at -19.3 0) (layer B.SilkS) hide)
    (fp_text value WeMos_mini (at -2.54 -15.875 90) (layer B.Fab) hide)
    (pad 16 thru_hole circle (at -8.89 11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 1 thru_hole circle (at -8.89 -11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -6.35 11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at -6.35 -11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 14 thru_hole circle (at -3.81 11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 -11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at -1.27 11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -1.27 -11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 1.27 11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 1.27 -11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 3.81 11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 3.81 -11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 6.35 11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 6.35 -11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 8.89 11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 8.89 -11.43 90) (size 1.8 1.8) (drill 1.016) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/SLW-108-01-G-S.wrl
      (offset (xyz 0 -11.39999982878918 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/SLW-108-01-G-S.wrl
      (offset (xyz 0 11.39999982878918 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/TSW-108-05-G-S.wrl
      (offset (xyz 0 -11.39999982878918 7.299999890364999))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 90 0 0))
    )
    (model ${KIPRJMOD}/3dshapes/wemos_d1_mini.3dshapes/TSW-108-05-G-S.wrl
      (offset (xyz 0 11.39999982878918 7.299999890364999))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 90 0 0))
    )
  )
  (gr_text 1Wire (at 36.195 33.655) (layer F.SilkS))
  (gr_text Gnd (at 30.48 33.655) (layer F.SilkS))
  (gr_text Vcc (at 41.91 33.655) (layer F.SilkS))
  (gr_text "Wireless\nDS18B20\nV2.0" (at 40.64 45.72) (layer F.SilkS))
  (gr_text 9 (at 45.72 32.258) (layer F.Fab))
  (gr_text 1 (at 26.67 49.403) (layer F.Fab))
  (gr_line (start 22.86 25.908) (end 22.86 50.8) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 24.892 25.908) (end 24.892 23.876) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.498 23.876) (end 24.892 23.876) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 47.498 25.908) (end 49.53 25.908) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.53 50.8) (end 49.53 25.908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 22.86 50.8) (end 49.53 50.8) (layer Edge.Cuts) (width 0.1))
)
