(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1~bpo10+1)
  (general
    (thickness 1.6)
    (drawings 32)
    (tracks 33)
    (zones 0)
    (modules 10)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2032)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.905 1.0668)
    (pad_drill 0.65)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 /SPI4_SCK)
  (net 4 /~FLASH_CS~)
  (net 5 /SPI4_MISO)
  (net 6 /SPI4_MOSI)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /SPI4_MISO)
    (add_net /SPI4_MOSI)
    (add_net /SPI4_SCK)
    (add_net /~FLASH_CS~)
    (add_net GND)
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer F.Cu) (tedit 5F033DAF)
    (at 85.09 65.405 90)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 1.695 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer F.Cu) (tedit 5F033DA0)
    (at 83.185 53.34)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference J9 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 1.695) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer F.Cu) (tedit 5F033D6B)
    (at 98.425 52.07)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference J8 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 1.695) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer F.Cu) (tedit 5F033D7D)
    (at 98.425 50.8)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference J7 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 1.695) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer F.Cu) (tedit 5F033D59)
    (at 98.425 54.61)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference J6 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 1.695) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x01_P1.27mm_Vertical (layer F.Cu) (tedit 5F033D8B)
    (at 98.425 48.26)
    (descr "Through hole straight pin header, 1x01, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.27mm single row")
    (fp_text reference J5 (at 0 -1.695) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 1.695) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x01_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical (layer F.Cu) (tedit 5F033D46)
    (at 98.425 58.42)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (fp_text reference J1 (at -1.27 -1.905) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 5.505) (layer F.Fab))
    (fp_text user %R (at 0 1.905 90) (layer F.Fab))
    (pad 4 thru_hole rect (at 0 3.81) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /SPI4_SCK))
    (pad 3 thru_hole rect (at 0 2.54) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /~FLASH_CS~))
    (pad 2 thru_hole rect (at 0 1.27) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 /SPI4_MISO))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 1.0668) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /SPI4_MOSI))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 93.98 51.435 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.54 0) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 87.63 51.435)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.54 0) (layer B.SilkS))
    (fp_text value 4k7 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 /~FLASH_CS~))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOIC-8_W5.6mm (layer B.Cu) (tedit 5D28A58E)
    (at 90.805 46.355 90)
    (attr smd)
    (fp_text reference U1 (at 1.905 -5.715 180) (layer B.SilkS))
    (fp_text value W25Q128JVSSIQ_TR (at 3.81 -0.635 180) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 8 smd rect (at -1.905 3.65 90) (size 0.65 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 7 smd rect (at -0.635 3.65 90) (size 0.65 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 6 smd rect (at 0.635 3.65 90) (size 0.65 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /SPI4_SCK))
    (pad 5 smd rect (at 1.905 3.65 90) (size 0.65 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /SPI4_MOSI))
    (pad 4 smd rect (at 1.905 -3.65 90) (size 0.65 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.635 -3.65 90) (size 0.65 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -0.635 -3.65 90) (size 0.65 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /SPI4_MISO))
    (pad 1 smd rect (at -1.905 -3.65 90) (size 0.65 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /~FLASH_CS~))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIJ-8_5.3x5.3mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 84.455 64.135) (end 84.455 53.975) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.885 64.135) (end 84.455 64.135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.885 53.975) (end 95.885 64.135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.455 53.975) (end 95.885 53.975) (layer Edge.Cuts) (width 0.1))
  (gr_text "STLINK\nV3MINI\nFLASH" (at 90.805 48.26) (layer F.SilkS))
  (gr_line (start 81.28 67.31) (end 81.28 42.545) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.33 67.31) (end 81.28 67.31) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100.33 42.545) (end 100.33 67.31) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 81.28 42.545) (end 100.33 42.545) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 80.645 41.91) (xy 100.965 41.91) (xy 100.965 67.31) (xy 80.645 67.31)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 80.01 52.07) (xy 80.01 41.275) (xy 101.6 41.275) (xy 101.6 67.945) (xy 80.01 67.945)
      )
    )
  )
)
