(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "-12V")
  (net 4 "Net-(D1-COM)")
  (net 5 "Net-(D2-COM)")
  (net 6 "/FACE")
  (net 7 "Net-(J1-Pin_1)")
  (net 8 "Net-(J1-Pin_10)")
  (net 9 "Net-(C4-Pad2)")
  (net 10 "/A'")
  (net 11 "/A_dc'")
  (net 12 "/B'")
  (net 13 "/B_dc'")
  (net 14 "/OUT_dc'")
  (net 15 "/OUT'")
  (net 16 "/GND'")
  (net 17 "unconnected-(J8-PadTN)")
  (net 18 "unconnected-(J9-PadTN)")
  (net 19 "unconnected-(J10-PadTN)")
  (net 20 "Net-(U1-carrier_in)")
  (net 21 "Net-(R4-Pad2)")
  (net 22 "Net-(U1-in_carrier)")
  (net 23 "Net-(R7-Pad2)")
  (net 24 "Net-(R10-Pad2)")
  (net 25 "Net-(R12-Pad1)")
  (net 26 "Net-(R13-Pad1)")
  (net 27 "Net-(R13-Pad2)")
  (net 28 "Net-(U1-bias)")
  (net 29 "Net-(U2A--)")
  (net 30 "Net-(R16-Pad2)")
  (net 31 "Net-(R17-Pad1)")
  (net 32 "Net-(U2A-+)")
  (net 33 "Net-(R21-Pad2)")
  (net 34 "Net-(U2B--)")
  (net 35 "Net-(R23-Pad2)")
  (net 36 "Net-(U1-gain-Pad2)")
  (net 37 "unconnected-(U1-n{slash}c-Pad7)")
  (net 38 "unconnected-(U1-n{slash}c-Pad9)")
  (net 39 "unconnected-(U1-n{slash}c-Pad11)")
  (net 40 "unconnected-(U1-n{slash}c-Pad13)")
  (net 41 "/_OUT")
  (net 42 "unconnected-(J2-Pin_3-Pad3)")
  (net 43 "/_OUT'")
  (net 44 "unconnected-(J3-Pin_3-Pad3)")
  (net 45 "/_A'")
  (net 46 "/_A")
  (net 47 "/_B'")
  (net 48 "/_B")
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 117.454 76.634 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -3.113 -0.127 90) (layer "F.SilkS"))
    (fp_text value "2.7K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.065 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 137.012 76.888 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 3.1989 0.0508 90) (layer "F.SilkS"))
    (fp_text value "15K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 32 "Net-(U2A-+)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 107.0195 81.46 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.8145 -0.254) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(D1-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(J1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 141.584 76.888 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 3.1989 0.0508 90) (layer "F.SilkS"))
    (fp_text value "15K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 29 "Net-(U2A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 30 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 115.168 76.634 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at -3.113 -0.127 90) (layer "F.SilkS"))
    (fp_text value "6.8K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 28 "Net-(U1-bias)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 123.55 80.952 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.778 90) (layer "F.SilkS"))
    (fp_text value "2.7K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 27 "Net-(R13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 119.74 76.634 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at -3.113 -0.127 90) (layer "F.SilkS"))
    (fp_text value "180K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 48 "/_B") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 149.352 108.278)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H10" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 139.298 76.8865 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at -3.1989 -0.1016 90) (layer "F.SilkS"))
    (fp_text value "15K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 31 "Net-(R17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 32 "Net-(U2A-+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 112.8708 88.826 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -2.7635 0.0112 90) (layer "F.SilkS"))
    (fp_text value "180K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 46 "/_A") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 20 "Net-(U1-carrier_in)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 140.822 89.08 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at -3.302 0 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 33 "Net-(R21-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 34 "Net-(U2B--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 107.17 87.81 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D2" (at -2.54 -2.416 90) (layer "F.SilkS"))
    (fp_text value "BAT54S" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D2-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 94.086 87.063)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 2.54 -0.523) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0 6.917) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 46 "/_A") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "/_B") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 136.504 81.355 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at -0.0034 -1.6764 90) (layer "F.SilkS"))
    (fp_text value "1.2K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 31 "Net-(R17-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 96.8 124.56)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H1" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount0" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "output"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 107.0195 84 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.8145 -0.254) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "Net-(D2-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(J1-Pin_10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 107.104 77.65 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D1" (at 2.54 -2.35 90) (layer "F.SilkS"))
    (fp_text value "BAT54S" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 145.14 83.895 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at -0.024 2.032 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 96.8 158.21)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H4" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 143.108 89.08 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 3.2019 0.0508 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 35 "Net-(R23-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 41 "/_OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (at 141.224 137.943)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H7" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "out" (at 0 -10.3 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 127.106 84.762 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "1.5K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 123.55 84.762 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at -0.189 1.778 90) (layer "F.SilkS"))
    (fp_text value "6.8K" (at 0.065 -1.524 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(R13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 27 "Net-(R13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 102.7176 101.9286 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J8" (at -5.9944 -3.4544 180 unlocked) (layer "F.SilkS"))
    (fp_text value "carrier" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 16 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 16 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "/A_dc'") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(J8-PadTN)") (pintype "passive+no_connect"))
    (model "/home/pstiverson/Projects/AR-808/hardware/EurorackKiCAD/Eurorack.pretty/models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 147.4 124.56)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H2" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 112.882 76.634 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at -3.113 0 90) (layer "F.SilkS"))
    (fp_text value "1.2K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 30 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 117.454 88.826 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 2.7635 -0.0112 90) (layer "F.SilkS"))
    (fp_text value "2.7K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 20 "Net-(U1-carrier_in)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 140.949 82.944 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "595-TL072CDR")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8")
    (property "ki_keywords" "dual opamp")
    (attr smd)
    (fp_text reference "U2" (at -2.605 -3.4 90) (layer "F.SilkS"))
    (fp_text value "TL072" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(R21-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(U2A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U2A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(U2B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(R23-Pad2)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 94.742 82.222)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H9" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 115.168 88.826 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 2.7635 -0.1382 90) (layer "F.SilkS"))
    (fp_text value "12K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 20 "Net-(U1-carrier_in)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 21 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 119.74 88.826 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.7635 -0.0042 90) (layer "F.SilkS"))
    (fp_text value "2.7K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 22 "Net-(U1-in_carrier)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 122.026 88.826 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 2.7635 -0.0042 90) (layer "F.SilkS"))
    (fp_text value "12K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 22 "Net-(U1-in_carrier)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 23 "Net-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 147.4 158.21)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H3" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 138.536 89.08 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 3.2019 -0.0508 90) (layer "F.SilkS"))
    (fp_text value "68K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 34 "Net-(U2B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 35 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Input" (layer "F.Cu")
    (at 102.7176 146.7196)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H5" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "carrier" (at 0 -10.3 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 149.987 73.3)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at -2.7404 -0.5028) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Socket" (at 0.89 7.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 41 "/_OUT") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(J2-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (at 116.692 82.73 -90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "863-MC1496BDR2G")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Balanced Modulators/Demodulators")
    (attr smd)
    (fp_text reference "U1" (at 0 -5.28 90) (layer "F.SilkS"))
    (fp_text value "MC1496" (at 0 5.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R13-Pad2)") (pinfunction "input") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -2.54 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(U1-gain-Pad2)") (pinfunction "gain") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.27 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(U1-gain-Pad2)") (pinfunction "gain") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(R10-Pad2)") (pinfunction "input") (pintype "input"))
    (pad "5" smd roundrect (at -2.475 1.27 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(U1-bias)") (pinfunction "bias") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(R16-Pad2)") (pinfunction "output") (pintype "output"))
    (pad "7" smd roundrect (at -2.475 3.81 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "unconnected-(U1-n{slash}c-Pad7)") (pinfunction "n/c") (pintype "no_connect"))
    (pad "8" smd roundrect (at 2.475 3.81 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U1-in_carrier)") (pinfunction "in_carrier") (pintype "input"))
    (pad "9" smd roundrect (at 2.475 2.54 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "unconnected-(U1-n{slash}c-Pad9)") (pinfunction "n/c") (pintype "no_connect"))
    (pad "10" smd roundrect (at 2.475 1.27 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(U1-carrier_in)") (pinfunction "carrier_in") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "unconnected-(U1-n{slash}c-Pad11)") (pinfunction "n/c") (pintype "no_connect"))
    (pad "12" smd roundrect (at 2.475 -1.27 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(R17-Pad1)") (pinfunction "output") (pintype "output"))
    (pad "13" smd roundrect (at 2.475 -2.54 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "unconnected-(U1-n{slash}c-Pad13)") (pinfunction "n/c") (pintype "no_connect"))
    (pad "14" smd roundrect (at 2.475 -3.81 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "V_ee") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 127.106 80.952 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 1.6764 90) (layer "F.SilkS"))
    (fp_text value "1.5K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 94.742 107.262)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H8" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 141.224 104.328 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J10" (at 4.064 -5.842 180 unlocked) (layer "F.SilkS"))
    (fp_text value "out" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 16 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 16 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 14 "/OUT_dc'") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(J10-PadTN)") (pintype "passive+no_connect"))
    (model "/home/pstiverson/Projects/AR-808/hardware/EurorackKiCAD/Eurorack.pretty/models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Input" (layer "F.Cu")
    (at 102.7176 135.5436)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H6" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "modulating" (at 0 -10.3 unlocked) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 102.7176 113.1046 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J9" (at -6.0452 3.6576 180 unlocked) (layer "F.SilkS"))
    (fp_text value "modulating" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 16 "/GND'") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 16 "/GND'") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 13 "/B_dc'") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J9-PadTN)") (pintype "passive+no_connect"))
    (model "/home/pstiverson/Projects/AR-808/hardware/EurorackKiCAD/Eurorack.pretty/models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 143.87 76.888 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 3.2497 0 90) (layer "F.SilkS"))
    (fp_text value "15K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 29 "Net-(U2A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 33 "Net-(R21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" (layer "F.Cu")
    (at 149.352 83.238)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H11" (at 0 -3.7) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 122.026 76.634 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at -3.113 -0.127 90) (layer "F.SilkS"))
    (fp_text value "6.8K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 25 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "B.Cu")
    (at 133.2738 109.5756 90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 3-pole, pins 1+2 closed/bridged")
    (property "ki_keywords" "Jumper SPDT")
    (attr through_hole)
    (fp_text reference "JP3" (at -0.0954 2.1486 90) (layer "B.SilkS"))
    (fp_text value "Jumper_3_Bridged12" (at 4.385 -7.35 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "/OUT'") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "/_OUT'") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "/OUT_dc'") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 149.987 98.34 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 2.7178 0.9586 180) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/GND'") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 43 "/_OUT'") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(J3-Pin_3-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "B.Cu")
    (at 124.6124 109.5734 90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 3-pole, pins 1+2 closed/bridged")
    (property "ki_keywords" "Jumper SPDT")
    (attr through_hole)
    (fp_text reference "JP1" (at -0.2478 2.1486 90) (layer "B.SilkS"))
    (fp_text value "Jumper_3_Bridged12" (at 4.385 -7.35 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/A'") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "/_A'") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/A_dc'") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal" (layer "B.Cu")
    (at 115.951 109.5734 90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 3-pole, pins 1+2 closed/bridged")
    (property "ki_keywords" "Jumper SPDT")
    (attr through_hole)
    (fp_text reference "JP2" (at -0.0954 2.047 90) (layer "B.SilkS"))
    (fp_text value "Jumper_3_Bridged12" (at 4.385 -7.35 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/B'") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "/_B'") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/B_dc'") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:PinHeader_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 103.614 77.65 180)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (property "PartNum" "A-2939")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -4.4323 4.4831) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.2446 -16.2052) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:C_Rect_Horizontal_L7.2mm_W11" (layer "B.Cu")
    (at 135.3566 115.1614 90)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at 0 -0.4507 270 unlocked) (layer "B.SilkS"))
    (fp_text value "1u box" (at 0 -1 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 270 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at -2.5 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 14 "/OUT_dc'") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 15 "/OUT'") (pintype "passive"))
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "B.Cu")
    (at 132.186 86.096 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Trim-potentiometer")
    (property "ki_keywords" "resistor variable trimpot trimmer")
    (attr through_hole)
    (fp_text reference "RV1" (at -2.54 3.66 90) (layer "B.SilkS"))
    (fp_text value "500" (at -2.54 -3.67 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 -0.005 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 21 "Net-(R4-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(R7-Pad2)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 109.964 89.269113 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at -2.096887 -1.654) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 109.964 78.601113 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at -2.096887 -1.654) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "B.Cu")
    (at 132.186 75.428 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Trim-potentiometer")
    (property "ki_keywords" "resistor variable trimpot trimmer")
    (attr through_hole)
    (fp_text reference "RV2" (at -2.54 3.66 90) (layer "B.SilkS"))
    (fp_text value "200" (at -2.54 -3.67 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 -0.005 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(R12-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "Net-(R13-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:C_Rect_Horizontal_L7.2mm_W11" (layer "B.Cu")
    (at 109.9599 115.1722 90)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 0 -0.3589 270 unlocked) (layer "B.SilkS"))
    (fp_text value "1u box" (at 0 -1 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 270 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at -2.5 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 12 "/B'") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 13 "/B_dc'") (pintype "passive"))
  )
  (footprint "Eurorack:C_Rect_Horizontal_L7.2mm_W11" (layer "B.Cu")
    (at 122.6599 115.1722 90)
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 0 -0.3589 270 unlocked) (layer "B.SilkS"))
    (fp_text value "1u box" (at 0 -1 270 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 270 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at -2.5 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 10 "/A'") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.524 1.524) (drill 0.762) (layers "*.Cu" "*.Mask")
      (net 11 "/A_dc'") (pintype "passive"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (at 94.086 112.103 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -2.286 -2.8298 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x03_Pin" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "/GND'") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 45 "/_A'") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 47 "/_B'") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 125.074 91.047113 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "balanced-modulator.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at -0.941575 3.5206 90) (layer "B.SilkS"))
    (fp_text value "100u 16V" (at 1.25 -3.75 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 91.8 121.56) (end 152.4 161.21)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 91.8 96.52) (end 152.4 119.02)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 91.8 71.48) (end 152.4 93.98)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "ac" (at 132.0292 98.8568) (layer "B.SilkS"))
  (gr_text "dc" (at 129.4892 98.8568) (layer "B.SilkS"))
  (gr_text "dc" (at 112.141 98.8568) (layer "B.SilkS"))
  (gr_text "car" (at 125.222 98.118) (layer "B.SilkS"))
  (gr_text "ac" (at 123.296 98.88) (layer "B.SilkS"))
  (gr_text "ac" (at 114.681 98.8568) (layer "B.SilkS"))
  (gr_text "dc" (at 120.756 98.88) (layer "B.SilkS"))
  (gr_text "mod" (at 116.967 98.0948) (layer "B.SilkS"))
  (gr_text "out" (at 134.3152 98.0948) (layer "B.SilkS"))
  (gr_text "thismatters/balanced-modulator/v0" (at 137.033 72.2122) (layer "B.SilkS"))
  (gr_text "balanced modulator" (at 122.809 160.401) (layer "F.SilkS"))
  (gr_text "thismatters/balanced-modulator/v0" (at 109.7788 97.3074) (layer "F.SilkS"))
  (gr_text "carrier" (at 108.077 135.509) (layer "F.SilkS"))
  (gr_text "thismatters/balanced-modulator/v0" (at 92.71 127.254 270) (layer "F.SilkS"))
  (gr_text "modulating" (at 108.077 146.685) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 91.038 70.772)
        (xy 153.014 70.772)
        (xy 153.014 94.648)
        (xy 91.038 94.648)
      )
    )
  )
  (zone (net 16) (net_name "/GND'") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 91.038 95.832)
        (xy 153.014 95.832)
        (xy 153.014 119.708)
        (xy 91.038 119.708)
      )
    )
  )
  (zone (net 6) (net_name "/FACE") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 91.038 121.004)
        (xy 153.014 121.004)
        (xy 153.014 162.152)
        (xy 91.038 162.152)
      )
    )
  )
)
