(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 60)
    (no_connects 0)
    (area 93.394999 74.3288 247.356002 100.703)
    (thickness 1.6)
    (drawings 4)
    (tracks 314)
    (zones 0)
    (modules 27)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 20 12)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /I2C_SCL)
  (net 3 /TOUCH_RST)
  (net 4 /I2C_SDA)
  (net 5 /TOUCH_CHG)
  (net 6 +3V3)
  (net 7 "Net-(R2-Pad2)")
  (net 8 "Net-(R3-Pad2)")
  (net 9 "Net-(R4-Pad2)")
  (net 10 "Net-(R5-Pad2)")
  (net 11 "Net-(R6-Pad2)")
  (net 12 "Net-(U2-Pad1)")
  (net 13 "Net-(U2-Pad2)")
  (net 14 "Net-(U2-Pad3)")
  (net 15 "Net-(U2-Pad4)")
  (net 16 "Net-(U2-Pad5)")
  (net 17 "Net-(U2-Pad6)")
  (net 18 "Net-(U2-Pad7)")
  (net 19 "Net-(U2-Pad8)")
  (net 20 "Net-(U2-Pad11)")
  (net 21 "Net-(U2-Pad14)")
  (net 22 "Net-(U2-Pad19)")
  (net 23 "Net-(U2-Pad20)")
  (net 24 "Net-(D4-Pad2)")
  (net 25 "Net-(D3-Pad2)")
  (net 26 "Net-(D2-Pad2)")
  (net 27 "Net-(D1-Pad2)")
  (net 28 "Net-(U2-Pad21)")
  (net 29 "Net-(D1-Pad1)")
  (net 30 "Net-(D2-Pad1)")
  (net 31 "Net-(D3-Pad1)")
  (net 32 "Net-(D4-Pad1)")
  (net 33 "Net-(U2-Pad28)")
  (net 34 /GUARD)
  (net 35 /TOUCH1)
  (net 36 /TOUCH2)
  (net 37 /TOUCH3)
  (net 38 /TOUCH4)
  (net 39 "Net-(U1-Pad7)")
  (net 40 "Net-(U1-Pad8)")
  (net 41 "Net-(U2-Pad26)")
  (net 42 "Net-(U2-Pad27)")
  (net 43 "Net-(P2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /I2C_SCL)
    (add_net /I2C_SDA)
    (add_net /TOUCH1)
    (add_net /TOUCH2)
    (add_net /TOUCH3)
    (add_net /TOUCH4)
    (add_net /TOUCH_CHG)
    (add_net /TOUCH_RST)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
  )
  (net_class Guard ""
    (clearance 1)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /GUARD)
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 113.792 82.9564 270)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value AT42QT1070 (at 0 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at -2.54 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.27 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 /I2C_SDA))
    (pad 4 smd rect (at 0 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 /TOUCH_RST))
    (pad 5 smd rect (at 1.27 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /TOUCH_CHG))
    (pad 6 smd rect (at 2.54 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 /I2C_SCL))
    (pad 7 smd rect (at 3.81 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 3.81 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 2.54 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (pad 11 smd rect (at 0 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (pad 12 smd rect (at -1.27 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R3-Pad2)"))
    (pad 13 smd rect (at -2.54 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R2-Pad2)"))
    (pad 14 smd rect (at -3.81 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.27 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03 (layer B.Cu) (tedit 0)
    (at 107.62 81.2038 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 5.1 180) (layer B.SilkS))
    (fp_text value CONN_02X03 (at 0 3.1 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 /I2C_SCL))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 /TOUCH_RST))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 /I2C_SDA))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 /TOUCH_CHG))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 541A9C03)
    (at 121.717 78.8924 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value C (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 122.58 88.3666 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /TOUCH_CHG))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 141.961 79.0956 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 4.7k-20k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 /GUARD))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 149.301 83.1596)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 /TOUCH1))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 149.377 86.4616 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 /TOUCH2))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 182.651 89.7382 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 /TOUCH3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 215.24 92.8116 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 38 /TOUCH4))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 104.8 91.7448 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 47k (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /TOUCH_RST))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 129.032 79.502)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 4.7k (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /I2C_SDA))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 228.448 94.7928 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 1.2k (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 195.555 94.869 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 1.2k (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 162.408 94.7928 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 1.2k (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 129.54 94.9706 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value 1.2k (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-28_5.3x10.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 112.344 93.2942 90)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 -6.25 90) (layer F.SilkS))
    (fp_text value MCP23017 (at 0 6.25 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -3.6 -3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -3.6 -2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -3.6 -2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -3.6 -0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -3.6 -0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -3.6 0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at -3.6 0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 10 smd rect (at -3.6 1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -3.6 2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at -3.6 2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 /I2C_SCL))
    (pad 13 smd rect (at -3.6 3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 /I2C_SDA))
    (pad 14 smd rect (at -3.6 4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 3.6 4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P2-Pad1)"))
    (pad 16 smd rect (at 3.6 3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 3.6 2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 3.6 2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 /TOUCH_RST))
    (pad 19 smd rect (at 3.6 1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 3.6 0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 3.6 0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 3.6 -0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D1-Pad1)"))
    (pad 23 smd rect (at 3.6 -0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D2-Pad1)"))
    (pad 24 smd rect (at 3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D3-Pad1)"))
    (pad 25 smd rect (at 3.6 -2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D4-Pad1)"))
    (pad 26 smd rect (at 3.6 -2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad26)"))
    (pad 27 smd rect (at 3.6 -3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 3.6 -4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad28)"))
    (model Housings_SSOP.3dshapes/SSOP-28_5.3x10.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:LED1206_rev_mount (layer F.Cu) (tedit 57FF83A8)
    (at 232.004 88.011)
    (tags LED)
    (fp_text reference D4 (at 3.8 0) (layer F.SilkS))
    (fp_text value Led_Small (at -2.6 0 90) (layer F.Fab) hide)
    (fp_text user - (at 1.6 -1.6) (layer F.SilkS))
    (fp_text user + (at 1.6 1.5) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 0 -2.2) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0 2.2) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D4-Pad2)"))
  )
  (module plan44:LED1206_rev_mount (layer F.Cu) (tedit 57FF83A8)
    (at 198.984 88.011)
    (tags LED)
    (fp_text reference D3 (at 3.8 0) (layer F.SilkS))
    (fp_text value Led_Small (at -2.6 0 90) (layer F.Fab) hide)
    (fp_text user - (at 1.6 -1.6) (layer F.SilkS))
    (fp_text user + (at 1.6 1.5) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 0 -2.2) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0 2.2) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D3-Pad2)"))
  )
  (module plan44:LED1206_rev_mount (layer F.Cu) (tedit 57FF83A8)
    (at 165.989 87.9856)
    (tags LED)
    (fp_text reference D2 (at 3.8 0) (layer F.SilkS))
    (fp_text value Led_Small (at -2.6 0 90) (layer F.Fab) hide)
    (fp_text user - (at 1.6 -1.6) (layer F.SilkS))
    (fp_text user + (at 1.6 1.5) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 0 -2.2) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0 2.2) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D2-Pad2)"))
  )
  (module plan44:LED1206_rev_mount (layer F.Cu) (tedit 57FF83A8)
    (at 132.994 87.9856)
    (tags LED)
    (fp_text reference D1 (at 3.8 0) (layer F.SilkS))
    (fp_text value Led_Small (at -2.6 0 90) (layer F.Fab) hide)
    (fp_text user - (at 1.6 -1.6) (layer F.SilkS))
    (fp_text user + (at 1.6 1.5) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 0 -2.2) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0 2.2) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D1-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 56C35ED0)
    (at 120.142 78.994)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TPD0 (at 0 2) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 34 /GUARD))
  )
  (module plan44:CONFIG-PAD-2P (layer F.Cu) (tedit 57FF90FF)
    (at 119.913 97.028)
    (fp_text reference P2 (at 0 1.8) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.55) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at -0.55 0) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P2-Pad1)"))
  )
  (module plan44:CONFIG-PAD-2P (layer F.Cu) (tedit 57FF90FF)
    (at 119.913 93.9546 180)
    (fp_text reference P3 (at 0 1.8 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.55 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.55 0 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(P2-Pad1)"))
  )
  (module plan44:Touchpad_12x20_with_LED (layer B.Cu) (tedit 57FFA6BA)
    (at 133 88)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference TPD1 (at 0 3) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 -4) (size 6 4) (layers B.Cu B.Paste B.Mask)
      (net 35 /TOUCH1) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at 0 4) (size 6 4) (layers B.Cu B.Paste B.Mask)
      (net 35 /TOUCH1) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at -6 0) (size 8 12) (layers B.Cu B.Paste B.Mask)
      (net 35 /TOUCH1) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at 6 0) (size 8 12) (layers B.Cu B.Paste B.Mask)
      (net 35 /TOUCH1) (clearance -1) (zone_connect 0))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Mask B.Cu))
  )
  (module plan44:Touchpad_12x20_with_LED (layer B.Cu) (tedit 57FFA6BA)
    (at 166 88)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference TPD2 (at 0 3) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 -4) (size 6 4) (layers B.Cu B.Paste B.Mask)
      (net 36 /TOUCH2) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at 0 4) (size 6 4) (layers B.Cu B.Paste B.Mask)
      (net 36 /TOUCH2) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at -6 0) (size 8 12) (layers B.Cu B.Paste B.Mask)
      (net 36 /TOUCH2) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at 6 0) (size 8 12) (layers B.Cu B.Paste B.Mask)
      (net 36 /TOUCH2) (clearance -1) (zone_connect 0))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Mask B.Cu))
  )
  (module plan44:Touchpad_12x20_with_LED (layer B.Cu) (tedit 57FFA6BA)
    (at 199 88)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference TPD3 (at 0 3) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 -4) (size 6 4) (layers B.Cu B.Paste B.Mask)
      (net 37 /TOUCH3) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at 0 4) (size 6 4) (layers B.Cu B.Paste B.Mask)
      (net 37 /TOUCH3) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at -6 0) (size 8 12) (layers B.Cu B.Paste B.Mask)
      (net 37 /TOUCH3) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at 6 0) (size 8 12) (layers B.Cu B.Paste B.Mask)
      (net 37 /TOUCH3) (clearance -1) (zone_connect 0))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Mask B.Cu))
  )
  (module plan44:Touchpad_12x20_with_LED (layer B.Cu) (tedit 57FFA6BA)
    (at 232 88)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference TPD4 (at 0 3) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at 0 -4) (size 6 4) (layers B.Cu B.Paste B.Mask)
      (net 38 /TOUCH4) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at 0 4) (size 6 4) (layers B.Cu B.Paste B.Mask)
      (net 38 /TOUCH4) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at -6 0) (size 8 12) (layers B.Cu B.Paste B.Mask)
      (net 38 /TOUCH4) (clearance -1) (zone_connect 0))
    (pad 1 smd rect (at 6 0) (size 8 12) (layers B.Cu B.Paste B.Mask)
      (net 38 /TOUCH4) (clearance -1) (zone_connect 0))
    (pad "" np_thru_hole circle (at 0 0) (size 2.8 2.8) (drill 2.8) (layers *.Mask B.Cu))
  )
  (gr_line (start 246.888 99.06) (end 102.616 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 246.888 76.708) (end 246.888 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.616 76.708) (end 246.888 76.708) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.616 99.06) (end 102.616 76.708) (angle 90) (layer Edge.Cuts) (width 0.15))
)
