(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.5748)
    (drawings 37)
    (tracks 76)
    (zones 0)
    (modules 13)
    (nets 12)
  )
  (page A)
  (title_block
    (title "7th Area QSO Party Pixie Plaque")
    (date 2017-03-14)
    (rev A)
    (company "Central Oregon DX Club")
    (comment 1 "Design by Martin Held, AE7EU")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.889)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (user_via 0.635 0.381)
    (user_via 0.635 0.381)
    (user_via 0.889 0.635)
    (user_via 0.889 0.635)
    (user_via 1.27 0.889)
    (user_via 1.27 0.889)
    (user_via 1.905 1.524)
    (user_via 1.905 1.524)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1.27 1.27)
    (mod_text_width 0.254)
    (pad_size 5.9944 5.9944)
    (pad_drill 3.1496)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /DC_BIAS)
  (net 3 /RF_OUT)
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(K1-Pad2)")
  (net 6 /COMMON)
  (net 7 /DIFFERENTIAL)
  (net 8 "Net-(T1-Pad4)")
  (net 9 "Net-(T1-Pad5)")
  (net 10 "Net-(T1-Pad6)")
  (net 11 "Net-(J2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /COMMON)
    (add_net /DC_BIAS)
    (add_net /DIFFERENTIAL)
    (add_net /RF_OUT)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(K1-Pad2)")
    (add_net "Net-(T1-Pad4)")
    (add_net "Net-(T1-Pad5)")
    (add_net "Net-(T1-Pad6)")
  )
  (module mheld_std:IND-7447669 (layer F.Cu) (tedit 5BBBF0AD)
    (at 59.69 48.768 180)
    (attr smd)
    (fp_text reference L1 (at 0 -4.318) (layer F.SilkS))
    (fp_text value 220uH (at 2.25 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0 2.6 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 0 -2.6 180) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /DC_BIAS))
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 73.152 53.848)
    (descr "SMT capacitor, 1210")
    (fp_text reference C1 (at 0.254 -2.794) (layer F.SilkS))
    (fp_text value "0.1uF 100V" (at -0.0254 1.7272) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 2 /DC_BIAS))
    (pad 1 smd rect (at 1.397 0) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:C1210 (layer F.Cu) (tedit 54088696)
    (at 60.706 39.116)
    (descr "SMT capacitor, 1210")
    (fp_text reference C2 (at 0 -2.794) (layer F.SilkS))
    (fp_text value "0.1uF 100V" (at -0.0254 1.7272) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 3 /RF_OUT))
    (pad 2 smd rect (at -1.397 0) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model smd/capacitors/c_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:SOD-123 (layer F.Cu) (tedit 5BBBE935)
    (at 66.802 53.34 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2 180) (layer F.SilkS))
    (fp_text value diode-1 (at 0 2.1 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 2 /DC_BIAS))
    (pad 1 smd rect (at 1.635 0 180) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module mheld_std:PANEL_UHF (layer F.Cu) (tedit 5BBBE554)
    (at 44.958 42.418)
    (fp_text reference J1 (at 0 9.652) (layer F.SilkS))
    (fp_text value BNC-1 (at 0 11.43) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 9.1186 -9.1186) (size 6.35 6.35) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 9.1186 9.1186) (size 6.35 6.35) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -9.1186 9.1186) (size 6.35 6.35) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -9.1186 -9.1186) (size 6.35 6.35) (drill 3.175) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 13.97 0) (size 2.54 2.54) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
  )
  (module mheld_std:IM_RELAY (layer F.Cu) (tedit 5BBBE770)
    (at 66.802 46.482 90)
    (fp_text reference K1 (at 6.35 0 180) (layer F.SilkS))
    (fp_text value IM_RELAY (at -5.78 -2.72 180) (layer F.SilkS) hide)
    (pad 8 smd rect (at -3.8 -3 90) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.6 -3 90) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /RF_OUT))
    (pad 6 smd rect (at 1.6 -3 90) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 7 /DIFFERENTIAL))
    (pad 5 smd rect (at 3.8 -3 90) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(K1-Pad2)"))
    (pad 4 smd rect (at 3.8 3 90) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 3 /RF_OUT))
    (pad 3 smd rect (at 1.6 3 90) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 6 /COMMON))
    (pad 2 smd rect (at -0.6 3 90) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(K1-Pad2)"))
    (pad 1 smd rect (at -3.8 3 90) (size 0.7 2) (layers F.Cu F.Paste F.Mask)
      (net 2 /DC_BIAS))
    (model 3DModels/IM_RELAY.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 90))
    )
  )
  (module mheld_std:R2512 (layer F.Cu) (tedit 54B6B8E8)
    (at 62.23 33.274 180)
    (descr "SMT resistor, 2512")
    (fp_text reference R1 (at -5.334 0 180) (layer F.SilkS))
    (fp_text value 51 (at 0 2.032 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 3.1877 0 180) (size 1.6002 3.175) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.1877 0 180) (size 1.6002 3.175) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(K1-Pad2)"))
    (model smd/resistors/r_2512.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mheld_std:TFORM_WBT_SMT (layer F.Cu) (tedit 5BBBE706)
    (at 78.486 36.576)
    (fp_text reference T1 (at 0 -5.08) (layer F.SilkS))
    (fp_text value transformer_PWB (at 0 5.588) (layer F.SilkS) hide)
    (pad 6 smd rect (at 6 -2.54) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(T1-Pad6)"))
    (pad 5 smd rect (at 6 0) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(T1-Pad5)"))
    (pad 4 smd rect (at 6 2.54) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(T1-Pad4)"))
    (pad 3 smd rect (at -6 2.54) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -6 0) (size 2 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -6 -2.54) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 7 /DIFFERENTIAL))
  )
  (module mheld_std:TFORM_WBT_SMT (layer F.Cu) (tedit 5BBBE706)
    (at 78.486 46.228)
    (fp_text reference T2 (at -1.524 5.334) (layer F.SilkS))
    (fp_text value transformer_PWB (at 0 5.588) (layer F.SilkS) hide)
    (pad 1 smd rect (at -6 -2.54) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 6 /COMMON))
    (pad 2 smd rect (at -6 0) (size 2 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -6 2.54) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 6 2.54) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad2)"))
    (pad 5 smd rect (at 6 0) (size 2 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 6 -2.54) (size 2 0.76) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(T1-Pad5)"))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BBBEBEA)
    (at 89.408 32.258)
    (fp_text reference TH1 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 10 "Net-(T1-Pad6)") (clearance 1.27))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BBBEBE5)
    (at 89.408 42.418)
    (fp_text reference TH2 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 8 "Net-(T1-Pad4)") (clearance 1.27))
  )
  (module mheld_std:TH_440 (layer F.Cu) (tedit 5BBBEBF2)
    (at 89.408 52.578)
    (fp_text reference TH3 (at -2.17 -4.29) (layer F.SilkS) hide)
    (fp_text value TP (at 3.29 -4.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.9944 5.9944) (drill 3.1496) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad2)") (clearance 1.27))
  )
  (module mheld_std:HDR2X1_P1 (layer F.Cu) (tedit 5BBBE906)
    (at 79.502 52.578 90)
    (fp_text reference J2 (at -2.54 -0.762 180) (layer F.SilkS))
    (fp_text value HDR2X1 (at 0.47 -1.94 90) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.524 1.524) (drill 0.9906) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_line (start 31.877 56.134) (end 31.877 56.388) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 28.702 56.134) (end 31.877 56.134) (angle -43.36342296) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 96.012 28.702) (end 92.837 28.702) (angle -28.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.837 28.448) (end 92.837 28.702) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.582 56.388) (end 93.218 56.388) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 82.296 56.642) (end 84.581999 56.388001) (angle -167.3196165) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 42.418 28.194) (end 44.703999 28.447999) (angle 167.3) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 40.132 28.448) (end 30.988 28.448) (layer Edge.Cuts) (width 0.1))
  (dimension 27.94 (width 0.3) (layer Dwgs.User)
    (gr_text "1.1000 in" (at 96.588 42.418 270) (layer Dwgs.User))
    (feature1 (pts (xy 93.218 56.388) (xy 95.074421 56.388)))
    (feature2 (pts (xy 93.218 28.448) (xy 95.074421 28.448)))
    (crossbar (pts (xy 94.488 28.448) (xy 94.488 56.388)))
    (arrow1a (pts (xy 94.488 56.388) (xy 93.901579 55.261496)))
    (arrow1b (pts (xy 94.488 56.388) (xy 95.074421 55.261496)))
    (arrow2a (pts (xy 94.488 28.448) (xy 93.901579 29.574504)))
    (arrow2b (pts (xy 94.488 28.448) (xy 95.074421 29.574504)))
  )
  (gr_text "WIRE\nHERE" (at 56.134 42.418) (layer F.SilkS))
  (gr_text "Rev A" (at 60.706 55.118) (layer F.SilkS))
  (gr_text "AE7EU Reversible Beverage\nRevision A\nOct 2018\nmartin.held@gmail.com\n\nNOT RATED FOR INPUT POWER\nRECEIVE ONLY" (at 85.598 39.878) (layer B.SilkS))
  (gr_text "AE7EU Reversible Beverage" (at 71.374 29.718) (layer F.SilkS))
  (dimension 62.23 (width 0.3) (layer Dwgs.User)
    (gr_text "2.4500 in" (at 62.103 24.824) (layer Dwgs.User))
    (feature1 (pts (xy 93.218 28.448) (xy 93.218 26.337579)))
    (feature2 (pts (xy 30.988 28.448) (xy 30.988 26.337579)))
    (crossbar (pts (xy 30.988 26.924) (xy 93.218 26.924)))
    (arrow1a (pts (xy 93.218 26.924) (xy 92.091496 27.510421)))
    (arrow1b (pts (xy 93.218 26.924) (xy 92.091496 26.337579)))
    (arrow2a (pts (xy 30.988 26.924) (xy 32.114504 27.510421)))
    (arrow2b (pts (xy 30.988 26.924) (xy 32.114504 26.337579)))
  )
  (gr_circle (center 44.958 42.418) (end 53.086 40.894) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 92.837 28.448) (end 44.704 28.448) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.218 56.388) (end 93.218 30.226) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 31.877 56.388) (end 80.01 56.388) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30.988 28.448) (end 30.988 53.975) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 93.218 56.388) (xy 93.218 28.448) (xy 30.988 28.448) (xy 30.988 56.388)
      )
    )
  )
)
