(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 279)
    (zones 0)
    (modules 26)
    (nets 73)
  )
  (page A1)
  (title_block
    (title "Golden Wing")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 478.85 280.34)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GRBR/HPMI_DAUGHTER_BOARD/"))
  )
  (net 0 "")
  (net 1 CLK)
  (net 2 "Net-(U1-Pad1)")
  (net 3 "Net-(U1-Pad2)")
  (net 4 SCL)
  (net 5 SDA)
  (net 6 "Net-(U2-Pad1)")
  (net 7 "Net-(U2-Pad2)")
  (net 8 "Net-(U2-Pad3)")
  (net 9 "Net-(U2-Pad4)")
  (net 10 "Net-(U2-Pad8)")
  (net 11 "Net-(U2-Pad9)")
  (net 12 "Net-(U2-Pad10)")
  (net 13 "Net-(U2-Pad11)")
  (net 14 "Net-(U2-Pad12)")
  (net 15 "Net-(U2-Pad13)")
  (net 16 "Net-(U2-Pad14)")
  (net 17 "Net-(U2-Pad15)")
  (net 18 "Net-(U2-Pad16)")
  (net 19 "Net-(U2-Pad17)")
  (net 20 "Net-(U2-Pad18)")
  (net 21 "Net-(U2-Pad20)")
  (net 22 "Net-(U2-Pad21)")
  (net 23 "Net-(U2-Pad22)")
  (net 24 "Net-(U2-Pad23)")
  (net 25 "Net-(U2-Pad24)")
  (net 26 "Net-(U2-Pad25)")
  (net 27 "Net-(U2-Pad26)")
  (net 28 "Net-(U2-Pad27)")
  (net 29 "Net-(U2-Pad28)")
  (net 30 "Net-(U2-Pad29)")
  (net 31 "Net-(U2-Pad30)")
  (net 32 "Net-(U2-Pad31)")
  (net 33 "Net-(U2-Pad35)")
  (net 34 "Net-(U2-Pad37)")
  (net 35 GND)
  (net 36 rot_enc_switch)
  (net 37 +12V)
  (net 38 rot_enc_data)
  (net 39 rot_enc_clk)
  (net 40 Y1)
  (net 41 Q)
  (net 42 Q*)
  (net 43 +5VD)
  (net 44 "Net-(R1-Pad1)")
  (net 45 "Net-(R1-Pad3)")
  (net 46 "Net-(U3-Pad1)")
  (net 47 "Net-(U3-Pad2)")
  (net 48 "Net-(U3-Pad4)")
  (net 49 "Net-(U3-Pad5)")
  (net 50 "Net-(U3-Pad12)")
  (net 51 "Net-(U3-Pad14)")
  (net 52 "Net-(U3-Pad15)")
  (net 53 "Net-(U4-Pad1)")
  (net 54 "Net-(U4-Pad2)")
  (net 55 "Net-(U4-Pad4)")
  (net 56 "Net-(U4-Pad5)")
  (net 57 "Net-(U4-Pad12)")
  (net 58 "Net-(U4-Pad14)")
  (net 59 "Net-(U4-Pad15)")
  (net 60 "Net-(U5-Pad15)")
  (net 61 "Net-(U5-Pad13)")
  (net 62 "Net-(U5-Pad12)")
  (net 63 "Net-(U5-Pad5)")
  (net 64 "Net-(U5-Pad4)")
  (net 65 "Net-(U5-Pad2)")
  (net 66 "Net-(U5-Pad1)")
  (net 67 CLK_IN)
  (net 68 "Net-(JP2-Pad2)")
  (net 69 Serial_TX)
  (net 70 "Net-(U6-Pad7)")
  (net 71 "Net-(U6-Pad6)")
  (net 72 "Net-(U6-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5VD)
    (add_net CLK)
    (add_net CLK_IN)
    (add_net GND)
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad3)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad35)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad14)")
    (add_net "Net-(U4-Pad15)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad13)")
    (add_net "Net-(U5-Pad15)")
    (add_net "Net-(U5-Pad2)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad6)")
    (add_net "Net-(U6-Pad7)")
    (add_net Q)
    (add_net Q*)
    (add_net SCL)
    (add_net SDA)
    (add_net Serial_TX)
    (add_net Y1)
    (add_net rot_enc_clk)
    (add_net rot_enc_data)
  )
  (net_class 12V_Power ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
  )
  (net_class 5V_Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net rot_enc_switch)
  )
  (net_class CLK ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module CaptainQWiC:ESP32-DevKitC-VB (layer F.Cu) (tedit 5EE59583)
    (at 323.91 291.77 90)
    (fp_text reference U2 (at 15.93 16.44 90) (layer F.SilkS))
    (fp_text value ESP32-DevKitC-VB (at 15.24 21.59 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(U2-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(U2-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(U2-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 rot_enc_clk))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 rot_enc_data))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 rot_enc_switch))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(U2-Pad8)"))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(U2-Pad9)"))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad10)"))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad11)"))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad12)"))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(U2-Pad13)"))
    (pad 14 thru_hole circle (at 0 33.02 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad14)"))
    (pad 15 thru_hole circle (at 0 35.56 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad15)"))
    (pad 16 thru_hole circle (at 0 38.1 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(U2-Pad16)"))
    (pad 17 thru_hole circle (at 0 40.64 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(U2-Pad17)"))
    (pad 18 thru_hole circle (at 0 43.18 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(U2-Pad18)"))
    (pad 19 thru_hole circle (at 0 45.72 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5VD))
    (pad 20 thru_hole circle (at 25.4 45.72 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(U2-Pad20)"))
    (pad 21 thru_hole circle (at 25.4 43.18 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(U2-Pad21)"))
    (pad 22 thru_hole circle (at 25.4 40.64 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(U2-Pad22)"))
    (pad 23 thru_hole circle (at 25.4 38.1 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(U2-Pad23)"))
    (pad 24 thru_hole circle (at 25.4 35.56 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad24)"))
    (pad 25 thru_hole circle (at 25.4 33.02 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(U2-Pad25)"))
    (pad 26 thru_hole circle (at 25.4 30.48 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(U2-Pad26)"))
    (pad 27 thru_hole circle (at 25.4 27.94 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(U2-Pad27)"))
    (pad 28 thru_hole circle (at 25.4 25.4 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad28)"))
    (pad 29 thru_hole circle (at 25.4 22.86 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad29)"))
    (pad 30 thru_hole circle (at 25.4 20.32 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad30)"))
    (pad 31 thru_hole circle (at 25.4 17.78 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad31)"))
    (pad 32 thru_hole circle (at 25.4 15.24 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 GND))
    (pad 33 thru_hole circle (at 25.4 12.7 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 SDA))
    (pad 34 thru_hole circle (at 25.4 10.16 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 69 Serial_TX))
    (pad 35 thru_hole circle (at 25.4 7.62 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad35)"))
    (pad 36 thru_hole circle (at 25.4 5.08 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 37 thru_hole circle (at 25.4 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad37)"))
    (pad 38 thru_hole circle (at 25.4 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 GND))
  )
  (module CaptainQWiC:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 338.975 288.84)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 3.375 0) (layer B.SilkS))
    (fp_text value "100 pF" (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 Y1))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:SMA_Amphenol_132289_EdgeMount (layer B.Cu) (tedit 5A1C1810)
    (at 337.1 261.09 90)
    (descr http://www.amphenolrf.com/132289.html)
    (tags SMA)
    (attr smd)
    (fp_text reference J2 (at -3.96 3) (layer B.SilkS))
    (fp_text value "Trig+ IN" (at 5 -6 270) (layer B.Fab))
    (fp_text user %R (at 4.79 0 180) (layer B.Fab))
    (pad 2 smd rect (at 0 -4.25) (size 1.5 5.08) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 2 smd rect (at 0 4.25) (size 1.5 5.08) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 2 smd rect (at 0 -4.25) (size 1.5 5.08) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 2 smd rect (at 0 4.25) (size 1.5 5.08) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 1 smd rect (at 0 0) (size 1.5 5.08) (layers B.Cu B.Paste B.Mask)
      (net 41 Q))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:SMA_Amphenol_132289_EdgeMount (layer B.Cu) (tedit 5A1C1810)
    (at 360.35 261.59 90)
    (descr http://www.amphenolrf.com/132289.html)
    (tags SMA)
    (attr smd)
    (fp_text reference J3 (at -3.96 3) (layer B.SilkS))
    (fp_text value "Trig- IN" (at 5 -6 270) (layer B.Fab))
    (fp_text user %R (at 4.79 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 5.08) (layers B.Cu B.Paste B.Mask)
      (net 42 Q*))
    (pad 2 smd rect (at 0 4.25) (size 1.5 5.08) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 2 smd rect (at 0 -4.25) (size 1.5 5.08) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 2 smd rect (at 0 4.25) (size 1.5 5.08) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 2 smd rect (at 0 -4.25) (size 1.5 5.08) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:PinSocket_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5A19A429)
    (at 366.35 270.34 90)
    (descr "Through hole angled socket strip, 1x03, 2.54mm pitch, 8.51mm socket length, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole angled socket strip THT 1x03 2.54mm single row")
    (fp_text reference J10 (at -4.38 -2.77 90) (layer F.SilkS))
    (fp_text value "12V to 5V DC" (at -4.38 7.85 90) (layer F.Fab))
    (fp_text user %R (at -5.775 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 +5VD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 +12V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:3296Y-1-501LF (layer B.Cu) (tedit 0)
    (at 324.6 286.59)
    (fp_text reference R1 (at 2.5273 1.3335) (layer B.SilkS))
    (fp_text value 3296Y-1-501LF (at 3.5 3.5) (layer B.SilkS))
    (fp_text user * (at 0 0) (layer B.Fab))
    (fp_text user * (at 0 0) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 1 thru_hole circle (at 5.08 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 44 "Net-(R1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 Y1))
    (pad 3 thru_hole rect (at 0 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 "Net-(R1-Pad3)"))
  )
  (module CaptainQWiC:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 338.975 285.84 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -3.375 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 +5VD))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 rot_enc_clk))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 338.975 287.34 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -3.375 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 +5VD))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 rot_enc_data))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 333.975 285.84 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 1.43) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 rot_enc_switch))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 +5VD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 333.975 288.84)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.625 0.5 180) (layer B.SilkS))
    (fp_text value 600 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 333.975 287.34 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -2.625 0) (layer B.SilkS))
    (fp_text value 15k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 GND))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 rot_enc_switch))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:SSD1306Module (layer B.Cu) (tedit 5EEBD852)
    (at 353.12 263.83 180)
    (fp_text reference Screen1 (at 4.02 -9.51) (layer B.SilkS))
    (fp_text value SSD1306_Module (at 3.683 -8.636) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 35 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 43 +5VD))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 SDA))
    (model "${KIPRJMOD}/3D Cad Files/SSD1306 Oled/OLED-128x64-0.96.step"
      (offset (xyz 38.15 -7.2 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm (layer B.Cu) (tedit 5EEBDABE)
    (at 331.45 283.34 90)
    (descr "Alps rotary encoder, EC12E... with switch, vertical shaft, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC11/EC11E15204A3.html")
    (tags "rotary encoder")
    (fp_text reference SW1 (at 2.8 4.7 90) (layer B.SilkS))
    (fp_text value Rotary_Encoder_Switch (at 7.5 -10.4 90) (layer B.Fab))
    (fp_text user %R (at 11.1 -6.3 90) (layer B.Fab))
    (pad S1 thru_hole circle (at 14.5 -5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 36 rot_enc_switch))
    (pad S2 thru_hole circle (at 14.5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 35 GND))
    (pad MP thru_hole rect (at 7.5 -8.1 90) (size 3.2 2) (drill oval 2.8 1.5) (layers *.Cu *.Mask))
    (pad MP thru_hole rect (at 7.5 3.1 90) (size 3.2 2) (drill oval 2.8 1.5) (layers *.Cu *.Mask))
    (pad B thru_hole circle (at 0 -5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 38 rot_enc_data))
    (pad C thru_hole circle (at 0 -2.5 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 35 GND))
    (pad A thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 39 rot_enc_clk))
    (model ${KISYS3DMOD}/Rotary_Encoder.3dshapes/RotaryEncoder_Alps_EC11E-Switch_Vertical_H20mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D Cad Files/Rotarty Encoder/EC11_Rotary_Encoder_Switched.step"
      (offset (xyz 7.6 -2.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CaptainQWiC:AdaSi5351 (layer F.Cu) (tedit 5ED674EE)
    (at 349.31 270.18 180)
    (fp_text reference U1 (at 0 -5.08) (layer F.SilkS))
    (fp_text value AdaSi5351 (at 0 -7.62) (layer F.Fab))
    (pad 0 thru_hole circle (at -7.62 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 CLK))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 4 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 SDA))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 GND))
    (pad 6 thru_hole circle (at 7.62 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 +5VD))
    (pad "" thru_hole circle (at -12.7 0 180) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 12.7 0 180) (size 4 4) (drill 3) (layers *.Cu *.Mask))
  )
  (module CaptainQWiC:SN74LV4051ADR (layer B.Cu) (tedit 5F38090F)
    (at 358.3778 279.705)
    (fp_text reference U3 (at 0 -1.27 -90) (layer B.SilkS))
    (fp_text value SN74LV4051ADR (at 0 3.81 -90) (layer B.Fab))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -1.6129 4.9276) (layer B.SilkS))
    (fp_text user * (at -1.6129 4.9276) (layer B.Fab))
    (fp_text user * (at -1.6129 4.9276) (layer B.Fab))
    (fp_text user * (at -1.6129 4.9276) (layer B.SilkS))
    (pad 1 smd rect (at -2.3622 4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -2.3622 3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -2.3622 1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 43 +5VD))
    (pad 4 smd rect (at -2.3622 0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -2.3622 -0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -2.3622 -1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 7 smd rect (at -2.3622 -3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 8 smd rect (at -2.3622 -4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 9 smd rect (at 2.3622 -4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 10 smd rect (at 2.3622 -3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 40 Y1))
    (pad 11 smd rect (at 2.3622 -1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 67 CLK_IN))
    (pad 12 smd rect (at 2.3622 -0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(U3-Pad12)"))
    (pad 13 smd rect (at 2.3622 0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 42 Q*))
    (pad 14 smd rect (at 2.3622 1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(U3-Pad14)"))
    (pad 15 smd rect (at 2.3622 3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(U3-Pad15)"))
    (pad 16 smd rect (at 2.3622 4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 43 +5VD))
  )
  (module CaptainQWiC:SN74LV4051ADR (layer B.Cu) (tedit 5F38090F)
    (at 349.214601 279.705)
    (fp_text reference U4 (at 0 -1.27 -90) (layer B.SilkS))
    (fp_text value SN74LV4051ADR (at 0 3.81 -90) (layer B.Fab))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at -1.6129 4.9276) (layer B.SilkS))
    (fp_text user * (at -1.6129 4.9276) (layer B.Fab))
    (fp_text user * (at -1.6129 4.9276) (layer B.Fab))
    (fp_text user * (at -1.6129 4.9276) (layer B.SilkS))
    (pad 1 smd rect (at -2.3622 4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -2.3622 3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(U4-Pad2)"))
    (pad 3 smd rect (at -2.3622 1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 43 +5VD))
    (pad 4 smd rect (at -2.3622 0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -2.3622 -0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at -2.3622 -1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 7 smd rect (at -2.3622 -3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 8 smd rect (at -2.3622 -4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 9 smd rect (at 2.3622 -4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 10 smd rect (at 2.3622 -3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 40 Y1))
    (pad 11 smd rect (at 2.3622 -1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 67 CLK_IN))
    (pad 12 smd rect (at 2.3622 -0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(U4-Pad12)"))
    (pad 13 smd rect (at 2.3622 0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 41 Q))
    (pad 14 smd rect (at 2.3622 1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(U4-Pad14)"))
    (pad 15 smd rect (at 2.3622 3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(U4-Pad15)"))
    (pad 16 smd rect (at 2.3622 4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 43 +5VD))
  )
  (module CaptainQWiC:SN74LV4051ADR (layer B.Cu) (tedit 5F38090F)
    (at 340.5978 279.705)
    (fp_text reference U5 (at 0 -1.27 -90) (layer B.SilkS))
    (fp_text value SN74LV4051ADR (at 0 3.81 -90) (layer B.Fab))
    (fp_text user * (at -1.6129 4.9276) (layer B.SilkS))
    (fp_text user * (at -1.6129 4.9276) (layer B.Fab))
    (fp_text user * (at -1.6129 4.9276) (layer B.Fab))
    (fp_text user * (at -1.6129 4.9276) (layer B.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 16 smd rect (at 2.3622 4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 43 +5VD))
    (pad 15 smd rect (at 2.3622 3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(U5-Pad15)"))
    (pad 14 smd rect (at 2.3622 1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 40 Y1))
    (pad 13 smd rect (at 2.3622 0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(U5-Pad13)"))
    (pad 12 smd rect (at 2.3622 -0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(U5-Pad12)"))
    (pad 11 smd rect (at 2.3622 -1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 67 CLK_IN))
    (pad 10 smd rect (at 2.3622 -3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 9 smd rect (at 2.3622 -4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 8 smd rect (at -2.3622 -4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 7 smd rect (at -2.3622 -3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 6 smd rect (at -2.3622 -1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 35 GND))
    (pad 5 smd rect (at -2.3622 -0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(U5-Pad5)"))
    (pad 4 smd rect (at -2.3622 0.635) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -2.3622 1.905) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 43 +5VD))
    (pad 2 smd rect (at -2.3622 3.175) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(U5-Pad2)"))
    (pad 1 smd rect (at -2.3622 4.445) (size 2.1844 0.5588) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U5-Pad1)"))
  )
  (module CaptainQWiC:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 356.225 286.09)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 1.43) (layer B.SilkS))
    (fp_text value "100 pF" (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 +5VD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 346.725 286.09)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 2.681 0 180) (layer B.SilkS))
    (fp_text value "100 pF" (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 43 +5VD))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CaptainQWiC:M3_Hole (layer F.Cu) (tedit 5E503261)
    (at 327.35 262)
    (fp_text reference H1 (at -4 2.25) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 -6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.5 6.5) (drill 3.3) (layers *.Cu *.Mask)
      (net 35 GND))
  )
  (module CaptainQWiC:M3_Hole (layer F.Cu) (tedit 5E503261)
    (at 370 262)
    (fp_text reference H2 (at 3 3.75) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 -6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.5 6.5) (drill 3.3) (layers *.Cu *.Mask)
      (net 35 GND))
  )
  (module CaptainQWiC:M3_Hole (layer F.Cu) (tedit 5E503261)
    (at 370 287)
    (fp_text reference H3 (at -5 0) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 -6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.5 6.5) (drill 3.3) (layers *.Cu *.Mask)
      (net 35 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged2Bar_Pad1.0x1.5mm (layer B.Cu) (tedit 5C756A82)
    (at 355.45 272.59)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 2 copper strips")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8) (layer B.SilkS))
    (fp_text value SolderJumper_2_Bridged (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 67 CLK_IN))
    (pad 2 smd rect (at 0.65 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 1 CLK))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm (layer F.Cu) (tedit 5A3EABFC)
    (at 340.1 278.59 270)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 -1.8 90) (layer F.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 68 "Net-(JP2-Pad2)"))
    (pad 1 smd rect (at -0.65 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 67 CLK_IN))
  )
  (module CaptainQWiC:CD40107BM (layer F.Cu) (tedit 5F38584B)
    (at 347.35 278.34)
    (fp_text reference U6 (at 0 0 90) (layer F.SilkS))
    (fp_text value CD40107BM (at 0 -3.81) (layer F.SilkS))
    (fp_text user * (at -2.7178 -3.6068) (layer F.SilkS))
    (fp_text user * (at -2.7178 -3.6068) (layer F.Fab))
    (fp_text user * (at -2.7178 -3.6068) (layer F.Fab))
    (fp_text user * (at -2.7178 -3.6068) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 8 smd rect (at 2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 43 +5VD))
    (pad 7 smd rect (at 2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U6-Pad7)"))
    (pad 6 smd rect (at 2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U6-Pad6)"))
    (pad 5 smd rect (at 2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U6-Pad5)"))
    (pad 4 smd rect (at -2.4638 1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 3 smd rect (at -2.4638 0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(JP2-Pad2)"))
    (pad 2 smd rect (at -2.4638 -0.635) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 69 Serial_TX))
    (pad 1 smd rect (at -2.4638 -1.905) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 CLK))
  )
  (module CaptainQWiC:BarrelJack_Horizontal (layer B.Cu) (tedit 5F39DCAC)
    (at 366.35 276.84 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at -8.45 -5.75) (layer B.SilkS))
    (fp_text value Barrel_Jack_Switch (at -6.2 5.5) (layer B.Fab))
    (fp_text user %R (at -3 2.95) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 37 +12V))
    (pad 2 thru_hole roundrect (at -6 0 180) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 35 GND))
    (pad 3 thru_hole roundrect (at -3 -4.7 180) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 35 GND))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "C:/Users/Paula/Documents/CaptainQWiC/3D Cad Files/KLDX-0202-B_rD3.IGS"
      (offset (xyz -13.75 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (gr_arc (start 325.85 289.59) (end 321.35 289.59) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 325.85 294.09) (end 369.6 294.09) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 374.1 262.84) (end 374.1 289.59) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 369.6 289.59) (end 369.6 294.09) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 321.35 262.84) (end 321.35 289.59) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 325.85 258.34) (end 369.6 258.34) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 369.6 262.84) (end 374.1 262.84) (angle -90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 325.85 262.84) (end 325.85 258.34) (angle -90) (layer Edge.Cuts) (width 0.1))
  (zone (net 35) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 377.35 295.09) (xy 320.35 295.09) (xy 320.35 255.84) (xy 377.35 255.84)
      )
    )
  )
  (zone (net 43) (net_name +5VD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 377.35 295.09) (xy 320.35 295.09) (xy 320.35 255.84) (xy 377.35 255.84)
      )
    )
  )
)
