(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 28)
    (no_connects 0)
    (area 145.8 82.448809 178.225001 105.575)
    (thickness 1.6)
    (drawings 9)
    (tracks 44)
    (zones 0)
    (modules 14)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.4)
    (user_trace_width 1.6)
    (user_trace_width 1.8)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4 0.3)
    (user_via 0.6 0.5)
    (user_via 0.8 0.6)
    (user_via 1.2 1)
    (user_via 1.4 1.2)
    (user_via 1.6 1.4)
    (user_via 1.8 1.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 GPIO2_5)
  (net 5 GPIO2)
  (net 6 GPIO0)
  (net 7 TX)
  (net 8 RX)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net GPIO0)
    (add_net GPIO2)
    (add_net GPIO2_5)
    (add_net RX)
    (add_net TX)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 166.75 93.75 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.75 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 6.15 -0.15 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 160.75 93.75 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.55 2.25 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 581095CE)
    (at 169.8 100)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 7 -1.8 180) (layer B.SilkS))
    (fp_text value CONN_01X01 (at 5 0.15 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GPIO2_5))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 161.8 98.4 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.4 -1.8 360) (layer F.SilkS))
    (fp_text value BSS138 (at 6.2 0.2 360) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 5 GPIO2))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 GPIO2_5))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 158 99.15 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.85 -2.6 360) (layer F.SilkS))
    (fp_text value 10k (at 3.85 -0.4 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 GPIO2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 166.75 98.6 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.4 1.75 270) (layer F.SilkS))
    (fp_text value 10k (at 5.2 -0.25 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GPIO2_5))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-01 (layer F.Cu) (tedit 5888BBC4)
    (at 152.105001 92.197)
    (descr "Module, ESP-8266, ESP-01, 8 pin")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U2 (at 4.894999 4.203 90) (layer B.SilkS))
    (fp_text value ESP-01v090 (at 0.144999 12.303 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 TX))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GPIO2))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GPIO0))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 RX))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 581095B5)
    (at 173.46 92 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -1.8 3.54 180) (layer B.SilkS))
    (fp_text value CONN_01X02 (at 5 -3.45 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 163.75076 93.8 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U1 (at 2.8 -0.84924 270) (layer F.SilkS))
    (fp_text value MCP1700 (at -7.6 -0.24924 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 173.46 100 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.6 -3.86 360) (layer B.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 581095A9)
    (at 174.6 94.8 270)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C5 (at 1.4 -1.6 450) (layer B.SilkS))
    (fp_text value 1000uf (at 1.25 4.4 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5888BBC0)
    (at 148.2 92.2)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 7.55 -7.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 TX))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GPIO0))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 RX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Wave (layer F.Cu) (tedit 0)
    (at 158 93.75 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Wave,")
    (tags "Tantal Cap. , Size B, EIA-3528, Wave,")
    (attr smd)
    (fp_text reference C4 (at -0.20066 -3.29946 90) (layer F.SilkS))
    (fp_text value 2.2uf (at -0.09906 3.59918 90) (layer F.Fab))
    (fp_text user + (at -3.79984 -2.49936 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.6256 0 90) (size 2.14884 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.6256 0 90) (size 2.14884 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Wave.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_Wave (layer F.Cu) (tedit 0)
    (at 169.5 93.472 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Wave,")
    (tags "Tantal Cap. , Size B, EIA-3528, Wave,")
    (attr smd)
    (fp_text reference C2 (at -0.20066 -3.29946 90) (layer F.SilkS))
    (fp_text value 2.2uf (at -0.09906 3.59918 90) (layer F.Fab))
    (fp_text user + (at -3.79984 -2.49936 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.6256 0 90) (size 2.14884 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.6256 0 90) (size 2.14884 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_Wave.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text GND (at 150 92.2 270) (layer B.SilkS))
  (gr_text TX (at 150 94.8 270) (layer B.SilkS))
  (gr_text RX (at 150 99.8 270) (layer B.SilkS))
  (gr_text G0 (at 150 97.2 270) (layer B.SilkS))
  (gr_line (start 146 90) (end 146 102) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 178 90) (end 178 102) (layer Edge.Cuts) (width 0.15))
  (gr_text "Takigama - HAStrip\nme@pjr.cc\n" (at 164.6 95.2 345) (layer B.SilkS))
  (gr_line (start 178 102) (end 146 102) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146 90) (end 178 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.2 102.2) (xy 145.8 102.2) (xy 145.8 89.8) (xy 178.2 89.8) (xy 178.2 102.2)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.8 89.8) (xy 145.8 102.2) (xy 163.6 102.2) (xy 163.6 89.8)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.8 89.8) (xy 163.8 102.2) (xy 178.2 102.2) (xy 178.2 89.8)
      )
    )
  )
)
