(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Top Layer")
		(31 "B.Cu" signal "Bottom Layer")
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user "Bottom Paste")
		(35 "F.Paste" user "Top Paste")
		(36 "B.SilkS" user "Bottom Overlay")
		(37 "F.SilkS" user "Top Overlay")
		(38 "B.Mask" user "Bottom Solder")
		(39 "F.Mask" user "Top Solder")
		(40 "Dwgs.User" user "Mechanical 10")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "Mechanical 11")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user "Mechanical 13")
		(49 "F.Fab" user "Mechanical 12")
		(50 "User.1" user "Mechanical 1")
		(51 "User.2" user "Mechanical 2")
		(52 "User.3" user "Mechanical 3")
		(53 "User.4" user "Mechanical 4")
		(54 "User.5" user "Mechanical 5")
		(55 "User.6" user "Mechanical 6")
		(56 "User.7" user "Mechanical 7")
		(57 "User.8" user "Mechanical 8")
		(58 "User.9" user "Mechanical 9")
	)
	(setup
		(pad_to_mask_clearance 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 124.3711 146.901295)
		(grid_origin 124.3711 146.901295)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "NetD2_A")
	(net 2 "NetD1_A")
	(net 3 "NetQ2_4")
	(net 4 "NetQ2_2")
	(net 5 "NetC1_2")
	(net 6 "NetC1_1")
	(net 7 "VCC")
	(net 8 "NetR1_1")
	(net 9 "NetL1_2")
	(net 10 "NetL1_1")
	(net 11 "NetC8_1")
	(net 12 "NetC3_2")
	(net 13 "NetC3_1")
	(net 14 "NetC2_2")
	(net 15 "NetC2_1")
	(net 16 "GND")
	(net 17 "NetC10_2")
	(net 18 "NetR10_1")
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 160.4391 135.979295 -90)
		(property "Reference" "R2"
			(at 1.524 1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 3.3147 1.6383 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
		)
		(pad "2" smd rect
			(at 0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "NetR1_1")
		)
	)
	(footprint "ClikThroughHole.PcbLib:DIODE400X100"
		(layer "F.Cu")
		(at 138.3411 84.671295 90)
		(property "Reference" "D2"
			(at 7.112 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -8.2169 -1.1557 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at -5.08 0 90)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "NetD2_A")
			(thermal_bridge_angle 90)
		)
		(pad "K" thru_hole rect
			(at 5.08 0 90)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "NetC3_2")
		)
	)
	(footprint "ClikGeneric.PcbLib:HDR2S156"
		(layer "F.Cu")
		(at 154.0891 142.075295 -90)
		(property "Reference" "J1"
			(at 0.508 -2.794 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -4.318 -0.762 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 4.318 3.048)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GND")
			(zone_connect 1)
			(thermal_bridge_width 1)
		)
		(pad "2" thru_hole oval
			(at 0 3.9624 270)
			(size 4.318 3.048)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "VCC")
			(zone_connect 1)
			(thermal_bridge_width 1)
		)
		(model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/026604020.stp"
			(offset
				(xyz 1.93048 -1.98108 2.032)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "ClikThroughHole.PcbLib:RES500X160"
		(layer "F.Cu")
		(at 160.1851 89.751295 90)
		(property "Reference" "R3"
			(at 1.524 4.318 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -9.4869 -1.9177 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 90)
			(size 1.524 1.524)
			(drill 0.7874)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "NetC2_1")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 90)
			(size 1.524 1.524)
			(drill 0.7874)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "NetC8_1")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 156.3751 125.311295 -90)
		(property "Reference" "C9"
			(at 4.064 -0.762 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 1.5367 1.8923 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "VCC")
		)
		(pad "2" smd rect
			(at 0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
		)
	)
	(footprint "ClikThroughHole.PcbLib:DIODE400X100"
		(layer "F.Cu")
		(at 143.4211 87.211295 -90)
		(property "Reference" "D3"
			(at -9.652 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 8.2169 1.1557 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at -5.08 0 270)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GND")
			(thermal_bridge_angle 90)
		)
		(pad "K" thru_hole rect
			(at 5.08 0 270)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "NetD2_A")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_SOT23"
		(layer "F.Cu")
		(at 144.9451 126.073295 180)
		(property "Reference" "U1"
			(at 3.302 -2.032 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 1.3589 -4.1783 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 1.1 180)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NetC10_2")
		)
		(pad "2" smd rect
			(at 0.95 1.1 180)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NetC10_2")
		)
		(pad "3" smd rect
			(at 0.00001 -1.1 180)
			(size 1 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
		)
	)
	(footprint "ClikGeneric.PcbLib:CTX2106XX"
		(layer "F.Cu")
		(at 127.3711 120.011295)
		(property "Reference" "T1"
			(at -2.5 -24.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "FL2015-2L"
			(at -8.1153 15.5321 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.coilcraft.com/getmedia/6651db01-d153-47d9-8a27-4758c28bff0d/fl.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Coilcraft FL2015-2L CCFL transformer"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 0)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "NetC1_1")
			(zone_connect 2)
		)
		(pad "2" smd rect
			(at 2.5 0)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "NetQ2_2")
		)
		(pad "3" smd rect
			(at 5 0)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "VCC")
		)
		(pad "4" smd rect
			(at 7.5 0)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "NetQ2_4")
		)
		(pad "5" smd rect
			(at 10 0)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "NetC1_2")
			(zone_connect 2)
		)
		(pad "6" smd rect
			(at 12.5 0)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "7" smd rect
			(at 12.5 -22.86)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "8" smd rect
			(at 10 -22.86)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "NetD2_A")
		)
		(pad "9" smd rect
			(at 2.5 -22.86)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "NetD1_A")
		)
		(pad "10" smd rect
			(at 0 -22.86)
			(size 1.27 1.91)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 141.1351 125.565295)
		(property "Reference" "R5"
			(at -0.95 -1.524 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -1.8923 1.5367 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0 90)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "VCC")
		)
		(pad "2" smd rect
			(at 0.95 0 90)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NetC10_2")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 160.4391 129.883295 -90)
		(property "Reference" "R6"
			(at 3.048 1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 1.5367 1.8923 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "NetC2_2")
		)
		(pad "2" smd rect
			(at 0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
		)
	)
	(footprint "ClikThroughHole.PcbLib:DIODE400X100"
		(layer "F.Cu")
		(at 133.2611 87.211295 -90)
		(property "Reference" "D4"
			(at -9.652 1.27 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 8.2169 1.1557 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at -5.08 0 270)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GND")
			(thermal_bridge_angle 90)
		)
		(pad "K" thru_hole rect
			(at 5.08 0 270)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "NetD1_A")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 150.7871 128.359295 180)
		(property "Reference" "R11"
			(at -2.286 -0.508 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 1.8923 -1.5367 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0 270)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NetC10_2")
		)
		(pad "2" smd rect
			(at 0.95 0 270)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
		)
	)
	(footprint "ClikGeneric.PcbLib:DR124"
		(layer "F.Cu")
		(at 152.0571 103.721295 180)
		(property "Reference" "L1"
			(at 6.985 7.0358 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 6.9723 -8.5725 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -5.125 0 180)
			(size 4 5.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "NetL1_1")
			(zone_connect 2)
		)
		(pad "2" smd rect
			(at 5.125 0 180)
			(size 4 5.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "NetL1_2")
			(zone_connect 2)
		)
	)
	(footprint "ClikThroughHole.PcbLib:CAP400X100"
		(layer "F.Cu")
		(at 150.7871 87.465295 90)
		(property "Reference" "C7"
			(at 4.826 -2.032 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -10.2743 -1.5113 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -3.81 -0.762 90)
			(size 1.778 1.778)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GND")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 3.81 0.762 90)
			(size 1.778 1.778)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "NetC3_2")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikGeneric.PcbLib:POT_TRIM BOURNS 3386F"
		(layer "F.Cu")
		(at 166.7891 132.931295 180)
		(property "Reference" "R1"
			(at 4.572 -6.604 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 4.6609 -7.2009 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 -2.54 180)
			(size 1.5748 1.5748)
			(drill 0.7874)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "NetR1_1")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54 180)
			(size 1.5748 1.5748)
			(drill 0.7874)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "NetC2_1")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 0 2.54 180)
			(size 1.5748 1.5748)
			(drill 0.7874)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "NetC2_1")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikThroughHole.PcbLib:CAP250X100"
		(layer "F.Cu")
		(at 162.9791 78.829295 180)
		(property "Reference" "C3"
			(at 0.889 2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0.7239 -6.3119 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -3.175 0 180)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "NetC3_1")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 3.175 0 180)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "NetC3_2")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 158.6611 125.311295 -90)
		(property "Reference" "R10"
			(at 4.826 -0.254 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 1.5367 1.8923 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "NetR10_1")
		)
		(pad "2" smd rect
			(at 0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
		)
	)
	(footprint "ClikThroughHole.PcbLib:CAP_R200x400"
		(layer "F.Cu")
		(at 142.4051 133.693295 90)
		(property "Reference" "C4"
			(at -5.334 -5.08 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 2.7305 0.9525 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 2.032 2.032)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "VCC")
			(zone_connect 1)
			(thermal_bridge_width 1)
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 2.032 2.032)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GND")
			(zone_connect 1)
			(thermal_bridge_width 1)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikThroughHole.PcbLib:CAP_R200x400"
		(layer "F.Cu")
		(at 130.7211 133.693295 90)
		(property "Reference" "C5"
			(at -5.334 3.556 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 2.7305 0.9525 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 2.032 2.032)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "VCC")
			(zone_connect 1)
			(thermal_bridge_width 1)
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 2.032 2.032)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GND")
			(zone_connect 1)
			(thermal_bridge_width 1)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 137.0711 125.565295)
		(property "Reference" "C6"
			(at -0.729 -1.557 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -1.8923 1.5367 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0 90)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "VCC")
		)
		(pad "2" smd rect
			(at 0.95 0 90)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
			(zone_connect 2)
		)
	)
	(footprint "ClikThroughHole.PcbLib:WIMAMKP2"
		(layer "F.Cu")
		(at 130.9751 125.311295)
		(property "Reference" "C1"
			(at -4.318 0.762 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -3.4671 4.9149 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.524 1.524)
			(drill 0.711)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "NetC1_1")
			(zone_connect 2)
			(thermal_bridge_width 1)
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.524 1.524)
			(drill 0.711)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "NetC1_2")
			(zone_connect 2)
			(thermal_bridge_width 1)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikGeneric.PcbLib:G_TO252M[D2PAK]"
		(layer "F.Cu")
		(at 163.4871 117.945295)
		(property "Reference" "Q1"
			(at 4.318 6.096 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -3.1877 7.9629 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "D" smd rect
			(at 0 -3.3)
			(size 10.6 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "NetL1_1")
			(zone_connect 2)
		)
		(pad "G" smd rect
			(at -2.54 6.3)
			(size 1.45 2.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "NetC2_2")
		)
		(pad "S" smd rect
			(at 2.54 6.3)
			(size 1.45 2.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
			(zone_connect 2)
		)
	)
	(footprint "ClikThroughHole.PcbLib:DIODE400X100"
		(layer "F.Cu")
		(at 128.1811 84.671295 90)
		(property "Reference" "D1"
			(at 7.112 -1.016 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -8.2169 -1.1557 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at -5.08 0 90)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "NetD1_A")
			(thermal_bridge_angle 90)
		)
		(pad "K" thru_hole rect
			(at 5.08 0 90)
			(size 1.524 1.524)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "NetC3_2")
		)
	)
	(footprint "ClikGeneric.PcbLib:HDR3S156M1"
		(layer "F.Cu")
		(at 149.0091 67.653295 90)
		(property "Reference" "J4"
			(at -0.762 10.668 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -3.5941 -0.2159 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 4.318 3.048)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "NetC8_1")
		)
		(pad "2" thru_hole oval
			(at 0 7.9248 90)
			(size 4.318 3.048)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GND")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 150.7871 130.645295)
		(property "Reference" "C10"
			(at 2.286 0.508 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -1.5113 10.2743 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0 90)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
		)
		(pad "2" smd rect
			(at 0.95 0 90)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NetC10_2")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 145.1991 121.501295 -90)
		(property "Reference" "R7"
			(at 0.762 1.524 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 3.3147 1.6383 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "NetQ2_4")
		)
		(pad "2" smd rect
			(at 0.95 0)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "VCC")
		)
	)
	(footprint "C__Data_FromLaptop_Projects_ClikPcb_ClikGeneric.PcbLib:M_MTHOLE"
		(layer "F.Cu")
		(at 129.4511 141.821295)
		(property "Reference" "UNK"
			(at -2.3876 -3.4036 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.08 5.08)
			(drill 3.81)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C__Data_FromLaptop_Projects_ClikPcb_ClikGeneric.PcbLib:M_MTHOLE"
		(layer "F.Cu")
		(at 167.5511 68.161295)
		(property "Reference" "UNK"
			(at -2.3876 -3.4036 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.08 5.08)
			(drill 3.81)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C__Data_FromLaptop_Projects_ClikPcb_ClikGeneric.PcbLib:M_MTHOLE"
		(layer "F.Cu")
		(at 165.0111 103.721295)
		(property "Reference" "UNK"
			(at -2.3876 -3.4036 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.08 5.08)
			(drill 3.81)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "NetL1_1")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikThroughHole.PcbLib:CAP400X100"
		(layer "F.Cu")
		(at 155.3591 87.465295 -90)
		(property "Reference" "C8"
			(at -4.826 -3.302 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 10.2743 1.5113 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -3.81 -0.762 270)
			(size 1.778 1.778)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "NetC8_1")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 3.81 0.762 270)
			(size 1.778 1.778)
			(drill 0.9398)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "GND")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C__Data_FromLaptop_Projects_ClikPcb_ClikGeneric.PcbLib:M_MTHOLE"
		(layer "F.Cu")
		(at 129.4511 68.161295)
		(property "Reference" "UNK"
			(at -2.3876 -3.4036 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.08 5.08)
			(drill 3.81)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikGeneric.PcbLib:G_0805[2012]"
		(layer "F.Cu")
		(at 150.7871 120.485295)
		(property "Reference" "C2"
			(at 2.286 0.508 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -1.8923 1.5367 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0 90)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "NetC2_1")
		)
		(pad "2" smd rect
			(at 0.95 0 90)
			(size 1.5 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "NetC2_2")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_1206[3216]"
		(layer "F.Cu")
		(at 153.0731 78.067295)
		(property "Reference" "R8"
			(at -1.27 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -0.7493 4.5847 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.4 0 90)
			(size 1.8 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "NetC3_2")
		)
		(pad "2" smd rect
			(at 1.4 0 90)
			(size 1.8 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "NetC8_1")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_1206[3216]"
		(layer "F.Cu")
		(at 164.7571 93.053295 90)
		(property "Reference" "R4"
			(at -1.27 3.048 90)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -4.3307 -0.7493 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.4 0 180)
			(size 1.8 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "NetC2_1")
		)
		(pad "2" smd rect
			(at 1.4 0 180)
			(size 1.8 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "NetC3_1")
		)
	)
	(footprint "ClikGeneric.PcbLib:G_SOT223-8"
		(layer "F.Cu")
		(at 151.5491 116.929295 180)
		(property "Reference" "Q2"
			(at -2.286 4.572 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0.8763 -3.7719 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 0.9398 2.794)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "NetL1_2")
			(zone_connect 2)
		)
		(pad "2" smd rect
			(at 0 1.524 270)
			(size 0.9398 2.794)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "NetQ2_2")
		)
		(pad "3" smd rect
			(at 0 3.048 270)
			(size 0.9398 2.794)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "NetL1_2")
			(zone_connect 2)
		)
		(pad "4" smd rect
			(at 0 4.572 270)
			(size 0.9398 2.794)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "NetQ2_4")
		)
		(pad "5" smd rect
			(at 6.8072 4.572 270)
			(size 0.9398 2.794)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "NetC1_1")
			(zone_connect 2)
		)
		(pad "6" smd rect
			(at 6.8072 3.048 270)
			(size 0.9398 2.794)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "NetC1_1")
			(zone_connect 2)
		)
		(pad "7" smd rect
			(at 6.8072 1.524 270)
			(size 0.9398 2.794)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "NetC1_2")
			(zone_connect 2)
		)
		(pad "8" smd rect
			(at 6.8072 0 270)
			(size 0.9398 2.794)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "NetC1_2")
			(zone_connect 2)
		)
	)
	(footprint "C__Data_FromLaptop_Projects_ClikPcb_ClikGeneric.PcbLib:M_MTHOLE"
		(layer "F.Cu")
		(at 167.5511 141.821295)
		(property "Reference" "UNK"
			(at -2.3876 -3.4036 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.08 5.08)
			(drill 3.81)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "ClikGeneric.PcbLib:G_SO8"
		(layer "F.Cu")
		(at 150.7871 124.295295)
		(property "Reference" "U2"
			(at -4.318 4.064 360)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at -1.3589 4.1783 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -2.54 -1.905)
			(size 2.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "2" smd oval
			(at -2.54 -0.635)
			(size 2.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "NetC2_1")
		)
		(pad "3" smd oval
			(at -2.54 0.635)
			(size 2.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NetC10_2")
		)
		(pad "4" smd oval
			(at -2.54 1.905)
			(size 2.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "GND")
		)
		(pad "5" smd oval
			(at 2.54 1.905)
			(size 2.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd oval
			(at 2.54 0.635)
			(size 2.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "NetC2_2")
		)
		(pad "7" smd oval
			(at 2.54 -0.635)
			(size 2.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "VCC")
		)
		(pad "8" smd oval
			(at 2.54 -1.905)
			(size 2.4 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "NetR10_1")
		)
	)
	(gr_line
		(start 126.91112 146.913605)
		(end 126.9111 146.913605)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.91113 146.925905)
		(end 126.91112 146.913605)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.6311 144.361295)
		(end 172.6311 144.385905)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 126.9111 146.913605)
		(mid 125.115045 146.169657)
		(end 124.3711 144.373605)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 124.3711 65.621295)
		(mid 125.115049 63.825244)
		(end 126.9111 63.081295)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.3711 144.361295)
		(end 124.3711 65.621295)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.0911 146.925905)
		(end 126.91113 146.925905)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.3711 144.373605)
		(end 124.3711 144.361295)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.6311 65.621295)
		(end 172.6311 144.361295)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.0911 63.081295)
		(mid 171.887151 63.825244)
		(end 172.6311 65.621295)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.9111 63.081295)
		(end 170.0911 63.081295)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.6311 144.385905)
		(mid 171.887148 146.18195)
		(end 170.0911 146.925905)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 155.0035 136.995295 90)
		(layer "F.SilkS")
	)
	(gr_text "HV"
		(at 149.7711 75.781295 90)
		(layer "F.SilkS")
	)
	(gr_text "(C) 2014 ERIC SCHLAEPFER"
		(at 170.8531 109.309295 90)
		(layer "F.SilkS")
	)
	(gr_text "VADJ"
		(at 163.9951 127.851295 360)
		(layer "F.SilkS")
	)
	(gr_text "DANGER"
		(at 132.7531 70.955295 360)
		(layer "F.SilkS")
	)
	(gr_text "SP1"
		(at 171.1071 114.897295 90)
		(layer "F.SilkS")
	)
	(gr_text "HIGH VOLTAGE"
		(at 128.6891 74.003295 360)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 157.8991 77.305295 90)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 151.0411 136.995295 90)
		(layer "F.SilkS")
	)
	(zone
		(net 10)
		(net_name "NetL1_1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 153.5811 97.879295) (xy 165.5191 97.879295) (xy 168.8211 101.181295) (xy 168.8211 118.961295)
				(xy 156.3751 118.961295) (xy 155.8671 118.453295) (xy 155.8671 112.611295) (xy 152.8191 109.563295)
				(xy 152.8191 98.641295)
			)
		)
	)
	(zone
		(net 9)
		(net_name "NetL1_2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 145.1991 97.625295) (xy 150.7871 97.625295) (xy 151.8031 98.641295) (xy 151.8031 110.833295)
				(xy 153.0731 112.103295) (xy 153.0731 118.199295) (xy 147.7391 118.199295) (xy 147.7391 111.849295)
				(xy 142.6591 106.769295) (xy 142.6591 100.165295)
			)
		)
	)
	(zone
		(net 7)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 129.1971 132.931295) (xy 129.7051 132.423295) (xy 141.1351 132.423295) (xy 142.1511 133.401295)
				(xy 146.6211 133.401295) (xy 151.8031 139.027295) (xy 151.8031 145.631295) (xy 134.2771 145.631295)
				(xy 133.5151 144.869295) (xy 133.5151 139.281295) (xy 132.2451 138.011295) (xy 130.2131 138.011295)
				(xy 129.1971 136.995295)
			)
		)
	)
	(zone
		(net 5)
		(net_name "NetC1_2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 136.1211 121.651295) (xy 133.3711 121.651295) (xy 132.1211 122.901295) (xy 132.1211 124.401295)
				(xy 132.1211 127.151295) (xy 132.8711 127.901295) (xy 134.6211 127.901295) (xy 135.1211 127.401295)
				(xy 135.1211 123.651295) (xy 135.8711 122.901295) (xy 138.1211 122.901295) (xy 138.6211 122.401295)
				(xy 138.6211 118.401295) (xy 139.6211 117.437295) (xy 146.4691 117.437295) (xy 146.4691 114.897295)
				(xy 138.5311 114.897295) (xy 136.1211 117.401295)
			)
		)
	)
	(zone
		(net 16)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 137.3711 127.651295) (xy 137.3711 124.401295) (xy 138.6211 124.401295) (xy 139.1211 124.901295)
				(xy 139.1211 125.819295) (xy 161.4551 125.819295) (xy 161.9631 125.311295) (xy 161.9631 120.993295)
				(xy 162.4711 120.485295) (xy 170.5991 120.485295) (xy 171.3611 121.247295) (xy 171.3611 145.123295)
				(xy 170.8531 145.631295) (xy 152.0571 145.631295) (xy 152.0571 138.011295) (xy 147.2311 132.931295)
				(xy 129.4511 132.931295) (xy 129.4511 128.105295) (xy 136.8711 128.105295)
			)
		)
	)
	(zone
		(net 6)
		(net_name "NetC1_1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 125.6531 125.901295) (xy 127.6731 127.851295) (xy 129.4511 127.851295) (xy 129.7051 127.597295)
				(xy 129.7051 122.901295) (xy 128.7011 121.901295) (xy 128.7011 118.961295) (xy 133.3711 114.401295)
				(xy 146.4691 114.389295) (xy 146.4691 111.849295) (xy 131.6211 111.901295) (xy 125.6531 117.691295)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 124.296364 65.606429) (xy 124.307742 65.578961) (xy 124.328766 65.557937) (xy 124.356234 65.546559)
				(xy 124.385966 65.546559) (xy 124.413434 65.557937) (xy 124.434458 65.578961) (xy 124.445836 65.606429)
				(xy 124.4473 65.621295) (xy 124.4473 144.361295) (xy 124.445836 144.376161) (xy 124.434458 144.403629)
				(xy 124.413434 144.424653) (xy 124.385966 144.436031) (xy 124.356234 144.436031) (xy 124.328766 144.424653)
				(xy 124.307742 144.403629) (xy 124.296364 144.376161) (xy 124.2949 144.361295) (xy 124.2949 65.621295)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 172.5549 144.361295) (xy 172.569453 144.316506) (xy 172.607553 144.288824) (xy 172.654647 144.288824)
				(xy 172.692747 144.316506) (xy 172.7073 144.361295) (xy 172.69085 144.654216) (xy 172.641706 144.943454)
				(xy 172.560488 145.225371) (xy 172.448215 145.496422) (xy 172.3063 145.753197) (xy 172.136528 145.992469)
				(xy 171.941033 146.211228) (xy 171.722274 146.406723) (xy 171.483002 146.576495) (xy 171.226227 146.71841)
				(xy 170.955176 146.830683) (xy 170.673259 146.911901) (xy 170.384021 146.961045) (xy 170.0911 146.977495)
				(xy 170.046311 146.962942) (xy 170.018629 146.924842) (xy 170.018629 146.877748) (xy 170.046311 146.839648)
				(xy 170.0911 146.825095) (xy 170.240132 146.825095) (xy 170.536024 146.789167) (xy 170.825428 146.717835)
				(xy 171.104123 146.61214) (xy 171.368046 146.473622) (xy 171.613349 146.304302) (xy 171.836454 146.106649)
				(xy 172.034107 145.883544) (xy 172.203427 145.638241) (xy 172.341945 145.374318) (xy 172.44764 145.095623)
				(xy 172.518972 144.806219) (xy 172.5549 144.510327) (xy 172.5549 144.361295)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.105966 146.826559) (xy 170.133434 146.837937) (xy 170.154458 146.858961) (xy 170.165836 146.886429)
				(xy 170.165836 146.916161) (xy 170.154458 146.943629) (xy 170.133434 146.964653) (xy 170.105966 146.976031)
				(xy 170.0911 146.977495) (xy 126.9111 146.977495) (xy 126.896234 146.976031) (xy 126.868766 146.964653)
				(xy 126.847742 146.943629) (xy 126.836364 146.916161) (xy 126.836364 146.886429) (xy 126.847742 146.858961)
				(xy 126.868766 146.837937) (xy 126.896234 146.826559) (xy 126.9111 146.825095) (xy 170.0911 146.825095)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.9111 146.825095) (xy 126.955889 146.839648) (xy 126.983571 146.877748) (xy 126.983571 146.924842)
				(xy 126.955889 146.962942) (xy 126.9111 146.977495) (xy 126.618179 146.961045) (xy 126.328941 146.911901)
				(xy 126.047024 146.830683) (xy 125.775973 146.71841) (xy 125.519198 146.576495) (xy 125.279926 146.406723)
				(xy 125.061167 146.211228) (xy 124.865672 145.992469) (xy 124.6959 145.753197) (xy 124.553985 145.496422)
				(xy 124.441712 145.225371) (xy 124.360494 144.943454) (xy 124.31135 144.654216) (xy 124.2949 144.361295)
				(xy 124.309453 144.316506) (xy 124.347553 144.288824) (xy 124.394647 144.288824) (xy 124.432747 144.316506)
				(xy 124.4473 144.361295) (xy 124.4473 144.510327) (xy 124.483228 144.806219) (xy 124.55456 145.095623)
				(xy 124.660255 145.374318) (xy 124.798773 145.638241) (xy 124.968093 145.883544) (xy 125.165746 146.106649)
				(xy 125.388851 146.304302) (xy 125.634154 146.473622) (xy 125.898077 146.61214) (xy 126.176772 146.717835)
				(xy 126.466176 146.789167) (xy 126.762068 146.825095) (xy 126.9111 146.825095)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 124.4473 65.621295) (xy 124.432747 65.666084) (xy 124.394647 65.693766) (xy 124.347553 65.693766)
				(xy 124.309453 65.666084) (xy 124.2949 65.621295) (xy 124.31135 65.328374) (xy 124.360494 65.039136)
				(xy 124.441712 64.757219) (xy 124.553985 64.486168) (xy 124.6959 64.229393) (xy 124.865672 63.990121)
				(xy 125.061167 63.771362) (xy 125.279926 63.575867) (xy 125.519198 63.406095) (xy 125.775973 63.26418)
				(xy 126.047024 63.151907) (xy 126.328941 63.070689) (xy 126.618179 63.021545) (xy 126.9111 63.005095)
				(xy 126.955889 63.019648) (xy 126.983571 63.057748) (xy 126.983571 63.104842) (xy 126.955889 63.142942)
				(xy 126.9111 63.157495) (xy 126.762068 63.157495) (xy 126.466176 63.193423) (xy 126.176772 63.264755)
				(xy 125.898077 63.37045) (xy 125.634154 63.508968) (xy 125.388851 63.678288) (xy 125.165746 63.875941)
				(xy 124.968093 64.099046) (xy 124.798773 64.344349) (xy 124.660255 64.608272) (xy 124.55456 64.886967)
				(xy 124.483228 65.176371) (xy 124.4473 65.472263) (xy 124.4473 65.621295)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.105966 63.006559) (xy 170.133434 63.017937) (xy 170.154458 63.038961) (xy 170.165836 63.066429)
				(xy 170.165836 63.096161) (xy 170.154458 63.123629) (xy 170.133434 63.144653) (xy 170.105966 63.156031)
				(xy 170.0911 63.157495) (xy 126.9111 63.157495) (xy 126.896234 63.156031) (xy 126.868766 63.144653)
				(xy 126.847742 63.123629) (xy 126.836364 63.096161) (xy 126.836364 63.066429) (xy 126.847742 63.038961)
				(xy 126.868766 63.017937) (xy 126.896234 63.006559) (xy 126.9111 63.005095) (xy 170.0911 63.005095)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.0911 63.157495) (xy 170.046311 63.142942) (xy 170.018629 63.104842) (xy 170.018629 63.057748)
				(xy 170.046311 63.019648) (xy 170.0911 63.005095) (xy 170.384021 63.021545) (xy 170.673259 63.070689)
				(xy 170.955176 63.151907) (xy 171.226227 63.26418) (xy 171.483002 63.406095) (xy 171.722274 63.575867)
				(xy 171.941033 63.771362) (xy 172.136528 63.990121) (xy 172.3063 64.229393) (xy 172.448215 64.486168)
				(xy 172.560488 64.757219) (xy 172.641706 65.039136) (xy 172.69085 65.328374) (xy 172.7073 65.621295)
				(xy 172.692747 65.666084) (xy 172.654647 65.693766) (xy 172.607553 65.693766) (xy 172.569453 65.666084)
				(xy 172.5549 65.621295) (xy 172.5549 65.472263) (xy 172.518972 65.176371) (xy 172.44764 64.886967)
				(xy 172.341945 64.608272) (xy 172.203427 64.344349) (xy 172.034107 64.099046) (xy 171.836454 63.875941)
				(xy 171.613349 63.678288) (xy 171.368046 63.508968) (xy 171.104123 63.37045) (xy 170.825428 63.264755)
				(xy 170.536024 63.193423) (xy 170.240132 63.157495) (xy 170.0911 63.157495)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 172.556364 65.606429) (xy 172.567742 65.578961) (xy 172.588766 65.557937) (xy 172.616234 65.546559)
				(xy 172.645966 65.546559) (xy 172.673434 65.557937) (xy 172.694458 65.578961) (xy 172.705836 65.606429)
				(xy 172.7073 65.621295) (xy 172.7073 144.361295) (xy 172.705836 144.376161) (xy 172.694458 144.403629)
				(xy 172.673434 144.424653) (xy 172.645966 144.436031) (xy 172.616234 144.436031) (xy 172.588766 144.424653)
				(xy 172.567742 144.403629) (xy 172.556364 144.376161) (xy 172.5549 144.361295) (xy 172.5549 65.621295)
			)
		)
	)
	(zone
		(net 16)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 132.4991 137.503295) (xy 133.2611 138.265295) (xy 151.5491 138.265295) (xy 152.0571 138.773295)
				(xy 152.0571 145.631295) (xy 161.9631 145.631295) (xy 163.4871 144.107295) (xy 163.4871 128.105295)
				(xy 161.2011 125.819295) (xy 130.4671 125.819295) (xy 128.4351 127.851295) (xy 128.4351 133.185295)
				(xy 129.1971 133.947295) (xy 131.4831 133.947295) (xy 132.4991 134.963295)
			)
		)
	)
	(zone
		(net 10)
		(net_name "NetL1_1")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 151.8031 97.879295) (xy 167.2971 97.879295) (xy 170.3451 100.927295) (xy 170.3451 124.803295)
				(xy 167.5511 127.597295) (xy 165.2651 127.597295) (xy 158.4071 120.739295) (xy 149.7711 120.739295)
				(xy 147.6211 118.461295) (xy 135.3711 118.461295) (xy 133.2611 116.401295) (xy 133.2611 104.229295)
				(xy 134.5311 102.959295) (xy 146.7231 102.959295)
			)
		)
	)
)
