(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 186)
    (zones 0)
    (modules 6)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user)
    (35 F.Paste user)
    (37 F.SilkS user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1.524)
    (pad_drill 0.85)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 BATT+)
  (net 3 BATT-)
  (net 4 5V)
  (net 5 RESET)
  (net 6 3.3V)
  (net 7 BT3)
  (net 8 BT1)
  (net 9 LED6)
  (net 10 SCL)
  (net 11 SDA)
  (net 12 BT2)
  (net 13 Data5)
  (net 14 RX1)
  (net 15 TX1)
  (net 16 Data4)
  (net 17 Data3)
  (net 18 Data2)
  (net 19 Data1)
  (net 20 LED1)
  (net 21 SP+)
  (net 22 SP-)
  (net 23 LED3)
  (net 24 LED4)
  (net 25 LED5)
  (net 26 LED2)
  (net 27 SWDIO)
  (net 28 SWDCLK)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3V)
    (add_net 5V)
    (add_net BATT+)
    (add_net BATT-)
    (add_net BT1)
    (add_net BT2)
    (add_net BT3)
    (add_net Data1)
    (add_net Data2)
    (add_net Data3)
    (add_net Data4)
    (add_net Data5)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net LED4)
    (add_net LED5)
    (add_net LED6)
    (add_net RESET)
    (add_net RX1)
    (add_net SCL)
    (add_net SDA)
    (add_net SP+)
    (add_net SP-)
    (add_net SWDCLK)
    (add_net SWDIO)
    (add_net TX1)
  )
  (net_class powa ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module lightsaber_parts:screw_hole (layer F.Cu) (tedit 582573F1)
    (at 54.61 71.12)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:screw_hole (layer F.Cu) (tedit 582573F1)
    (at 54.61 101.6)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module lightsaber_parts:screw_hole (layer F.Cu) (tedit 582573F1)
    (at 97.79 101.6)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 59650533)
    (at 52.07 81.28 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 BATT+))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 BATT-))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 5V))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 3.3V))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 RX1))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 TX1))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SDA))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 SCL))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 SWDIO))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 SWDCLK))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 BT1))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 BT2))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 BT3))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 LED6))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 Data5))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 LED5))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 Data4))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 LED4))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 Data3))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 LED3))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 Data2))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 LED2))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 Data1))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 LED1))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 SP+))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 SP-))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lightsaber_parts:ProffieBoardV2.0 (layer F.Cu) (tedit 5C7097F3)
    (at 76.2 94.615)
    (fp_text reference U1 (at 0 2.54) (layer F.SilkS))
    (fp_text value ProffieBoardV2_0 (at 0 -2.54) (layer F.Fab))
    (pad 11 thru_hole circle (at 10.16 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 3 BATT-))
    (pad 20 thru_hole circle (at 10.16 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 3 BATT-))
    (pad 10 thru_hole circle (at 7.62 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 21 SP+))
    (pad 9 thru_hole circle (at 5.08 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 22 SP-))
    (pad 17 thru_hole circle (at 15.24 -5.08) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 26 LED2))
    (pad 16 thru_hole circle (at 15.24 -2.54) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 23 LED3))
    (pad 15 thru_hole circle (at 15.24 2.54) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 24 LED4))
    (pad 14 thru_hole circle (at 15.24 5.08) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 25 LED5))
    (pad 13 thru_hole circle (at 15.24 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 12 BT2))
    (pad 18 thru_hole circle (at 15.24 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 8 BT1))
    (pad 22 thru_hole circle (at 5.08 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 2 BATT+))
    (pad 26 thru_hole circle (at -5.08 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 27 thru_hole circle (at -7.62 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 6 3.3V))
    (pad 28 thru_hole circle (at -10.16 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 19 Data1))
    (pad 29 thru_hole circle (at -12.7 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 15 TX1))
    (pad 30 thru_hole circle (at -15.24 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 16 Data4))
    (pad 1 thru_hole circle (at -15.24 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 13 Data5))
    (pad 2 thru_hole circle (at -12.7 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 18 Data2))
    (pad 3 thru_hole circle (at -10.16 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 10 SCL))
    (pad 4 thru_hole circle (at -7.62 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 27 SWDIO))
    (pad 5 thru_hole circle (at -5.08 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 28 SWDCLK))
    (pad 6 thru_hole circle (at -2.54 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 14 RX1))
    (pad 7 thru_hole circle (at 0 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 17 Data3))
    (pad 8 thru_hole circle (at 2.54 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 7 BT3))
    (pad 12 thru_hole circle (at 12.7 7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 9 LED6))
    (pad 19 thru_hole circle (at 12.7 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 20 LED1))
    (pad 21 thru_hole circle (at 7.62 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 23 thru_hole circle (at 2.54 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 4 5V))
    (pad 24 thru_hole circle (at 0 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 11 SDA))
    (pad 25 thru_hole circle (at -2.54 -7.62) (size 1.75 1.75) (drill 1.05) (layers *.Cu *.Mask F.SilkS)
      (net 5 RESET))
  )
  (module lightsaber_parts:screw_hole (layer F.Cu) (tedit 582573F1)
    (at 97.79 71.12)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value screw_hole (at 0 -0.5) (layer F.Fab))
    (pad 0 thru_hole circle (at 0 0) (size 7 7) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "Proffieboard V2" (at 75.692 71.12) (layer F.Cu))
  (gr_line (start 50.8 71.12) (end 50.8 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 67.31) (end 54.61 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.6 101.6) (end 101.6 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97.79 71.12) (end 97.79 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 54.61 71.12) (end 50.8 71.12) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 54.61 105.41) (end 97.79 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 97.79 101.6) (end 101.6 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 54.61 101.6) (end 54.61 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.18 66.04) (xy 106.68 66.04) (xy 106.68 106.68) (xy 43.18 106.68)
      )
    )
  )
  (zone (net 3) (net_name BATT-) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43.18 66.04) (xy 106.68 66.04) (xy 106.68 106.68) (xy 43.18 106.68)
      )
    )
  )
)
