(kicad_pcb (version 20171130) (host pcbnew "(5.1.9)-1")
  (general
    (thickness 1.6)
    (drawings 44)
    (tracks 132)
    (zones 0)
    (modules 17)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 3.1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 55.8292 21.3868 270)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference GPIO (at -1.9304 2.6416 270) (layer F.SilkS) hide)
    (fp_text value PinSocket_2x20_P2.54mm_Vertical (at -1.27 -51.03 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -24.13) (layer B.Fab))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 81.3308 37.6428)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 220Ω (at 4.8768 2.54) (layer F.SilkS))
    (fp_text value R3 (at 5.08 0) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 82.55 27.7368)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 220Ω (at 5.2832 2.4892) (layer F.SilkS))
    (fp_text value R2 (at 5.08 0) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 67.2084 27.6352)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 220Ω (at 5.1816 2.5908) (layer F.SilkS))
    (fp_text value R1 (at 5.08 0) (layer F.SilkS))
    (fp_text user %R (at 5.08 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x07_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 56.8452 52.3748)
    (descr "Through hole straight pin header, 2x07, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.54mm double row")
    (fp_text reference "DIP SWITCH" (at 1.27 18.542) (layer F.SilkS))
    (fp_text value PinHeader_2x07_P2.54mm_Vertical (at 1.27 17.57) (layer F.Fab))
    (fp_text user %R (at 1.27 7.62 90) (layer F.Fab))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 55.4736 46.8376)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C1 (at 2.4765 0.0635 180) (layer F.SilkS))
    (fp_text value 0.1uf (at 2.6416 -2.1844) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module segastv:Generic_0.96in-128x64-OLED-Display-IIC (layer F.Cu) (tedit 590F4B36)
    (at 79.4512 58.7756)
    (descr http://www.ebay.com/itm/0-96-I2C-IIC-SPI-Serial-128X64-White-OLED-LCD-LED-Display-Module-for-Arduino-BU/361916106520)
    (fp_text reference DS1 (at 0 -15) (layer F.SilkS) hide)
    (fp_text value "OLED PANEL  (128x64)" (at -0.1016 0.1524) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 10.35 11.6) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -10.35 11.6) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -10.35 -11.6) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 3.81 -11.95) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 1.27 -11.95) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1.27 -11.95) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at -3.81 -11.95) (size 2.1 2.1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.35 -11.6) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 55.88 30.5816 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C2 (at 2.4765 0.0635 270) (layer F.SilkS))
    (fp_text value 0.1uf (at 2.6924 -2.1336 90) (layer F.SilkS))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:USB_A_Female_UE27AC54100 (layer F.Cu) (tedit 5D25FE01)
    (at 101.3968 33.8328 90)
    (fp_text reference "RPi USB PWR" (at 9.4488 3.5941) (layer F.SilkS))
    (fp_text value USB_A_Female_UE27AC54100 (at 0 12 90) (layer F.Fab))
    (fp_text user %R (at -0.025 0.975 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 3.5 -2.71 90) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 1 -2.71 90) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -1 -2.71 90) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.5 -2.71 90) (size 1.9 1.9) (drill 0.92) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at 6.57 0 90) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at -6.57 0 90) (size 3.3 3.3) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_TopOnly (layer F.Cu) (tedit 607D7681)
    (at 109.8296 71.5772)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_TopOnly (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 connect circle (at 0 0) (size 5 5) (layers F.Cu F.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_TopOnly (layer F.Cu) (tedit 607D764D)
    (at 49.276 71.5264)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_TopOnly (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.1) (layers *.Cu *.Mask))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers F.Cu F.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_TopOnly (layer F.Cu) (tedit 607D7672)
    (at 109.7788 19.177)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_TopOnly (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.1) (layers *.Cu *.Mask))
    (pad 1 connect circle (at 0 0) (size 5 5) (layers F.Cu F.Mask))
  )
  (module MountingHole:MountingHole_2.5mm_Pad_TopOnly (layer F.Cu) (tedit 607D765E)
    (at 49.276 19.177)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm_Pad_TopOnly (at 0 3.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 connect circle (at 0 0) (size 5 5) (layers F.Cu F.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.1) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 108.6104 46.2788 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 220Ω (at 5.207 -2.4765 90) (layer F.SilkS))
    (fp_text value R4 (at 5.08 0 90) (layer F.SilkS))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 97.028 65.786)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SELECT (at 3.25 7.3406) (layer F.SilkS))
    (fp_text value SW_PUSH_6mm (at 3.75 6.7) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 96.9518 55.372)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference DOWN (at 3.25 7.5184) (layer F.SilkS))
    (fp_text value SW_PUSH_6mm (at 3.75 6.7) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5A02FE31)
    (at 96.9264 46.7868)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference UP (at 3.0988 -2.9972) (layer F.SilkS))
    (fp_text value SW_PUSH_6mm (at 3.75 6.7) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 54.1528 22.4536) (layer F.SilkS))
  (gr_text 14 (at 62.484 67.9196 -90) (layer F.SilkS))
  (gr_text 2 (at 62.3824 52.578 -90) (layer F.SilkS))
  (gr_text 6 (at 62.4332 57.5564 -90) (layer F.SilkS))
  (gr_text 10 (at 62.4332 62.8396 -90) (layer F.SilkS))
  (gr_text 8 (at 62.4332 60.1472 -90) (layer F.SilkS))
  (gr_text 4 (at 62.3824 55.1688 -90) (layer F.SilkS))
  (gr_text 12 (at 62.4332 65.3796 -90) (layer F.SilkS))
  (gr_line (start 110.0582 74.3712) (end 49.022 74.3585) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 49.022 16.383) (end 110.0582 16.383) (layer Edge.Cuts) (width 0.05))
  (gr_text 13 (at 53.848 67.9196 90) (layer F.SilkS))
  (gr_text "CPSII-Pi MULTI SELECTOR" (at 48.9712 68.4784 90) (layer F.SilkS))
  (gr_text 11 (at 53.7972 65.3796 90) (layer F.SilkS))
  (gr_text 9 (at 53.7972 62.8396 90) (layer F.SilkS))
  (gr_text 7 (at 53.7972 60.1472 90) (layer F.SilkS))
  (gr_text 5 (at 53.7972 57.5564 90) (layer F.SilkS))
  (gr_text 3 (at 53.7464 55.1688 90) (layer F.SilkS))
  (gr_text SDA (at 83.4136 43.688) (layer F.SilkS))
  (gr_text SCL (at 80.772 43.688) (layer F.SilkS))
  (gr_text GND (at 75.6412 43.688) (layer F.SilkS))
  (gr_text VCC (at 78.3336 43.688) (layer F.SilkS))
  (gr_text "(5V)" (at 95.3008 37.3888 270) (layer F.SilkS))
  (gr_text VCC (at 96.5073 37.4396 270) (layer F.SilkS))
  (gr_text GND (at 96.4184 30.4292 270) (layer F.SilkS))
  (gr_text 1 (at 53.7464 52.578 90) (layer F.SilkS))
  (gr_arc (start 110.0582 71.8312) (end 110.0582 74.3712) (angle -89.14062776) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 49.022 71.8185) (end 46.482 71.8185) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 49.022 18.923) (end 49.022 16.383) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 110.0582 18.923) (end 112.5982 18.923) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "BladeZX  rev1.1" (at 111.4044 62.2808 90) (layer F.SilkS))
  (gr_line (start 46.482 71.8185) (end 46.482 18.923) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112.5982 18.923) (end 112.5982 71.8693) (layer Edge.Cuts) (width 0.05))
)
