(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 97)
    (no_connects 0)
    (area 139.924999 89.924999 160.075001 110.075001)
    (thickness 1.6002)
    (drawings 26)
    (tracks 414)
    (zones 0)
    (modules 38)
    (nets 25)
  )
  (page A4)
  (layers
    (0 Top signal)
    (1 Ground power hide)
    (2 Power jumper hide)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.127)
    (user_trace_width 0.3)
    (trace_clearance 0.127)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4572)
    (via_min_drill 0.254)
    (user_via 0.4572 0.254)
    (user_via 1 0.5)
    (uvia_size 0.4572)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.5 0.5)
    (mod_text_width 0.1)
    (pad_size 3.45 3.45)
    (pad_drill 0)
    (pad_to_mask_clearance 0.125)
    (aux_axis_origin 0 0)
    (visible_elements 7FFECF7D)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 +5V)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D3-Pad2)")
  (net 7 LED)
  (net 8 "Net-(B1-Pad1)")
  (net 9 "Net-(B1-Pad2)")
  (net 10 "Net-(C1-Pad1)")
  (net 11 "Net-(J5-Pad1)")
  (net 12 "Net-(J6-Pad1)")
  (net 13 "Net-(B2-Pad1)")
  (net 14 USART2_TX)
  (net 15 USART2_RX)
  (net 16 I2C1_SCL)
  (net 17 I2C1_SDA)
  (net 18 "Net-(C12-Pad1)")
  (net 19 IMU_INT1)
  (net 20 IMU_INT2)
  (net 21 USART1_TX)
  (net 22 USART1_RX)
  (net 23 "Net-(C15-Pad2)")
  (net 24 "Net-(C5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
    (add_net I2C1_SCL)
    (add_net I2C1_SDA)
    (add_net IMU_INT1)
    (add_net IMU_INT2)
    (add_net LED)
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(B1-Pad2)")
    (add_net "Net-(B2-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net USART1_RX)
    (add_net USART1_TX)
    (add_net USART2_RX)
    (add_net USART2_TX)
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.3)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.4572)
    (uvia_drill 0.254)
    (add_net +3V3)
    (add_net +5V)
    (add_net +BATT)
    (add_net GND)
  )
  (module local:MIC-5353 (layer Bottom) (tedit 5938A71D)
    (at 155.45 104.9 90)
    (fp_text reference U1 (at -1.6 0 360) (layer B.SilkS))
    (fp_text value MIC5353-3.3YMT-TR (at 1.6 0 360) (layer B.Fab))
    (pad 6 smd rect (at -0.5 0.7 90) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 24 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -0.5 -0.7 90) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 5 smd rect (at 0 0.7 90) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 2 smd rect (at 0 -0.7 90) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.5 0.7 90) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0.5 -0.7 90) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 7 smd rect (at 0 0 90) (size 1.4 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer Bottom) (tedit 58AA8408)
    (at 141.7 102.9 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0 0.8 450) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at -1.475 0.1 360) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-1000P (layer Bottom) (tedit 590E3C35)
    (at 142.5 98.5)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference B1 (at 1.1 -2) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 2.5) (layer B.Fab))
    (pad 1 smd rect (at -1.7 0) (size 0.9 1.7) (layers Bottom B.Paste B.Mask)
      (net 8 "Net-(B1-Pad1)"))
    (pad 2 smd rect (at 1.7 0) (size 0.9 1.7) (layers Bottom B.Paste B.Mask)
      (net 9 "Net-(B1-Pad2)"))
  )
  (module Resistors_SMD:R_0402 (layer Bottom) (tedit 590E3C5D)
    (at 144.1 105.2 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 1.45 0 180) (layer B.SilkS))
    (fp_text value 2k2 (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 16 I2C1_SCL))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer Bottom) (tedit 5863D73A)
    (at 141.325 106.4 90)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D2 (at -1.975 -0.1 270) (layer B.SilkS))
    (fp_text value D (at 0 1.5 90) (layer B.Fab))
    (pad 1 smd rect (at -0.85 0 90) (size 0.6 0.8) (layers Bottom B.Paste B.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.85 0 90) (size 0.6 0.8) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
  )
  (module Resistors_SMD:R_0402 (layer Bottom) (tedit 590E3C4E)
    (at 143.9 100.7 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at -1.3 -0.2 180) (layer B.SilkS))
    (fp_text value 2K2 (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 17 I2C1_SDA))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:MS5637 (layer Bottom) (tedit 5902BB28)
    (at 144 102.9 270)
    (fp_text reference U5 (at -2.35 0 270) (layer B.SilkS))
    (fp_text value MS5637 (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -1 1 270) (size 1 1) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -1 -1 270) (size 1 1) (layers Bottom B.Paste B.Mask)
      (net 17 I2C1_SDA))
    (pad 4 smd rect (at 1 1 270) (size 1 1) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 -1 270) (size 1 1) (layers Bottom B.Paste B.Mask)
      (net 16 I2C1_SCL))
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 5904EC8F)
    (at 151.05 96)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 1.8 0) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer Bottom) (tedit 5904EF8B)
    (at 158.45 101.9)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J2 (at -1.375 -0.525) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers Bottom B.Mask)
      (net 23 "Net-(C15-Pad2)"))
  )
  (module local:CPH3225A (layer Bottom) (tedit 590E3C70)
    (at 144.025 107.25 90)
    (descr http://www.sii.co.jp/en/me/files/2016/02/English_Micro-Battery-2016.pdf)
    (tags "battery super capacitor")
    (fp_text reference BT1 (at -1.975 0 180) (layer B.SilkS))
    (fp_text value Battery_Cell (at 2.6 0 360) (layer B.Fab))
    (pad 2 smd rect (at 0 1.1 90) (size 1.4 1.4) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -1.1 90) (size 1.4 1.4) (layers Bottom B.Paste B.Mask)
      (net 1 +BATT))
  )
  (module LEDs:LED_0402 (layer Top) (tedit 5904F0A3)
    (at 158.85 95.125 270)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 1.7 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.7) (layers Top F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.7) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer Top) (tedit 5904F0B8)
    (at 158.85 92.9 90)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 1.775 0 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.4 90) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.7) (layers Top F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.7) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled (layer Bottom) (tedit 5904D798)
    (at 150 106.75 180)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J1 (at -4.525 -2.625 180) (layer B.SilkS))
    (fp_text value CONN_01X04_MALE (at 0 -4.5 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5 1.9375 180) (size 0.6 1.55) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -0.5 1.9375 180) (size 0.6 1.55) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 3 smd rect (at 0.5 1.9375 180) (size 0.6 1.55) (layers Bottom B.Paste B.Mask)
      (net 21 USART1_TX))
    (pad 4 smd rect (at 1.5 1.9375 180) (size 0.6 1.55) (layers Bottom B.Paste B.Mask)
      (net 22 USART1_RX))
    (pad "" smd rect (at -2.8 -1.9375 180) (size 1.2 1.8) (layers Bottom B.Paste B.Mask))
    (pad "" smd rect (at 2.8 -1.9375 180) (size 1.2 1.8) (layers Bottom B.Paste B.Mask))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer Bottom) (tedit 5904EF68)
    (at 158.45 99.35)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J3 (at -1.625 0.05) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers Bottom B.Mask)
      (net 2 GND))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer Bottom) (tedit 5904EFD3)
    (at 158.45 104.45)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J5 (at 1.375 0.425) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers Bottom B.Mask)
      (net 11 "Net-(J5-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer Bottom) (tedit 5904EFD8)
    (at 158.45 107)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J6 (at 0 2) (layer B.SilkS) hide)
    (fp_text value TEST_1P (at 0 -2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers Bottom B.Mask)
      (net 12 "Net-(J6-Pad1)"))
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 5904ECA0)
    (at 151.05 95.125)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 1.75 0.025) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 590E3BBB)
    (at 141.55 93.15 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 0.875 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 5904ED19)
    (at 148.25 93)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at -1.45 0) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 5904EC59)
    (at 148.25 95.65)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at -1.45 0.025) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 5904EC3C)
    (at 148.25 96.525)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -1.45 -0.025) (layer B.SilkS))
    (fp_text value 10nF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 590E3C86)
    (at 155.65 106.45 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -0.9 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 24 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 590E3CAD)
    (at 153.95 102.35)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 1.7 0.05) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 5938B134)
    (at 153.95 101.475)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 1.7 -0.025) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 5904EC68)
    (at 148.25 94.775)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at -1.65 0.025) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 590E3BD9)
    (at 145.325 96.425)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0.325 0.925) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 18 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 590E3CB7)
    (at 155.475 103.35 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 1.825 0 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Bottom) (tedit 590E2196)
    (at 141.2 96.2 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 0.95 180) (layer B.SilkS))
    (fp_text value 510R (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 8 "Net-(B1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Bottom) (tedit 590E3C9C)
    (at 153.75 100.35 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at -1.55 0 180) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Bottom) (tedit 590E3C95)
    (at 153.75 99.35 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -1.6 0 180) (layer B.SilkS))
    (fp_text value 100R (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 7 LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer Bottom) (tedit 590E3D13)
    (at 146.1 98.6 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.1 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 9 "Net-(B1-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 592B7E45)
    (at 148.25 93.9)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at -1.65 -0.025) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:FXOS8700CQ (layer Bottom) (tedit 5903F1C8)
    (at 144 94 90)
    (fp_text reference U4 (at 2.675 0 180) (layer B.SilkS))
    (fp_text value FXOS8700CQ (at 0 -2.875 90) (layer B.Fab))
    (pad 1 smd rect (at -1.275 1) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -1.275 0.5) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 18 "Net-(C12-Pad1)"))
    (pad 3 smd rect (at -1.275 0) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.275 -0.5) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 16 I2C1_SCL))
    (pad 5 smd rect (at -1.275 -1) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -0.5 -1.275 90) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 17 I2C1_SDA))
    (pad 7 smd rect (at 0 -1.275 90) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 0.5 -1.275 90) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 9 smd rect (at 1.275 -1) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 20 IMU_INT2))
    (pad 10 smd rect (at 1.275 -0.5) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 1.275 0) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 19 IMU_INT1))
    (pad 12 smd rect (at 1.275 0.5) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 1.275 1) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 0.5 1.275 90) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at 0 1.275 90) (size 0.3 0.8) (layers Bottom B.Paste B.Mask))
    (pad 16 smd rect (at -0.5 1.275 90) (size 0.3 0.8) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
  )
  (module local:UFQFPN32 (layer Bottom) (tedit 590403A1)
    (at 150 100 270)
    (fp_text reference U2 (at -2.3 -3.65 360) (layer B.SilkS))
    (fp_text value STM32F042K6Ux (at 0 -3.5 270) (layer B.Fab))
    (pad 1 smd rect (at -2.35 1.75 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -2.35 1.25 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 3 smd rect (at -2.35 0.75 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 4 smd rect (at -2.35 0.25 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 23 "Net-(C15-Pad2)"))
    (pad 5 smd rect (at -2.35 -0.25 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 6 smd rect (at -2.35 -0.75 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 19 IMU_INT1))
    (pad 7 smd rect (at -2.35 -1.25 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 20 IMU_INT2))
    (pad 8 smd rect (at -2.35 -1.75 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 14 USART2_TX))
    (pad 9 smd rect (at -1.75 -2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 15 USART2_RX))
    (pad 10 smd rect (at -1.25 -2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(B2-Pad1)"))
    (pad 11 smd rect (at -0.75 -2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 7 LED))
    (pad 12 smd rect (at -0.25 -2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 13 smd rect (at 0.25 -2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 14 smd rect (at 0.75 -2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 15 smd rect (at 1.25 -2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 16 smd rect (at 1.75 -2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 17 smd rect (at 2.35 -1.75 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
    (pad 18 smd rect (at 2.35 -1.25 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 19 smd rect (at 2.35 -0.75 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 21 USART1_TX))
    (pad 20 smd rect (at 2.35 -0.25 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 22 USART1_RX))
    (pad 21 smd rect (at 2.35 0.25 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 22 smd rect (at 2.35 0.75 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 23 smd rect (at 2.35 1.25 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 11 "Net-(J5-Pad1)"))
    (pad 24 smd rect (at 2.35 1.75 180) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 12 "Net-(J6-Pad1)"))
    (pad 25 smd rect (at 1.75 2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 26 smd rect (at 1.25 2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 27 smd rect (at 0.75 2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 28 smd rect (at 0.25 2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 29 smd rect (at -0.25 2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 16 I2C1_SCL))
    (pad 30 smd rect (at -0.75 2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 17 I2C1_SDA))
    (pad 31 smd rect (at -1.25 2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask)
      (net 9 "Net-(B1-Pad2)"))
    (pad 32 smd rect (at -1.75 2.35 270) (size 0.3 0.6) (layers Bottom B.Paste B.Mask))
    (pad 33 smd rect (at 0 0 270) (size 3.45 3.45) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-3000P (layer Bottom) (tedit 5904D714)
    (at 156.025 91.65 180)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference B2 (at 1.3 -2.15 180) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -2.5 180) (layer B.Fab))
    (fp_text user %R (at 0 3 180) (layer B.Fab))
    (pad 1 smd rect (at -1.7 0 180) (size 0.9 1.7) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(B2-Pad1)"))
    (pad 2 smd rect (at 1.7 0 180) (size 0.9 1.7) (layers Bottom B.Paste B.Mask)
      (net 3 +3V3))
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 592C7E97)
    (at 151.05 93.8 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at 0 0.9 180) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 23 "Net-(C15-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer Bottom) (tedit 5938A105)
    (at 153.8 105.55 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 1.45 0 360) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers Bottom B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:SAM-M8Q (layer Top) (tedit 58E6FB10)
    (at 150 100)
    (fp_text reference U3 (at 0.05 -8.95) (layer F.SilkS))
    (fp_text value SAM-M8Q (at 0 10.5) (layer F.Fab))
    (pad 1 smd rect (at -6.6 -3.8 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -6.6 -1.9 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -6.6 0 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd rect (at -6.6 1.9 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -6.6 3.8 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -3.8 6.6) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -1.9 6.6) (size 1.7 2) (layers Top F.Paste F.Mask))
    (pad 8 smd rect (at 0 6.6) (size 1.7 2) (layers Top F.Paste F.Mask))
    (pad 9 smd rect (at 1.9 6.6) (size 1.7 2) (layers Top F.Paste F.Mask))
    (pad 10 smd rect (at 3.8 6.6) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 6.6 3.8 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 6.6 1.9 90) (size 1.7 2) (layers Top F.Paste F.Mask))
    (pad 13 smd rect (at 6.6 0 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 15 USART2_RX))
    (pad 14 smd rect (at 6.6 -1.9 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 14 USART2_TX))
    (pad 15 smd rect (at 6.6 -3.8 90) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 3.8 -6.6) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 1.9 -6.6) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 3 +3V3))
    (pad 18 smd rect (at 0 -6.6) (size 1.7 2) (layers Top F.Paste F.Mask))
    (pad 19 smd rect (at -1.9 -6.6) (size 1.7 2) (layers Top F.Paste F.Mask))
    (pad 20 smd rect (at -3.8 -6.6) (size 1.7 2) (layers Top F.Paste F.Mask)
      (net 2 GND))
  )
  (gr_text Boot0 (at 141.9 100.6) (layer B.SilkS))
  (gr_text SWDCLK (at 157.075 107.5 90) (layer B.SilkS))
  (gr_text SWDIO (at 157.1 104.425 90) (layer B.SilkS))
  (gr_text NRST (at 157.1 101.925 90) (layer B.SilkS))
  (gr_text GND (at 157.025 99.35 90) (layer B.SilkS))
  (gr_text +Y (at 155.3 108.5) (layer F.SilkS))
  (gr_text +X (at 158.6 105.5) (layer F.SilkS))
  (gr_text GND (at 151.95 103.5) (layer B.SilkS))
  (gr_text 5V (at 150.575 103.525) (layer B.SilkS))
  (gr_text Tx (at 149.45 103.5) (layer B.SilkS))
  (gr_text Rx (at 148.45 103.5) (layer B.SilkS))
  (gr_text "GPS Diamond V1.1\n" (at 148.7 108.7) (layer F.SilkS))
  (gr_line (start 158 110) (end 142 110) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160 92) (end 160 108) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 142 108) (end 142 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158 108) (end 160 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158 92) (end 158 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 142 92) (end 140 92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142 90) (end 158 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 108) (end 140 92) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 90) (xy 160 90) (xy 160 110) (xy 140 110)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Ground) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 90) (xy 160 90) (xy 160 110) (xy 140 110)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer Power) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140 90) (xy 160 90) (xy 160 110) (xy 140 110)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.16)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.3) (smoothing chamfer))
    (polygon
      (pts
        (xy 140 90) (xy 160 90) (xy 160 110) (xy 140 110)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch none 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.325 93.325) (xy 144.675 93.325) (xy 144.675 94.675) (xy 143.325 94.675)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Power) (hatch none 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.325 93.325) (xy 144.675 93.325) (xy 144.675 94.675) (xy 143.325 94.675)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Ground) (hatch none 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.325 93.325) (xy 144.675 93.325) (xy 144.675 94.675) (xy 143.325 94.675)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Top) (hatch none 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.325 93.325) (xy 144.675 93.325) (xy 144.675 94.675) (xy 143.325 94.675)
      )
    )
  )
)
