(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "W7ZOI TIA")
    (date "2024-01-16")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-In)")
  (net 2 "Net-(Q1-B)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(Q2-C)")
  (net 5 "GND")
  (net 6 "Net-(Q1-E)")
  (net 7 "Net-(C5-Pad2)")
  (net 8 "Net-(C6-Pad1)")
  (net 9 "Net-(J2-In)")
  (net 10 "+12V")
  (net 11 "Net-(Q1-C)")
  (net 12 "Net-(Q2-E)")
  (net 13 "Net-(Q3-E)")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 146.05 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 4.56 0 180) (layer "F.SilkS"))
    (fp_text value "15" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm" (layer "F.Cu")
    (at 133.39 92.71)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 1.11 2.34) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-In)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 133.35 88.9 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 4.5 0 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(Q1-B)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 144.78 86.36 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at -2.21 -0.02 180) (layer "F.SilkS"))
    (fp_text value "330" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(Q1-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad_Via" (layer "F.Cu")
    (at 129.19 84.19)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
  )
  (footprint "Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm" (layer "F.Cu")
    (at 160.02 92.71)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 1.105 2.34) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.55) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-In)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad_Via" (layer "F.Cu")
    (at 167.71 84.19)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
  )
  (footprint "Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm" (layer "F.Cu")
    (at 150.3 87.6 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 1.48 2.29) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.55) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm" (layer "F.Cu")
    (at 142.24 97.79 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 4.56 -0.01 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.55 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-E)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 128.27 93.35 180)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr smd)
    (fp_text reference "J1" (at 0.07 6.6 180) (layer "F.SilkS") hide)
    (fp_text value "Conn_Coaxial" (at 5 6) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J1-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 134.62 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 4.56 -0.03 180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 4.06 2.47 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(Q1-B)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad_Via" (layer "F.Cu")
    (at 129.19 102.48)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 149.86 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 4.56 0.01 180) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Q2-E)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 160.02 87.63 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at 2.63 1.18 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Pin" (at 0 4.87 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 149.86 93.98 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q3" (at -1.42 -2.59 180) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q3-E)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Q2-E)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 168.61 93.35)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr smd)
    (fp_text reference "J2" (at -0.0275 -6.6 180) (layer "F.SilkS") hide)
    (fp_text value "Conn_Coaxial" (at 5 6) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 4.79 0 270) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(J2-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 154.94 92.71)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 1.31 2.415) (layer "F.SilkS") hide)
    (fp_text value "47" (at 1.27 2.37) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q3-E)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(C6-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 144.78 93.98 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q2" (at -1.42 -2.42 180) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(Q2-E)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(Q1-C)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 139.7 93.98 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at -1.42 -2.33 180) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-E)") (pinfunction "E") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(Q1-B)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 90) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(Q1-C)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad_Via" (layer "F.Cu")
    (at 167.71 102.48)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pad" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input"))
    (pad "1" thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
    (pad "1" thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pinfunction "1") (pintype "input") (zone_connect 2))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 153.67 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 4.56 0.04 180) (layer "F.SilkS"))
    (fp_text value "470" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(Q3-E)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D3.8mm_W2.6mm_P2.50mm" (layer "F.Cu")
    (at 137.16 86.4 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.8*2.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.8mm width 2.6mm Capacitor")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at -2 0.01 180) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.55 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.8mm_W2.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 138.43 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 4.56 0.03 180) (layer "F.SilkS"))
    (fp_text value "180" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-E)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 140.97 86.36 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at -2.21 -0.03 -180) (layer "F.SilkS"))
    (fp_text value "680" (at 1.27 2.37 90) (layer "F.Fab") hide)
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(Q1-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "F.Cu")
    (at 153.67 87.63)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "tia_amp.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 1.27 -2.32) (layer "F.SilkS"))
    (fp_text value "10" (at 1.27 2.37) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 -2.37) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q2-C)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 125.449 80.65) (end 171.45 106.013)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "R9" (at 156.07 95.05) (layer "F.SilkS"))
  (gr_text "TIA Amp\nW7ZOI & K3NHI\nPCB: VE3CBW\nRev 1.0" (at 155.58 102.93) (layer "F.SilkS"))
  (zone (net 5) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.5 80.67)
        (xy 125.51 106.02)
        (xy 171.59 106.05)
        (xy 171.37 80.75)
      )
    )
  )
  (zone (net 5) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 125.51 80.68)
        (xy 125.51 105.96)
        (xy 171.44 105.98)
        (xy 171.39 80.72)
      )
    )
  )
)
