(kicad_pcb (version 20171130) (host pcbnew "(5.1.12-1-10_14)")
  (general
    (thickness 1.6002)
    (drawings 17)
    (tracks 76)
    (zones 0)
    (modules 17)
    (nets 15)
  )
  (page USLetter)
  (title_block
    (rev 1)
  )
  (layers
    (0 Front signal hide)
    (31 Back signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.6858 0.3302)
    (user_via 0.889 0.381)
    (uvia_size 0.6858)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.0381)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.127)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerbers"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 LED1)
  (net 4 "Net-(D1-Pad1)")
  (net 5 VDC)
  (net 6 "Net-(Q1-Pad4)")
  (net 7 V_IN)
  (net 8 "Net-(R1-Pad2)")
  (net 9 "Net-(R2-Pad2)")
  (net 10 "Net-(R2-Pad1)")
  (net 11 LED3)
  (net 12 LED2)
  (net 13 "Net-(U2-Pad5)")
  (net 14 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.6858)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net GND)
    (add_net LED1)
    (add_net LED2)
    (add_net LED3)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(Q1-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U2-Pad5)")
    (add_net VCC)
    (add_net VDC)
    (add_net V_IN)
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer Front) (tedit 5A02FF57)
    (at 125.7554 73.9648 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 3.22072 -3.43916 180) (layer F.SilkS))
    (fp_text value AMS1117-5.0 (at 3.23088 -1.61036 180) (layer F.Fab))
    (fp_text user %R (at -0.05588 0.47244) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers Front F.Paste F.Mask)
      (net 7 V_IN))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers Front F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers Front F.Paste F.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer Front) (tedit 5995936A)
    (at 144.1958 93.1164 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 1.50368 -0.04572 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 LED3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer Front) (tedit 5995936A)
    (at 137.3378 93.1164 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 1.50368 -0.05588 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 LED2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer Front) (tedit 5995936A)
    (at 130.6068 93.1164 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.45288 -0.08636 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 LED1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type011_RT05502HBWC_1x02_P5.00mm_Horizontal (layer Front) (tedit 5B294E99)
    (at 120.2944 82.7786 270)
    (descr "terminal block Metz Connect Type011_RT05502HBWC, 2 pins, pitch 5mm, size 10x10.5mm^2, drill diamater 1.4mm, pad diameter 2.8mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_310111_RT055xxHBLC_OFF-022717S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
    (tags "THT terminal block Metz Connect Type011_RT05502HBWC pitch 5mm size 10x10.5mm^2 drill 1.4mm pad 2.8mm")
    (fp_text reference J2 (at 6.4516 -4.2926 180) (layer F.SilkS) hide)
    (fp_text value Screw_Terminal_01x02 (at 2.5 5.06 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.32664 -4.37896 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 5 VDC))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type011_RT05502HBWC_1x02_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1%2C5-2-5.08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer Front) (tedit 56D1B4CB)
    (at 154.7114 92.71)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer Front) (tedit 56D1B4CB)
    (at 154.7114 71.882)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer Front) (tedit 56D1B4CB)
    (at 118.11 71.882)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer Front) (tedit 56D1B4CB)
    (at 118.11 92.71)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Front) (tedit 5AE5139B)
    (at 137.4013 71.1454 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 4.8387 -0.1016 90) (layer F.SilkS))
    (fp_text value 330 (at 0.88392 -0.0635 90) (layer F.Fab))
    (fp_text user %R (at 4.1148 0.0127 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(Q1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer Front) (tedit 5AE50EF0)
    (at 119.2784 75.7936 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 0.00508 0.0762 180) (layer F.SilkS))
    (fp_text value "22uF tantalum" (at 1.25 3.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25984 -0.01016 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer Front) (tedit 5A02E8C5)
    (at 130.1877 87.503 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 6.8072 10.05586 180) (layer F.SilkS))
    (fp_text value ATtiny85-20PU (at 8.128 3.70586 180) (layer F.Fab))
    (fp_text user %R (at 3.67284 3.45186 180) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 LED1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 LED3))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 LED2))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad5)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H9.5mm (layer Front) (tedit 5A02FE31)
    (at 144.2847 71.0946)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=9.5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.49758 2.2987) (layer F.SilkS))
    (fp_text value SW_SPST (at 3.15722 6.54304) (layer F.Fab) hide)
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H9.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Front) (tedit 5AE5139B)
    (at 124.8156 92.8116 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 4.318 1.48336) (layer F.SilkS))
    (fp_text value 10k (at 0.46228 0.17272) (layer F.Fab))
    (fp_text user %R (at 4.0894 -0.0254) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer Front) (tedit 5AE5139B)
    (at 140.7668 71.1454 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 4.8006 -0.0889 90) (layer F.SilkS))
    (fp_text value 10k (at 0.92456 -0.04572 90) (layer F.Fab))
    (fp_text user %R (at 3.9116 -0.04572 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer Front) (tedit 5D9F72B1)
    (at 132.8801 73.279 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference Q1 (at 2.47904 -3.50266 180) (layer F.SilkS))
    (fp_text value FDS4559 (at 0 3.4 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDC))
    (pad 7 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDC))
    (pad 6 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDC))
    (pad 5 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 VDC))
    (pad 4 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(Q1-Pad4)"))
    (pad 3 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(J1-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 V_IN))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer Front) (tedit 5A1DBF6A)
    (at 142.5194 83.8962 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at -9.76376 -5.84708) (layer F.SilkS) hide)
    (fp_text value Barrel_Jack (at -6.2 -5.5) (layer F.Fab) hide)
    (fp_text user %R (at -4.7498 0.06604) (layer F.Fab))
    (pad 3 thru_hole roundrect (at -3 4.7 180) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (pad 2 thru_hole roundrect (at -6 0 180) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/barrel-jack-horizontal.step
      (offset (xyz -14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text KM6BSQ (at 150.96236 90.39098) (layer F.SilkS))
  (gr_text "+\n" (at 117.221 87.69604 90) (layer B.SilkS))
  (gr_text - (at 117.27688 82.63636 90) (layer B.SilkS))
  (gr_text github.com/ikatkov/24h-timer-switch (at 155.28036 82.27568 90) (layer B.SilkS))
  (gr_text "24h timer switch v1\n" (at 153.48712 82.27568 90) (layer B.SilkS))
  (gr_text * (at 131.064 74.0664) (layer F.SilkS))
  (gr_text - (at 117.094 82.80908 90) (layer F.SilkS))
  (gr_text + (at 117.13972 87.7316) (layer F.SilkS))
  (gr_text * (at 131.064 85.217) (layer F.SilkS))
  (gr_text + (at 133.3627 89.1032) (layer F.SilkS))
  (gr_text + (at 140.0048 89.1286) (layer F.SilkS))
  (gr_text + (at 146.7612 89.1413) (layer F.SilkS))
  (gr_line (start 115.57 95.25) (end 115.5446 69.3674) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 156.2514 95.25) (end 115.57 95.25) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 156.2514 69.3674) (end 156.2514 95.25) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 115.5446 69.3674) (end 156.2514 69.3674) (layer Edge.Cuts) (width 0.0381))
  (zone (net 1) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.11806 69.95668) (xy 152.11806 94.7928) (xy 118.14302 94.5642) (xy 118.28272 69.7738)
      )
    )
  )
)
