(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 130)
    (no_connects 0)
    (area 43.612999 45.644999 258.139001 111.835001)
    (thickness 1.6)
    (drawings 22)
    (tracks 480)
    (zones 0)
    (modules 51)
    (nets 65)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 1)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 172.974 24.638)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(350ma1-Pad3)")
  (net 2 "Net-(350ma1-Pad4)")
  (net 3 +24V)
  (net 4 GNDPWR)
  (net 5 /led0)
  (net 6 GND)
  (net 7 "Net-(350ma2-Pad3)")
  (net 8 "Net-(350ma2-Pad4)")
  (net 9 /led1)
  (net 10 "Net-(350ma3-Pad3)")
  (net 11 "Net-(350ma3-Pad4)")
  (net 12 "Net-(350ma4-Pad3)")
  (net 13 "Net-(350ma4-Pad4)")
  (net 14 /led3)
  (net 15 "Net-(350ma5-Pad3)")
  (net 16 "Net-(350ma5-Pad4)")
  (net 17 /led4)
  (net 18 "Net-(350ma6-Pad3)")
  (net 19 "Net-(350ma6-Pad4)")
  (net 20 /led5)
  (net 21 "Net-(350ma7-Pad3)")
  (net 22 "Net-(350ma7-Pad4)")
  (net 23 /led6)
  (net 24 "Net-(350ma8-Pad3)")
  (net 25 "Net-(350ma8-Pad4)")
  (net 26 /led7)
  (net 27 "Net-(350ma9-Pad3)")
  (net 28 "Net-(350ma9-Pad4)")
  (net 29 "Net-(350ma10-Pad3)")
  (net 30 "Net-(350ma10-Pad4)")
  (net 31 /led9)
  (net 32 "Net-(350ma11-Pad3)")
  (net 33 "Net-(350ma11-Pad4)")
  (net 34 /led10)
  (net 35 "Net-(350ma12-Pad3)")
  (net 36 "Net-(350ma12-Pad4)")
  (net 37 /led11)
  (net 38 "Net-(350ma13-Pad3)")
  (net 39 "Net-(350ma13-Pad4)")
  (net 40 /led12)
  (net 41 "Net-(350ma14-Pad3)")
  (net 42 "Net-(350ma14-Pad4)")
  (net 43 /led13)
  (net 44 "Net-(350ma15-Pad3)")
  (net 45 "Net-(350ma15-Pad4)")
  (net 46 /led14)
  (net 47 "Net-(J1-Pad7)")
  (net 48 "Net-(J1-Pad8)")
  (net 49 "Net-(J2-Pad7)")
  (net 50 "Net-(J2-Pad8)")
  (net 51 "Net-(J3-Pad7)")
  (net 52 "Net-(J3-Pad8)")
  (net 53 "Net-(J4-Pad7)")
  (net 54 "Net-(J4-Pad8)")
  (net 55 "Net-(J5-Pad7)")
  (net 56 "Net-(J5-Pad8)")
  (net 57 VCC)
  (net 58 "Net-(U1-Pad16)")
  (net 59 "Net-(U1-Pad17)")
  (net 60 "Net-(U1-Pad21)")
  (net 61 /led2)
  (net 62 /led8)
  (net 63 /sda)
  (net 64 /scl)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /led0)
    (add_net /led1)
    (add_net /led10)
    (add_net /led11)
    (add_net /led12)
    (add_net /led13)
    (add_net /led14)
    (add_net /led2)
    (add_net /led3)
    (add_net /led4)
    (add_net /led5)
    (add_net /led6)
    (add_net /led7)
    (add_net /led8)
    (add_net /led9)
    (add_net /scl)
    (add_net /sda)
    (add_net GND)
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad21)")
    (add_net VCC)
  )
  (net_class 24vpower ""
    (clearance 0.2)
    (trace_width 4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +24V)
    (add_net GNDPWR)
  )
  (net_class 350power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(350ma1-Pad3)")
    (add_net "Net-(350ma1-Pad4)")
    (add_net "Net-(350ma10-Pad3)")
    (add_net "Net-(350ma10-Pad4)")
    (add_net "Net-(350ma11-Pad3)")
    (add_net "Net-(350ma11-Pad4)")
    (add_net "Net-(350ma12-Pad3)")
    (add_net "Net-(350ma12-Pad4)")
    (add_net "Net-(350ma13-Pad3)")
    (add_net "Net-(350ma13-Pad4)")
    (add_net "Net-(350ma14-Pad3)")
    (add_net "Net-(350ma14-Pad4)")
    (add_net "Net-(350ma15-Pad3)")
    (add_net "Net-(350ma15-Pad4)")
    (add_net "Net-(350ma2-Pad3)")
    (add_net "Net-(350ma2-Pad4)")
    (add_net "Net-(350ma3-Pad3)")
    (add_net "Net-(350ma3-Pad4)")
    (add_net "Net-(350ma4-Pad3)")
    (add_net "Net-(350ma4-Pad4)")
    (add_net "Net-(350ma5-Pad3)")
    (add_net "Net-(350ma5-Pad4)")
    (add_net "Net-(350ma6-Pad3)")
    (add_net "Net-(350ma6-Pad4)")
    (add_net "Net-(350ma7-Pad3)")
    (add_net "Net-(350ma7-Pad4)")
    (add_net "Net-(350ma8-Pad3)")
    (add_net "Net-(350ma8-Pad4)")
    (add_net "Net-(350ma9-Pad3)")
    (add_net "Net-(350ma9-Pad4)")
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 578D37A7)
    (at 66.294 49.53)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF11 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FF66)
    (at 232.664 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF10 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FF69)
    (at 218.694 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF9 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FF73)
    (at 195.834 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF8 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FF7B)
    (at 172.974 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF7 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FF7F)
    (at 150.114 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF6 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 578D37B0)
    (at 232.664 49.53)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF3 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FFB4)
    (at 66.294 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF2 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FFB9)
    (at 85.09 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF1 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 192.024 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 /led0))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 205.994 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 /led1))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 219.964 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 61 /led2))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 178.054 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R4 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 /led3))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 164.084 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R5 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 /led4))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 150.114 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R6 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 /led5))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 94.234 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R7 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 23 /led6))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 136.144 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R8 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 26 /led7))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 122.174 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R9 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 62 /led8))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 66.294 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R10 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 31 /led9))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 80.264 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R11 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 /led10))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 108.204 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R12 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 37 /led11))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 51.054 83.82)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R13 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 /led12))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 66.294 83.82)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R14 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 43 /led13))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56648415)
    (at 51.054 78.74)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R15 (at 5.32892 -3.50012) (layer F.SilkS))
    (fp_text value 10k (at 5.08 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 57 VCC))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 46 /led14))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 0)
    (at 207.264 104.14)
    (tags RJ45)
    (fp_text reference J1 (at 0.254 4.826) (layer F.SilkS))
    (fp_text value RJ45 (at 0.14224 -0.1016) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 5.93852 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(350ma1-Pad4)"))
    (pad 2 thru_hole circle (at -3.175 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(350ma1-Pad3)"))
    (pad 3 thru_hole circle (at -1.905 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(350ma2-Pad4)"))
    (pad 4 thru_hole circle (at -0.635 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(350ma2-Pad3)"))
    (pad 5 thru_hole circle (at 0.635 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(350ma3-Pad4)"))
    (pad 6 thru_hole circle (at 1.905 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(350ma3-Pad3)"))
    (pad 7 thru_hole circle (at 3.175 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 4.445 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(J1-Pad8)"))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 0)
    (at 184.404 104.14)
    (tags RJ45)
    (fp_text reference J2 (at 0.254 4.826) (layer F.SilkS))
    (fp_text value RJ45 (at 0.14224 -0.1016) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 5.93852 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(350ma4-Pad4)"))
    (pad 2 thru_hole circle (at -3.175 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(350ma4-Pad3)"))
    (pad 3 thru_hole circle (at -1.905 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(350ma5-Pad4)"))
    (pad 4 thru_hole circle (at -0.635 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(350ma5-Pad3)"))
    (pad 5 thru_hole circle (at 0.635 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(350ma6-Pad4)"))
    (pad 6 thru_hole circle (at 1.905 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(350ma6-Pad3)"))
    (pad 7 thru_hole circle (at 3.175 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at 4.445 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(J2-Pad8)"))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 0)
    (at 138.684 104.14)
    (tags RJ45)
    (fp_text reference J3 (at 0.254 4.826) (layer F.SilkS))
    (fp_text value RJ45 (at 0.14224 -0.1016) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 5.93852 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(350ma10-Pad4)"))
    (pad 2 thru_hole circle (at -3.175 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(350ma10-Pad3)"))
    (pad 3 thru_hole circle (at -1.905 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(350ma11-Pad4)"))
    (pad 4 thru_hole circle (at -0.635 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(350ma11-Pad3)"))
    (pad 5 thru_hole circle (at 0.635 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(350ma12-Pad4)"))
    (pad 6 thru_hole circle (at 1.905 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(350ma12-Pad3)"))
    (pad 7 thru_hole circle (at 3.175 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(J3-Pad7)"))
    (pad 8 thru_hole circle (at 4.445 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(J3-Pad8)"))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 0)
    (at 161.544 104.14)
    (tags RJ45)
    (fp_text reference J4 (at 0.254 4.826) (layer F.SilkS))
    (fp_text value RJ45 (at 0.14224 -0.1016) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 5.93852 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(350ma7-Pad4)"))
    (pad 2 thru_hole circle (at -3.175 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(350ma7-Pad3)"))
    (pad 3 thru_hole circle (at -1.905 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(350ma8-Pad4)"))
    (pad 4 thru_hole circle (at -0.635 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(350ma8-Pad3)"))
    (pad 5 thru_hole circle (at 0.635 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(350ma9-Pad4)"))
    (pad 6 thru_hole circle (at 1.905 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(350ma9-Pad3)"))
    (pad 7 thru_hole circle (at 3.175 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(J4-Pad7)"))
    (pad 8 thru_hole circle (at 4.445 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(J4-Pad8)"))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 0)
    (at 115.824 104.14)
    (tags RJ45)
    (fp_text reference J5 (at 0.254 4.826) (layer F.SilkS))
    (fp_text value RJ45 (at 0.14224 -0.1016) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 5.93852 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(350ma13-Pad4)"))
    (pad 2 thru_hole circle (at -3.175 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(350ma13-Pad3)"))
    (pad 3 thru_hole circle (at -1.905 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(350ma14-Pad4)"))
    (pad 4 thru_hole circle (at -0.635 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(350ma14-Pad3)"))
    (pad 5 thru_hole circle (at 0.635 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(350ma15-Pad4)"))
    (pad 6 thru_hole circle (at 1.905 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(350ma15-Pad3)"))
    (pad 7 thru_hole circle (at 3.175 -6.35) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(J5-Pad7)"))
    (pad 8 thru_hole circle (at 4.445 -8.89) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(J5-Pad8)"))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FFAA)
    (at 103.124 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF4 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 5789FF9F)
    (at 127.254 102.87)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference REF5 (at 0 -3.50012) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module lighting:pwm_pca9685 (layer F.Cu) (tedit 5789F769)
    (at 237.744 55.88 270)
    (fp_text reference U1 (at 10.16 -12.7 270) (layer F.SilkS))
    (fp_text value EBAYPCA9685 (at 10.16 -15.24 270) (layer F.Fab))
    (pad 16 thru_hole circle (at 0 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(U1-Pad16)"))
    (pad 15 thru_hole circle (at 2.54 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 46 /led14))
    (pad 14 thru_hole circle (at 5.08 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 43 /led13))
    (pad 13 thru_hole circle (at 7.62 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 40 /led12))
    (pad 12 thru_hole circle (at 12.7 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 37 /led11))
    (pad 11 thru_hole circle (at 15.24 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 34 /led10))
    (pad 10 thru_hole circle (at 17.78 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 31 /led9))
    (pad 9 thru_hole circle (at 20.32 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 62 /led8))
    (pad 8 thru_hole circle (at 27.94 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 26 /led7))
    (pad 7 thru_hole circle (at 30.48 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 /led6))
    (pad 6 thru_hole circle (at 33.02 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 20 /led5))
    (pad 5 thru_hole circle (at 35.56 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 17 /led4))
    (pad 4 thru_hole circle (at 40.64 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 14 /led3))
    (pad 3 thru_hole circle (at 43.18 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 61 /led2))
    (pad 2 thru_hole circle (at 45.72 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 /led1))
    (pad 1 thru_hole circle (at 48.26 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 /led0))
    (pad 17 thru_hole circle (at -5.08 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at -5.08 -7.62 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 57 VCC))
    (pad 19 thru_hole circle (at -5.08 -10.16 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 63 /sda))
    (pad 20 thru_hole circle (at -5.08 -12.7 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 64 /scl))
    (pad 21 thru_hole circle (at -5.08 -15.24 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at -5.08 -17.78 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 23 thru_hole circle (at 53.34 -5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 24 thru_hole circle (at 53.34 -7.62 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole circle (at 53.34 -10.16 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole circle (at 53.34 -12.7 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole circle (at 53.34 -15.24 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole circle (at 53.34 -17.78 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole circle (at 0 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole circle (at 2.54 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole circle (at 5.08 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole circle (at 7.62 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 33 thru_hole circle (at 12.7 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 34 thru_hole circle (at 15.24 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 35 thru_hole circle (at 17.78 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole circle (at 20.32 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole circle (at 27.94 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 38 thru_hole circle (at 30.48 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 39 thru_hole circle (at 33.02 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 40 thru_hole circle (at 35.56 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 41 thru_hole circle (at 40.64 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 42 thru_hole circle (at 43.18 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 43 thru_hole circle (at 45.72 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 44 thru_hole circle (at 48.26 -2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 45 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 46 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 47 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 48 thru_hole circle (at 7.62 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 49 thru_hole circle (at 12.7 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 50 thru_hole circle (at 15.24 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 51 thru_hole circle (at 17.78 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 52 thru_hole circle (at 20.32 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 53 thru_hole circle (at 27.94 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 54 thru_hole circle (at 30.48 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 55 thru_hole circle (at 33.02 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 56 thru_hole circle (at 35.56 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 57 thru_hole circle (at 40.64 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 58 thru_hole circle (at 43.18 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 59 thru_hole circle (at 45.72 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
    (pad 60 thru_hole circle (at 48.26 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 578D069F)
    (at 227.584 107.95 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference ICC1 (at 0 -3.048 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /sda))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 /scl))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 578D06A2)
    (at 223.774 107.95 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference ICC2 (at 0 -3.048 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /sda))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 /scl))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lighting:350ma_constant_current_xl4001 (layer F.Cu) (tedit 578D07BE)
    (at 191.389 90.17)
    (fp_text reference 350ma1 (at 5.08 -12.7) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(350ma1-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(350ma1-Pad4)"))
    (pad 1 thru_hole rect (at 0 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 /led0))
    (pad 6 thru_hole circle (at 0 -20.32) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer B.Cu) (tedit 578D07BE)
    (at 223.139 90.17 180)
    (fp_text reference 350ma2 (at 5.08 12.7 180) (layer B.SilkS))
    (fp_text value Led_Driver (at 5.08 15.24 180) (layer B.Fab))
    (pad 3 thru_hole rect (at 0 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(350ma2-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(350ma2-Pad4)"))
    (pad 1 thru_hole rect (at 0 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 22.86 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 9 /led1))
    (pad 6 thru_hole circle (at 0 20.32 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer F.Cu) (tedit 578D07BE)
    (at 216.789 90.17)
    (fp_text reference 350ma3 (at 5.08 -12.7) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(350ma3-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(350ma3-Pad4)"))
    (pad 1 thru_hole rect (at 0 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 61 /led2))
    (pad 6 thru_hole circle (at 0 -20.32) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer B.Cu) (tedit 578D07BE)
    (at 197.739 90.17 180)
    (fp_text reference 350ma4 (at 5.08 12.7 180) (layer B.SilkS))
    (fp_text value Led_Driver (at 5.08 15.24 180) (layer B.Fab))
    (pad 3 thru_hole rect (at 0 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(350ma4-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 13 "Net-(350ma4-Pad4)"))
    (pad 1 thru_hole rect (at 0 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 22.86 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 14 /led3))
    (pad 6 thru_hole circle (at 0 20.32 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer F.Cu) (tedit 578D07BE)
    (at 166.751 90.17)
    (fp_text reference 350ma5 (at 5.08 -12.7) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(350ma5-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(350ma5-Pad4)"))
    (pad 1 thru_hole rect (at 0 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 17 /led4))
    (pad 6 thru_hole circle (at 0 -20.32) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer B.Cu) (tedit 578D07BE)
    (at 173.863 90.17 180)
    (fp_text reference 350ma6 (at 5.08 12.7 180) (layer B.SilkS))
    (fp_text value Led_Driver (at 5.08 15.24 180) (layer B.Fab))
    (pad 3 thru_hole rect (at 0 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(350ma6-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(350ma6-Pad4)"))
    (pad 1 thru_hole rect (at 0 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 22.86 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 20 /led5))
    (pad 6 thru_hole circle (at 0 20.32 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer F.Cu) (tedit 578D07BE)
    (at 119.761 90.17)
    (fp_text reference 350ma7 (at 5.08 -12.7) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(350ma7-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(350ma7-Pad4)"))
    (pad 1 thru_hole rect (at 0 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 /led6))
    (pad 6 thru_hole circle (at 0 -20.32) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer B.Cu) (tedit 578D07BE)
    (at 150.749 90.17 180)
    (fp_text reference 350ma8 (at 5.08 12.7 180) (layer B.SilkS))
    (fp_text value Led_Driver (at 5.08 15.24 180) (layer B.Fab))
    (pad 3 thru_hole rect (at 0 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 24 "Net-(350ma8-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(350ma8-Pad4)"))
    (pad 1 thru_hole rect (at 0 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 22.86 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 26 /led7))
    (pad 6 thru_hole circle (at 0 20.32 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer F.Cu) (tedit 578D07BE)
    (at 142.875 90.17)
    (fp_text reference 350ma9 (at 5.08 -12.7) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(350ma9-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(350ma9-Pad4)"))
    (pad 1 thru_hole rect (at 0 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 62 /led8))
    (pad 6 thru_hole circle (at 0 -20.32) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer F.Cu) (tedit 578D07BE)
    (at 96.139 90.17)
    (fp_text reference 350ma10 (at 5.08 -12.7) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(350ma10-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(350ma10-Pad4)"))
    (pad 1 thru_hole rect (at 0 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 31 /led9))
    (pad 6 thru_hole circle (at 0 -20.32) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer B.Cu) (tedit 578D07BE)
    (at 103.505 90.17 180)
    (fp_text reference 350ma11 (at 5.08 12.7 180) (layer B.SilkS))
    (fp_text value Led_Driver (at 5.08 15.24 180) (layer B.Fab))
    (pad 3 thru_hole rect (at 0 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 32 "Net-(350ma11-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 33 "Net-(350ma11-Pad4)"))
    (pad 1 thru_hole rect (at 0 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 22.86 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 34 /led10))
    (pad 6 thru_hole circle (at 0 20.32 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer B.Cu) (tedit 578D07BE)
    (at 127.381 90.17 180)
    (fp_text reference 350ma12 (at 5.08 12.7 180) (layer B.SilkS))
    (fp_text value Led_Driver (at 5.08 15.24 180) (layer B.Fab))
    (pad 3 thru_hole rect (at 0 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 35 "Net-(350ma12-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 36 "Net-(350ma12-Pad4)"))
    (pad 1 thru_hole rect (at 0 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 22.86 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 37 /led11))
    (pad 6 thru_hole circle (at 0 20.32 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer F.Cu) (tedit 578D07BE)
    (at 72.517 90.17)
    (fp_text reference 350ma13 (at 5.08 -12.7) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(350ma13-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(350ma13-Pad4)"))
    (pad 1 thru_hole rect (at 0 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 40 /led12))
    (pad 6 thru_hole circle (at 0 -20.32) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer B.Cu) (tedit 578D07BE)
    (at 79.629 90.17 180)
    (fp_text reference 350ma14 (at 5.08 12.7 180) (layer B.SilkS))
    (fp_text value Led_Driver (at 5.08 15.24 180) (layer B.Fab))
    (pad 3 thru_hole rect (at 0 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 41 "Net-(350ma14-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 42 "Net-(350ma14-Pad4)"))
    (pad 1 thru_hole rect (at 0 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 30.48 180) (size 4 4) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 22.86 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 43 /led13))
    (pad 6 thru_hole circle (at 0 20.32 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 6 GND))
  )
  (module lighting:350ma_constant_current_xl4001 (layer F.Cu) (tedit 578D07BE)
    (at 48.133 90.17)
    (fp_text reference 350ma15 (at 5.08 -12.7) (layer F.SilkS))
    (fp_text value Led_Driver (at 5.08 -15.24) (layer F.Fab))
    (pad 3 thru_hole rect (at 0 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(350ma15-Pad3)"))
    (pad 4 thru_hole rect (at 12.7 0) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(350ma15-Pad4)"))
    (pad 1 thru_hole rect (at 0 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole rect (at 12.7 -30.48) (size 4 4) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 5 thru_hole circle (at 0 -22.86) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 46 /led14))
    (pad 6 thru_hole circle (at 0 -20.32) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 0)
    (at 134.239 51.308)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference BLK1 (at 0 -5.08) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 3 +24V))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 0)
    (at 152.019 51.308)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference BLK2 (at 0 -5.08) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 4 GNDPWR))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 66.04 (width 0.3) (layer Dwgs.User)
    (gr_text "2.6000 in" (at 274.654 79.248 270) (layer Dwgs.User))
    (feature1 (pts (xy 256.794 112.268) (xy 276.004 112.268)))
    (feature2 (pts (xy 256.794 46.228) (xy 276.004 46.228)))
    (crossbar (pts (xy 273.304 46.228) (xy 273.304 112.268)))
    (arrow1a (pts (xy 273.304 112.268) (xy 272.717579 111.141496)))
    (arrow1b (pts (xy 273.304 112.268) (xy 273.890421 111.141496)))
    (arrow2a (pts (xy 273.304 46.228) (xy 272.717579 47.354504)))
    (arrow2b (pts (xy 273.304 46.228) (xy 273.890421 47.354504)))
  )
  (dimension 214.63 (width 0.3) (layer Dwgs.User)
    (gr_text "8.4500 in" (at 150.749 34.718) (layer Dwgs.User))
    (feature1 (pts (xy 258.064 46.228) (xy 258.064 33.368)))
    (feature2 (pts (xy 43.434 46.228) (xy 43.434 33.368)))
    (crossbar (pts (xy 43.434 36.068) (xy 258.064 36.068)))
    (arrow1a (pts (xy 258.064 36.068) (xy 256.937496 36.654421)))
    (arrow1b (pts (xy 258.064 36.068) (xy 256.937496 35.481579)))
    (arrow2a (pts (xy 43.434 36.068) (xy 44.560504 36.654421)))
    (arrow2b (pts (xy 43.434 36.068) (xy 44.560504 35.481579)))
  )
  (gr_text 4 (at 125.349 109.728) (layer F.SilkS))
  (gr_text 3 (at 148.209 109.728) (layer F.SilkS))
  (gr_text 2 (at 171.069 109.728) (layer F.SilkS))
  (gr_text 1 (at 193.929 109.728) (layer F.SilkS))
  (gr_text 0 (at 216.789 109.728) (layer F.SilkS))
  (gr_text - (at 145.034 50.673) (layer F.SilkS))
  (gr_text + (at 141.224 50.673) (layer F.SilkS))
  (gr_text sda (at 234.696 106.172) (layer F.SilkS))
  (gr_text gnd (at 231.648 98.806) (layer F.SilkS))
  (gr_text "vcc\n" (at 231.648 107.95) (layer F.SilkS))
  (gr_text "This board can take up to 30V and drive 5 20W RGB \nLEDs. Do not use common anode or common\ncathode LEDs with this board." (at 45.466 96.266) (layer F.SilkS))
  (gr_text - (at 159.004 50.673) (layer F.SilkS))
  (gr_text + (at 127.254 50.673) (layer F.SilkS))
  (gr_line (start 43.688 111.76) (end 43.688 45.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 258.064 111.76) (end 43.688 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 258.064 45.72) (end 258.064 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 258.064 45.72) (end 43.688 45.72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name +24V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.029 46.228) (xy 232.029 56.388) (xy 44.069 56.388) (xy 44.069 46.228)
      )
    )
  )
  (zone (net 4) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 232.029 46.228) (xy 232.029 56.388) (xy 44.069 56.388) (xy 44.069 46.228)
      )
    )
  )
)
