(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 5)
    (zones 0)
    (modules 11)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 /Bat-)
  (net 3 /Pwr+)
  (net 4 /Bat+)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Bat+)
    (add_net /Bat-)
    (add_net /Pwr+)
    (add_net "Net-(D1-Pad2)")
  )
  (module LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 132.3625 64.95 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 /Bat-))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PDB17:ATC_Fuse_Holder (layer F.Cu) (tedit 5A053E5A)
    (at 109.75 64.65 180)
    (fp_text reference F1 (at -0.25 1.65 180) (layer F.SilkS))
    (fp_text value Fuse (at -0.1 -1.35 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.735 -1.7 180) (size 2.55 2.55) (drill 1.85) (layers *.Cu *.Mask)
      (net 3 /Pwr+))
    (pad 1 thru_hole circle (at -6.735 1.7 180) (size 2.55 2.55) (drill 1.85) (layers *.Cu *.Mask)
      (net 3 /Pwr+))
    (pad 2 thru_hole circle (at 6.735 1.7 180) (size 2.55 2.55) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 2 thru_hole circle (at 6.738 -1.7 180) (size 2.55 2.55) (drill 1.85) (layers *.Cu *.Mask)
      (net 4 /Bat+))
  )
  (module Connector_Molex:Molex_Mega-Fit_76825-0008_2x04_P5.70mm_Horizontal (layer F.Cu) (tedit 5A11601C)
    (at 103.5 52.95)
    (descr "Molex Mega-Fit Power Connectors, 76825-0008 (compatible alternatives: 172064-0008, 172064-1008), 4 Pins per row (http://www.molex.com/pdm_docs/sd/1720640002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mega-Fit top entry")
    (fp_text reference J1 (at 8.5 -10.95) (layer F.SilkS))
    (fp_text value Conn_02x04_Counter_Clockwise (at 8.55 8.55) (layer F.Fab))
    (fp_text user %R (at 8.5 -12.95) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 2 thru_hole circle (at 5.7 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 3 thru_hole circle (at 11.4 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 4 thru_hole circle (at 17.1 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 5 thru_hole circle (at 0 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 6 thru_hole circle (at 5.7 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 7 thru_hole circle (at 11.4 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 8 thru_hole circle (at 17.1 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad "" np_thru_hole circle (at 0 -7.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 17.1 -7.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mega-Fit_76825-0008_2x04_P5.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mega-Fit_76825-0004_2x02_P5.70mm_Horizontal (layer F.Cu) (tedit 5A11601C)
    (at 128.3 52.95)
    (descr "Molex Mega-Fit Power Connectors, 76825-0004 (compatible alternatives: 172064-0004, 172064-1004), 2 Pins per row (http://www.molex.com/pdm_docs/sd/1720640002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mega-Fit top entry")
    (fp_text reference J2 (at 2.7 -10.95) (layer F.SilkS))
    (fp_text value Conn_02x02_Counter_Clockwise (at 2.85 8.55) (layer F.Fab))
    (fp_text user %R (at 2.7 -12.95) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /Pwr+))
    (pad 2 thru_hole circle (at 5.7 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /Pwr+))
    (pad 3 thru_hole circle (at 0 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 4 thru_hole circle (at 5.7 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad "" np_thru_hole circle (at 2.85 -7.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mega-Fit_76825-0004_2x02_P5.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal (layer F.Cu) (tedit 5A11601C)
    (at 152.65 52.95)
    (descr "Molex Mega-Fit Power Connectors, 76825-0002 (compatible alternatives: 172064-0002, 172064-1002), 1 Pins per row (http://www.molex.com/pdm_docs/sd/1720640002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mega-Fit top entry")
    (fp_text reference J3 (at 0 -10.95) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 8.55) (layer F.Fab))
    (fp_text user %R (at 0 -12.95) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /Pwr+))
    (pad 2 thru_hole circle (at 0 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad "" np_thru_hole circle (at 0 -7.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal (layer F.Cu) (tedit 5A11601C)
    (at 162.45 52.95)
    (descr "Molex Mega-Fit Power Connectors, 76825-0002 (compatible alternatives: 172064-0002, 172064-1002), 1 Pins per row (http://www.molex.com/pdm_docs/sd/1720640002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mega-Fit top entry")
    (fp_text reference J4 (at -0.45 -10.95) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 8.55) (layer F.Fab))
    (fp_text user %R (at -0.45 -12.95) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 -7.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 1 thru_hole rect (at 0 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /Pwr+))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal (layer F.Cu) (tedit 5A11601C)
    (at 172.15 52.95)
    (descr "Molex Mega-Fit Power Connectors, 76825-0002 (compatible alternatives: 172064-0002, 172064-1002), 1 Pins per row (http://www.molex.com/pdm_docs/sd/1720640002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mega-Fit top entry")
    (fp_text reference J5 (at -0.15 -10.95) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 8.55) (layer F.Fab))
    (fp_text user %R (at 0 -12.95) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /Pwr+))
    (pad 2 thru_hole circle (at 0 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad "" np_thru_hole circle (at 0 -7.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal (layer F.Cu) (tedit 5A11601C)
    (at 142.85 52.95)
    (descr "Molex Mega-Fit Power Connectors, 76825-0002 (compatible alternatives: 172064-0002, 172064-1002), 1 Pins per row (http://www.molex.com/pdm_docs/sd/1720640002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mega-Fit top entry")
    (fp_text reference J6 (at 0 -10.95) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 8.55) (layer F.Fab))
    (fp_text user %R (at 0 -12.95) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 -7.3) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 5.5) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 1 thru_hole rect (at 0 0) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 3 /Pwr+))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PDB17:Molex_EXTreme_Ten60Power (layer F.Cu) (tedit 5C905092)
    (at 96 54 90)
    (fp_text reference J7 (at 15 -9 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -11.43 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 7.5 -2.5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 7.5 -5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 7.5 -7.5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 4.5 0 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 4.5 -2.5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 4.5 -5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at 0 -2.5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at 0 -5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at 0 -7.5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at -3 0 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at -3 -2.5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at -3 -5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 2 thru_hole circle (at 4.5 -7.5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 1 thru_hole circle (at -3 -7.5 90) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
  )
  (module PDB17:Molex_EXTreme_Ten60Power (layer F.Cu) (tedit 5C905092)
    (at 180.8 50.1 270)
    (fp_text reference J8 (at -11.1 -9.2) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -11.43 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -3 -7.5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 2 thru_hole circle (at 4.5 -7.5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 1 thru_hole circle (at -3 -5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at -3 -2.5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at -3 0 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at 0 -7.5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at 0 -5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at 0 -2.5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 4 /Bat+))
    (pad 2 thru_hole circle (at 4.5 -5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 4.5 -2.5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 4.5 0 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 7.5 -7.5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 7.5 -5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 7.5 -2.5 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 1.75 1.75) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 /Bat-))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 123.3 64.8)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 /Pwr+))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Power Distribution Board 2018-19\nUtah Student Robotics (24V)" (at 156 64) (layer F.SilkS))
  (gr_line (start 84 69) (end 84 36) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193 69) (end 84 69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193 67) (end 193 69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193 36) (end 193 67) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84 36) (end 193 36) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name /Bat-) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 84 36) (xy 193 36) (xy 193 69) (xy 84 69)
      )
    )
  )
  (zone (net 3) (net_name /Pwr+) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 109.5 55.5) (xy 109.5 69) (xy 178.5 69) (xy 178.5 47.5) (xy 124.5 47.5)
        (xy 124.5 55.5)
      )
    )
  )
  (zone (net 4) (net_name /Bat+) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 84 69) (xy 84 36) (xy 193 36) (xy 193 69) (xy 179 69)
        (xy 179 47) (xy 124 47) (xy 124 55) (xy 109 55) (xy 109 69)
      )
    )
  )
)
