(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 12)
    (no_connects 0)
    (area 142.30858 91.0463 165.09238 109.78896)
    (thickness 1.6002)
    (drawings 5)
    (tracks 28)
    (zones 0)
    (modules 3)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "Net-(J2-Pad2)")
  (net 9 "Net-(J2-Pad3)")
  (net 10 "Net-(J2-Pad4)")
  (net 11 "Net-(J2-Pad5)")
  (net 12 "Net-(J2-Pad6)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X06_NO_SILK placed (layer F.Cu) (tedit 59684301)
    (at 144.78 93.98 270)
    (descr "PLATED THROUGH HOLE - 6 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 6 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J1 (at 0.254 2.54 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0.5588 1.7272 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(J1-Pad6)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X06_NO_SILK placed (layer F.Cu) (tedit 59684319)
    (at 162.56 106.68 90)
    (descr "PLATED THROUGH HOLE - 6 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 6 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J2 (at 0 3.81 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0.5588 1.7272 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(J2-Pad6)"))
  )
  (module EAGLE-POWER_MAGNETICS-rev17c:EAGLE-POWER_MAGNETICS-rev17c-WE-FLEX_ER11_5 placed (layer F.Cu) (tedit 5968142A)
    (at 153.67 100.33)
    (attr smd)
    (fp_text reference T1 (at 2.87274 -8.0899) (layer F.SilkS) hide)
    (fp_text value WE-FLEX_ER11/5 (at 0.07366 8.13816) (layer F.SilkS))
    (fp_text user 6 (at -3.2131 4.9149) (layer Dwgs.User))
    (fp_text user 7 (at 3.83286 4.96316) (layer Dwgs.User))
    (fp_text user 12 (at 3.6195 -5.23494) (layer Dwgs.User))
    (pad 1 smd rect (at -5.97408 -4.99872 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at -5.97408 -2.99974 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -5.97408 -0.99822 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -5.97408 0.99822 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -5.97408 2.99974 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -5.97408 4.99872 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at 5.97408 4.99872 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 8 smd rect (at 5.97408 2.99974 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 9 smd rect (at 5.97408 0.99822 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 10 smd rect (at 5.97408 -0.99822 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad4)"))
    (pad 11 smd rect (at 5.97408 -2.99974 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad5)"))
    (pad 12 smd rect (at 5.97408 -4.99872 270) (size 1.4986 2.2479) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad6)"))
  )
  (gr_line (start 163.83 91.44) (end 163.83 91.44) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 163.83 109.22) (end 163.83 91.44) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 143.51 109.22) (end 163.83 109.22) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 143.51 91.44) (end 143.51 109.22) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 163.83 91.44) (end 143.51 91.44) (layer Edge.Cuts) (width 0.127))
)
