(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 5)
    (no_connects 1)
    (area 138.924999 89.924999 154.075001 124.075001)
    (thickness 1.6)
    (drawings 20)
    (tracks 9)
    (zones 0)
    (modules 4)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.01)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VBUS)
  (net 2 D+)
  (net 3 D-)
  (net 4 GND)
  (net 5 "Net-(J1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net D+)
    (add_net D-)
    (add_net GND)
    (add_net "Net-(J1-Pad6)")
    (add_net VBUS)
  )
  (module Parts:Wurth_Micro_USB_2.0_Type_B_Vertical (layer F.Cu) (tedit 59AFECC7)
    (at 148.775 107.225 90)
    (fp_text reference J1 (at 0 -3 90) (layer F.SilkS) hide)
    (fp_text value USB_OTG (at 0 3.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.3 -0.5 90) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 VBUS))
    (pad 2 thru_hole circle (at -0.65 0.5 90) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 3 D-))
    (pad 3 thru_hole circle (at 0 -0.5 90) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 D+))
    (pad 4 thru_hole circle (at 0.65 0.5 90) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 1.3 -0.5 90) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 6 thru_hole oval (at -3.575 -0.28 90) (size 0.9 1.9) (drill oval 0.35 1.35) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (pad 6 thru_hole oval (at 3.575 -0.28 90) (size 0.9 1.9) (drill oval 0.35 1.35) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (model /home/ron/mod/kicad/3D/Wurth_USB_TYPE_B.wrl
      (at (xyz 0 0.0125 0.055))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59AFECCA)
    (at 141.6 111.325 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 9.95 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VBUS))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 D+))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 D-))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 59AFECD8)
    (at 148 95)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference M1 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value Mechanical_mounting (at 0 4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.25 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.59099 1.59099) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.25) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.59099 1.59099) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.25 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.59099 -1.59099) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.25) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.59099 -1.59099) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 59AFECD4)
    (at 148 119)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (fp_text reference M2 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value Mechanical_mounting (at 0 4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.25 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.59099 1.59099) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 2.25) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.59099 1.59099) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -2.25 0) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.59099 -1.59099) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -2.25) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.59099 -1.59099) (size 0.6 0.6) (drill 0.5) (layers *.Cu *.Mask))
  )
  (gr_arc (start 149 103.65) (end 149.01 103.55) (angle 162.979698) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.99 103.75) (end 149 103.75) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.98 103.55) (end 149.01 103.55) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.99 103.65) (end 147.99 103.75) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.99 110.8) (end 147.99 110.9) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.99 110.9) (end 149.02 110.9) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149 110.8) (end 149.01 110.7) (angle 162.9795862) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.98 110.7) (end 149.01 110.7) (layer Edge.Cuts) (width 0.15))
  (gr_text D- (at 144.75 106 90) (layer B.SilkS))
  (gr_text D+ (at 144.75 109 90) (layer B.SilkS))
  (gr_text VBUS (at 141.75 116 90) (layer B.SilkS))
  (gr_text GND (at 141.75 99.5 90) (layer B.SilkS))
  (gr_text GND (at 141.75 99.25 90) (layer F.SilkS))
  (gr_text VBUS (at 141.75 115.75 90) (layer F.SilkS))
  (gr_text D- (at 144.75 105.75 90) (layer F.SilkS))
  (gr_text D+ (at 144.75 109.25 90) (layer F.SilkS))
  (gr_line (start 139 124) (end 139 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 124) (end 139 124) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 90) (end 154 124) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 90) (end 154 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139 90) (xy 154 90) (xy 154 124) (xy 139 124)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139 90) (xy 154 90) (xy 154 124) (xy 139 124)
      )
    )
  )
)
