(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 60)
    (no_connects 0)
    (area 135.424999 94.174999 156.325001 118.575001)
    (thickness 1.6)
    (drawings 32)
    (tracks 253)
    (zones 0)
    (modules 37)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C6-Pad2)")
  (net 7 "Net-(C7-Pad1)")
  (net 8 "Net-(C7-Pad2)")
  (net 9 "Net-(R1-Pad1)")
  (net 10 "Net-(R2-Pad1)")
  (net 11 "Net-(R3-Pad2)")
  (net 12 "Net-(U1-Pad1)")
  (net 13 "Net-(U1-Pad2)")
  (net 14 "Net-(U1-Pad3)")
  (net 15 "Net-(U1-Pad11)")
  (net 16 "Net-(U1-Pad13)")
  (net 17 "Net-(U1-Pad14)")
  (net 18 "Net-(U1-Pad15)")
  (net 19 "Net-(U1-Pad16)")
  (net 20 "Net-(U1-Pad21)")
  (net 21 "Net-(U1-Pad22)")
  (net 22 "Net-(U1-Pad23)")
  (net 23 "Net-(U2-Pad2)")
  (net 24 "Net-(U2-Pad4)")
  (net 25 "Net-(R5-Pad2)")
  (net 26 "Net-(R7-Pad2)")
  (net 27 "Net-(Q1-Pad1)")
  (net 28 "Net-(R10-Pad1)")
  (net 29 "Net-(R10-Pad2)")
  (net 30 "Net-(R11-Pad1)")
  (net 31 "Net-(R11-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad4)")
    (add_net VDD)
  )
  (net_class VDD ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Ultra:QFN-28-LM49270 (layer F.Cu) (tedit 57E9D2D1)
    (at 148.5 105)
    (attr smd)
    (fp_text reference U1 (at 3.5 -14.25) (layer F.SilkS) hide)
    (fp_text value LM49270 (at -18.25 -3) (layer F.Fab))
    (pad 1 smd rect (at -2.45 -1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -2.45 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.45 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.45 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 5 smd rect (at -2.45 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 6 smd rect (at -2.45 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R1-Pad1)"))
    (pad 7 smd rect (at -2.45 1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 8 smd rect (at -1.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 9 smd rect (at -1 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 10 smd rect (at -0.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 0 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 0.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 13 smd rect (at 1 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 1.5 2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 2.45 1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at 2.45 1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 2.45 0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 18 smd rect (at 2.45 0) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 2.45 -0.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 20 smd rect (at 2.45 -1) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 21 smd rect (at 2.45 -1.5) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 1.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 1 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 0.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 25 smd rect (at 0 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 26 smd rect (at -0.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 27 smd rect (at -1 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(Q1-Pad1)"))
    (pad 28 smd rect (at -1.5 -2.45 90) (size 0.7 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 29 smd rect (at 0 0) (size 3 3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module "Thru pad" (layer F.Cu) (tedit 57E9D2C7)
    (at 137 100.5 90)
    (fp_text reference REF** (at 6 -8.25 90) (layer F.SilkS) hide)
    (fp_text value "Thru pad" (at 0.2 -6.05 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(Q1-Pad1)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 579C9E7B)
    (at 154.75 98.25 90)
    (fp_text reference REF** (at 8.5 2 90) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 4.25 4.25 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U1-Pad23)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 579C9E78)
    (at 154.75 101.25 90)
    (fp_text reference REF** (at 10 -4.25 90) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 4.25 7.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-Pad22)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 57E9CF9E)
    (at 137 100.5 90)
    (fp_text reference REF** (at -13.5 -15 90) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at -1.25 -16.25 90) (layer F.Fab))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 57E9CFA2)
    (at 137 103.5 90)
    (fp_text reference REF** (at -10 -11.5 90) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 0 -11 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad1)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 57E9CFA0)
    (at 137 106.5 90)
    (fp_text reference REF** (at -7.25 -13.75 90) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 3 -14 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U1-Pad2)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 57E9CFA4)
    (at 137 109.5 90)
    (fp_text reference REF** (at -6.25 -9.25 90) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 6.5 -19.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad3)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 579C9E70)
    (at 154.75 111.75 90)
    (fp_text reference REF** (at 3.75 10.5 90) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 1.5 6.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad13)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 579C9E74)
    (at 154.75 108.75 90)
    (fp_text reference REF** (at 6.5 10.75 90) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 4.25 5.75 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U1-Pad14)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 579C9E57)
    (at 137 117)
    (fp_text reference REF** (at -6.25 -2.5) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at -5.5 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VDD))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 579C9E5A)
    (at 140 117)
    (fp_text reference REF** (at -10.75 -4.25) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at -1.5 3) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 579C9E60)
    (at 143 117)
    (fp_text reference REF** (at -13.75 -11.5) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at -3 6.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(R5-Pad2)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 579C9E65)
    (at 146 117)
    (fp_text reference REF** (at -13 1) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 9 2.75) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(R7-Pad2)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 57E9D134)
    (at 152 117)
    (fp_text reference REF** (at 12.5 -2.5) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 1.25 6.25) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R11-Pad1)"))
  )
  (module Test_Point_2mx2mm (layer F.Cu) (tedit 57E9D141)
    (at 155 117)
    (fp_text reference REF** (at 4.25 1) (layer F.SilkS) hide)
    (fp_text value Test_Point_2mx2mm (at 0.75 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(R10-Pad2)"))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57924941)
    (at 143 105 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 13 -5.75 180) (layer F.SilkS) hide)
    (fp_text value C (at 9.5 12.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57924922)
    (at 143.75 106.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 9.75 -8.25 180) (layer F.SilkS) hide)
    (fp_text value C (at 11 12.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5792495B)
    (at 148.5 109.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -10.25 6 180) (layer F.SilkS) hide)
    (fp_text value C (at -10.25 2.75 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5792493E)
    (at 149 114.25 270)
    (attr smd)
    (fp_text reference C5 (at -8.5 -8.75 270) (layer F.SilkS) hide)
    (fp_text value CP (at 2 17.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57924937)
    (at 146.25 110 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at -8.5 -11.5 270) (layer F.SilkS) hide)
    (fp_text value C (at 2.75 12.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5792491D)
    (at 143.75 110 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at -1.75 -14 270) (layer F.SilkS) hide)
    (fp_text value C (at -0.5 10.75 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57924902)
    (at 154 105.75 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 9.75 14.75 180) (layer F.SilkS) hide)
    (fp_text value C (at 7 17.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57924908)
    (at 150.5 97.25 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at -7.75 3.5 270) (layer F.SilkS) hide)
    (fp_text value C (at -8.25 5.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57924955)
    (at 139.25 97 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 2.25 5.5 270) (layer F.SilkS) hide)
    (fp_text value C (at 3 7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57924906)
    (at 147.5 100.5 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -6 10.25 180) (layer F.SilkS) hide)
    (fp_text value R (at 5.5 8.75 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5792490A)
    (at 149 99.25 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at -1.75 10.75 180) (layer F.SilkS) hide)
    (fp_text value R (at -3.75 11 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 57E9D23A)
    (at 144.25 97)
    (descr "8-Lead Thermally Enhanced Plastic Small Outline (SE) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value PIC12F1822 (at -7.5 -7.75) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R11-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R3-Pad2)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R10-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-8-1EP_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57E9CF99)
    (at 154 104.25 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at -0.75 11.25 180) (layer F.SilkS) hide)
    (fp_text value C (at 8 12.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57924918)
    (at 143.25 112 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 11.75 1.25 180) (layer F.SilkS) hide)
    (fp_text value R (at 10.75 3.75 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57924924)
    (at 143.5 113.75 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at -8.25 11.25 270) (layer F.SilkS) hide)
    (fp_text value R (at 2.25 9.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5792491F)
    (at 145.75 112 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 14.5 5.25 180) (layer F.SilkS) hide)
    (fp_text value R (at -11.5 1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57924927)
    (at 146 113.75 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at -5.25 17.25 270) (layer F.SilkS) hide)
    (fp_text value R (at 0.75 -11.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57E9D0D6)
    (at 139.25 99 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference REF** (at 13 -15.25 180) (layer F.SilkS) hide)
    (fp_text value C_0402 (at -13.25 18 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R11-Pad2)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 57E9D241)
    (at 148.75 97.25 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference REF** (at 9.25 -8.25 90) (layer F.SilkS) hide)
    (fp_text value C_0402 (at 7.5 -6.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R10-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57E9D226)
    (at 154.5 114)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 57E9D223)
    (at 152.5 114)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0 -1.8) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text LOUT- (at 151.45 101.25) (layer B.SilkS))
  (gr_text LOUT+ (at 151.45 98.25) (layer B.SilkS))
  (gr_text ROUT- (at 151.45 108.75) (layer B.SilkS))
  (gr_text ROUT+ (at 151.45 111.75) (layer B.SilkS))
  (gr_text HP- (at 139.65 106.5) (layer B.SilkS))
  (gr_text UP (at 155 115.25) (layer B.SilkS))
  (gr_text DN (at 152 115.25) (layer B.SilkS))
  (gr_text RIN (at 146 115.25) (layer B.SilkS))
  (gr_text LIN (at 143 115.25) (layer B.SilkS))
  (gr_text GND (at 140 115.25) (layer B.SilkS))
  (gr_text 5v (at 137 115.25) (layer B.SilkS))
  (gr_text HPL (at 139.75 109.5) (layer B.SilkS))
  (gr_text HPR (at 139.75 103.5) (layer B.SilkS))
  (gr_text HPS (at 139.75 100.5) (layer B.SilkS))
  (gr_text HPS (at 139.5 100.5) (layer F.SilkS))
  (gr_text HPR (at 139.5 103.5) (layer F.SilkS))
  (gr_text HP- (at 139.65 106.5) (layer F.SilkS))
  (gr_text HPL (at 139.5 109.5) (layer F.SilkS))
  (gr_text LOUT- (at 151.85 101.25) (layer F.SilkS))
  (gr_text LOUT+ (at 151.85 98.25) (layer F.SilkS))
  (gr_text ROUT+ (at 151.85 111.75) (layer F.SilkS))
  (gr_text ROUT- (at 151.85 108.75) (layer F.SilkS))
  (gr_text UP (at 155 115.35) (layer F.SilkS))
  (gr_text DN (at 152 115.35) (layer F.SilkS))
  (gr_text RIN (at 146 115.35) (layer F.SilkS))
  (gr_text LIN (at 143 115.35) (layer F.SilkS))
  (gr_text GND (at 140 115.35) (layer F.SilkS))
  (gr_text 5v (at 137 115.35) (layer F.SilkS))
  (gr_line (start 156.25 94.25) (end 135.5 94.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.25 118.5) (end 156.25 94.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.5 94.25) (end 135.5 118.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.5 118.5) (end 156.25 118.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.5) (smoothing fillet))
    (polygon
      (pts
        (xy 156.25 118.5) (xy 135.5 118.5) (xy 135.5 94.25) (xy 156.25 94.25) (xy 156.25 118.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 156.25 118.5) (xy 135.5 118.5) (xy 135.5 94.25) (xy 156.25 94.25) (xy 156.25 118.5)
      )
    )
  )
  (zone (net 1) (net_name VDD) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.75 106.25) (xy 147.25 106.25) (xy 147.25 103.75) (xy 149.75 103.75) (xy 149.75 106.25)
      )
    )
  )
)
