<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<text>CV/Audio Output</text>
<text>Biodata Sonification MIDI Arduino Shield</text>
<text>v004</text>
<text>Electrodes</text>
<text>Biodata Sonification MIDI Arduino Shield</text>
<text>v004</text>
<text>Electrode Input</text>
<text>GND</text>
<text>220</text>
<text>red</text>
<text>red</text>
<text>yellow</text>
<text>green</text>
<text>blue</text>
<text>white</text>
<text>Electrodes</text>
<text>Electricity for Progress 2017</text>
<text>Electricity for Progress 2017</text>
<text>CV/Audio Output</text>
<text>R1</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="DIL08-ROUND">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="ARDUINO">
<description>&lt;b&gt;Arduino Uno&lt;/b&gt;
&lt;p&gt;
Make a shield with ease, this package has all the named pins as well as the two mounting drill holes and an outline of the USB and DC power connector. The outline is on the DIMENSION layer, so if your board house uses it they will cut the outline to match.</description>
</package>
<package name="0805-THM-7">
</package>
<package name="STX3100">
<description>&lt;b&gt;MIC/HEADPHONE JACK&lt;/b&gt;&lt;p&gt;
KS-S stereo microphone/headphone jack&lt;p&gt;
 PG203JN (Schukat)</description>
</package>
<package name="CP-2350">
<description>Female &lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
5 pins 90 deg. with shield, horizontal (DIN 41524)</description>
</package>
<package name="1X1-BIGPOGO">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML1206">
<description>&lt;b&gt;SML10XXKH-TR (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;SML10R3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10E3KH-TR&lt;/td&gt;&lt;td&gt;SUPER REDSUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10O3KH-TR&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PY3KH-TR&lt;/td&gt;&lt;td&gt;PURE YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10OY3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10AG3KH-TR&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10BG3KH-TR&lt;/td&gt;&lt;td&gt;BLUE GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PB1KH-TR&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10CW1KH-TR&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;

Source: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="5,5-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 5.5 mm, round</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="5-2,5">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pot_sam">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EVUFXK">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt; Single Type with Bushing, Vertical, Snap-in&lt;p&gt;
Source: Panasonic</description>
</package>
</packages>
</library>
<library name="switch-omron_circ">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="555" library="adafruit" package="DIL08-ROUND" value="555">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0805-THM-7" value="220"/>
<element name="R2" library="adafruit" package="0805-THM-7" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0805-THM-7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="0805-THM-7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="0805-THM-7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="0805-THM-7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="0805-THM-7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="0805-THM-7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CAP-PTH-SMALL" value=".0042uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="SparkFun-LED" package="LED5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="LED7" library="led" package="SML1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="SML1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED9" library="led" package="SML1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED10" library="led" package="SML1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED11" library="led" package="SML1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED12" library="led" package="SML1206" value="">
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Passives" package="1206" value="01.uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Passives" package="1206" value=".0042uF">
<attribute name="NAME"/>
</element>
<element name="U$3" library="adafruit" package="ARDUINO" value="ARDUINOUNO"/>
<element name="X1" library="adafruit" package="STX3100" value="STEREOJACK">
<attribute name="NAME"/>
</element>
<element name="X2" library="adafruit" package="STX3100" value="STEREOJACK">
<attribute name="NAME"/>
</element>
<element name="MIDI" library="adafruit" package="CP-2350" value="MIDIJACK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="pot_sam" package="EVUFXK" value="EVUF2K">
<attribute name="NAME"/>
</element>
<element name="R10" library="adafruit" package="0805-THM-7" value="3.9k / 10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="5,5-PAD" value="MOUNT-PAD-ROUND5.5"/>
<element name="H2" library="holes" package="5,5-PAD" value="MOUNT-PAD-ROUND5.5"/>
<element name="PAD1" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD6" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="PAD7" library="wirepad" package="5-2,5" value="WIREPADSMD5-2,5">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="adafruit" package="1X1-BIGPOGO" value=""/>
<element name="R11" library="adafruit" package="0805-THM-7" value="0.1uF / 1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-omron_circ" package="B3F-10XX" value="B3F-1000">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="555" pad="4"/>
<contactref element="555" pad="8"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R9" pad="3"/>
<contactref element="U$3" pad="5V"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED3" pad="K"/>
<contactref element="LED4" pad="K"/>
<contactref element="LED5" pad="K"/>
<contactref element="LED6" pad="K"/>
<contactref element="555" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED10" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED8" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="C7" pad="2"/>
<contactref element="LED11" pad="C"/>
<contactref element="R9" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="U$3" pad="GND1"/>
<contactref element="U$3" pad="GND2"/>
<contactref element="JP1" pad="P$1"/>
<contactref element="R11" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="U$3" pad="GND"/>
</signal>
<signal name="PROBE1">
<contactref element="555" pad="6"/>
<contactref element="555" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="X2" pad="1"/>
<contactref element="H1" pad="B5,5"/>
<contactref element="PAD1" pad="1"/>
<contactref element="PAD7" pad="1"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="OUTPUT">
<contactref element="555" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="U$3" pad="D2"/>
</signal>
<signal name="PROBE2">
<contactref element="555" pad="7"/>
<contactref element="R2" pad="2"/>
<contactref element="X2" pad="5"/>
<contactref element="H2" pad="B5,5"/>
<contactref element="PAD5" pad="1"/>
<contactref element="PAD6" pad="1"/>
<contactref element="PAD4" pad="1"/>
<contactref element="PAD3" pad="1"/>
</signal>
<signal name="MIDIOUT">
<contactref element="U$3" pad="D1"/>
<contactref element="MIDI" pad="5"/>
</signal>
<signal name="POT">
<contactref element="U$3" pad="A0"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="LED7" pad="A"/>
<contactref element="R4" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$18">
<contactref element="LED8" pad="A"/>
<contactref element="R5" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$19">
<contactref element="LED9" pad="A"/>
<contactref element="R6" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="LED10" pad="A"/>
<contactref element="R7" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$21">
<contactref element="LED11" pad="A"/>
<contactref element="R8" pad="2"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="LED12" pad="A"/>
<contactref element="R3" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="CV1">
<contactref element="X1" pad="5"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U$3" pad="VIN"/>
</signal>
<signal name="3V">
<contactref element="U$3" pad="3V"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="1"/>
<contactref element="U$3" pad="D5"/>
</signal>
<signal name="CVOUT">
<contactref element="U$3" pad="D11"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R8" pad="1"/>
<contactref element="U$3" pad="D10"/>
</signal>
<signal name="N$7">
<contactref element="R7" pad="1"/>
<contactref element="U$3" pad="D9"/>
</signal>
<signal name="N$4">
<contactref element="U$3" pad="D3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U$3" pad="D6"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="1"/>
<contactref element="MIDI" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="C3" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="A1"/>
<contactref element="S1" pad="4"/>
<contactref element="S1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
