(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 69)
    (zones 0)
    (modules 10)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (trace_clearance 0.1778)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.4064)
    (via_drill 0.254)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (user_via 0.4064 0.254)
    (uvia_size 0.4064)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.4064)
    (uvia_min_drill 0.254)
    (edge_width 0.0254)
    (segment_width 0.1778)
    (pcb_text_width 0.2032)
    (pcb_text_size 1.2192 1.2192)
    (mod_edge_width 0.127)
    (mod_text_size 0.7112 0.7112)
    (mod_text_width 0.1016)
    (pad_size 1.397 1.397)
    (pad_drill 0.8382)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 147.32 96.52)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 "Net-(C5-Pad1)")
  (net 8 +3V3)
  (net 9 /DTR_TTL)
  (net 10 /DSR_TTL)
  (net 11 /TX_TTL)
  (net 12 /RX_TTL)
  (net 13 /DTR_232)
  (net 14 /DCD_232)
  (net 15 /DSR_232)
  (net 16 /CTS_232)
  (net 17 /RTS_232)
  (net 18 /RX_232)
  (net 19 /TX_232)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.4064)
    (via_drill 0.254)
    (uvia_dia 0.4064)
    (uvia_drill 0.254)
    (diff_pair_width 0.1778)
    (diff_pair_gap 0.1778)
    (add_net +3V3)
    (add_net /CTS_232)
    (add_net /DCD_232)
    (add_net /DSR_232)
    (add_net /DSR_TTL)
    (add_net /DTR_232)
    (add_net /DTR_TTL)
    (add_net /RI_232)
    (add_net /RTS_232)
    (add_net /RX_232)
    (add_net /RX_TTL)
    (add_net /TX_232)
    (add_net /TX_TTL)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad31)")
    (add_net "Net-(J1-Pad32)")
    (add_net "Net-(J1-Pad33)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad40)")
    (add_net "Net-(J1-Pad41)")
    (add_net "Net-(J1-Pad42)")
    (add_net "Net-(J1-Pad43)")
    (add_net "Net-(J1-Pad44)")
    (add_net "Net-(J1-Pad45)")
    (add_net "Net-(J1-Pad46)")
    (add_net "Net-(J1-Pad47)")
    (add_net "Net-(J1-Pad48)")
    (add_net "Net-(J1-Pad49)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad50)")
    (add_net "Net-(J1-Pad52)")
    (add_net "Net-(J1-Pad53)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad9)")
  )
  (module 0_LOCAL:Teensy_MounT_stagger_6mil (layer F.Cu) (tedit 5F63C04C)
    (at 147.32 96.52 180)
    (fp_text reference J1 (at 0 -10.16) (layer F.SilkS) hide)
    (fp_text value Teensy (at 0 10.16) (layer F.Fab))
    (fp_text user MK66FX1MBVMD18/ (at 1.27 0) (layer F.SilkS) hide)
    (fp_text user MK64FX512VMD12 (at 1.27 1.143) (layer F.SilkS) hide)
    (pad 17 thru_hole circle (at 11.43 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 13.97 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 16.51 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 19.05 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 8.89 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 6.35 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 3.81 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 21.59 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 24.13 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 26.67 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 29.21 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 29.21 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 26.67 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 24.13 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 21.59 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 19.05 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 16.51 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 13.97 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at 11.43 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 1.2446 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -1.27 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -3.81 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -6.35 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -8.89 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -11.43 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 /DSR_TTL))
    (pad 7 thru_hole circle (at -13.97 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 9 /DTR_TTL))
    (pad 6 thru_hole circle (at -16.51 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -19.05 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -21.59 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -24.13 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 /TX_TTL))
    (pad 2 thru_hole circle (at -26.67 7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 12 /RX_TTL))
    (pad 1 thru_hole roundrect (at -29.21 7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (pad 38 thru_hole circle (at 8.89 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 6.35 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole circle (at 3.81 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 41 thru_hole circle (at 1.27 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 42 thru_hole circle (at -1.27 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at -3.81 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at -6.35 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 45 thru_hole circle (at -8.89 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 46 thru_hole circle (at -11.43 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 47 thru_hole circle (at -13.97 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 48 thru_hole circle (at -16.51 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at -19.05 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 50 thru_hole circle (at -21.59 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 51 thru_hole circle (at -24.13 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask)
      (net 8 +3V3))
    (pad 52 thru_hole circle (at -26.67 -7.6962 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
    (pad 53 thru_hole circle (at -29.21 -7.5438 180) (size 1.397 1.397) (drill 0.9144) (layers *.Cu *.Mask))
  )
  (module 0_LOCAL:DSUB-25_Male_Vertical_P2.77x2.84mm (layer B.Cu) (tedit 5F4932F5)
    (at 163.957 95.0468 180)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference J2 (at 1.4605 -1.2827 180) (layer B.SilkS) hide)
    (fp_text value DB25_Male (at 16.62 -8.73 180) (layer B.Fab))
    (fp_text user %R (at 16.62 -1.42 180) (layer B.Fab))
    (pad 25 thru_hole circle (at 31.855 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at 29.085 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at 26.315 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at 23.545 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at 20.775 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 18.005 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 13 /DTR_232))
    (pad 19 thru_hole circle (at 15.235 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 18 thru_hole circle (at 12.465 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 9.695 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 6.925 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 4.155 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at 1.385 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at 33.24 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 30.47 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 27.7 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 24.93 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 22.16 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 19.39 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 14 /DCD_232))
    (pad 7 thru_hole circle (at 16.62 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 13.85 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 15 /DSR_232))
    (pad 5 thru_hole circle (at 11.08 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 16 /CTS_232))
    (pad 4 thru_hole circle (at 8.31 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 17 /RTS_232))
    (pad 3 thru_hole circle (at 5.54 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 18 /RX_232))
    (pad 2 thru_hole circle (at 2.77 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 19 /TX_232))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/A_DS_25_PP_Z_cut.step
      (offset (xyz 16.625 -1.42 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:PinHeader_1x02_P2.54mm_Horizontal (layer B.Cu) (tedit 5F492FFB)
    (at 121.92 101.6 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 4.385 2.27 90) (layer B.SilkS) hide)
    (fp_text value Jumper_2_Bridged (at 4.385 -4.81 90) (layer B.Fab))
    (fp_text user %R (at 2.77 -1.27 180) (layer B.Fab))
    (pad 2 thru_hole custom (at 0 -2.54 90) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 /CTS_232) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
      ))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.651 1.651) (drill 0.9144) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 17 /RTS_232))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 169.3164 100.7364 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -0.0508 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 171.1198 98.806 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0.0254 0 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C2-Pad2)"))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 175.7426 100.7364 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -0.0254 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C1-Pad2)"))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 175.7426 98.806 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.0254 -0.0254 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 smd roundrect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:C_0805 (layer F.Cu) (tedit 5F4898F2)
    (at 176.6824 94.361 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.0254 0) (layer F.SilkS))
    (fp_text value 0.1uf (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 2 smd roundrect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:NetTie-2_SMD_10 (layer F.Cu) (tedit 5F3D08F8)
    (at 147.32 96.4692 180)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference NT1 (at 0 -1.2) (layer F.SilkS) hide)
    (fp_text value Net-Tie_2 (at 0 1.2) (layer F.Fab))
    (pad 2 smd circle (at 0.254 0 180) (size 0.254 0.254) (layers F.Cu)
      (net 14 /DCD_232))
    (pad 1 smd circle (at -0.254 0 180) (size 0.254 0.254) (layers F.Cu)
      (net 15 /DSR_232))
  )
  (module 0_LOCAL:SOIC-16_W3.90mm (layer B.Cu) (tedit 5F3A577D)
    (at 172.212 98.044 180)
    (attr smd)
    (fp_text reference U1 (at 0 0.762) (layer B.SilkS) hide)
    (fp_text value MAX3232 (at 0 0) (layer B.SilkS))
    (fp_text user REF** (at 0 0) (layer B.Fab))
    (pad 16 smd roundrect (at -4.445 2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 15 smd roundrect (at -3.175 2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 14 smd roundrect (at -1.905 2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 /RX_232))
    (pad 13 smd roundrect (at -0.635 2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 /TX_232))
    (pad 12 smd roundrect (at 0.635 2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 /RX_TTL))
    (pad 11 smd roundrect (at 1.905 2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /TX_TTL))
    (pad 10 smd roundrect (at 3.175 2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /DTR_TTL))
    (pad 9 smd roundrect (at 4.445 2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /DSR_TTL))
    (pad 8 smd roundrect (at 4.445 -2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 /DTR_232))
    (pad 7 smd roundrect (at 3.175 -2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /DSR_232))
    (pad 6 smd roundrect (at 1.905 -2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C5-Pad1)"))
    (pad 5 smd roundrect (at 0.635 -2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C2-Pad2)"))
    (pad 4 smd roundrect (at -0.635 -2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C2-Pad1)"))
    (pad 3 smd roundrect (at -1.905 -2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C1-Pad2)"))
    (pad 2 smd roundrect (at -3.175 -2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -4.445 -2.7 180) (size 0.6 1.27) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text USB (at 174.371 96.52) (layer F.SilkS))
  (gr_text "SD CARD" (at 123.19 96.52) (layer F.SilkS))
  (gr_text "Teensy MounT" (at 163.703 91.186) (layer F.SilkS))
  (gr_line (start 177.9016 105.5116) (end 177.9016 87.5284) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 116.7384 105.5116) (end 177.9016 105.5116) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 116.7384 87.5284) (end 116.7384 105.5116) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 177.9016 87.5284) (end 116.7384 87.5284) (layer Edge.Cuts) (width 0.0254))
  (gr_text CTS (at 119.38 90.5764) (layer B.SilkS))
  (gr_text RTS (at 121.92 90.5764) (layer B.SilkS))
  (gr_text "DB25M this side" (at 147.32 96.52) (layer B.SilkS))
  (gr_text "Teensy this side" (at 147.32 96.52) (layer F.SilkS))
  (gr_text "Teensy MounT" (at 147.32 90.932) (layer B.SilkS))
  (gr_text github.com/bkw777/MounT (at 147.32 102.362) (layer B.SilkS))
  (gr_text "C* 0.1uf" (at 173.863 102.235) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 177.9016 105.5116) (xy 116.7384 105.5116) (xy 116.7384 87.5284) (xy 177.9016 87.5284)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.254) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 177.9016 105.5116) (xy 116.7384 105.5116) (xy 116.7384 87.5284) (xy 177.9016 87.5284)
      )
    )
  )
)
