(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 474)
    (tracks 933)
    (zones 0)
    (modules 126)
    (nets 123)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power hide)
    (2 In2.Cu power hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.4572 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.1)
    (pad_size 1.3 1.3)
    (pad_drill 0.75)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 /COMP-BLUE)
  (net 5 -5V)
  (net 6 /H2-1)
  (net 7 /H3-1)
  (net 8 /COMP-GREEN)
  (net 9 /COMP-SYN)
  (net 10 /H4-1)
  (net 11 /COMP-RED)
  (net 12 /H2-6)
  (net 13 /VID0)
  (net 14 /VID1)
  (net 15 /VID2)
  (net 16 /VID3)
  (net 17 /H3-6)
  (net 18 /VID4)
  (net 19 /VID5)
  (net 20 /VID6)
  (net 21 /VID7)
  (net 22 /H4-6)
  (net 23 /VID8)
  (net 24 /VID9)
  (net 25 /VID10)
  (net 26 /VID11)
  (net 27 /J11-1)
  (net 28 "Net-(J11-Pad3)")
  (net 29 /L4-1)
  (net 30 /L3-1)
  (net 31 /UC2-8)
  (net 32 /R13-1)
  (net 33 /MONO-COLOR)
  (net 34 /Q2-3)
  (net 35 +12V)
  (net 36 /R114-1)
  (net 37 /R8-2)
  (net 38 "Net-(U1-Pad4)")
  (net 39 "Net-(U1-Pad3)")
  (net 40 "Net-(U2-Pad1)")
  (net 41 /28M)
  (net 42 "Net-(U2-Pad2)")
  (net 43 "Net-(U2-Pad5)")
  (net 44 /UC2-20)
  (net 45 /UC2-10)
  (net 46 /UC2-19)
  (net 47 /UC2-9)
  (net 48 "Net-(UB2-Pad18)")
  (net 49 /UC2-17)
  (net 50 /UC2-7)
  (net 51 /UC2-16)
  (net 52 /UC2-6)
  (net 53 /UC2-5)
  (net 54 /UC2-4)
  (net 55 /UC2-13)
  (net 56 /UC2-3)
  (net 57 /UC2-12)
  (net 58 /UC2-11)
  (net 59 "Net-(C8-Pad2)")
  (net 60 CREF.H)
  (net 61 CREF.L)
  (net 62 /STRETCH.L)
  (net 63 /UG3-7)
  (net 64 /UG3-5)
  (net 65 /VBL.L)
  (net 66 /BABUS12)
  (net 67 /FLIP7.H)
  (net 68 /A2R-W.H)
  (net 69 /3.5DIK)
  (net 70 /UG3-6)
  (net 71 /M2SEL.L)
  (net 72 /HDSEL.H)
  (net 73 /FLIP6.H)
  (net 74 /RESET.L)
  (net 75 /PH0.H)
  (net 76 /UH2-43)
  (net 77 /IRQ.L)
  (net 78 /RABUS7)
  (net 79 /RABUS5)
  (net 80 /RABUS3)
  (net 81 /RABUS1)
  (net 82 /MDBUS7)
  (net 83 /MDBUS5)
  (net 84 /MDBUS3)
  (net 85 /UH2-44)
  (net 86 /U18TEST)
  (net 87 /UH2-40)
  (net 88 /RABUS6)
  (net 89 /RABUS4)
  (net 90 /RABUS2)
  (net 91 /RABUS0)
  (net 92 /MDBUS6)
  (net 93 /MDBUS4)
  (net 94 /MDBUS2)
  (net 95 /MDBUS0)
  (net 96 /RGB2.H)
  (net 97 /RGB8.H)
  (net 98 /ADBUS1)
  (net 99 /ADBUS3)
  (net 100 /ADBUS5)
  (net 101 /ADBUS7)
  (net 102 /14M.H)
  (net 103 /MDBUS1)
  (net 104 /RGB1.H)
  (net 105 /RGB4.H)
  (net 106 /ADBUS0)
  (net 107 /ADBUS2)
  (net 108 /ADBUS4)
  (net 109 /ADBUS6)
  (net 110 /R54-1)
  (net 111 /R17-1)
  (net 112 /R135-1)
  (net 113 /R14-2)
  (net 114 /R54-2)
  (net 115 /COMSYNC)
  (net 116 /UG3-1)
  (net 117 /R114-2)
  (net 118 /SYNC.L)
  (net 119 /14MD.H)
  (net 120 "Net-(J25-Pad20)")
  (net 121 "Net-(J10-Pad6)")
  (net 122 "Net-(J10-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /14M.H)
    (add_net /14MD.H)
    (add_net /28M)
    (add_net /3.5DIK)
    (add_net /A2R-W.H)
    (add_net /ADBUS0)
    (add_net /ADBUS1)
    (add_net /ADBUS2)
    (add_net /ADBUS3)
    (add_net /ADBUS4)
    (add_net /ADBUS5)
    (add_net /ADBUS6)
    (add_net /ADBUS7)
    (add_net /BABUS12)
    (add_net /COMP-BLUE)
    (add_net /COMP-GREEN)
    (add_net /COMP-RED)
    (add_net /COMP-SYN)
    (add_net /COMSYNC)
    (add_net /FLIP6.H)
    (add_net /FLIP7.H)
    (add_net /H2-1)
    (add_net /H2-6)
    (add_net /H3-1)
    (add_net /H3-6)
    (add_net /H4-1)
    (add_net /H4-6)
    (add_net /HDSEL.H)
    (add_net /IRQ.L)
    (add_net /J11-1)
    (add_net /L3-1)
    (add_net /L4-1)
    (add_net /M2SEL.L)
    (add_net /MDBUS0)
    (add_net /MDBUS1)
    (add_net /MDBUS2)
    (add_net /MDBUS3)
    (add_net /MDBUS4)
    (add_net /MDBUS5)
    (add_net /MDBUS6)
    (add_net /MDBUS7)
    (add_net /MONO-COLOR)
    (add_net /PH0.H)
    (add_net /Q2-3)
    (add_net /R114-1)
    (add_net /R114-2)
    (add_net /R13-1)
    (add_net /R135-1)
    (add_net /R14-2)
    (add_net /R17-1)
    (add_net /R54-1)
    (add_net /R54-2)
    (add_net /R8-2)
    (add_net /RABUS0)
    (add_net /RABUS1)
    (add_net /RABUS2)
    (add_net /RABUS3)
    (add_net /RABUS4)
    (add_net /RABUS5)
    (add_net /RABUS6)
    (add_net /RABUS7)
    (add_net /RESET.L)
    (add_net /RGB1.H)
    (add_net /RGB2.H)
    (add_net /RGB4.H)
    (add_net /RGB8.H)
    (add_net /STRETCH.L)
    (add_net /SYNC.L)
    (add_net /U18TEST)
    (add_net /UC2-10)
    (add_net /UC2-11)
    (add_net /UC2-12)
    (add_net /UC2-13)
    (add_net /UC2-16)
    (add_net /UC2-17)
    (add_net /UC2-19)
    (add_net /UC2-20)
    (add_net /UC2-3)
    (add_net /UC2-4)
    (add_net /UC2-5)
    (add_net /UC2-6)
    (add_net /UC2-7)
    (add_net /UC2-8)
    (add_net /UC2-9)
    (add_net /UG3-1)
    (add_net /UG3-5)
    (add_net /UG3-6)
    (add_net /UG3-7)
    (add_net /UH2-40)
    (add_net /UH2-43)
    (add_net /UH2-44)
    (add_net /VBL.L)
    (add_net /VID0)
    (add_net /VID1)
    (add_net /VID10)
    (add_net /VID11)
    (add_net /VID2)
    (add_net /VID3)
    (add_net /VID4)
    (add_net /VID5)
    (add_net /VID6)
    (add_net /VID7)
    (add_net /VID8)
    (add_net /VID9)
    (add_net CREF.H)
    (add_net CREF.L)
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(J10-Pad4)")
    (add_net "Net-(J10-Pad6)")
    (add_net "Net-(J11-Pad3)")
    (add_net "Net-(J25-Pad20)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(UB2-Pad18)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.3048)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net -5V)
    (add_net GND)
  )
  (module "My Libraries:BE5v2" (layer F.Cu) (tedit 5FBC48F5)
    (at 114.6556 124.7394)
    (descr "Imported from BE5.svg")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 8.048) (layer F.SilkS) hide)
  )
  (module "My Libraries:BE5v2" (layer B.Cu) (tedit 5FBC48F5)
    (at 155.0416 88.7476 180)
    (descr "Imported from BE5.svg")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference svg2mod (at 0 3.048) (layer B.SilkS) hide)
    (fp_text value G*** (at 0 -8.048) (layer B.SilkS) hide)
  )
  (module Symbol:KiCad-Logo_5mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 120.7008 106.2482 270)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF** (at 0 5.08 90) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo_5mm_SilkScreen (at 0 -3.81 90) (layer B.Fab) hide)
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 170.7896 71.0946 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 150.0886 87.3506)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 83.78 63.46)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H8 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 193.08 63.46)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H7 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 83.78 132.12)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H6 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 56D1B4CB)
    (at 193.08 132.12)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference H5 (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Package_TO_SOT_THT:TO-92 (layer F.Cu) (tedit 60AB141F)
    (at 187.833 115.189 180)
    (descr "TO-92 leads molded, narrow, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference TF1 (at -2.159 1.397) (layer F.SilkS))
    (fp_text value CapacitiveTransformer (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 27 /J11-1))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 37 /R8-2))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1.3 1.3) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer B.Cu) (tedit 5F9F0FC9)
    (at 95.758 83.058)
    (fp_text reference TP5 (at 0.127 1.524) (layer B.SilkS) hide)
    (fp_text value TestPoint (at 0 1.778) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 3.45 1.85) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 149.86 93.726)
    (fp_text reference TP4 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 187.452 82.931)
    (fp_text reference TP3 (at 0.127 1.905) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 171.958 127)
    (fp_text reference TP2 (at 0 1.905) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 180.467 99.441 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at -0.127 1.651 90) (layer F.SilkS))
    (fp_text value 1u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 +12V))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 183.388 71.374)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C24 (at 4.826 0 90) (layer F.SilkS))
    (fp_text value 10u (at 1.25 3.75) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 +12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.924 70.993 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C102 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 120p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /COMP-BLUE))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 147.447 67.945 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J28 (at 0 -2.33) (layer F.SilkS))
    (fp_text value -5V_In (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 -5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 101.092 69.85 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value +5V_IN (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 179.197 71.12 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J27 (at -2.159 1.016 180) (layer F.SilkS) hide)
    (fp_text value 12V_IN (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 +12V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 120.396 86.36 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C22 (at -1.651 2.54 270) (layer F.SilkS))
    (fp_text value 10u (at 1.25 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 105.41 73.66 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C21 (at 4.191 2.159 180) (layer F.SilkS))
    (fp_text value 10u (at 1.25 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LCC:PLCC-68_THT-Socket (layer F.Cu) (tedit 5A02ECC8)
    (at 120.65 93.98)
    (descr "PLCC, 68 pins, through hole")
    (tags "plcc leaded")
    (fp_text reference UF2 (at 0 -3.825) (layer F.SilkS))
    (fp_text value VGC (at 0 29.225) (layer F.Fab))
    (fp_text user %R (at 0 12.7) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /VID8))
    (pad 4 thru_hole circle (at -2.54 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /VID10))
    (pad 6 thru_hole circle (at -5.08 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /COMP-SYN))
    (pad 8 thru_hole circle (at -7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 68 thru_hole circle (at 2.54 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /VID6))
    (pad 66 thru_hole circle (at 5.08 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /VID4))
    (pad 64 thru_hole circle (at 7.62 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VID2))
    (pad 62 thru_hole circle (at 10.16 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VID0))
    (pad 1 thru_hole rect (at 0 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /VID7))
    (pad 3 thru_hole circle (at -2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /VID9))
    (pad 5 thru_hole circle (at -5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /VID11))
    (pad 7 thru_hole circle (at -7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /MONO-COLOR))
    (pad 9 thru_hole circle (at -10.16 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 67 thru_hole circle (at 2.54 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /VID5))
    (pad 65 thru_hole circle (at 5.08 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /VID3))
    (pad 63 thru_hole circle (at 7.62 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /VID1))
    (pad 11 thru_hole circle (at -10.16 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /28M))
    (pad 13 thru_hole circle (at -10.16 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 /ADBUS6))
    (pad 15 thru_hole circle (at -10.16 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 /ADBUS4))
    (pad 17 thru_hole circle (at -10.16 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 /ADBUS2))
    (pad 19 thru_hole circle (at -10.16 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 /ADBUS0))
    (pad 21 thru_hole circle (at -10.16 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 /RGB4.H))
    (pad 23 thru_hole circle (at -10.16 17.78) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 /RGB1.H))
    (pad 25 thru_hole circle (at -10.16 20.32) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /MDBUS1))
    (pad 10 thru_hole circle (at -12.7 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 /14M.H))
    (pad 12 thru_hole circle (at -12.7 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 /ADBUS7))
    (pad 14 thru_hole circle (at -12.7 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 /ADBUS5))
    (pad 16 thru_hole circle (at -12.7 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 /ADBUS3))
    (pad 18 thru_hole circle (at -12.7 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 /ADBUS1))
    (pad 20 thru_hole circle (at -12.7 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /RGB8.H))
    (pad 22 thru_hole circle (at -12.7 17.78) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 /RGB2.H))
    (pad 24 thru_hole circle (at -12.7 20.32) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 /MDBUS0))
    (pad 26 thru_hole circle (at -12.7 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 /MDBUS2))
    (pad 28 thru_hole circle (at -10.16 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 /MDBUS4))
    (pad 30 thru_hole circle (at -7.62 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 /MDBUS6))
    (pad 32 thru_hole circle (at -5.08 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 /RABUS0))
    (pad 34 thru_hole circle (at -2.54 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 /RABUS2))
    (pad 36 thru_hole circle (at 0 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 /RABUS4))
    (pad 38 thru_hole circle (at 2.54 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 /RABUS6))
    (pad 40 thru_hole circle (at 5.08 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 /UH2-40))
    (pad 42 thru_hole circle (at 7.62 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /U18TEST))
    (pad 44 thru_hole circle (at 12.7 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /UH2-44))
    (pad 27 thru_hole circle (at -10.16 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 /MDBUS3))
    (pad 29 thru_hole circle (at -7.62 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 /MDBUS5))
    (pad 31 thru_hole circle (at -5.08 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 /MDBUS7))
    (pad 33 thru_hole circle (at -2.54 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 /RABUS1))
    (pad 35 thru_hole circle (at 0 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 /RABUS3))
    (pad 37 thru_hole circle (at 2.54 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 /RABUS5))
    (pad 39 thru_hole circle (at 5.08 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 /RABUS7))
    (pad 41 thru_hole circle (at 7.62 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /IRQ.L))
    (pad 43 thru_hole circle (at 10.16 25.4) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 /UH2-43))
    (pad 45 thru_hole circle (at 10.16 22.86) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 /PH0.H))
    (pad 47 thru_hole circle (at 10.16 20.32) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /RESET.L))
    (pad 49 thru_hole circle (at 10.16 17.78) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 /FLIP6.H))
    (pad 51 thru_hole circle (at 10.16 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 /HDSEL.H))
    (pad 53 thru_hole circle (at 10.16 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 /M2SEL.L))
    (pad 55 thru_hole circle (at 10.16 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 /UG3-1))
    (pad 57 thru_hole circle (at 10.16 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask))
    (pad 59 thru_hole circle (at 10.16 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 61 thru_hole circle (at 10.16 0) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 /3.5DIK))
    (pad 46 thru_hole circle (at 12.7 20.32) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 /A2R-W.H))
    (pad 48 thru_hole circle (at 12.7 17.78) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 /FLIP7.H))
    (pad 50 thru_hole circle (at 12.7 15.24) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 /BABUS12))
    (pad 52 thru_hole circle (at 12.7 12.7) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 /VBL.L))
    (pad 54 thru_hole circle (at 12.7 10.16) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 /UG3-5))
    (pad 56 thru_hole circle (at 12.7 7.62) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /UG3-7))
    (pad 58 thru_hole circle (at 12.7 5.08) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 60 thru_hole circle (at 12.7 2.54) (size 1.4224 1.4224) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 /STRETCH.L))
    (model ${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-68_THT-Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 150.495 78.994 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C61 (at 1.25 -6.25 90) (layer F.SilkS))
    (fp_text value 470u (at 1.25 6.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 92.456 71.882 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C16 (at 1.143 5.969 90) (layer F.SilkS))
    (fp_text value 470u (at 1.25 6.25 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 171.831 114.173)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C6 (at 1.25 -6.25) (layer F.SilkS))
    (fp_text value 1000u (at 1.25 6.25) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 /R54-1))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /UC2-9))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 159.639 84.201)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C13 (at -3.302 0) (layer F.SilkS))
    (fp_text value 22uF (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /UC2-3))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /H4-6))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 159.639 90.1954)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C5 (at -3.048 0.1016) (layer F.SilkS))
    (fp_text value 22uF (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /UC2-4))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /H3-6))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 159.639 96.139)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at -3.048 0.254) (layer F.SilkS))
    (fp_text value 22uF (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /UC2-5))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /H2-6))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 160.655 82.169 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6alt1 (at 4.064 0.762) (layer F.SilkS) hide)
    (fp_text value 22uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /H4-6))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /UC2-3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 160.655 88.011 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5alt1 (at 4.064 0.508) (layer F.SilkS) hide)
    (fp_text value 22uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /H3-6))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /UC2-4))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 160.589 94.107 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4alt1 (at 3.998 0.762) (layer F.SilkS) hide)
    (fp_text value 22uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /H2-6))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 /UC2-5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 190.373 108.077 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0 -2.54) (layer F.SilkS))
    (fp_text value 100n (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 164.465 119.507 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C60 (at 1.27 -3.429 90) (layer F.SilkS))
    (fp_text value 22u (at 1.25 3.75 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 /R14-2))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 131.064 125.984 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 1 +5V))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 86 /U18TEST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 96.52 88.9)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J20 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "RGB In" (at 0 20.11) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 /RGB2.H))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 /RGB2.H))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 /RGB1.H))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 /RGB1.H))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 /RGB8.H))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 /RGB8.H))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 /RGB4.H))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 /RGB4.H))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.33 106.68 180)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "Aux Data Bus" (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 /ADBUS7))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 /ADBUS6))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /ADBUS5))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 /ADBUS4))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 /ADBUS3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 /ADBUS2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /ADBUS1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /ADBUS0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 121.92 130.81 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J26 (at -0.7874 -2.286 90) (layer F.SilkS) hide)
    (fp_text value SYNC (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 /SYNC.L))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 /SYNC.L))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 143.51 128.27 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J23 (at -0.254 -2.159) (layer F.SilkS) hide)
    (fp_text value "VGC Extra" (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /A2R-W.H))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /A2R-W.H))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /RESET.L))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /RESET.L))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /IRQ.L))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /IRQ.L))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 143.51 119.38 180)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference J22 (at 1.143 14.5415 180) (layer F.SilkS))
    (fp_text value "Memory Control" (at 1.27 15.03) (layer F.Fab))
    (fp_text user %R (at 1.27 6.35 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /STRETCH.L))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /STRETCH.L))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /M2SEL.L))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /M2SEL.L))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /BABUS12))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /BABUS12))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /HDSEL.H))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /HDSEL.H))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /FLIP7.H))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /FLIP7.H))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /FLIP6.H))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /FLIP6.H))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 185.547 95.885 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J19 (at -0.508 4.572 90) (layer F.SilkS) hide)
    (fp_text value CREF (at 1.27 4.87 90) (layer F.Fab))
    (fp_text user %R (at 1.27 1.27) (layer F.Fab))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 CREF.L))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 CREF.L))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 CREF.H))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 CREF.H))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 86.36 80.01)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J25 (at 1.27 -2.33) (layer F.SilkS) hide)
    (fp_text value Bald-Ext-1 (at 1.27 50.59) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 90) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /PH0.H))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 /MDBUS7))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 /RABUS7))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 /MDBUS6))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 /RABUS6))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 /MDBUS5))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /RABUS5))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /RABUS4))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 /MDBUS4))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 /MDBUS3))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 /RABUS3))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 /MDBUS2))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 /RABUS2))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /RABUS1))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(J25-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 /MDBUS1))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 /RABUS0))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 /MDBUS0))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /ADBUS0))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /ADBUS1))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 /ADBUS2))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 /ADBUS4))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 /ADBUS3))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 /ADBUS6))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /ADBUS5))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 /ADBUS7))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 /14MD.H))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 129.54 130.81 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J24 (at 0.127 4.699 90) (layer F.SilkS) hide)
    (fp_text value CLK_PH0 (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /PH0.H))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.33 81.28)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J21 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CLK_14M (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 /14MD.H))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 162.306 75.692 270)
    (fp_text reference TP127 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.778 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 36 /R114-1))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer B.Cu) (tedit 5F9F0FC9)
    (at 137.16 114.3 180)
    (fp_text reference TP112 (at 0.254 -2.286) (layer B.SilkS))
    (fp_text value TestPoint (at 0 1.778) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.45 1.85) (layers B.Cu B.Paste B.Mask)
      (net 85 /UH2-44))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer B.Cu) (tedit 5F9F0FC9)
    (at 127.508 125.73 90)
    (fp_text reference TP93 (at 0 -1.651 90) (layer B.SilkS))
    (fp_text value TestPoint (at 0 1.778 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.45 1.85) (layers B.Cu B.Paste B.Mask)
      (net 87 /UH2-40))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 188.087 88.773 90)
    (fp_text reference TP67 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.778 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 112 /R135-1))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 158.623 122.301)
    (fp_text reference TP61 (at 2.54 -0.762 90) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 111 /R17-1))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 154.559 115.951 180)
    (fp_text reference TP60 (at 0 1.524) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 34 /Q2-3))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 149.225 122.555)
    (fp_text reference TP59 (at 0 1.651) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 32 /R13-1))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "My Libraries:Harwin-S1751-46-Test-Point" (layer F.Cu) (tedit 5F9F0FC9)
    (at 161.417 105.029)
    (fp_text reference TP1 (at -1.016 -1.524) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.45 1.85) (layers F.Cu F.Paste F.Mask)
      (net 47 /UC2-9))
    (model "C:/Users/balde/Dropbox/KiCad/Downloaded Libraries/s1751-46.stp"
      (offset (xyz 0 0.825 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.33 76.2 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R206 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 75 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 119 /14MD.H))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 102 /14M.H))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 123.698 125.984 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R196 (at -1.397 1.524 90) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 1 +5V))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 87 /UH2-40))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.227 116.205)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R193 (at -0.889 -2.286 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 35 +12V))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 113 /R14-2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 152.781 130.429)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R191 (at 0 1.524) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 33 /MONO-COLOR))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 181.737 82.423 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R138 (at 0 1.778) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 44 /UC2-20))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 185.801 88.773 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R135 (at -2.413 -0.508) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 112 /R135-1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 168.91 72.263 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R114 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 117 /R114-2))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 36 /R114-1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 181.864 113.03)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R54 (at 0 -1.397) (layer F.SilkS))
    (fp_text value 75 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 114 /R54-2))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 110 /R54-1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 127.254 127.508 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 2.3114 -0.0508 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 118 /SYNC.L))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 76 /UH2-43))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.6642 100.5586)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -2.9772 0.1524) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 31 /UC2-8))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 152.527 96.901 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 2.921 0) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 30 /L3-1))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 52 /UC2-6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.369 126.873)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0.127 1.524) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 55 /UC2-13))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 111 /R17-1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.989 81.915 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 51k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 59 "Net-(C8-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 51 /UC2-16))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 183.515 88.773 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 2.286 -0.381) (layer F.SilkS))
    (fp_text value 1.5k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 61 CREF.L))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 112 /R135-1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 161.925 115.443 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -2.159 0.127 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 34 /Q2-3))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 113 /R14-2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 150.241 119.253 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -2.667 0 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 32 /R13-1))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 34 /Q2-3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 154.559 122.809)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -2.032 0.127 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 32 /R13-1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 169.926 76.2)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 1.5K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 36 /R114-1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 165.6642 102.997)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -2.4692 0.381) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 47 /UC2-9))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 181.864 115.316)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0.127 1.397) (layer F.SilkS))
    (fp_text value 75 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 37 /R8-2))
    (pad 1 smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 110 /R54-1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.115 115.443 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.159 0 90) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439014634146341)
      (net 71 /M2SEL.L))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2 (layer F.Cu) (tedit 5AE59B05)
    (at 173.863 77.724)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (fp_text reference L12 (at 5.08 -2.47) (layer F.SilkS))
    (fp_text value 1.5u (at 5.08 2.47) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 /COMSYNC))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 /R114-2))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 184.023 108.839 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J18 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value RCA (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /J11-1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 190.5 123.19 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J17 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "RCA Shunt Select" (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J11-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 143.51 97.79 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J16 (at 0 2.159 180) (layer B.SilkS))
    (fp_text value RTC (at 0 -12.49) (layer B.Fab))
    (fp_text user %R (at 0 -5.08 270) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /3.5DIK))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 /UG3-1))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /UG3-7))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 /UG3-6))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /UG3-5))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 143.51 102.87)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J15 (at 2.159 0 90) (layer F.SilkS) hide)
    (fp_text value VBL (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 /VBL.L))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 148.844 127.254 270)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J14 (at 1.778 0 180) (layer F.SilkS) hide)
    (fp_text value Mono-Color (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /MONO-COLOR))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 187.833 77.851 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J13 (at -2.286 0 180) (layer F.SilkS) hide)
    (fp_text value COMSYNC (at 0 2.33 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 /COMSYNC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 100.33 110.49)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "Main Data Bus" (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 /MDBUS7))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 /MDBUS6))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 /MDBUS5))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 /MDBUS4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 /MDBUS3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 /MDBUS2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 /MDBUS1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 /MDBUS0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 168.656 65.405 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value VID_OUT (at 0 22.65 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16) (layer F.Fab))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 /R54-2))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 /COMSYNC))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(J10-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(J10-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /COMP-RED))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /COMP-GREEN))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /COMP-BLUE))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 166.116 77.978)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "Composite Sync" (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /COMP-SYN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 96.52 110.49)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J8 (at -0.127 19.939) (layer F.SilkS) hide)
    (fp_text value "RAM Addr Bus" (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 /RABUS7))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 /RABUS6))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /RABUS5))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /RABUS4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 /RABUS3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 /RABUS2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 /RABUS1))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 /RABUS0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 120.65 80.01 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J7 (at 0 9.779) (layer F.SilkS))
    (fp_text value "Video Binary R" (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /VID11))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /VID10))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /VID9))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /VID8))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 153.035 65.428 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value COMP_RGB (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /COMP-RED))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /COMP-GREEN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /COMP-BLUE))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 130.81 80.01 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J5 (at 0.127 9.779) (layer F.SilkS))
    (fp_text value "Video Binary G" (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /VID7))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /VID6))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VID5))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VID4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 115.062 65.532 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "DAC RGB" (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /H4-1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /H3-1))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /H2-1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 140.97 80.01 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 9.779) (layer F.SilkS))
    (fp_text value "Video Binary B" (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /VID3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /VID2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /VID1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /VID0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.496 70.866 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C101 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 120p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /COMP-GREEN))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 162.941 70.739 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C100 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 120p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /COMP-RED))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 137.16 110.236 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C59 (at 3.048 0 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.68 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 85 /UH2-44))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 180.975 88.793 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 2.266 0.127 180) (layer F.SilkS))
    (fp_text value 220p (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /UC2-17))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 112 /R135-1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 162.941 68.58)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at 2.794 0) (layer F.SilkS))
    (fp_text value 33p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /COMP-RED))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.496 68.58)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C31 (at 1.778 -1.143) (layer F.SilkS))
    (fp_text value 33p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /COMP-GREEN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 127.254 125.222)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 56p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 /UH2-43))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.924 68.58)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at -2.794 0) (layer F.SilkS))
    (fp_text value 33p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /COMP-BLUE))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.369 124.587 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at -2.794 -0.127) (layer F.SilkS))
    (fp_text value 56p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /R13-1))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 111 /R17-1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 158.115 119.253 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 0.127 1.397 90) (layer F.SilkS))
    (fp_text value .001u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /Q2-3))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /UC2-10))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 147.955 119.253 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -2.667 0 90) (layer F.SilkS))
    (fp_text value 27p (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /R13-1))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /Q2-3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 156.337 130.429 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /MONO-COLOR))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 181.737 85.217)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 2.286 -0.635 90) (layer F.SilkS))
    (fp_text value 0.01u (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /UC2-19))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.6842 98.0694 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -0.0508 1.9304) (layer F.SilkS))
    (fp_text value 0.01u (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /UC2-7))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 180.467 104.521 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /UC2-12))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 180.467 108.331 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /UC2-11))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 170.053 78.613 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 1n (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(C8-Pad2)"))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 180.975 93.853 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.921 -0.127 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /UC2-16))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 155.829 100.457 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.68 90) (layer F.SilkS))
    (fp_text value 18p (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /L3-1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 165.801 106.045 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 18p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /UC2-8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 157.099 106.045)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 56p (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /L4-1))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 187.325 102.489 270)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference UE7-1 (at -1.651 -5.08 90) (layer F.SilkS))
    (fp_text value 74LS02 (at 0 5.28 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 14 smd roundrect (at 2.475 -3.81 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 13 smd roundrect (at 2.475 -2.54 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 2.475 -1.27 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 2.475 0 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 2.475 1.27 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 2.475 2.54 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at 2.475 3.81 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -2.475 3.81 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 6 smd roundrect (at -2.475 2.54 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 5 smd roundrect (at -2.475 1.27 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 CREF.H))
    (pad 4 smd roundrect (at -2.475 0 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 CREF.L))
    (pad 3 smd roundrect (at -2.475 -1.27 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -2.475 -2.54 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -2.475 -3.81 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-20_W7.62mm_Socket (layer F.Cu) (tedit 5A02E8C5)
    (at 169.545 82.677)
    (descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference UB2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MC1377 (at 3.81 25.19) (layer F.Fab))
    (fp_text user %R (at 3.81 11.43) (layer F.Fab))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /UC2-20))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /UC2-10))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /UC2-19))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /UC2-9))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(UB2-Pad18)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /UC2-8))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /UC2-17))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /UC2-7))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /UC2-16))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /UC2-6))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /UC2-5))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 +12V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /UC2-4))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /UC2-13))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /UC2-3))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /UC2-12))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /COMP-SYN))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 /UC2-11))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C8-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_SMD_IDT_JU6-6_7.0x5.0mm_P2.54mm (layer F.Cu) (tedit 5DB72B02)
    (at 107.95 82.55 270)
    (descr "SMD Crystal Oscillator IDT https://www.idt.com/document/dst/xu-family-datasheet#page=17, 7.0x5.0mm")
    (tags "SMD SMT crystal oscillator")
    (attr smd)
    (fp_text reference U2 (at 0 -4.63 90) (layer F.SilkS))
    (fp_text value "28.636360 MHz" (at -0.03 4.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.1 -2.54 180) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U2-Pad1)"))
    (pad 3 smd rect (at -2.1 2.54 180) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.1 2.54 180) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 41 /28M))
    (pad 6 smd rect (at 2.1 -2.54 180) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -2.1 0 180) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad2)"))
    (pad 5 smd rect (at 2.1 0 180) (size 1.8 2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U2-Pad5)"))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_IDT_JU6-6_7.0x5.0mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 110.236 74.93)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9) (layer F.SilkS))
    (fp_text value MIC5504-3.3YM5 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 159.004 75.057 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0.508 -2.286) (layer F.SilkS))
    (fp_text value "BC817 " (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 1.88 4.56 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 +12V))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 /R114-1))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 /COMP-SYN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 154.559 119.253 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.159 90) (layer F.SilkS))
    (fp_text value "BC817 " (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 /Q2-3))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /R13-1))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 154.559 126.111 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value "BC817 " (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /R13-1))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 /MONO-COLOR))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2 (layer F.Cu) (tedit 5AE59B05)
    (at 156.337 109.601)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (fp_text reference L4 (at 5.207 2.413) (layer F.SilkS))
    (fp_text value 10u (at 5.08 2.47) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /UC2-8))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /L4-1))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2 (layer F.Cu) (tedit 5AE59B05)
    (at 152.545 99.441 270)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=6.6*2.7mm^2, Vishay, IM-2, http://www.vishay.com/docs/34030/im.pdf")
    (tags "Inductor Axial series Axial Horizontal pin pitch 10.16mm  length 6.6mm diameter 2.7mm Vishay IM-2")
    (fp_text reference L3 (at 5.08 2.177 90) (layer F.SilkS))
    (fp_text value 10u (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /L4-1))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /L3-1))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L6.6mm_D2.7mm_P10.16mm_Horizontal_Vishay_IM-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "My Downloaded Libraries:Jack_RCA_Switchcraft_PJRAN1X1UxxX" (layer F.Cu) (tedit 604FB660)
    (at 182.88 124.968)
    (fp_text reference J11 (at -3 -7) (layer F.SilkS) hide)
    (fp_text value "RCA MONO OUT" (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.5 2.3) (drill oval 2.5 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -3.75 -3.7) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask)
      (net 27 /J11-1))
    (pad 3 thru_hole oval (at 3.75 -3.7) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask)
      (net 28 "Net-(J11-Pad3)"))
  )
  (module Resistor_THT:R_Array_SIP7 (layer F.Cu) (tedit 5A14249F)
    (at 115.57 69.85 270)
    (descr "7-pin Resistor SIP pack")
    (tags R)
    (fp_text reference H4 (at 17.526 0 180) (layer F.SilkS))
    (fp_text value VideoThingy (at 8.89 2.4 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /H4-6))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /VID8))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /VID9))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /VID10))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /VID11))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /H4-1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP7 (layer F.Cu) (tedit 5A14249F)
    (at 125.73 69.85 270)
    (descr "7-pin Resistor SIP pack")
    (tags R)
    (fp_text reference H3 (at 17.526 0 180) (layer F.SilkS))
    (fp_text value VideoThingy (at 8.89 2.4 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /H3-6))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /VID4))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /VID5))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /VID6))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /VID7))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /H3-1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP7 (layer F.Cu) (tedit 5A14249F)
    (at 135.89 69.85 270)
    (descr "7-pin Resistor SIP pack")
    (tags R)
    (fp_text reference H2 (at 17.526 -0.254 180) (layer F.SilkS))
    (fp_text value VideoThingy (at 8.89 2.4 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 7 thru_hole oval (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 12.7 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /H2-6))
    (pad 5 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VID0))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /VID1))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VID2))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /VID3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /H2-1))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Array_SIP10 (layer F.Cu) (tedit 5A14249F)
    (at 120.269 65.278)
    (descr "10-pin Resistor SIP pack")
    (tags R)
    (fp_text reference H1 (at 23.241 2.286) (layer F.SilkS))
    (fp_text value Video_Sync (at 12.7 2.4) (layer F.Fab))
    (fp_text user %R (at 11.43 0) (layer F.Fab))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /COMP-BLUE))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 -5V))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /H2-1))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /H3-1))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /COMP-GREEN))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /COMP-SYN))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /H4-1))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /COMP-RED))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Array_SIP10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 110.17 77.978 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -2.479 -0.127 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.95 0 180) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 100.838 73.152)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Hi Chat!\nThank You!\n*rj was right" (at 86.36 68.58 90) (layer B.SilkS))
  (gr_text "Golden Delicious \nVGC Proto PCB rev1.1\n@baldengineer\nrev1" (at 175.26 128.27) (layer B.SilkS))
  (gr_text VBL.L (at 146.8755 102.8065) (layer B.SilkS))
  (gr_text +5V (at 108.712 69.85 180) (layer B.SilkS))
  (gr_text +5V (at 108.712 69.85) (layer F.SilkS))
  (gr_text +12V (at 176.276 73.406 180) (layer B.SilkS))
  (gr_text +12V (at 176.2252 73.7616) (layer F.SilkS))
  (gr_text H4-6 (at 117.602 82.804 90) (layer B.SilkS))
  (gr_text H3-6 (at 128.524 82.804 180) (layer B.SilkS))
  (gr_text H2-6 (at 138.938 82.55 180) (layer B.SilkS))
  (gr_text H4-6 (at 117.602 82.804 90) (layer F.SilkS))
  (gr_text H2-6 (at 138.938 82.55) (layer F.SilkS))
  (gr_text H3-6 (at 128.524 82.804) (layer F.SilkS))
  (gr_text H4-1 (at 117.856 69.596 90) (layer B.SilkS))
  (gr_text H3-1 (at 128.016 69.596 90) (layer B.SilkS))
  (gr_text H2-1 (at 138.176 69.596 90) (layer B.SilkS))
  (gr_text H4-1 (at 117.856 69.596 90) (layer F.SilkS))
  (gr_text H3-1 (at 128.016 69.596 90) (layer F.SilkS))
  (gr_text H2-1 (at 138.176 69.596 90) (layer F.SilkS))
  (gr_text 1 (at 138.557 77.6605) (layer B.SilkS))
  (gr_text 0 (at 138.4935 80.2005) (layer B.SilkS))
  (gr_text 3 (at 138.6205 72.5805) (layer B.SilkS))
  (gr_text 2 (at 138.6205 75.1205) (layer B.SilkS))
  (gr_text 5 (at 128.397 77.47) (layer B.SilkS))
  (gr_text 4 (at 128.3335 80.01) (layer B.SilkS))
  (gr_text 6 (at 128.4605 74.93) (layer B.SilkS))
  (gr_text 7 (at 128.4605 72.39) (layer B.SilkS))
  (gr_text 10 (at 118.364 74.93) (layer B.SilkS))
  (gr_text 9 (at 118.364 77.47) (layer B.SilkS))
  (gr_text 8 (at 118.364 79.9465) (layer B.SilkS))
  (gr_text 11 (at 118.364 72.39) (layer B.SilkS))
  (gr_text 1 (at 138.557 77.6605) (layer F.SilkS))
  (gr_text 0 (at 138.6205 80.2005) (layer F.SilkS))
  (gr_text 2 (at 138.4935 75.1205) (layer F.SilkS))
  (gr_text 3 (at 138.4935 72.5805) (layer F.SilkS))
  (gr_text 4 (at 128.397 80.01) (layer F.SilkS))
  (gr_text 5 (at 128.3335 77.47) (layer F.SilkS))
  (gr_text 6 (at 128.27 74.93) (layer F.SilkS))
  (gr_text 7 (at 128.27 72.39) (layer F.SilkS))
  (gr_text 8 (at 118.364 79.9465) (layer F.SilkS))
  (gr_text 9 (at 118.364 77.47) (layer F.SilkS))
  (gr_text 10 (at 118.364 74.93) (layer F.SilkS))
  (gr_text 11 (at 118.364 72.39) (layer F.SilkS))
  (gr_text L3 (at 152.654 104.648 90) (layer B.SilkS))
  (gr_text L4 (at 161.544 109.474) (layer B.SilkS))
  (gr_text L12 (at 179.07 77.47 180) (layer B.SilkS))
  (gr_text +12V (at 179.197 98.171 90) (layer B.SilkS))
  (gr_text +12V (at 179.197 98.298 90) (layer F.SilkS))
  (gr_text UC2-10 (at 169.418 107.696 180) (layer B.SilkS))
  (gr_text UC2-10 (at 169.291 107.696) (layer F.SilkS))
  (gr_text UC2-4 (at 165.989 90.297) (layer B.SilkS))
  (gr_text UC2-3 (at 165.989 87.757) (layer B.SilkS))
  (gr_text UC2-5 (at 166.116 92.837) (layer B.SilkS))
  (gr_text 7 (at 167.767 98.171) (layer F.SilkS))
  (gr_text UC2-5 (at 165.862 92.837) (layer F.SilkS))
  (gr_text UC2-4 (at 165.989 90.297) (layer F.SilkS))
  (gr_text UC2-3 (at 165.989 87.757) (layer F.SilkS))
  (gr_text "COMP-\nSYN" (at 166.37 85.344) (layer F.SilkS))
  (gr_text UG3-1 (at 140.265167 90.3605) (layer B.SilkS))
  (gr_text 3.5DIK (at 140.131833 87.5665) (layer B.SilkS))
  (gr_text UG3-6 (at 140.265167 95.3135) (layer B.SilkS))
  (gr_text UG3-7 (at 140.265167 92.9005) (layer B.SilkS))
  (gr_text UG3-5 (at 140.265167 97.8535) (layer B.SilkS))
  (gr_text 3.5DIK (at 140.030167 87.5665) (layer F.SilkS))
  (gr_text UG3-1 (at 139.896833 90.3605) (layer F.SilkS))
  (gr_text UG3-7 (at 139.896833 92.9005) (layer F.SilkS))
  (gr_text UG3-6 (at 139.896833 95.3135) (layer F.SilkS))
  (gr_text UG3-5 (at 139.896833 97.8535) (layer F.SilkS))
  (gr_text VBL.L (at 146.8755 102.9335) (layer F.SilkS))
  (gr_text Stretch (at 147.182333 106.4895) (layer B.SilkS))
  (gr_text BAUS12 (at 147.353762 111.633) (layer B.SilkS))
  (gr_text Flip6 (at 145.542 119.888 270) (layer B.SilkS))
  (gr_text HDSEL (at 146.934714 114.173) (layer B.SilkS))
  (gr_text M2SEL (at 146.953762 109.093) (layer B.SilkS))
  (gr_text Flip7 (at 145.542 116.713 270) (layer B.SilkS))
  (gr_text Flip6 (at 145.415 120.015 90) (layer F.SilkS))
  (gr_text Flip7 (at 145.415 116.84 90) (layer F.SilkS))
  (gr_text HDSEL (at 146.881881 114.3) (layer F.SilkS))
  (gr_text BAUS12 (at 147.300929 111.76) (layer F.SilkS))
  (gr_text M2SEL (at 146.900929 109.22) (layer F.SilkS))
  (gr_text Stretch (at 147.1295 106.6165) (layer F.SilkS))
  (gr_text "RCA\nShunt" (at 193.167 120.015 270) (layer F.SilkS))
  (gr_text "RCA\nShunt" (at 193.167 120.0785 -90) (layer B.SilkS))
  (gr_text "RCA\nOut" (at 186.4995 111.5695) (layer F.SilkS))
  (gr_text "RCA\nOut" (at 186.436 111.5695) (layer B.SilkS))
  (gr_text CREF.H (at 182.9308 94.6404 90) (layer F.SilkS))
  (gr_text CREF.H (at 183.515 94.615 90) (layer B.SilkS))
  (gr_text CREF.L (at 190.8556 94.488 90) (layer F.SilkS))
  (gr_text CREF.L (at 190.246 94.615 90) (layer B.SilkS))
  (gr_text "COM\nSYNC" (at 187.833 75.438) (layer B.SilkS))
  (gr_text "COM\nSYNC" (at 187.833 75.438) (layer F.SilkS))
  (gr_text "COM-\nSYNC" (at 166.243 75.565) (layer B.SilkS))
  (gr_text "COM-\nSYNC" (at 166.243 75.565) (layer F.SilkS))
  (gr_text "COM\nSYNC" (at 183.769 62.611 270) (layer B.SilkS))
  (gr_text "COM\nSYNC" (at 183.769 62.484 -90) (layer F.SilkS))
  (gr_text CGRN (at 170.942 62.611 -90) (layer F.SilkS))
  (gr_text CGRN (at 171.069 62.541143 -90) (layer B.SilkS))
  (gr_text CRED (at 173.609 62.668143 -90) (layer B.SilkS))
  (gr_text CRED (at 173.482 62.738 -90) (layer F.SilkS))
  (gr_text CBLU (at 168.656 62.738 -90) (layer F.SilkS))
  (gr_text CBLU (at 168.656 62.738 270) (layer B.SilkS))
  (gr_text CRED (at 163.195 62.865 -90) (layer F.SilkS))
  (gr_text CRED (at 163.322 62.795143 -90) (layer B.SilkS))
  (gr_text CGRN (at 157.861 62.738 -90) (layer F.SilkS))
  (gr_text CGRN (at 157.988 62.668143 -90) (layer B.SilkS))
  (gr_text CBLU (at 152.908 62.865 -90) (layer F.SilkS))
  (gr_text CBLU (at 153.035 62.795143 270) (layer B.SilkS))
  (gr_text -5V (at 147.574 62.504238 270) (layer B.SilkS))
  (gr_text -5V (at 147.447 62.484 270) (layer F.SilkS))
  (gr_text CBLU (at 140.462 62.541143 270) (layer B.SilkS))
  (gr_text -5V (at 138.049 62.504238 270) (layer B.SilkS))
  (gr_text +5V (at 143.129 62.504238 270) (layer B.SilkS))
  (gr_text H2 (at 135.636 63.074286) (layer B.SilkS))
  (gr_text +5V (at 143.002 62.484 -90) (layer F.SilkS))
  (gr_text -5V (at 137.922 62.484 270) (layer F.SilkS))
  (gr_text CGRN (at 127.762 62.484 270) (layer B.SilkS))
  (gr_text CRED (at 120.269 62.526857 270) (layer B.SilkS))
  (gr_text CSYN (at 125.349 62.541143 270) (layer B.SilkS))
  (gr_text H3 (at 130.175 63.074286) (layer B.SilkS))
  (gr_text H4 (at 122.555 63.074286) (layer B.SilkS))
  (gr_text CRED (at 120.269 62.484 -90) (layer F.SilkS))
  (gr_text CBLU (at 140.335 62.611 -90) (layer F.SilkS))
  (gr_text CGRN (at 127.762 62.484 -90) (layer F.SilkS))
  (gr_text CSYN (at 125.349 62.484 270) (layer F.SilkS))
  (gr_text H4 (at 109.982 63.246) (layer B.SilkS))
  (gr_text H2 (at 114.935 63.246) (layer B.SilkS))
  (gr_text H3 (at 112.395 63.246) (layer B.SilkS))
  (gr_text H2 (at 135.509 63.119 180) (layer F.SilkS))
  (gr_text H3 (at 130.175 63.119 180) (layer F.SilkS))
  (gr_text H4 (at 122.555 63.119 180) (layer F.SilkS))
  (gr_text H2 (at 114.935 63.119 180) (layer F.SilkS))
  (gr_text H3 (at 112.395 63.119 180) (layer F.SilkS))
  (gr_text H4 (at 109.982 63.119 180) (layer F.SilkS))
  (gr_text "Mono\nColor" (at 148.844 130.302 270) (layer F.SilkS))
  (gr_text "Mono\nColor" (at 148.844 130.302 -90) (layer B.SilkS))
  (gr_text RESET (at 137.388572 125.73) (layer B.SilkS))
  (gr_text A2RW (at 137.617143 123.19) (layer B.SilkS))
  (gr_text PH0 (at 137.922 128.27) (layer B.SilkS))
  (gr_text A2RW (at 137.617143 123.19) (layer F.SilkS))
  (gr_text RESET (at 137.388572 125.73) (layer F.SilkS))
  (gr_text PH0 (at 137.998096 128.27) (layer F.SilkS))
  (gr_text PH0 (at 127.508 131.318 270) (layer B.SilkS))
  (gr_text PH0 (at 129.3876 133.1722) (layer F.SilkS))
  (gr_text SYNC (at 123.19 132.842) (layer B.SilkS))
  (gr_text SYNC (at 123.19 132.842) (layer F.SilkS))
  (gr_text 28M (at 108.839 94.996 135) (layer B.SilkS))
  (gr_text 14M (at 106.426 96.266 90) (layer B.SilkS))
  (gr_text MC (at 113.03 92.202 90) (layer B.SilkS))
  (gr_text COMP_SYN (at 115.57 100.838 90) (layer B.SilkS))
  (gr_text VID (at 123.698 99.314) (layer B.SilkS))
  (gr_text 1 (at 128.299 92.583 -90) (layer B.SilkS))
  (gr_text 3 (at 125.759 92.583 -90) (layer B.SilkS))
  (gr_text 5 (at 123.219 92.583 -90) (layer B.SilkS))
  (gr_text 7 (at 120.552 92.583 -90) (layer B.SilkS))
  (gr_text 9 (at 118.139 92.583 -90) (layer B.SilkS))
  (gr_text "1\n1" (at 115.472 92.583 -90) (layer B.SilkS))
  (gr_text "10\n" (at 118.081 98.425 90) (layer B.SilkS))
  (gr_text 8 (at 120.621 98.044 90) (layer B.SilkS))
  (gr_text 6 (at 123.161 98.044 90) (layer B.SilkS))
  (gr_text 4 (at 125.701 98.044 90) (layer B.SilkS))
  (gr_text 2 (at 128.368 98.044 90) (layer B.SilkS))
  (gr_text STRETCH (at 134.874 94.742 270) (layer B.SilkS))
  (gr_text 5V (at 135.128 99.06) (layer B.SilkS))
  (gr_text VBL (at 134.874 106.934 90) (layer B.SilkS))
  (gr_text M2SEL (at 127.762 106.934) (layer B.SilkS))
  (gr_text HDSEL (at 127.762 109.22) (layer B.SilkS))
  (gr_text 7 (at 135.001 111.789) (layer B.SilkS))
  (gr_text FLIP6 (at 128.016 111.76) (layer B.SilkS))
  (gr_text RW (at 134.903 114.173 90) (layer B.SilkS))
  (gr_text RESET (at 127.889 114.3) (layer B.SilkS))
  (gr_text PH0 (at 132.334 118.364 135) (layer B.SilkS))
  (gr_text IRQ (at 128.397 121.441 90) (layer B.SilkS))
  (gr_text 7 (at 125.701 120.777 -90) (layer B.SilkS))
  (gr_text 5 (at 123.161 120.777 -90) (layer B.SilkS))
  (gr_text 3 (at 120.621 120.777 -90) (layer B.SilkS))
  (gr_text 1 (at 118.081 120.777 -90) (layer B.SilkS))
  (gr_text 0 (at 115.541 115.443 -90) (layer B.SilkS))
  (gr_text 2 (at 118.081 115.443 270) (layer B.SilkS))
  (gr_text 4 (at 120.621 115.443 -90) (layer B.SilkS))
  (gr_text 6 (at 123.161 115.443 -90) (layer B.SilkS))
  (gr_text "RAM Addr" (at 119.253 114.3) (layer B.SilkS))
  (gr_text "Main Data" (at 110.998 122.428) (layer B.SilkS))
  (gr_text 4 (at 109.191 118.237 -45) (layer B.SilkS))
  (gr_text 1 (at 111.887 114.271) (layer B.SilkS))
  (gr_text 2 (at 113.001 115.443 270) (layer B.SilkS))
  (gr_text 7 (at 115.541 120.777 270) (layer B.SilkS))
  (gr_text 5 (at 113.001 120.777 270) (layer B.SilkS))
  (gr_text 3 (at 110.461 120.777 270) (layer B.SilkS))
  (gr_text 2 (at 106.553 116.811) (layer B.SilkS))
  (gr_text 0 (at 106.553 114.271) (layer B.SilkS))
  (gr_text RGB (at 113.03 110.236 270) (layer B.SilkS))
  (gr_text 1 (at 111.887 111.731) (layer B.SilkS))
  (gr_text 4 (at 111.887 108.937) (layer B.SilkS))
  (gr_text 8 (at 106.553 109.191) (layer B.SilkS))
  (gr_text 2 (at 106.553 111.731) (layer B.SilkS))
  (gr_text "Aux Data" (at 113.157 102.587 270) (layer B.SilkS))
  (gr_text 0 (at 111.887 106.651) (layer B.SilkS))
  (gr_text 2 (at 111.887 104.111) (layer B.SilkS))
  (gr_text 4 (at 111.887 101.571) (layer B.SilkS))
  (gr_text 6 (at 111.887 99.031) (layer B.SilkS))
  (gr_text 7 (at 106.553 99.031) (layer B.SilkS))
  (gr_text 5 (at 106.553 101.571) (layer B.SilkS))
  (gr_text 3 (at 106.553 104.111) (layer B.SilkS))
  (gr_text 1 (at 106.553 106.651) (layer B.SilkS))
  (gr_text 14M (at 91.789238 80.01 180) (layer B.SilkS))
  (gr_text 14M (at 102.108 81.026 270) (layer B.SilkS))
  (gr_text 14M (at 102.108 81.026 90) (layer F.SilkS))
  (gr_text AD (at 100.33 86.741) (layer B.SilkS))
  (gr_text 6 (at 102.362 91.567 270) (layer B.SilkS))
  (gr_text 1 (at 102.362 104.14 270) (layer B.SilkS))
  (gr_text 7 (at 102.362 89.027 270) (layer B.SilkS))
  (gr_text 3 (at 102.362 99.06 270) (layer B.SilkS))
  (gr_text 4 (at 102.362 96.52 270) (layer B.SilkS))
  (gr_text 2 (at 102.362 101.6 270) (layer B.SilkS))
  (gr_text 0 (at 102.362 106.68 270) (layer B.SilkS))
  (gr_text 5 (at 102.362 93.98 270) (layer B.SilkS))
  (gr_text 6 (at 102.391 91.567 90) (layer F.SilkS))
  (gr_text 1 (at 102.391 104.14 90) (layer F.SilkS))
  (gr_text 7 (at 102.391 89.027 90) (layer F.SilkS))
  (gr_text 3 (at 102.391 99.06 90) (layer F.SilkS))
  (gr_text 4 (at 102.391 96.52 90) (layer F.SilkS))
  (gr_text 2 (at 102.391 101.6 90) (layer F.SilkS))
  (gr_text 0 (at 102.391 106.68 90) (layer F.SilkS))
  (gr_text 5 (at 102.391 93.98 90) (layer F.SilkS))
  (gr_text AD (at 100.33 86.741) (layer F.SilkS))
  (gr_text RA (at 96.647 130.556 180) (layer B.SilkS))
  (gr_text MD (at 100.457 130.429 180) (layer B.SilkS))
  (gr_text 6 (at 102.616 125.73 90) (layer B.SilkS))
  (gr_text 1 (at 102.616 113.157 90) (layer B.SilkS))
  (gr_text 7 (at 102.616 128.27 90) (layer B.SilkS))
  (gr_text 3 (at 102.616 118.237 90) (layer B.SilkS))
  (gr_text 4 (at 102.616 120.777 90) (layer B.SilkS))
  (gr_text 2 (at 102.616 115.697 90) (layer B.SilkS))
  (gr_text 0 (at 102.616 110.617 90) (layer B.SilkS))
  (gr_text 5 (at 102.616 123.317 90) (layer B.SilkS))
  (gr_text 7 (at 94.488 128.27 90) (layer B.SilkS))
  (gr_text RGB8 (at 94.488 95.25 90) (layer B.SilkS))
  (gr_text RGB1 (at 94.488 100.33 90) (layer B.SilkS))
  (gr_text RGB4 (at 94.488 90.17 90) (layer B.SilkS))
  (gr_text RGB2 (at 94.488 105.41 90) (layer B.SilkS))
  (gr_text 1 (at 94.488 113.157 90) (layer B.SilkS))
  (gr_text 4 (at 94.488 120.777 90) (layer B.SilkS))
  (gr_text 0 (at 94.361 110.617 90) (layer B.SilkS))
  (gr_text 2 (at 94.488 115.697 90) (layer B.SilkS))
  (gr_text 5 (at 94.488 123.317 90) (layer B.SilkS))
  (gr_text 3 (at 94.488 118.237 90) (layer B.SilkS))
  (gr_text 6 (at 94.488 125.73 90) (layer B.SilkS))
  (gr_text MD3 (at 91.694 110.617) (layer B.SilkS))
  (gr_text MD4 (at 91.694 113.157) (layer B.SilkS))
  (gr_text AD4 (at 91.694 90.17) (layer B.SilkS))
  (gr_text MD0 (at 91.694 97.917) (layer B.SilkS))
  (gr_text "MD1\n" (at 91.694 100.457) (layer B.SilkS))
  (gr_text MD5 (at 91.694 118.237) (layer B.SilkS))
  (gr_text MD2 (at 91.694 108.077) (layer B.SilkS))
  (gr_text N/C (at 91.821 102.997) (layer B.SilkS))
  (gr_text AD6 (at 91.694 87.63) (layer B.SilkS))
  (gr_text AD2 (at 91.694 92.71) (layer B.SilkS))
  (gr_text MD7 (at 91.694 123.317) (layer B.SilkS))
  (gr_text MD6 (at 91.694 120.777) (layer B.SilkS))
  (gr_text AD7 (at 83.693 85.09 180) (layer B.SilkS))
  (gr_text AD5 (at 83.693 87.63 180) (layer B.SilkS))
  (gr_text AD3 (at 83.693 90.17 180) (layer B.SilkS))
  (gr_text AD1 (at 83.693 95.25 180) (layer B.SilkS))
  (gr_text AD0 (at 83.693 97.663 180) (layer B.SilkS))
  (gr_text RA6 (at 83.693 120.65 180) (layer B.SilkS))
  (gr_text RA4 (at 83.693 115.57 180) (layer B.SilkS))
  (gr_text RA1 (at 83.693 105.537 180) (layer B.SilkS))
  (gr_text RA0 (at 83.693 100.457 180) (layer B.SilkS))
  (gr_text RA5 (at 83.693 118.11 180) (layer B.SilkS))
  (gr_text RA7 (at 83.693 123.19 180) (layer B.SilkS))
  (gr_text RA3 (at 83.693 110.617 180) (layer B.SilkS))
  (gr_text RA2 (at 83.693 108.077 180) (layer B.SilkS))
  (gr_text PH0 (at 83.693 128.27 180) (layer B.SilkS))
  (gr_text N/C (at 91.567 102.997) (layer F.SilkS))
  (gr_text AD4 (at 91.694 90.17) (layer F.SilkS))
  (gr_text MD0 (at 91.694 97.917) (layer F.SilkS))
  (gr_text "MD1\n" (at 91.694 100.457) (layer F.SilkS))
  (gr_text MD2 (at 91.694 108.077) (layer F.SilkS))
  (gr_text MD3 (at 91.694 110.617) (layer F.SilkS))
  (gr_text MD4 (at 91.694 113.157) (layer F.SilkS))
  (gr_text MD5 (at 91.694 118.237) (layer F.SilkS))
  (gr_text MD6 (at 91.694 120.777) (layer F.SilkS))
  (gr_text MD7 (at 91.694 123.317) (layer F.SilkS))
  (gr_text 7 (at 102.489 128.27 270) (layer F.SilkS))
  (gr_text 1 (at 102.489 113.157 270) (layer F.SilkS))
  (gr_text 4 (at 102.489 120.777 270) (layer F.SilkS))
  (gr_text 0 (at 102.489 110.617 270) (layer F.SilkS))
  (gr_text 2 (at 102.489 115.697 270) (layer F.SilkS))
  (gr_text 5 (at 102.489 123.317 270) (layer F.SilkS))
  (gr_text 3 (at 102.489 118.237 270) (layer F.SilkS))
  (gr_text 6 (at 102.489 125.73 270) (layer F.SilkS))
  (gr_text 7 (at 94.361 128.27 -90) (layer F.SilkS))
  (gr_text MD (at 100.33 130.556) (layer F.SilkS))
  (gr_text RA (at 96.52 130.429) (layer F.SilkS))
  (gr_text 0 (at 94.488 110.617 -90) (layer F.SilkS))
  (gr_text 1 (at 94.361 113.157 -90) (layer F.SilkS))
  (gr_text 2 (at 94.361 115.697 -90) (layer F.SilkS))
  (gr_text 3 (at 94.361 118.237 -90) (layer F.SilkS))
  (gr_text 4 (at 94.361 120.777 -90) (layer F.SilkS))
  (gr_text 5 (at 94.361 123.317 -90) (layer F.SilkS))
  (gr_text 6 (at 94.361 125.73 -90) (layer F.SilkS))
  (gr_text PH0 (at 83.693 128.27 180) (layer F.SilkS))
  (gr_text RA7 (at 83.693 123.19 180) (layer F.SilkS))
  (gr_text RA6 (at 83.693 120.65 180) (layer F.SilkS))
  (gr_text RA5 (at 83.693 118.11 180) (layer F.SilkS))
  (gr_text RA4 (at 83.693 115.57 180) (layer F.SilkS))
  (gr_text RA3 (at 83.693 110.617 180) (layer F.SilkS))
  (gr_text RA2 (at 83.693 108.077 180) (layer F.SilkS))
  (gr_text RA1 (at 83.693 105.537 180) (layer F.SilkS))
  (gr_text RA0 (at 83.693 100.457 180) (layer F.SilkS))
  (gr_text AD0 (at 83.693 97.663 180) (layer F.SilkS))
  (gr_text RGB2 (at 94.361 105.41 -90) (layer F.SilkS))
  (gr_text RGB1 (at 94.361 100.33 -90) (layer F.SilkS))
  (gr_text RGB8 (at 94.361 95.25 -90) (layer F.SilkS))
  (gr_text RGB4 (at 94.361 90.17 -90) (layer F.SilkS))
  (gr_text 14M (at 91.789238 80.01) (layer F.SilkS))
  (gr_text AD6 (at 91.694 87.63) (layer F.SilkS))
  (gr_text AD2 (at 91.694 92.71) (layer F.SilkS))
  (gr_text AD1 (at 83.693 95.25 180) (layer F.SilkS))
  (gr_text AD3 (at 83.693 90.17 180) (layer F.SilkS))
  (gr_text AD5 (at 83.693 87.63 180) (layer F.SilkS))
  (gr_text AD7 (at 83.693 85.09 180) (layer F.SilkS))
  (gr_line (start 81.28 134.62) (end 81.28 60.96) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 195.58 134.62) (end 81.28 134.62) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 195.58 60.96) (end 195.58 134.62) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 81.28 60.96) (end 195.58 60.96) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.009 52.07) (xy 199.009 147.32) (xy 76.835 147.447) (xy 77.851 51.816)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.009 52.07) (xy 199.009 147.32) (xy 76.835 147.447) (xy 77.851 51.816)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.009 52.07) (xy 199.009 147.32) (xy 76.835 147.447) (xy 77.851 51.816)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199.009 52.07) (xy 199.009 147.32) (xy 76.835 147.447) (xy 77.851 51.816)
      )
    )
  )
)
