<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="59.07015" y1="79.74768125" x2="60.12880625" y2="81.44450625" width="0" layer="20" curve="180"/>
<wire x1="59.07015" y1="79.74768125" x2="52.0623" y2="83.143371875" width="0" layer="20" curve="12.214793"/>
<wire x1="52.73798125" y1="85.02578125" x2="52.0623" y2="83.14336875" width="0" layer="20" curve="180"/>
<wire x1="60.128809375" y1="81.444509375" x2="52.737978125" y2="85.025775" width="0" layer="20" curve="12.214799"/>
<wire x1="8.64928125" y1="68.07015" x2="6.95245" y2="69.128809375" width="0" layer="20" curve="179.999659"/>
<wire x1="8.64928125" y1="68.07015" x2="5.253590625" y2="61.0623" width="0" layer="20" curve="12.214794"/>
<wire x1="3.371190625" y1="61.73798125" x2="5.253590625" y2="61.0623" width="0" layer="20" curve="180"/>
<wire x1="6.95245" y1="69.128809375" x2="3.3711875" y2="61.73798125" width="0" layer="20" curve="12.214793"/>
<wire x1="20.326809375" y1="17.64928125" x2="19.26815" y2="15.95245" width="0" layer="20" curve="180.000152"/>
<wire x1="20.326809375" y1="17.64928125" x2="27.334659375" y2="14.25359375" width="0" layer="20" curve="12.214792"/>
<wire x1="26.65898125" y1="12.371190625" x2="27.334659375" y2="14.253590625" width="0" layer="20" curve="179.999831"/>
<wire x1="19.26815" y1="15.95245" x2="26.658978125" y2="12.3711875" width="0" layer="20" curve="12.214794"/>
<wire x1="70.74768125" y1="29.326809375" x2="72.444509375" y2="28.26815" width="0" layer="20" curve="180.000551"/>
<wire x1="70.74768125" y1="29.326809375" x2="74.14336875" y2="36.334659375" width="0" layer="20" curve="12.214791"/>
<wire x1="76.02578125" y1="35.65898125" x2="74.14336875" y2="36.334659375" width="0" layer="20" curve="179.99971"/>
<wire x1="72.444509375" y1="28.26815" x2="76.025775" y2="35.658984375" width="0" layer="20" curve="12.214804"/>
<wire x1="69.69848125" y1="0" x2="64.69848125" y2="0" width="0" layer="20"/>
<wire x1="69.69848125" y1="0" x2="72.19848125" y2="1" width="0" layer="20"/>
<wire x1="76.19848125" y1="2.772790625" x2="72.19848125" y2="1" width="0" layer="20"/>
<wire x1="76.19848125" y1="2.772790625" x2="78.66473125" y2="4.23223125" width="0" layer="20" curve="0.842809"/>
<wire x1="78.66473125" y1="4.23223125" x2="88.396965625" y2="43.69848125" width="0" layer="20" curve="30.387397"/>
<wire x1="88.39696875" y1="48.69848125" x2="88.39696875" y2="43.69848125" width="0" layer="20"/>
<wire x1="88.39696875" y1="48.69848125" x2="87.39696875" y2="49.69848125" width="0" layer="20"/>
<wire x1="87.39696875" y1="49.69848125" x2="77.39696875" y2="49.69848125" width="0" layer="20"/>
<wire x1="77.39696875" y1="49.69848125" x2="77.39696875" y2="73.69848125" width="0" layer="20"/>
<wire x1="87.39696875" y1="73.69848125" x2="88.39696875" y2="74.69848125" width="0" layer="20"/>
<wire x1="88.39696875" y1="78.69848125" x2="88.39696875" y2="74.69848125" width="0" layer="20"/>
<wire x1="88.39696875" y1="78.69848125" x2="87.39696875" y2="79.69848125" width="0" layer="20"/>
<wire x1="72.8685" y1="79.69848125" x2="87.39696875" y2="79.69848125" width="0" layer="20"/>
<wire x1="70.77355" y1="80.551109375" x2="72.8685" y2="79.698478125" width="0" layer="20" curve="44.29208"/>
<wire x1="70.77355" y1="80.551109375" x2="59.8052" y2="88.396965625" width="0" layer="20" curve="17.430499"/>
<wire x1="59.8052" y1="88.39696875" x2="17.841759375" y2="88.39696875" width="0" layer="20"/>
<wire x1="17.841759375" y1="88.39696875" x2="-0.00000625" y2="68.805203125" width="0" layer="20" curve="36.276865"/>
<wire x1="0" y1="68.8052" x2="0" y2="28.591759375" width="0" layer="20"/>
<wire x1="0" y1="28.591759375" x2="8.23223125" y2="17.23223125" width="0" layer="20" curve="18.138428"/>
<wire x1="8.23223125" y1="17.23223125" x2="34.69848125" y2="0" width="0" layer="20" curve="30.387394"/>
<wire x1="38.69848125" y1="0" x2="34.69848125" y2="0" width="0" layer="20"/>
<wire x1="38.69848125" y1="0" x2="39.69848125" y2="1" width="0" layer="20"/>
<wire x1="39.69848125" y1="1" x2="39.69848125" y2="11" width="0" layer="20"/>
<wire x1="39.69848125" y1="11" x2="63.69848125" y2="11" width="0" layer="20"/>
<wire x1="63.69848125" y1="11" x2="63.69848125" y2="1" width="0" layer="20"/>
<wire x1="63.69848125" y1="1" x2="64.69848125" y2="0" width="0" layer="20"/>
<wire x1="38.4825" y1="19.4625" x2="38.48" y2="14.72135" width="0" layer="20"/>
<wire x1="38.48" y1="14.72135" x2="38.4875" y2="14.72125" width="0" layer="20"/>
<wire x1="40.8875" y1="19.4625" x2="40.89" y2="14.72135" width="0" layer="20"/>
<wire x1="40.89" y1="14.72135" x2="40.8875" y2="14.72125" width="0" layer="20"/>
<wire x1="38.4825" y1="19.4625" x2="40.8875" y2="19.4625" width="0" layer="20" curve="-352.94"/>
<wire x1="38.48" y1="14.72135" x2="40.89" y2="14.72135" width="0" layer="20" curve="-355.94"/>
<hole x="37.5225" y="4.88875" drill="1.8"/>
<hole x="65.8740625" y="4.9021875" drill="1.8"/>
<hole x="83.53625" y="47.6475" drill="1.8"/>
<hole x="83.4978125" y="75.9740625" drill="1.8"/>
<wire x1="87.39696875" y1="73.69848125" x2="77.39696875" y2="73.69848125" width="0" layer="20"/>
<hole x="39.661875" y="15.148125" drill="0.5"/>
<hole x="39.7" y="19" drill="0.5"/>
<hole x="38.893125" y="18.98625" drill="0.5"/>
<hole x="40.475" y="19.025" drill="0.5"/>
<hole x="38.844375" y="15.1775" drill="0.5"/>
<hole x="40.46" y="15.173125" drill="0.5"/>
<hole x="37.136875" y="74.744375" drill="0.5"/>
<hole x="38.09" y="74.73" drill="0.5"/>
<hole x="39.02125" y="74.73" drill="0.5"/>
<hole x="37.18" y="82.15875" drill="0.5"/>
<hole x="38.100625" y="82.238125" drill="0.5"/>
<hole x="39.031875" y="82.238125" drill="0.5"/>
<text>LED-IN</text>
<text>SERVO1</text>
<text>SERVO2</text>
<text>LED-IN</text>
<text>SERVO1</text>
<text>SERVO2</text>
<text>LED-IN</text>
<text>SERVO1</text>
<text>SERVO2</text>
<text>LED-IN</text>
<text>SERVO1</text>
<text>SERVO2</text>
<wire x1="36.75" y1="74.25" x2="36.75" y2="82.5" width="0" layer="20"/>
<wire x1="36.75" y1="82.5" x2="36.750625" y2="82.5" width="0" layer="20"/>
<wire x1="36.750625" y1="82.5" x2="36.750625" y2="82.470625" width="0" layer="20"/>
<wire x1="36.750625" y1="82.5" x2="36.750625" y2="82.629375" width="0" layer="20"/>
<wire x1="39.5" y1="82.75" x2="39.5" y2="74.25" width="0" layer="20"/>
<wire x1="39.5" y1="74.25" x2="50.05" y2="74.25" width="0" layer="20"/>
<wire x1="50.05" y1="74.25" x2="52.75" y2="71.25" width="0" layer="20"/>
<wire x1="52.75" y1="71.25" x2="52.75" y2="63.25" width="0" layer="20"/>
<wire x1="52.75" y1="63.25" x2="24.25" y2="63.25" width="0" layer="20"/>
<wire x1="24.25" y1="63.25" x2="24.25" y2="70.25" width="0" layer="20"/>
<wire x1="24.25" y1="70.25" x2="27.95" y2="74.25" width="0" layer="20"/>
<wire x1="27.95" y1="74.25" x2="36.75" y2="74.25" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>S1</text>
<text>S2</text>
<text>S-LED</text>
<text>+</text>
<text>S</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>S</text>
<text>-</text>
<text>+</text>
<text>by Ron de Leos</text>
<text>BB-8</text>
<text>LED LOGICS</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>&lt;--</text>
<text>LED</text>
<text>IN</text>
<text>R</text>
<text>R</text>
<text>R</text>
<text>by Ron de Leos</text>
<text>BB-8</text>
<text>LED LOGICS</text>
<text>v1</text>
<text>by Ron de Leos</text>
<text>150</text>
<text>33</text>
<text>33</text>
<text>P-OUT</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>LED-OUT</text>
<text>+</text>
<text>-</text>
<text>INPUT</text>
<text>S1</text>
<text>S2</text>
<text>LED-S</text>
<text>SERVO2</text>
<text>P-OUT</text>
<text>BATT</text>
<text>+</text>
<text>-</text>
<text>SERVO1</text>
<text>S</text>
<text>-</text>
<text>+</text>
<text>S</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<circle x="6.0194125" y="6.35658125" radius="6.020796875" width="0.008" layer="20"/>
<hole x="10.356871875" y="11.27681875" drill="0.6"/>
<hole x="11.797028125" y="12.68641875" drill="0.6"/>
<hole x="12.5017875" y="11.950975" drill="0.6"/>
<hole x="11.061628125" y="13.391221875" drill="0.6"/>
<hole x="11.061628125" y="10.572015625" drill="0.6"/>
<hole x="9.614384375" y="11.914715625" drill="0.6"/>
<wire x1="8.725996875" y1="11.7338375" x2="11.153096875" y2="14.1609375" width="0.008" layer="20"/>
<wire x1="11.153096875" y1="14.1609375" x2="11.18739375" y2="14.1609375" width="0.008" layer="20"/>
<wire x1="11.0164625" y1="9.6913125" x2="13.418034375" y2="12.092884375" width="0.008" layer="20"/>
<wire x1="13.418034375" y1="12.092884375" x2="13.418034375" y2="12.109865625" width="0.008" layer="20"/>
<hole x="1.75" y="6.5" drill="1.2"/>
<hole x="10" y="6.5" drill="1.2"/>
<text>BB-8</text>
<circle x="62.7694125" y="57.35658125" radius="6.020796875" width="0.008" layer="20"/>
<text>-</text>
<text>+</text>
<text>BB-8</text>
<text>Voice</text>
<text>LED</text>
<hole x="63" y="53.25" drill="1.2"/>
<wire x1="67.775" y1="60.65" x2="70.4" y2="63.275" width="0.008" layer="20"/>
<wire x1="70.4" y1="63.275" x2="70.4" y2="63.325" width="0.008" layer="20"/>
<wire x1="68.775" y1="57.8" x2="71.525" y2="60.55" width="0.008" layer="20"/>
<wire x1="71.525" y1="60.55" x2="71.55" y2="60.6" width="0.008" layer="20"/>
<hole x="68.825" y="59.8" drill="0.6"/>
<hole x="69.15" y="58.875" drill="0.6"/>
<hole x="68.425" y="60.6" drill="0.6"/>
<hole x="70.625" y="61.65" drill="0.6"/>
<hole x="70.975" y="60.825" drill="0.6"/>
<hole x="70.25" y="62.475" drill="0.6"/>
<text>+</text>
<text>HP Servo Mount Plus v2</text>
<text>HP Servo Mount Plus v2</text>
<text>150</text>
<text>BATT</text>
<text>LM338</text>
<text>LM338</text>
<text>INPUT</text>
<text>-</text>
<text>-</text>
<text>HP Servo Mount Plus v2</text>
<text>by Ron de Leos</text>
<text>RADAR EYE</text>
<text>FRONT LOGICS</text>
<text>LED</text>
<text>VOICE</text>
<text>LED</text>
<text>LED</text>
<text>IN</text>
</plain>
<libraries>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="317TS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_2.54_SCREWTERM">
</package>
<package name="1X03">
</package>
<package name="1X02">
</package>
<package name="1X02_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LM338" library="v-reg" package="317TS" value="">
<attribute name="VALUE"/>
</element>
<element name="BATT" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="127">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.4" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SERVO1" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="SERVO2" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="INPUT" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED-IN" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.4" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="IN" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.4" value="33">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.4" value="33">
<attribute name="VALUE"/>
</element>
<element name="OPT" library="led" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.4" value="150"/>
<element name="LED-OUT" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="P-OUT" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="VOICE-IN" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="R" library="SparkFun-Connectors" package="1X02_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VOICE-IN1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED3MM" value="">
<attribute name="PROD_ID" value="DIO-08794"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="120uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="1uF"/>
</elements>
<signals>
<signal name="N$2">
</signal>
<signal name="N$1">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="RAW">
<contactref element="BATT" pad="P1"/>
<contactref element="LM338" pad="3"/>
<contactref element="P-OUT" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="GND1">
<contactref element="BATT" pad="P2"/>
<contactref element="R2" pad="P$1"/>
<contactref element="SERVO1" pad="1"/>
<contactref element="SERVO2" pad="1"/>
<contactref element="LED-OUT" pad="2"/>
<contactref element="P-OUT" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="LM338" pad="1"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="6V">
<contactref element="LM338" pad="2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="SERVO1" pad="2"/>
<contactref element="SERVO2" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="SRVSIG1">
<contactref element="SERVO1" pad="3"/>
<contactref element="INPUT" pad="3"/>
</signal>
<signal name="SRVSIG2">
<contactref element="SERVO2" pad="3"/>
<contactref element="INPUT" pad="2"/>
</signal>
<signal name="N$8">
</signal>
<signal name="GND2">
<contactref element="R4" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="LED-IN" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LED-IN" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="LED3" pad="K"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="LED2" pad="K"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="LED4" pad="K"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="IN" pad="1"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED7" pad="A"/>
<contactref element="OPT" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="LED7" pad="K"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="LED5" pad="K"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$17">
<contactref element="LED6" pad="K"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="LED8" pad="K"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="GND3">
<contactref element="IN" pad="2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="N$19">
<contactref element="OPT" pad="K"/>
<contactref element="R8" pad="P$1"/>
</signal>
<signal name="LEDSIG">
<contactref element="INPUT" pad="1"/>
<contactref element="LED-OUT" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="VOICE-IN" pad="2"/>
<contactref element="R" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="GND4">
<contactref element="D2" pad="K"/>
<contactref element="VOICE-IN" pad="1"/>
</signal>
<signal name="GND5">
<contactref element="D1" pad="K"/>
<contactref element="VOICE-IN1" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="VOICE-IN1" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
