(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 22)
    (no_connects 0)
    (area 64.659364 107.839364 108.060636 151.240636)
    (thickness 1.6)
    (drawings 102)
    (tracks 83)
    (zones 0)
    (modules 23)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2.5)
    (trace_clearance 1)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 3)
    (pad_drill 2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 102.87 118.11)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /L_OUT)
  (net 2 /MOC_PIN4)
  (net 3 /L)
  (net 4 /N)
  (net 5 /MOC_PIN6)
  (net 6 /PE)
  (net 7 /PHASE)
  (net 8 /3.3V)
  (net 9 /GND)
  (net 10 /EN)
  (net 11 "Net-(J5-Pad1)")
  (net 12 "Net-(J1-Pad1)")
  (net_class Default "Это класс цепей по умолчанию."
    (clearance 1)
    (trace_width 2.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3V)
    (add_net /GND)
    (add_net /L)
    (add_net /L_OUT)
    (add_net /N)
    (add_net /PHASE)
  )
  (net_class FAT ""
    (clearance 2)
    (trace_width 2.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J5-Pad1)")
  )
  (net_class lv ""
    (clearance 0.4)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /EN)
    (add_net /MOC_PIN4)
    (add_net /MOC_PIN6)
    (add_net /PE)
    (add_net "Net-(J1-Pad1)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 59E70513)
    (at 68.58 111.76)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 59E70516)
    (at 104.14 111.76)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 59E7050A)
    (at 104.14 147.32)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module .pretty:TO-220_Horizontal_2 (layer B.Cu) (tedit 59885C32)
    (at 104.775 132.08 270)
    (descr "TO-220, Horizontal, RM 2.54mm")
    (tags "TO-220 Horizontal RM 2.54mm")
    (fp_text reference D1 (at 2.54 20.58 270) (layer B.SilkS) hide)
    (fp_text value BT137-600 (at 2.54 -1.9 270) (layer B.Fab))
    (fp_text user %R (at 2.54 20.58 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 /L_OUT))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 /MOC_PIN4))
    (pad 2 smd circle (at 2.55 16.65 270) (size 3.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 7 /PHASE))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Horizontal.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuseholder_Fuse_TR5_Littlefuse-No560_No460 (layer F.Cu) (tedit 59885A32)
    (at 69.85 119.38 270)
    (descr "Fuse, Fuseholder, TR5, Littlefuse/Wickmann, No. 460, No560,")
    (tags "Fuse Fuseholder TR5 Littlefuse/Wickmann No. 460 No560 ")
    (fp_text reference F1 (at 2.39 -6.89 270) (layer F.SilkS) hide)
    (fp_text value Fuse (at 2.39 7.43 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 /L))
    (pad 2 thru_hole circle (at 5.08 0.01 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /PHASE))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 59885D79)
    (at 87.63 149.225 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 0 2.39 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -4.929999 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /3.3V))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /3.3V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer B.Cu) (tedit 59885D7E)
    (at 99.06 146.685)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 0 2.39) (layer B.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 -4.929999) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 59885D33)
    (at 67.31 135.255)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.39) (layer F.SilkS) hide)
    (fp_text value MOC3063M (at 3.81 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /EN))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /MOC_PIN4))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /MOC_PIN6))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 598BEB71)
    (at 75.565 111.76)
    (fp_text reference J2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 2) (layers *.Cu *.Mask)
      (net 3 /L))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 598863B4)
    (at 99.695 126.365)
    (fp_text reference J3 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 2) (layers *.Cu *.Mask)
      (net 4 /N))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 59E700BE)
    (at 80.645 110.49)
    (fp_text reference J4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 6 /PE))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 59E700C4)
    (at 92.075 110.49)
    (fp_text reference J6 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 6 /PE))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 598BEB7B)
    (at 86.36 111.76)
    (fp_text reference J7 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 2) (layers *.Cu *.Mask)
      (net 4 /N))
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 598BEB81)
    (at 97.155 111.76)
    (fp_text reference J5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 2) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad1)"))
  )
  (module .pretty:HLK-PM12 (layer F.Cu) (tedit 59A8FCA3)
    (at 96.52 113.792 270)
    (fp_text reference U2 (at 18 -2 270) (layer F.SilkS) hide)
    (fp_text value HI-LINKPM12 (at 18 -4 270) (layer F.Fab))
    (fp_text user GND (at 31.75 -0.127 270) (layer F.SilkS) hide)
    (fp_text user AC (at 5 12 270) (layer F.SilkS) hide)
    (fp_text user AC (at 5 8 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 2.3 7.5 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /N))
    (pad 2 thru_hole circle (at 2.3 12.5 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /PHASE))
    (pad 3 thru_hole circle (at 31.7 2.3 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /GND))
    (pad 4 thru_hole circle (at 31.7 17.7 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /3.3V))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59885D77)
    (at 73.66 144.145 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 2.39 90) (layer B.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 -2.39 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 59E7050F)
    (at 68.58 147.32)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 59E7020D)
    (at 71.12 139.065 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 1.85 270) (layer B.SilkS) hide)
    (fp_text value 150 (at 0 -1.95 270) (layer B.Fab))
    (fp_text user %R (at 0 1.85 270) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 10 /EN))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58AADA9E)
    (at 71.12 130.175)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 1.85) (layer B.SilkS))
    (fp_text value 360 (at 0 -1.95) (layer B.Fab))
    (fp_text user %R (at 0 1.85) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 7 /PHASE))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /MOC_PIN6))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 58AADA9E)
    (at 98.425 134.62 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 360 (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /L_OUT))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /MOC_PIN4))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module .pretty:iTerm (layer B.Cu) (tedit 59E70132)
    (at 102.87 118.11 270)
    (tags "varistor SIOV")
    (fp_text reference TH1 (at 3.75 -5.3 270) (layer B.SilkS) hide)
    (fp_text value Thermistor_NTC (at 3.75 2.6 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.4) (layers *.Cu *.Mask)
      (net 11 "Net-(J5-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 -2.7 270) (size 2 2) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 /L_OUT))
  )
  (module .pretty:iRV_Disc_D15.5_W3.9_P7.5 (layer B.Cu) (tedit 59E6FF71)
    (at 82.55 121.92)
    (tags "varistor SIOV")
    (fp_text reference RV1 (at 3.75 -3.65) (layer B.SilkS) hide)
    (fp_text value Varistor (at 3.75 2.25) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.4) (layers *.Cu *.Mask)
      (net 7 /PHASE))
    (pad 2 thru_hole circle (at 7.5 -1.4) (size 2 2) (drill 1.4) (layers *.Cu *.Mask)
      (net 4 /N))
  )
  (module .pretty:LOGO_SILK (layer F.Cu) (tedit 595F8ADD)
    (at 82.47 132.51 90)
    (fp_text reference G*** (at 0.4 -8.1 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.2 -10.8 90) (layer F.SilkS) hide)
  )
  (gr_line (start 67.87 121.71) (end 67.87 122.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.67 121.71) (end 67.87 121.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.67 122.11) (end 75.67 121.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 67.87 122.11) (end 75.67 122.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.27 118.91) (end 85.87 118.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.27 123.71) (end 86.27 118.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.87 123.71) (end 86.27 123.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.87 118.91) (end 85.87 123.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.67 127.71) (end 88.47 127.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.47 128.51) (end 88.67 127.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.87 128.51) (end 89.47 128.51) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.87 128.91) (end 94.87 128.51) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.27 127.91) (end 88.47 127.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.27 128.91) (end 88.27 127.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94.87 128.91) (end 89.27 128.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.47 114.11) (end 84.67 113.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.87 117.51) (end 84.47 114.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 88.07 117.31) (end 87.87 117.51) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.67 113.91) (end 88.07 117.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.27 141.31) (end 72.87 141.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.27 133.51) (end 73.27 141.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.87 132.11) (end 73.27 133.51) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.67 132.11) (end 71.87 132.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.27 132.11) (end 71.67 132.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.27 132.51) (end 66.27 132.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.67 132.51) (end 66.27 132.51) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.87 133.71) (end 71.67 132.51) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.87 141.31) (end 72.87 133.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 86.36 129.54) (end 64.709365 142.04) (angle -30) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 86.36 129.54) (end 98.86 151.190635) (angle -30) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 86.36 129.54) (end 108.010635 117.04) (angle -30) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 86.36 129.54) (end 73.86 107.889365) (angle -30) (layer Edge.Cuts) (width 0.1))
  (dimension 50.289434 (width 0.3) (layer Margin)
    (gr_text "50,289 мм" (at 59.370406 156.529594 315) (layer Margin))
    (feature1 (pts (xy 104.14 147.32) (xy 76.195812 175.264188)))
    (feature2 (pts (xy 68.58 111.76) (xy 40.635812 139.704188)))
    (crossbar (pts (xy 42.545 137.795) (xy 78.105 173.355)))
    (arrow1a (pts (xy 78.105 173.355) (xy 76.893779 172.973104)))
    (arrow1b (pts (xy 78.105 173.355) (xy 77.723104 172.143779)))
    (arrow2a (pts (xy 42.545 137.795) (xy 42.926896 139.006221)))
    (arrow2b (pts (xy 42.545 137.795) (xy 43.756221 138.176896)))
  )
  (gr_line (start 101.6 128.143) (end 101.727 128.016) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.235 128.778) (end 101.6 128.143) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.981 123.698) (end 102.108 123.825) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.346 124.333) (end 101.981 123.698) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99.695 126.365) (end 102.108 123.825) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99.695 126.365) (end 101.346 124.333) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.125 142.16) (end 84.925 142.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.125 141.76) (end 83.125 142.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.125 141.76) (end 83.125 141.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.125 142.16) (end 95.125 141.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.925 142.16) (end 95.125 142.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 43.18 (width 0.3) (layer Margin)
    (gr_text "43,180 мм" (at 86.36 98.98) (layer Margin))
    (feature1 (pts (xy 107.95 132.08) (xy 107.95 97.63)))
    (feature2 (pts (xy 64.77 132.08) (xy 64.77 97.63)))
    (crossbar (pts (xy 64.77 100.33) (xy 107.95 100.33)))
    (arrow1a (pts (xy 107.95 100.33) (xy 106.823496 100.916421)))
    (arrow1b (pts (xy 107.95 100.33) (xy 106.823496 99.743579)))
    (arrow2a (pts (xy 64.77 100.33) (xy 65.896504 100.916421)))
    (arrow2b (pts (xy 64.77 100.33) (xy 65.896504 99.743579)))
  )
  (gr_line (start 71.325 127.96) (end 71.325 128.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.125 127.96) (end 71.325 127.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.125 128.36) (end 76.125 127.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.325 128.36) (end 76.125 128.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.725 129.36) (end 97.725 130.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.525 129.36) (end 97.725 129.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.525 130.16) (end 101.525 129.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.725 130.16) (end 101.525 130.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.725 134.36) (end 103.725 135.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.725 134.36) (end 103.725 134.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.725 135.16) (end 105.725 134.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.725 135.16) (end 105.725 135.16) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text N (at 99.695 122.555 180) (layer B.SilkS))
  (gr_text LO (at 97.79 115.57 90) (layer B.SilkS))
  (gr_text PE (at 92.075 113.665 90) (layer F.SilkS))
  (gr_text N (at 87.47 114.31 90) (layer B.SilkS))
  (gr_text PE (at 80.645 113.665 90) (layer F.SilkS))
  (gr_text LI (at 74.93 115.57 90) (layer B.SilkS))
  (gr_text N (at 99.695 122.555 180) (layer F.SilkS))
  (gr_text N (at 87.47 114.31 90) (layer F.SilkS))
  (gr_text LO (at 97.79 115.57 90) (layer F.SilkS))
  (gr_text PE (at 92.075 113.665 90) (layer B.SilkS))
  (gr_text PE (at 80.645 113.665 90) (layer B.SilkS))
  (gr_text LI (at 74.93 115.57 90) (layer F.SilkS))
  (dimension 25.4 (width 0.3) (layer Margin)
    (gr_text "25,400 мм" (at 86.36 163.275) (layer Margin))
    (feature1 (pts (xy 99.06 144.145) (xy 99.06 164.625)))
    (feature2 (pts (xy 73.66 144.145) (xy 73.66 164.625)))
    (crossbar (pts (xy 73.66 161.925) (xy 99.06 161.925)))
    (arrow1a (pts (xy 99.06 161.925) (xy 97.933496 162.511421)))
    (arrow1b (pts (xy 99.06 161.925) (xy 97.933496 161.338579)))
    (arrow2a (pts (xy 73.66 161.925) (xy 74.786504 162.511421)))
    (arrow2b (pts (xy 73.66 161.925) (xy 74.786504 161.338579)))
  )
  (dimension 11.43 (width 0.3) (layer Margin)
    (gr_text "11,430 мм" (at 79.375 155.02) (layer Margin))
    (feature1 (pts (xy 73.66 149.225) (xy 73.66 156.37)))
    (feature2 (pts (xy 85.09 149.225) (xy 85.09 156.37)))
    (crossbar (pts (xy 85.09 153.67) (xy 73.66 153.67)))
    (arrow1a (pts (xy 73.66 153.67) (xy 74.786504 153.083579)))
    (arrow1b (pts (xy 73.66 153.67) (xy 74.786504 154.256421)))
    (arrow2a (pts (xy 85.09 153.67) (xy 83.963496 153.083579)))
    (arrow2b (pts (xy 85.09 153.67) (xy 83.963496 154.256421)))
  )
  (dimension 11.43 (width 0.3) (layer Margin)
    (gr_text "11,430 мм" (at 93.345 155.02) (layer Margin))
    (feature1 (pts (xy 99.06 149.225) (xy 99.06 156.37)))
    (feature2 (pts (xy 87.63 149.225) (xy 87.63 156.37)))
    (crossbar (pts (xy 87.63 153.67) (xy 99.06 153.67)))
    (arrow1a (pts (xy 99.06 153.67) (xy 97.933496 154.256421)))
    (arrow1b (pts (xy 99.06 153.67) (xy 97.933496 153.083579)))
    (arrow2a (pts (xy 87.63 153.67) (xy 88.756504 154.256421)))
    (arrow2b (pts (xy 87.63 153.67) (xy 88.756504 153.083579)))
  )
  (dimension 2.54 (width 0.3) (layer Margin)
    (gr_text "2,540 мм" (at 112.475 147.955 270) (layer Margin))
    (feature1 (pts (xy 99.06 149.225) (xy 113.825 149.225)))
    (feature2 (pts (xy 99.06 146.685) (xy 113.825 146.685)))
    (crossbar (pts (xy 111.125 146.685) (xy 111.125 149.225)))
    (arrow1a (pts (xy 111.125 149.225) (xy 110.538579 148.098496)))
    (arrow1b (pts (xy 111.125 149.225) (xy 111.711421 148.098496)))
    (arrow2a (pts (xy 111.125 146.685) (xy 110.538579 147.811504)))
    (arrow2b (pts (xy 111.125 146.685) (xy 111.711421 147.811504)))
  )
  (gr_line (start 73.86 151.190635) (end 98.86 151.190635) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 64.709365 117.04) (end 64.709365 142.04) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.86 107.889365) (end 73.86 107.889365) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 108.010635 142.04) (end 108.010635 117.04) (layer Edge.Cuts) (width 0.1))
  (dimension 50 (width 0.3) (layer Margin)
    (gr_text "50,000 мм" (at 164.5 44.65) (layer Margin))
    (feature1 (pts (xy 139.5 61.5) (xy 139.5 43.3)))
    (feature2 (pts (xy 189.5 61.5) (xy 189.5 43.3)))
    (crossbar (pts (xy 189.5 46) (xy 139.5 46)))
    (arrow1a (pts (xy 139.5 46) (xy 140.626504 45.413579)))
    (arrow1b (pts (xy 139.5 46) (xy 140.626504 46.586421)))
    (arrow2a (pts (xy 189.5 46) (xy 188.373496 45.413579)))
    (arrow2b (pts (xy 189.5 46) (xy 188.373496 46.586421)))
  )
  (zone (net 9) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 64.77 132.715) (xy 71.755 132.715) (xy 71.755 142.24) (xy 107.95 142.24) (xy 107.315 151.13)
        (xy 64.77 151.13)
      )
    )
  )
  (zone (net 9) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 64.77 132.715) (xy 71.755 132.715) (xy 71.755 142.24) (xy 107.95 142.24) (xy 107.315 151.13)
        (xy 64.77 151.13)
      )
    )
  )
  (zone (net 7) (net_name /PHASE) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.217 129.54) (xy 85.217 139.7) (xy 91.821 139.7) (xy 91.821 137.414) (xy 95.123 137.414)
        (xy 95.123 131.572) (xy 91.821 131.572) (xy 91.821 129.54)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Paste) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.059 130.048) (xy 91.059 132.08) (xy 94.361 132.08) (xy 94.361 136.906) (xy 91.059 136.906)
        (xy 91.059 139.192) (xy 85.979 139.192) (xy 85.725 139.192) (xy 85.725 130.048)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.27 129.51) (xy 91.67 129.51) (xy 91.67 131.51) (xy 95.07 131.51) (xy 95.07 137.51)
        (xy 91.87 137.51) (xy 91.87 139.71) (xy 85.27 139.71)
      )
    )
  )
)
