(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 52)
    (tracks 320)
    (zones 0)
    (modules 26)
    (nets 22)
  )
  (page A4)
  (title_block
    (title "ATTINY1614 mini board")
    (date 2018-12-10)
    (rev 1)
    (comment 1 creativecommons.org/licenses/by-sa/4.0/)
    (comment 2 "License: CC BY-SA 4.0")
    (comment 3 "(C) Vlad Belous")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.6096)
    (trace_clearance 0.2032)
    (zone_clearance 0.3556)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.0762)
    (edge_width 0.0254)
    (via_size 0.6096)
    (via_drill 0.3048)
    (via_min_size 0.6096)
    (via_min_drill 0.3048)
    (user_via 0.6096 0.3048)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.1778)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.0762)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.1016)
    (pad_size 1.905 1.905)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1524)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.076200)
      (plotframeref true)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plot"))
  )
  (net 0 "")
  (net 1 VIN)
  (net 2 GND)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 /RX)
  (net 6 /TX)
  (net 7 /SCK)
  (net 8 /MISO)
  (net 9 /MOSI)
  (net 10 /SCL)
  (net 11 /SDA)
  (net 12 "Net-(Q1-Pad1)")
  (net 13 "Net-(Q2-Pad1)")
  (net 14 /~RESET)
  (net 15 VOUT1-~EN)
  (net 16 "Net-(R7-Pad1)")
  (net 17 VEXT-EN)
  (net 18 UPDI)
  (net 19 /EXT_LOAD-)
  (net 20 /EXT_VIN_LOAD+)
  (net 21 /VOUT1)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.6096)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.2032)
    (add_net /EXT_LOAD-)
    (add_net /EXT_VIN_LOAD+)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RX)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net /VOUT1)
    (add_net /~RESET)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net UPDI)
    (add_net VEXT-EN)
    (add_net VIN)
    (add_net VOUT1-~EN)
  )
  (module local_footprints:SOIC-14_3.9x8.7mm_Pitch1.27mm_HS (layer F.Cu) (tedit 5C120D77)
    (at 148.59 138.43 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value attiny1614 (at 0 5.375 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -2.95 -3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VIN))
    (pad 2 smd roundrect (at -2.95 -2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 VOUT1-~EN))
    (pad 3 smd roundrect (at -2.95 -1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 VEXT-EN))
    (pad 4 smd roundrect (at -2.95 0 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad2)"))
    (pad 5 smd roundrect (at -2.95 1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad3)"))
    (pad 6 smd roundrect (at -2.95 2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RX))
    (pad 7 smd roundrect (at -2.95 3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /TX))
    (pad 8 smd roundrect (at 2.95 3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /SDA))
    (pad 9 smd roundrect (at 2.95 2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /SCL))
    (pad 10 smd roundrect (at 2.95 1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /~RESET))
    (pad 11 smd roundrect (at 2.95 0 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /MOSI))
    (pad 12 smd roundrect (at 2.95 -1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /MISO))
    (pad 13 smd roundrect (at 2.95 -2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /SCK))
    (pad 14 smd roundrect (at 2.95 -3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:SOIC-14_3.9x8.7mm_Pitch1.27mm_HS (layer F.Cu) (tedit 5C120D7A)
    (at 148.59 138.43 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value attiny1614 (at 0 5.375 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -2.95 -3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VIN))
    (pad 2 smd roundrect (at -2.95 -2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 VOUT1-~EN))
    (pad 3 smd roundrect (at -2.95 -1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 VEXT-EN))
    (pad 4 smd roundrect (at -2.95 0 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad2)"))
    (pad 5 smd roundrect (at -2.95 1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad3)"))
    (pad 6 smd roundrect (at -2.95 2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /RX))
    (pad 7 smd roundrect (at -2.95 3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /TX))
    (pad 8 smd roundrect (at 2.95 3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /SDA))
    (pad 9 smd roundrect (at 2.95 2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /SCL))
    (pad 10 smd roundrect (at 2.95 1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /~RESET))
    (pad 11 smd roundrect (at 2.95 0 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /MOSI))
    (pad 12 smd roundrect (at 2.95 -1.27 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /MISO))
    (pad 13 smd roundrect (at 2.95 -2.54 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /SCK))
    (pad 14 smd roundrect (at 2.95 -3.81 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 142.748 140.716 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 VIN))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:1206_Diode_HS (layer F.Cu) (tedit 5C0E1507)
    (at 129.54 134.62)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference D1 (at 0.508 0 90) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 1.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.65 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /EXT_LOAD-))
    (pad 1 smd roundrect (at -1.65 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /EXT_VIN_LOAD+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5C120D19)
    (at 139.7 144.78 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at 0 13.335 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /TX))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S2B-PH-K_02x2.00mm_Angled (layer F.Cu) (tedit 5C120D25)
    (at 128.27 142.24 270)
    (descr "JST PH series connector, S2B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J3 (at 1.5 -2.45 270) (layer F.SilkS) hide)
    (fp_text value BAT_JST_PH (at 1 7.25 270) (layer F.Fab) hide)
    (fp_text user %R (at 1 2.5 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S2B-PH-K_02x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5C120D21)
    (at 134.62 144.78 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5C120D16)
    (at 152.4 144.78 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5C120D1D)
    (at 132.08 144.78 270)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value VOUT1 (at 0 2.54 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.54 90) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 270) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /VOUT1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5C120CE5)
    (at 127 132.08 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value EXT_VIN (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /EXT_VIN_LOAD+))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5C120CEC)
    (at 129.54 132.08 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value EXT_LOAD+ (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /EXT_VIN_LOAD+))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5C120CE8)
    (at 132.08 132.08 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value EXT_LOAD- (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /EXT_LOAD-))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:SOT-23_HS (layer B.Cu) (tedit 5C0C84E5)
    (at 129.54 139.192)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 0 -90) (layer B.SilkS))
    (fp_text value DMP2035U (at 0 -2.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 3 smd roundrect (at 1.2 0) (size 1.3 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 /VOUT1))
    (pad 2 smd roundrect (at -1.2 -0.95) (size 1.3 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 VIN))
    (pad 1 smd roundrect (at -1.2 0.95) (size 1.3 0.8) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:SOT-23_HS (layer F.Cu) (tedit 5C0C84E5)
    (at 129.54 137.668)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 0 90) (layer F.SilkS))
    (fp_text value NTR3C21NZ (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.2 -0.95) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at -1.2 0.95) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 3 smd roundrect (at 1.2 0) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /EXT_LOAD-))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 142.748 136.398 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 0) (layer F.SilkS))
    (fp_text value 3.3k (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /~RESET))
    (pad 1 smd roundrect (at -1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 UPDI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer B.Cu) (tedit 5C0C83D5)
    (at 129.413 135.255)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 0 -90) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.15 0) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 VOUT1-~EN))
    (pad 1 smd roundrect (at -1.15 0) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:1206_HS (layer B.Cu) (tedit 5C0C843B)
    (at 125.73 137.16 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 0 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.95 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.65 0 270) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 VOUT1-~EN))
    (pad 2 smd roundrect (at 1.65 0 270) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer B.Cu) (tedit 5C0C83D5)
    (at 149.86 135.636 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 VIN))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer B.Cu) (tedit 5C0C83D5)
    (at 152.4 135.636 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /SDA))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 VIN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:1206_HS (layer B.Cu) (tedit 5C0C843B)
    (at 137.3505 137.668 90)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 0) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.95 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.65 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.65 0 90) (size 1.3 1.7) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 126.365 137.795 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(Q2-Pad1)"))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 VEXT-EN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 124.46 137.795 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 VEXT-EN))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5923F252)
    (at 133.604 135.255)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 3.81 2.413) (layer F.SilkS))
    (fp_text value SW_SPST (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 /~RESET))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(R7-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 /~RESET))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5C120D3F)
    (at 137.16 132.08 270)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value UPDI (at 0 2.54 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.54 90) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 270) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 UPDI))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C120D3C)
    (at 139.7 132.08 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -2.032 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 14.986 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /SCK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /MISO))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /MOSI))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /SCL))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5C120CDB)
    (at 124.46 132.08 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value GND (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.54 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.651) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "rev 1" (at 147.447 137.668) (layer B.SilkS))
  (gr_text GND (at 126.111 144.272) (layer B.SilkS))
  (gr_text VIN (at 126.238 142.24) (layer B.SilkS))
  (gr_text GND (at 134.874 143.002) (layer B.SilkS))
  (gr_text VOUT1 (at 131.699 143.002) (layer B.SilkS))
  (gr_text "CC BY-SA 4.0" (at 145.161 136.525) (layer B.SilkS))
  (gr_text Belous (at 143.51 135.382) (layer B.SilkS))
  (gr_text Vlad (at 146.304 135.382) (layer B.SilkS))
  (gr_text © (at 148.082 135.382) (layer B.SilkS))
  (gr_text UPDI (at 137.033 133.858) (layer B.SilkS))
  (gr_text PB1 (at 152.273 138.43) (layer B.SilkS))
  (gr_text PB0 (at 149.86 138.43) (layer B.SilkS))
  (gr_text PA1 (at 147.32 133.858) (layer B.SilkS))
  (gr_text PA2 (at 144.78 133.858) (layer B.SilkS))
  (gr_text PA3 (at 142.24 133.858) (layer B.SilkS))
  (gr_text GND (at 139.7 133.731) (layer B.SilkS))
  (gr_text TXD (at 149.86 141.986) (layer B.SilkS))
  (gr_text RXD (at 147.32 141.986) (layer B.SilkS))
  (gr_text GND (at 152.273 143.002) (layer B.SilkS))
  (gr_text PB2 (at 149.86 143.002) (layer B.SilkS))
  (gr_text PB3 (at 147.32 143.002) (layer B.SilkS))
  (gr_text PA7 (at 144.78 143.002) (layer B.SilkS))
  (gr_text PA6 (at 142.24 143.002) (layer B.SilkS))
  (gr_text VIN (at 139.573 143.002) (layer B.SilkS))
  (gr_text GND (at 135.128 143.002) (layer F.SilkS))
  (gr_text VOUT1 (at 131.953 143.002) (layer F.SilkS))
  (gr_text VIN (at 139.7 143.002) (layer F.SilkS))
  (gr_text PA6 (at 142.24 143.002) (layer F.SilkS))
  (gr_text PA7 (at 144.78 143.002) (layer F.SilkS))
  (gr_text RXD (at 147.32 143.002) (layer F.SilkS))
  (gr_text TXD (at 149.86 143.002) (layer F.SilkS))
  (gr_text GND (at 152.4 143.002) (layer F.SilkS))
  (gr_text SDA (at 152.4 133.858) (layer F.SilkS))
  (gr_text SCL (at 149.86 133.858) (layer F.SilkS))
  (gr_text MOSI (at 147.32 133.858) (layer F.SilkS))
  (gr_text MISO (at 144.78 133.858) (layer F.SilkS))
  (gr_text SCK (at 142.367 133.858) (layer F.SilkS))
  (gr_text GND (at 139.7 133.858) (layer F.SilkS))
  (gr_text UPDI (at 135.382 132.334 90) (layer F.SilkS))
  (gr_text L- (at 131.953 133.731) (layer B.SilkS))
  (gr_text L+ (at 129.667 133.731) (layer B.SilkS))
  (gr_text VEXT (at 127.254 133.858) (layer B.SilkS))
  (gr_text GND (at 124.46 133.858) (layer B.SilkS))
  (gr_text attiny1614 (at 148.59 138.557) (layer F.SilkS))
  (dimension 15.24 (width 0.1778) (layer Cmts.User)
    (gr_text "0.6000 in" (at 161.3916 138.43 90) (layer Cmts.User))
    (feature1 (pts (xy 158.75 130.81) (xy 160.606421 130.81)))
    (feature2 (pts (xy 158.75 146.05) (xy 160.606421 146.05)))
    (crossbar (pts (xy 160.02 146.05) (xy 160.02 130.81)))
    (arrow1a (pts (xy 160.02 130.81) (xy 160.606421 131.936504)))
    (arrow1b (pts (xy 160.02 130.81) (xy 159.433579 131.936504)))
    (arrow2a (pts (xy 160.02 146.05) (xy 160.606421 144.923496)))
    (arrow2b (pts (xy 160.02 146.05) (xy 159.433579 144.923496)))
  )
  (dimension 30.48 (width 0.1778) (layer Cmts.User)
    (gr_text "1.2000 in" (at 138.43 152.5016) (layer Cmts.User))
    (feature1 (pts (xy 153.67 149.86) (xy 153.67 151.716421)))
    (feature2 (pts (xy 123.19 149.86) (xy 123.19 151.716421)))
    (crossbar (pts (xy 123.19 151.13) (xy 153.67 151.13)))
    (arrow1a (pts (xy 153.67 151.13) (xy 152.543496 151.716421)))
    (arrow1b (pts (xy 153.67 151.13) (xy 152.543496 150.543579)))
    (arrow2a (pts (xy 123.19 151.13) (xy 124.316504 151.716421)))
    (arrow2b (pts (xy 123.19 151.13) (xy 124.316504 150.543579)))
  )
  (gr_line (start 123.19 130.81) (end 153.67 130.81) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 123.19 146.05) (end 123.19 130.81) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 153.67 146.05) (end 123.19 146.05) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 153.67 130.81) (end 153.67 146.05) (layer Edge.Cuts) (width 0.0254))
  (dimension 33.02 (width 0.1778) (layer F.SilkS)
    (gr_text "1.3000 in" (at 137.16 158.8516) (layer F.SilkS))
    (feature1 (pts (xy 120.65 156.21) (xy 120.65 158.066421)))
    (feature2 (pts (xy 153.67 156.21) (xy 153.67 158.066421)))
    (crossbar (pts (xy 153.67 157.48) (xy 120.65 157.48)))
    (arrow1a (pts (xy 120.65 157.48) (xy 121.776504 156.893579)))
    (arrow1b (pts (xy 120.65 157.48) (xy 121.776504 158.066421)))
    (arrow2a (pts (xy 153.67 157.48) (xy 152.543496 156.893579)))
    (arrow2b (pts (xy 153.67 157.48) (xy 152.543496 158.066421)))
  )
  (dimension 17.78 (width 0.1778) (layer F.SilkS)
    (gr_text "0.7000 in" (at 166.4716 137.16 90) (layer F.SilkS))
    (feature1 (pts (xy 163.83 128.27) (xy 165.686421 128.27)))
    (feature2 (pts (xy 163.83 146.05) (xy 165.686421 146.05)))
    (crossbar (pts (xy 165.1 146.05) (xy 165.1 128.27)))
    (arrow1a (pts (xy 165.1 128.27) (xy 165.686421 129.396504)))
    (arrow1b (pts (xy 165.1 128.27) (xy 164.513579 129.396504)))
    (arrow2a (pts (xy 165.1 146.05) (xy 165.686421 144.923496)))
    (arrow2b (pts (xy 165.1 146.05) (xy 164.513579 144.923496)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.3048)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.92 129.54) (xy 154.94 129.54) (xy 154.94 147.32) (xy 121.92 147.32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0) (thermal_bridge_width 0))
    (polygon
      (pts
        (xy 125.6538 132.715) (xy 126.0602 133.1214) (xy 126.3396 133.1214) (xy 125.857 132.6388)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.3048)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.7922 132.6896) (xy 140.9446 132.842) (xy 141.3256 132.9944) (xy 141.1478 132.6388)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3556))
    (min_thickness 0.3048)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.2098 143.4084) (xy 129.7432 142.7226) (xy 129.1336 143.1544)
      )
    )
  )
)
