<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="105.7275" y2="0" width="0.1524" layer="20"/>
<wire x1="105.7275" y1="0" x2="105.7275" y2="12.7" width="0.1524" layer="20"/>
<wire x1="105.7275" y1="12.7" x2="99.568" y2="12.7" width="0.1524" layer="20"/>
<wire x1="99.568" y1="12.7" x2="95.631" y2="8.89" width="0.1524" layer="20"/>
<wire x1="95.631" y1="8.89" x2="10.16" y2="8.89" width="0.1524" layer="20"/>
<wire x1="10.16" y1="8.89" x2="6.35" y2="12.7" width="0.1524" layer="20"/>
<wire x1="6.35" y1="12.7" x2="0" y2="12.7" width="0.1524" layer="20"/>
<wire x1="0" y1="12.7" x2="0" y2="0" width="0.1524" layer="20"/>
<text>RV-Project.Com LED Halo Light Board B
V1.2     2/9/2019</text>
<text>A</text>
<text>A</text>
<text>C</text>
<text>C</text>
<text>Side C</text>
<text>Side D</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="PAD-1.5X4.5">
</package>
<package name="LED-1206">
</package>
<package name="1206-RES">
</package>
<package name="1X01_HEADER">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="a-lib" package="PAD-1.5X4.5" value=""/>
<element name="JP2" library="a-lib" package="PAD-1.5X4.5" value=""/>
<element name="JP3" library="a-lib" package="PAD-1.5X4.5" value=""/>
<element name="JP4" library="a-lib" package="PAD-1.5X4.5" value=""/>
<element name="LED1" library="a-lib" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="a-lib" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="a-lib" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="a-lib" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="P$1"/>
<contactref element="JP4" pad="P$1"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="P$1"/>
<contactref element="JP3" pad="P$1"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R4" pad="1"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
