(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1~bpo10+1)
  (general
    (thickness 1.6)
    (drawings 24)
    (tracks 0)
    (zones 0)
    (modules 0)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (gr_text "York Modular 2021" (at 99.25 100 90) (layer B.SilkS))
  (gr_text VC2 (at 104.75 51.25) (layer F.Mask))
  (gr_text VC2 (at 104.75 51.25) (layer F.Cu))
  (gr_text I/O (at 99 119.5 90) (layer F.Mask))
  (gr_text I/O (at 99 142.5 90) (layer F.Mask))
  (gr_text SWITCH (at 99 79.5 90) (layer F.Mask))
  (gr_text I/O (at 99 62.25 90) (layer F.Mask))
  (gr_text I/O (at 99 142.5 90) (layer F.Cu))
  (gr_text I/O (at 99 119.5 90) (layer F.Cu))
  (gr_text SWITCH (at 99 79.5 90) (layer F.Cu))
  (gr_text I/O (at 99 62.25 90) (layer F.Cu))
  (gr_circle (center 104.75 167.805) (end 106.25 167.805) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 104.75 45.305) (end 106.25 45.305) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.25 42.405) (end 112.15 42.405) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 109.25 90.98) (end 111 90.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.15 42.405) (end 112.15 170.805) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 109.25 130.98) (end 111 130.98) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 105.75 62.23) (end 108.75 62.23) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.25 170.805) (end 97.25 42.405) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 105.75 142.48) (end 108.75 142.48) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 105.75 119.48) (end 108.75 119.48) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.15 170.805) (end 97.25 170.805) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 105.75 79.73) (end 108.75 79.73) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 109.25 153.75) (end 111 153.75) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114 175) (xy 93.75 172.75) (xy 95.75 41) (xy 113.25 41)
      )
    )
  )
)
