(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "Polyimide") (epsilon_r 3.2) (loss_tangent 0.004))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
      (edge_connector yes)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers-only-lower-20220926/")
    )
  )
  (net 0 "")
  (net 1 "Net-(GND1-Pad1)")
  (net 2 "Net-(JCONN2-Pad15)")
  (net 3 "Net-(HPL1-Pad1)")
  (net 4 "Net-(JCONN2-Pad5)")
  (net 5 "Net-(HPR1-Pad1)")
  (net 6 "Net-(JCONN2-Pad3)")
  (net 7 "Net-(HPSW1-Pad1)")
  (net 8 "Net-(JCONN2-Pad4)")
  (net 9 "Net-(JCONN1-Pad1)")
  (net 10 "Net-(JCONN1-Pad2)")
  (net 11 "Net-(JCONN1-Pad6)")
  (net 12 "Net-(JCONN1-Pad7)")
  (net 13 "Net-(JCONN1-Pad8)")
  (net 14 "Net-(JCONN1-Pad14)")
  (net 15 "Net-(JCONN2-Pad1)")
  (net 16 "Net-(JCONN2-Pad2)")
  (net 17 "Net-(JCONN2-Pad6)")
  (net 18 "Net-(JCONN2-Pad7)")
  (net 19 "Net-(JCONN2-Pad8)")
  (net 20 "Net-(JCONN2-Pad9)")
  (net 21 "Net-(JCONN2-Pad10)")
  (net 22 "Net-(JCONN2-Pad11)")
  (net 23 "Net-(JCONN2-Pad12)")
  (net 24 "Net-(JCONN2-Pad13)")
  (net 25 "Net-(JCONN1-Pad9)")
  (net 26 "Net-(JCONN1-Pad10)")
  (net 27 "Net-(JCONN1-Pad11)")
  (net 28 "Net-(JCONN1-Pad12)")
  (net 29 "Net-(JCONN1-Pad13)")
  (net 30 "Net-(JCONN2-Pad14)")
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" locked (layer "F.Cu")
    (tedit 5A0F774F)
    (at 75 94.25)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "VCC2" (at -2.5 -0.5) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle locked (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(JCONN2-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 25.25 69.75)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "VCC1" (at 0 3 90) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(JCONN1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 27.75 68.25)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "SW-VCC1" (at 0 4 90) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(JCONN1-Pad2)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 35.8 68.8)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "HPR1" (at -1.55 -1.05 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 7.4 -5.4 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.4 -3.9 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "Net-(HPR1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 49 99.6)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P112" (at 2 -0.1 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 20 "Net-(JCONN2-Pad9)") (pinfunction "1") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 73 96)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "SW-VCC2" (at -3.75 -0.75 180) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 16 "Net-(JCONN2-Pad2)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 77.2 72.3)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P10" (at -1.95 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -9.2 -5.3 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -4.2 -3.8 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 26 "Net-(JCONN1-Pad10)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 49.4 96.7)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P122" (at 2.1 0.3 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 22 "Net-(JCONN2-Pad11)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:ground solder" (layer "F.Cu")
    (tedit 0)
    (at 30.712132 77.462132 45)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "GND1" (at 0 -1.414214 45 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 45 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 45 unlocked) (layer "F.Fab"))
    (pad "1" connect custom (at 0 -0.3 45) (size 0.456 0.456) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(GND1-Pad1)") (pinfunction "1") (pintype "input")
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1.25 0)
            (xy 1.25 0.55)
            (xy 0.75 0.55)
            (xy 0.5 0.2)
            (xy -0.3 0.2)
            (xy -0.6 0.55)
            (xy -1 0.55)
            (xy -1 0)
            (xy -0.5 -0.45)
            (xy 0.75 -0.45)
          ) (width 0.1) (fill yes))
      ))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 62.8 105.1)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "HPL2" (at -2.05 0.15 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(JCONN2-Pad5)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 83 72)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "VDD1" (at 0 2 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 9 0 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.5 1.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 29 "Net-(JCONN1-Pad13)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 33.8 68.8)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "HPSW1" (at -2.3 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -5.3 -5.1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.3 -3.6 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(HPSW1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 78.4 74.6)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P13" (at 1.85 -0.1 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 8.55 2.85 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.6 4.4 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 13 "Net-(JCONN1-Pad8)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 78.4 76.1)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P15" (at 1.85 -0.1 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -10.9 6.9 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.9 5.4 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 12 "Net-(JCONN1-Pad7)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 62.8 106.8)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "HPR2" (at -2.05 0.2 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(JCONN2-Pad3)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 50.1 101.4)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P132" (at 2.15 0.1 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 19 "Net-(JCONN2-Pad8)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 84.5 81)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "VEE1" (at -0.75 -1.75 -45 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 8.95 1.45 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12 3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 14 "Net-(JCONN1-Pad14)") (pinfunction "1") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 66.25 100.5)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "HPSW2" (at -2.25 -1.75 180) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 8 "Net-(JCONN2-Pad4)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 50 87.6)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P152" (at 0 2.4 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 18 "Net-(JCONN2-Pad7)") (pinfunction "1") (pintype "input"))
  )
  (footprint "Connector_FFC-FPC:Hirose_FH12-15S-0.5SH_1x15-1MP_P0.50mm_Horizontal" (layer "F.Cu")
    (tedit 5D24667B)
    (at 69.5 89.95 180)
    (descr "Hirose FH12, FFC/FPC connector, FH12-15S-0.5SH, 15 Pins per row (https://www.hirose.com/product/en/products/FH12/FH12-24S-0.5SH(55)/), generated with kicad-footprint-generator")
    (tags "connector Hirose FH12 horizontal")
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "JCONN2" (at -7.25 3.95) (layer "F.SilkS"))
    (fp_text value "Conn_01x15_Female" (at 0 5.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.7) (layer "F.Fab"))
    (pad "1" smd rect (at -3.5 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(JCONN2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at -3 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(JCONN2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -2.5 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(JCONN2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at -2 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(JCONN2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -1.5 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(JCONN2-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at -1 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(JCONN2-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at -0.5 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(JCONN2-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 0 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(JCONN2-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at 0.5 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(JCONN2-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 1 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(JCONN2-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at 1.5 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(JCONN2-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 2 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(JCONN2-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at 2.5 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(JCONN2-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 3 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(JCONN2-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at 3.5 -1.85 180) (size 0.3 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(JCONN2-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "MP" smd rect (at -5.4 1.4 180) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "MP" smd rect (at 5.4 1.4 180) (size 1.8 2.2) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/Hirose_FH12-15S-0.5SH_1x15-1MP_P0.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 77.2 75.3)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P14" (at -1.95 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 28 "Net-(JCONN1-Pad12)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:0.5 pitch edge" (layer "F.Cu")
    (tedit 0)
    (at 26.5 161.25 90)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "JCONN1" (at 9.25 3.35 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x15_Male" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" connect rect (at 7.25 0 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(JCONN1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" connect rect (at 7.25 0.5 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(JCONN1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" connect rect (at 7.25 1 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(HPR1-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" connect rect (at 7.25 1.5 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(HPSW1-Pad1)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" connect rect (at 7.25 2 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(HPL1-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" connect rect (at 7.25 2.5 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 11 "Net-(JCONN1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" connect rect (at 7.25 3 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 12 "Net-(JCONN1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" connect rect (at 7.25 3.5 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 13 "Net-(JCONN1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" connect rect (at 7.25 4 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 25 "Net-(JCONN1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" connect rect (at 7.25 4.5 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 26 "Net-(JCONN1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" connect rect (at 7.25 5 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 27 "Net-(JCONN1-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" connect rect (at 7.25 5.5 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 28 "Net-(JCONN1-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" connect rect (at 7.25 6 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 29 "Net-(JCONN1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" connect rect (at 7.25 6.5 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 14 "Net-(JCONN1-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" connect rect (at 7.25 7 90) (size 2.5 0.4) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(GND1-Pad1)") (pinfunction "Pin_15") (pintype "passive"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 77.2 73.8)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P12" (at -1.95 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -9.2 -2.3 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -4.2 -0.8 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 27 "Net-(JCONN1-Pad11)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 55.2 107.8)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "VEE2" (at -1.95 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 30 "Net-(JCONN2-Pad14)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 78.4 73.1)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P11" (at 1.85 -0.1 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 5.1 -5.1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.1 -3.6 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 "Net-(JCONN1-Pad9)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 57.8 92.5)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "GND2" (at 1.95 -0.05 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(JCONN2-Pad15)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 62 87.6)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P142" (at 0.25 2.4 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 23 "Net-(JCONN2-Pad12)") (pinfunction "1") (pintype "input"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 67.5 97.5)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "SPKR2" (at -3 -1 180) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 17 "Net-(JCONN2-Pad6)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 35.8 70.6)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "HPL1" (at -1.8 -0.6 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(HPL1-Pad1)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" (layer "F.Cu")
    (tedit 0)
    (at 37.5 69.6)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SPKR1" (at 0 2.4 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at 8.5 -0.8 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.5 0.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(JCONN1-Pad6)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 48.6 101.5)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P102" (at -1.1 -1.25 90 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 21 "Net-(JCONN2-Pad10)") (pinfunction "1") (pintype "input"))
  )
  (footprint "some-stuff:solder-to-via" locked (layer "F.Cu")
    (tedit 0)
    (at 82 86.6)
    (property "Sheetfile" "boards.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "VDD2" (at -1.5 -0.85 unlocked) (layer "F.SilkS"))
    (fp_text value "MountingHole_Pad" (at -8.4 0.75 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.35 2.3 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 24 "Net-(JCONN2-Pad13)") (pinfunction "1") (pintype "input"))
  )
  (gr_line (start 85 82.25) (end 84 82.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 75.75 70) (end 80 70) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 83 86) (end 83 87) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 26 148.6) (end 26 155.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 51 105) (end 51 103.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 49.5 86.5) (end 50.55 86.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 64.75 105.75) (end 64.75 106) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 36.25 66.75) (end 38.75 69.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 79.75 78) (end 37 78) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 81.35 87.4) (end 82.6 87.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 36.75 85) (end 36.9 85.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 82.6 87.4) (end 83 87) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 84 82.25) (end 79.75 78) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 51 105) (end 51 110) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 30.6 77.695) (end 31.1 77.3) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 61.4 91) (end 61.4 86.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 26 155.4) (end 34 155.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 38.75 69.25) (end 38.75 72.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 31.39 77.41) (end 32.75 76) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 39.5 73) (end 38.75 72.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 30.6 78.2) (end 30.6 77.695) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 63.25 107.75) (end 64 107) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 72.1 97.4) (end 73.8 97.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 29.1 145.5) (end 26 148.6) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 72.1 97.4) (end 64.75 104.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 32.75 76) (end 35 76) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 23.75 69.25) (end 26.25 66.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 23.75 69.25) (end 23.75 69.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 35 83.25) (end 36.75 85) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 76.5 87.7) (end 76.5 94.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 39.5 73) (end 72.75 73) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 50.55 86.5) (end 50.55 91) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 52.75 111.75) (end 57.25 111.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 23.75 71.5) (end 23.75 69.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 81.35 87.4) (end 80.65 86.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 29.1 145.5) (end 29.1 87.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 30.25 78.6) (end 30.6 78.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 46.75 96.5) (end 49 94.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 51 110) (end 52.75 111.75) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 59.987259 100.6) (end 58.387259 99) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_line (start 30.25 78.6) (end 30.25 79.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 62.5 85) (end 61.4 86.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 80.65 86.7) (end 77.5 86.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 61.25 107.75) (end 63.25 107.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 22.25 73.25) (end 23.75 71.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 76.5 94.9) (end 74 97.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 34 148.9) (end 34 155.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 46.75 102) (end 46.75 96.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 57.25 111.75) (end 61.25 107.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 29 86.875) (end 29.1 87.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 30.75 80.25) (end 30.25 79.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 64.75 106) (end 64 106.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 84.25 78.75) (end 85.75 80.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 83.5 70.75) (end 84.25 71.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 49 94.25) (end 49 88.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 33.25 81.5) (end 35 83.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 26.25 66.75) (end 36.25 66.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line locked (start 22.25 80.125) (end 29 86.875) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 47.75 103) (end 46.75 102) (layer "Edge.Cuts") (width 0.1))
  (gr_line locked (start 36.9 146) (end 34 148.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 33.25 81.5) (end 32 80.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 64 106.75) (end 64 107) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 64.75 104.75) (end 64.75 105.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 22.25 73.25) (end 22.25 80.125) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 49 87) (end 49.5 86.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 85.75 80.25) (end 85.75 81.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 72.75 73) (end 75.75 70) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 49 88.5) (end 49 87) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 50.55 91) (end 61.4 91) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 50.25 103) (end 51 103.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 50.25 103) (end 47.75 103) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 74 97.4) (end 73.8 97.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 36.9 146) (end 36.9 85.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 32 80.25) (end 30.75 80.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 80.75 70.75) (end 83.5 70.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 35 76) (end 37 78) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 76.5 87.7) (end 77.5 86.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 31.1 77.3) (end 31.39 77.41) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 82 85) (end 83 86) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 80 70) (end 80.75 70.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 85.75 81.5) (end 85 82.25) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 84.25 71.5) (end 84.25 78.75) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 62.5 85) (end 82 85) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 23.75 71.75) (end 23.75 71.5) (layer "Edge.Cuts") (width 0.1))
  (gr_text "MGB-SP v0.2\nAllison Parrish\nwww.decontextualize.com" (at 49.5 94) (layer "F.SilkS"))
)
