(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 14)
    (no_connects 0)
    (area 133.286499 85.026499 155.003501 102.933501)
    (thickness 1.6)
    (drawings 47)
    (tracks 27)
    (zones 0)
    (modules 11)
    (nets 7)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 2 2)
    (pad_drill 1)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(A1-Pad2)")
  (net 4 "Net-(A2-Pad2)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(R3-Pad2)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.3)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A2-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net VCC)
  )
  (module BRICE:DS18B20 placed (layer Top) (tedit 590B66B4)
    (at 135.89 90.17 90)
    (fp_text reference "SWITCH A" (at -0.254 -1.524 270) (layer F.SilkS))
    (fp_text value SWITCH-A (at 0 -4.826 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad2)"))
  )
  (module BRICE:DS18B20 placed (layer Top) (tedit 590DED59)
    (at 135.89 97.79 90)
    (fp_text reference "SWITCH B" (at 0.254 -1.524 90) (layer F.SilkS))
    (fp_text value SWITCH-B (at -0.508 -4.826 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(A2-Pad2)"))
  )
  (module BRICE:Power_Pad_2x_1mmDrill (layer Top) (tedit 590DEDC8)
    (at 152.4 88.646 270)
    (fp_text reference 5VCC (at 0.254 -1.524 270) (layer F.SilkS))
    (fp_text value Power (at 0 -5.08 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.524 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -1.016 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module BRICE:Power_Pad_2x_1mmDrill (layer Top) (tedit 590DEF9F)
    (at 152.4 96.52 90)
    (fp_text reference VIA (at 0 1.524 90) (layer F.SilkS))
    (fp_text value Power (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer Top) (tedit 590DEDFA)
    (at 152.4 95.25)
    (fp_text reference pb0 (at -1.524 0 90) (layer F.SilkS))
    (fp_text value pb0 (at 4.572 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad2)"))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer Top) (tedit 590DEDE9)
    (at 152.4 92.71 270)
    (fp_text reference pb1 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value pb1 (at 4.572 -0.254 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(R3-Pad2)"))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer Top) (tedit 590E1564)
    (at 138.938 88.392)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R1 1 Mohm" (at 5.08 0) (layer F.SilkS))
    (fp_text value R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer Top) (tedit 590E157B)
    (at 138.938 92.202)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R2 1 MOhm" (at 5.08 0) (layer F.SilkS))
    (fp_text value R (at 2.794 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer Top) (tedit 590E158F)
    (at 138.938 96.266)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R3 1 MOhm" (at 5.08 0) (layer F.SilkS))
    (fp_text value R (at 2.794 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A2-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(R3-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer Top) (tedit 590E15A5)
    (at 138.938 100.076)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference "R4 1 MOhm" (at 5.08 0) (layer F.SilkS))
    (fp_text value R (at 2.794 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A2-Pad2)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 143.51 97.536 270)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (gr_line (start 133.35 87.63) (end 133.35 100.33) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 135.89 85.09) (end 152.4 85.09) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 152.4 102.87) (end 135.89 102.87) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 154.94 100.33) (end 154.94 87.63) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text "DESIGN IN FRENCH" (at 146.304 90.678 90) (layer B.SilkS))
  (gr_text + (at 150.876 97.79) (layer F.SilkS))
  (gr_text - (at 150.876 100.33 90) (layer F.SilkS))
  (gr_text https://easydomoticz.com (at 144.018 101.6 180) (layer B.SilkS))
  (gr_arc (start 152.4 87.63) (end 152.4 85.09) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 152.4 100.33) (end 154.94 100.33) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 135.89 87.63) (end 133.35 87.63) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 135.89 100.33) (end 135.89 102.87) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text 2017 (at 140.462 90.17 90) (layer B.SilkS))
  (gr_text + (at 150.876 90.17) (layer F.SilkS))
  (gr_text - (at 150.876 87.63 90) (layer F.SilkS))
  (gr_text pb0 (at 137.414 90.17 90) (layer F.SilkS))
  (gr_text GND (at 137.414 92.71 90) (layer F.SilkS))
  (gr_text VCC (at 137.414 87.63 90) (layer F.SilkS))
  (gr_text "ZIONIII \nEXTENSION\nSONDE B V2.1" (at 143.764 90.932 90) (layer B.SilkS))
  (gr_text pb1 (at 137.414 97.79 90) (layer F.SilkS))
  (gr_text VCC (at 137.414 95.25 90) (layer F.SilkS))
  (gr_text GND (at 137.414 100.33 90) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 85.09) (xy 154.94 85.09) (xy 154.94 102.87) (xy 133.35 102.87)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 85.09) (xy 154.94 85.09) (xy 154.94 102.87) (xy 133.35 102.87)
      )
    )
  )
)
