(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 48)
    (tracks 233)
    (zones 0)
    (modules 23)
    (nets 37)
  )
  (page A4)
  (title_block
    (title "DMX Demonstrator - Frame Scrambler (DMX-FS1)")
    (date 2023-12-24)
    (rev 1.1)
    (company "Sparky Bobo Designs")
    (comment 2 "Designed by: SparkyBobo")
    (comment 3 "https://creativecommons.org/licenses/by-sa/4.0/ ")
    (comment 4 "Released under the Creative Commons Attribution Share-Alike 4.0 License")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "grb/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /A1)
  (net 3 GND)
  (net 4 "Net-(D6-Pad2)")
  (net 5 "Net-(D5-Pad2)")
  (net 6 "Net-(D4-Pad2)")
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D2-Pad2)")
  (net 9 "Net-(D3-Pad2)")
  (net 10 "Net-(A1-Pad32)")
  (net 11 "Net-(A1-Pad31)")
  (net 12 "Net-(A1-Pad1)")
  (net 13 "Net-(A1-Pad2)")
  (net 14 "Net-(A1-Pad3)")
  (net 15 "Net-(A1-Pad4)")
  (net 16 "Net-(A1-Pad8)")
  (net 17 "Net-(A1-Pad25)")
  (net 18 /A2)
  (net 19 /A4)
  (net 20 "Net-(A1-Pad15)")
  (net 21 "Net-(A1-Pad16)")
  (net 22 /A5)
  (net 23 /RX)
  (net 24 /RXCLK)
  (net 25 "Net-(A1-Pad30)")
  (net 26 "Net-(A1-Pad9)")
  (net 27 /~DATA_RX)
  (net 28 /~DATA_TX)
  (net 29 /TX)
  (net 30 /TXCLK)
  (net 31 /A3)
  (net 32 /~CLK_RX)
  (net 33 /~CLK_TX)
  (net 34 /~SCRAM)
  (net 35 /~EN)
  (net 36 /EN)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /EN)
    (add_net /RX)
    (add_net /RXCLK)
    (add_net /TX)
    (add_net /TXCLK)
    (add_net /~CLK_RX)
    (add_net /~CLK_TX)
    (add_net /~DATA_RX)
    (add_net /~DATA_TX)
    (add_net /~EN)
    (add_net /~SCRAM)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(A1-Pad31)")
    (add_net "Net-(A1-Pad32)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 1.27)
    (via_drill 0.635)
    (uvia_dia 1.27)
    (uvia_drill 0.635)
    (diff_pair_width 0.3048)
    (diff_pair_gap 0.3048)
    (add_net +5V)
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 133.7945 69.342 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 4.8895 0) (layer F.SilkS))
    (fp_text value 330 (at 5.08 2.37 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad25)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels (layer F.Cu) (tedit 656EBC42)
    (at 159.385 74.9935)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8) (layer F.SilkS))
    (fp_text value EN/RX (at 0 1.9) (layer F.Fab))
    (fp_text user 3 (at 2.6 0) (layer F.SilkS) hide)
    (fp_text user 1 (at -2.6 0) (layer F.SilkS) hide)
    (pad 1 smd custom (at -1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 31 /A3) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
        (gr_poly (pts
           (xy 0.4 -0.3) (xy 0.9 -0.3) (xy 0.9 0.3) (xy 0.4 0.3)) (width 0))
      ))
    (pad 3 smd custom (at 1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 23 /RX) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 36 /EN))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 170.8785 70.612)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 2.794 2.667 90) (layer F.SilkS))
    (fp_text value Display (at 4.385 7.35) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /A4))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /EN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 144.907 92.329 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -1.778 180) (layer F.SilkS))
    (fp_text value DIM1 (at 1.27 3.96 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 /~EN))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 138.303 87.3125)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 5.08 -0.0635) (layer F.SilkS))
    (fp_text value 330 (at 5.08 2.37) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 173.482 103.886)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 2.794 2.6035 270) (layer F.SilkS))
    (fp_text value Output (at 4.385 7.35) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /RXCLK))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:ARDUINO_R3_NO_HOLES (layer F.Cu) (tedit 5FA36CC6)
    (at 150.622 89.916)
    (descr "ARDUINO UNO R3 FOOTPRINT")
    (tags "ARDUINO UNO R3 FOOTPRINT")
    (attr virtual)
    (fp_text reference A1 (at -32.766 -25.908) (layer F.SilkS) hide)
    (fp_text value Arduino_UNO_R3 (at -29.718 -24.892) (layer F.SilkS) hide)
    (fp_text user SCL (at -15.5194 -20.5232 90) (layer Dwgs.User))
    (fp_text user SDA (at -12.9794 -20.5232 90) (layer Dwgs.User))
    (fp_text user AREF (at -10.4394 -20.9296 90) (layer Dwgs.User))
    (fp_text user GND (at -7.8994 -20.5232 90) (layer Dwgs.User))
    (fp_text user D13 (at -5.3594 -20.5232 90) (layer Dwgs.User))
    (fp_text user D12 (at -2.8194 -20.5232 90) (layer Dwgs.User))
    (fp_text user D11 (at -0.2794 -20.5232 90) (layer Dwgs.User))
    (fp_text user D10 (at 2.2606 -20.5232 90) (layer Dwgs.User))
    (fp_text user D9 (at 4.79806 -20.1168 90) (layer Dwgs.User))
    (fp_text user D8 (at 7.3406 -20.1168 90) (layer Dwgs.User))
    (fp_text user D7 (at 11.4046 -20.1168 90) (layer Dwgs.User))
    (fp_text user D6 (at 13.9446 -20.1168 90) (layer Dwgs.User))
    (fp_text user D5 (at 16.4846 -20.1168 90) (layer Dwgs.User))
    (fp_text user D4 (at 19.0246 -20.1168 90) (layer Dwgs.User))
    (fp_text user D3 (at 21.5646 -20.1168 90) (layer Dwgs.User))
    (fp_text user D2 (at 24.1046 -20.1168 90) (layer Dwgs.User))
    (fp_text user D0/RXI (at 29.05506 -19.2024 90) (layer Dwgs.User))
    (fp_text user D1/TXO (at 26.5176 -19.2024 90) (layer Dwgs.User))
    (fp_text user !RESET! (at -1.6764 20.0152 90) (layer Dwgs.User))
    (fp_text user 3.3V (at 0.8636 21.2344 90) (layer Dwgs.User))
    (fp_text user 5V (at 3.4036 22.0472 90) (layer Dwgs.User))
    (fp_text user GND (at 5.9436 21.6408 90) (layer Dwgs.User))
    (fp_text user GND (at 8.4836 21.6408 90) (layer Dwgs.User))
    (fp_text user VIN (at 11.0236 21.6408 90) (layer Dwgs.User))
    (fp_text user A0 (at 16.1036 22.0472 90) (layer Dwgs.User))
    (fp_text user A1 (at 18.6436 22.0472 90) (layer Dwgs.User))
    (fp_text user A2 (at 21.1836 22.0472 90) (layer Dwgs.User))
    (fp_text user A3 (at 23.7236 22.0472 90) (layer Dwgs.User))
    (fp_text user A4 (at 26.2636 22.0472 90) (layer Dwgs.User))
    (fp_text user A5 (at 28.80106 22.0472 90) (layer Dwgs.User))
    (fp_text user IOREF (at -4.2164 20.828 90) (layer Dwgs.User))
    (pad 4 thru_hole circle (at 1.27 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad4)") (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 3.81 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 16.51 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad9)") (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 19.05 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /A1) (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 21.59 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /A2) (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 24.13 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /A3) (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 26.67 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 /A4) (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 29.21 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /A5) (solder_mask_margin 0.1016))
    (pad 30 thru_hole circle (at -10.414 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad30)") (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 29.21 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad15)") (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 26.67 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad16)") (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at 24.13 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /~DATA_RX) (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at 21.59 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /~CLK_RX) (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 19.05 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /~DATA_TX) (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 16.51 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /~CLK_TX) (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 13.97 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /~SCRAM) (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 11.43 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /~EN) (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 7.366 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /TX) (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at 4.826 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /TXCLK) (solder_mask_margin 0.1016))
    (pad 25 thru_hole circle (at 2.286 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad25)") (solder_mask_margin 0.1016))
    (pad 26 thru_hole circle (at -0.254 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad25)") (solder_mask_margin 0.1016))
    (pad 27 thru_hole circle (at -2.794 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 /RX) (solder_mask_margin 0.1016))
    (pad 28 thru_hole circle (at -5.334 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 /RXCLK) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 6.35 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 8.89 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 29 thru_hole circle (at -7.874 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -3.81 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -6.35 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad1)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -1.27 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad3)") (solder_mask_margin 0.1016))
    (pad 32 thru_hole circle (at -15.494 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad32)") (solder_mask_margin 0.1016))
    (pad 31 thru_hole circle (at -12.954 -24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad31)") (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 11.43 24.13) (size 1.9304 1.9304) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad8)") (solder_mask_margin 0.1016))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 154.1145 81.2165)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0) (layer F.SilkS))
    (fp_text value 330 (at 5.08 -0.508) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 154.1145 84.2645)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 5.08 0) (layer F.SilkS))
    (fp_text value 330 (at 5.08 0.635) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 154.1145 78.1685)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0) (layer F.SilkS))
    (fp_text value 330 (at 5.08 -0.508) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 154.1145 87.3125)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 5.08 0) (layer F.SilkS))
    (fp_text value 330 (at 5.08 0.635) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 138.303 84.2645)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 5.08 0) (layer F.SilkS))
    (fp_text value 330 (at 5.08 0.635) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Switches:TACTILE_SWITCH_PTH_12MM (layer F.Cu) (tedit 200000)
    (at 159.258 104.013)
    (descr "MOMENTARY SWITCH (PUSHBUTTON) - SPST - PTH, 12MM SQUARE")
    (tags "MOMENTARY SWITCH (PUSHBUTTON) - SPST - PTH, 12MM SQUARE")
    (attr virtual)
    (fp_text reference S2 (at 0 4.191) (layer F.SilkS))
    (fp_text value SCRAMBLE (at 0 5.08) (layer F.SilkS))
    (pad 1 thru_hole circle (at 6.2484 2.49936) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -6.2484 2.49936) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 6.2484 -2.49936) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (net 18 /A2) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -6.2484 -2.49936) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 182.245 96.52 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -1.778 180) (layer F.SilkS))
    (fp_text value DATA_OUT (at 1.27 3.96 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 /~DATA_RX))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Switches:TACTILE_SWITCH_PTH_12MM (layer F.Cu) (tedit 200000)
    (at 143.3576 104.013)
    (descr "MOMENTARY SWITCH (PUSHBUTTON) - SPST - PTH, 12MM SQUARE")
    (tags "MOMENTARY SWITCH (PUSHBUTTON) - SPST - PTH, 12MM SQUARE")
    (attr virtual)
    (fp_text reference S3 (at 0.0254 4.191) (layer F.SilkS))
    (fp_text value ENABLE (at 0 5.08) (layer F.SilkS))
    (pad 4 thru_hole circle (at -6.2484 -2.49936) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 6.2484 -2.49936) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (net 22 /A5) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -6.2484 2.49936) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 6.2484 2.49936) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
  )
  (module Switches:TACTILE_SWITCH_PTH_12MM (layer F.Cu) (tedit 200000)
    (at 143.4084 74.25436 180)
    (descr "MOMENTARY SWITCH (PUSHBUTTON) - SPST - PTH, 12MM SQUARE")
    (tags "MOMENTARY SWITCH (PUSHBUTTON) - SPST - PTH, 12MM SQUARE")
    (attr virtual)
    (fp_text reference S1 (at -0.0254 4.23164 180) (layer F.SilkS))
    (fp_text value CLEAR (at 0 5.12064 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 6.2484 2.49936 180) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -6.2484 2.49936 180) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 6.2484 -2.49936 180) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 /A1) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -6.2484 -2.49936 180) (size 2.159 2.159) (drill 1.19888) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 171.1325 96.4565)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 1.27 1.778) (layer F.SilkS))
    (fp_text value DATA_IN (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 /~DATA_TX))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 171.1325 83.5985)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D4 (at 1.27 1.778) (layer F.SilkS))
    (fp_text value CLOCK_IN (at 1.27 3.96) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 /~CLK_TX))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 160.909 92.329 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -1.778 180) (layer F.SilkS))
    (fp_text value DIM1 (at 1.27 3.96 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 /~SCRAM))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 129.54 108.966 180)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 2.794 2.54 90) (layer F.SilkS))
    (fp_text value Input (at 5.08 2.54 270) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /TX))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /TXCLK))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm (layer F.Cu) (tedit 5995936A)
    (at 182.245 83.662 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -1.778 180) (layer F.SilkS))
    (fp_text value CLOCK_OUT (at 1.27 3.96 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 /~CLK_RX))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:OSHW-LOGO-S locked (layer F.Cu) (tedit 200000)
    (at 119.126 114.3)
    (descr "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (tags "OPEN-SOURCE HARDWARE (OSHW) LOGO - SMALL - SILKSCREEN")
    (attr virtual)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
  )
  (module footprints:logo_cr_5x5 locked (layer B.Cu) (tedit 0)
    (at 120.142 109.474 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text RX (at 162.4965 75.057) (layer F.SilkS))
  (gr_text EN (at 156.1465 75.057) (layer F.SilkS))
  (gr_text Output (at 180.34 78.74) (layer F.SilkS))
  (gr_text Input (at 172.4025 78.74) (layer F.SilkS))
  (gr_text "E G S" (at 168.656 73.2155 90) (layer F.SilkS))
  (gr_text Display (at 166.116 73.2155 90) (layer F.SilkS))
  (gr_text Data (at 172.593 92.202) (layer F.SilkS))
  (gr_text Clock (at 172.593 87.884) (layer F.SilkS))
  (gr_text "C G D" (at 131.826 106.68 270) (layer F.SilkS))
  (gr_text Input (at 134.366 106.68 270) (layer F.SilkS))
  (gr_arc (start 181.61 115.824) (end 181.61 116.586) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 117.094 115.824) (end 116.332 115.824) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 117.094 64.008) (end 117.094 63.246) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.332 115.824) (end 116.332 64.008) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.61 116.586) (end 117.094 116.586) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 114.046) (end 182.372 115.824) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.912 111.506) (end 182.372 114.046) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.912 78.74) (end 184.912 111.506) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 76.2) (end 184.912 78.74) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.372 64.77) (end 182.372 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.848 63.246) (end 182.372 64.77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.094 63.246) (end 180.848 63.246) (layer Edge.Cuts) (width 0.15))
  (gr_text "DMX-FS1, Rev 1.1\nSparky Bobo Designs" (at 125.984 114.3) (layer B.SilkS))
  (gr_text DMX-FS1 (at 126.492 114.3) (layer F.SilkS))
  (gr_text Clock (at 180.975 87.884) (layer F.SilkS))
  (gr_text Output (at 168.656 106.426 90) (layer F.SilkS))
  (gr_text "Clear All" (at 143.383 81.788) (layer F.SilkS))
  (gr_text Scrambled (at 159.639 96.393) (layer F.SilkS))
  (gr_text Enabled (at 143.637 96.393) (layer F.SilkS))
  (gr_text Scramble (at 159.385 111.379) (layer F.SilkS))
  (gr_text Enable (at 143.383 111.379) (layer F.SilkS))
  (gr_text "D G C" (at 171.196 106.426 90) (layer F.SilkS))
  (gr_text Data (at 180.975 92.202) (layer F.SilkS))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.586 63.754) (xy 116.84 63.5) (xy 180.848 63.5) (xy 182.118 64.77) (xy 182.118 76.454)
        (xy 184.658 78.994) (xy 184.658 111.252) (xy 182.118 113.792) (xy 182.118 116.078) (xy 181.864 116.332)
        (xy 116.84 116.332) (xy 116.586 116.078)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.586 63.754) (xy 116.84 63.5) (xy 180.848 63.5) (xy 182.118 64.77) (xy 182.118 76.454)
        (xy 184.658 78.994) (xy 184.658 111.252) (xy 182.118 113.792) (xy 182.118 116.078) (xy 181.864 116.332)
        (xy 116.84 116.332) (xy 116.586 116.078)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.482 114.6175) (xy 176.022 114.681) (xy 176.022 116.3955) (xy 173.482 116.332)
      )
    )
  )
)
